From af0eabf8ee0d6e3a677f0f4e2e7339a44f635586 Mon Sep 17 00:00:00 2001
From: Tad <tad@spotco.us>
Date: Wed, 26 Oct 2016 21:26:42 -0400
Subject: [PATCH] Enable LTE

Change-Id: Ia918caa4bdde40807a24b157f8a825bfb501d351
---
 overlay/frameworks/base/core/res/res/values/config.xml          | 2 +-
 overlay/frameworks/base/packages/SystemUI/res/values/config.xml | 3 +++
 overlay/packages/services/Telephony/res/values/config.xml       | 3 +++
 3 files changed, 7 insertions(+), 1 deletion(-)

diff --git a/overlay/frameworks/base/core/res/res/values/config.xml b/overlay/frameworks/base/core/res/res/values/config.xml
index 7029fe9..807ad28 100644
--- a/overlay/frameworks/base/core/res/res/values/config.xml
+++ b/overlay/frameworks/base/core/res/res/values/config.xml
@@ -224,7 +224,7 @@
          Empty is viewed as "all".  Only used on devices which
          don't support RIL_REQUEST_GET_RADIO_CAPABILITY
          format is UMTS|LTE|... -->
-    <string translatable="false" name="config_radio_access_family">GSM | WCDMA | LTE</string>
+    <string translatable="false" name="config_radio_access_family">GPRS|EDGE|UMTS|HSDPA|HSUPA|HSPA|LTE|HSPAP|GSM|WCDMA</string>
 
     <!-- Set to true to add links to Cell Broadcast app from Settings and MMS app. -->
     <bool name="config_cellBroadcastAppLinks">true</bool>
diff --git a/overlay/frameworks/base/packages/SystemUI/res/values/config.xml b/overlay/frameworks/base/packages/SystemUI/res/values/config.xml
index f9febfe..e41fbaf 100644
--- a/overlay/frameworks/base/packages/SystemUI/res/values/config.xml
+++ b/overlay/frameworks/base/packages/SystemUI/res/values/config.xml
@@ -40,5 +40,8 @@
 
     <!-- Doze: shake accelerometer threshold -->
     <integer name="doze_shake_accelerometer_threshold">10</integer>
+
+    <!-- Show enabled lte option for lte device -->
+    <bool name="config_enabled_lte" translatable="false">true</bool>
 </resources>
 
diff --git a/overlay/packages/services/Telephony/res/values/config.xml b/overlay/packages/services/Telephony/res/values/config.xml
index af352a4..22c65ea 100644
--- a/overlay/packages/services/Telephony/res/values/config.xml
+++ b/overlay/packages/services/Telephony/res/values/config.xml
@@ -21,4 +21,7 @@
          are routed through the android.media.AudioManager class (true) or through
          the com.android.internal.telephony.Phone interface (false). -->
     <bool name="send_mic_mute_to_AudioManager">true</bool>
+
+    <!-- Show enabled lte option for lte device -->
+    <bool name="config_enabled_lte" translatable="false">true</bool>
 </resources>
-- 
2.9.3

