From d94b190ec3f1b1acc84d3149b6bfd5e486c19144 Mon Sep 17 00:00:00 2001
From: Zefan Li <lizefan@huawei.com>
Date: Tue, 14 Apr 2015 17:34:05 +0800
Subject: [PATCH] Linux 3.4.107
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

spi: dw: Fix dynamic speed change.

commit 0a8727e69778683495058852f783eeda141a754e upstream.

An IOCTL call that calls spi_setup() and then dw_spi_setup() will
overwrite the persisted last transfer speed. On each transfer, the
SPI speed is compared to the last transfer speed to determine if the
clock divider registers need to be updated (did the speed change?).
This bug was observed with the spidev driver using spi-config to
update the max transfer speed.

This fix: Don't overwrite the persisted last transaction clock speed
when updating the SPI parameters in dw_spi_setup(). On the next
transaction, the new speed won't match the persisted last speed
and the hardware registers will be updated.
On initialization, the persisted last transaction clock
speed will be 0 but will be updated after the first SPI
transaction.

Move zeroed clock divider check into clock change test because
chip->clk_div is zero on startup and would cause a divide-by-zero
error. The calculation was wrong as well (can't support odd #).

Reported-by: Vlastimil Setka <setka@vsis.cz>
Signed-off-by: Vlastimil Setka <setka@vsis.cz>
Signed-off-by: Thor Thayer <tthayer@opensource.altera.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: serial: cp210x: add IDs for CEL MeshConnect USB Stick

commit ffcfe30ebd8dd703d0fc4324ffe56ea21f5479f4 upstream.

Signed-off-by: Preston Fick <pffick@gmail.com>
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

iio: Fix IIO_EVENT_CODE_EXTRACT_DIR bit mask

commit ccf54555da9a5e91e454b909ca6a5303c7d6b910 upstream.

The direction field is set on 7 bits, thus we need to AND it with 0111 111 mask
in order to retrieve it, that is 0x7F, not 0xCF as it is now.

Fixes: ade7ef7ba (staging:iio: Differential channel handling)
Signed-off-by: Cristina Ciocan <cristina.ciocan@intel.com>
Signed-off-by: Jonathan Cameron <jic23@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb: serial: ftdi_sio: add PIDs for Matrix Orbital products

commit 204ec6e07ea7aff863df0f7c53301f9cbbfbb9d3 upstream.

Add PIDs for new Matrix Orbital GTT series products.

Signed-off-by: Troy Clark <tclark@matrixorbital.ca>
[johan: shorten commit message ]
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: keyspan: fix tty line-status reporting

commit 5d1678a33c731b56e245e888fdae5e88efce0997 upstream.

Fix handling of TTY error flags, which are not bitmasks and must
specifically not be ORed together as this prevents the line discipline
from recognising them.

Also insert null characters when reporting overrun errors as these are
not associated with the received character.

Fixes: 1da177e4c3f4 ("Linux-2.6.12-rc2")
Signed-off-by: Johan Hovold <johan@kernel.org>
[lizf: Backported to 3.4:
 - s/&port->port/tty/
 - adjust context
 - adjust indentation]
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: keyspan: fix overrun-error reporting

commit 855515a6d3731242d85850a206f2ec084c917338 upstream.

Fix reporting of overrun errors, which are not associated with a
character. Instead insert a null character and report only once.

Fixes: 1da177e4c3f4 ("Linux-2.6.12-rc2")
Signed-off-by: Johan Hovold <johan@kernel.org>
[lizf: Backported to 3.4:
 - s/&port->port/tty
 - adjust context
 - adjust indentation]
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: ssu100: fix overrun-error reporting

commit 75bcbf29c284dd0154c3e895a0bd1ef0e796160e upstream.

Fix reporting of overrun errors, which should only be reported once
using the inserted null character.

Fixes: 6b8f1ca5581b ("USB: ssu100: set tty_flags in ssu100_process_packet")
Signed-off-by: Johan Hovold <johan@kernel.org>
[lizf: Backported to 3.4:
 - adjust context
 - lookup tty using tty_port_tty_get()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

SUNRPC: Fix locking around callback channel reply receive

commit 093a1468b6edb0e568be7311b8d2228d205702db upstream.

Both xprt_lookup_rqst() and xprt_complete_rqst() require that you
take the transport lock in order to avoid races with xprt_transmit().

Signed-off-by: Trond Myklebust <trond.myklebust@primarydata.com>
Reviewed-by: Jeff Layton <jlayton@primarydata.com>
Signed-off-by: J. Bruce Fields <bfields@redhat.com>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

nfsd: Fix slot wake up race in the nfsv4.1 callback code

commit c6c15e1ed303ffc47e696ea1c9a9df1761c1f603 upstream.

The currect code for nfsd41_cb_get_slot() and nfsd4_cb_done() has no
locking in order to guarantee atomicity, and so allows for races of
the form.

Task 1                                  Task 2
======                                  ======
if (test_and_set_bit(0) != 0) {
                                        clear_bit(0)
                                        rpc_wake_up_next(queue)
        rpc_sleep_on(queue)
        return false;
}

This patch breaks the race condition by adding a retest of the bit
after the call to rpc_sleep_on().

Signed-off-by: Trond Myklebust <trond.myklebust@primarydata.com>
Signed-off-by: J. Bruce Fields <bfields@redhat.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

bnx2fc: do not add shared skbs to the fcoe_rx_list

commit 01a4cc4d0cd6a836c7b923760e8eb1cbb6a47258 upstream.

In some cases, the fcoe_rx_list may contains multiple instances
of the same skb (the so called "shared skbs").

the bnx2fc_l2_rcv thread is a loop that extracts a skb from the list,
modifies (and destroys) its content and then proceed to the next one.
The problem is that if the skb is shared, the remaining instances will
be corrupted.

The solution is to use skb_share_check() before adding the skb to the
fcoe_rx_list.

[ 6286.808725] ------------[ cut here ]------------
[ 6286.808729] WARNING: at include/scsi/fc_frame.h:173 bnx2fc_l2_rcv_thread+0x425/0x450 [bnx2fc]()
[ 6286.808748] Modules linked in: bnx2x(-) mdio dm_service_time bnx2fc cnic uio fcoe libfcoe 8021q garp stp mrp libfc llc scsi_transport_fc scsi_tgt sg iTCO_wdt iTCO_vendor_support coretemp kvm_intel kvm crct10dif_pclmul crc32_pclmul crc32c_intel e1000e ghash_clmulni_intel aesni_intel lrw gf128mul glue_helper ablk_helper ptp cryptd hpilo serio_raw hpwdt lpc_ich pps_core ipmi_si pcspkr mfd_core ipmi_msghandler shpchp pcc_cpufreq mperf nfsd auth_rpcgss nfs_acl lockd sunrpc dm_multipath xfs libcrc32c ata_generic pata_acpi sd_mod crc_t10dif crct10dif_common mgag200 syscopyarea sysfillrect sysimgblt i2c_algo_bit ata_piix drm_kms_helper ttm drm libata i2c_core hpsa dm_mirror dm_region_hash dm_log dm_mod [last unloaded: mdio]
[ 6286.808750] CPU: 3 PID: 1304 Comm: bnx2fc_l2_threa Not tainted 3.10.0-121.el7.x86_64 #1
[ 6286.808750] Hardware name: HP ProLiant DL120 G7, BIOS J01 07/01/2013
[ 6286.808752]  0000000000000000 000000000b36e715 ffff8800deba1e00 ffffffff815ec0ba
[ 6286.808753]  ffff8800deba1e38 ffffffff8105dee1 ffffffffa05618c0 ffff8801e4c81888
[ 6286.808754]  ffffe8ffff663868 ffff8801f402b180 ffff8801f56bc000 ffff8800deba1e48
[ 6286.808754] Call Trace:
[ 6286.808759]  [<ffffffff815ec0ba>] dump_stack+0x19/0x1b
[ 6286.808762]  [<ffffffff8105dee1>] warn_slowpath_common+0x61/0x80
[ 6286.808763]  [<ffffffff8105e00a>] warn_slowpath_null+0x1a/0x20
[ 6286.808765]  [<ffffffffa054f415>] bnx2fc_l2_rcv_thread+0x425/0x450 [bnx2fc]
[ 6286.808767]  [<ffffffffa054eff0>] ? bnx2fc_disable+0x90/0x90 [bnx2fc]
[ 6286.808769]  [<ffffffff81085aef>] kthread+0xcf/0xe0
[ 6286.808770]  [<ffffffff81085a20>] ? kthread_create_on_node+0x140/0x140
[ 6286.808772]  [<ffffffff815fc76c>] ret_from_fork+0x7c/0xb0
[ 6286.808773]  [<ffffffff81085a20>] ? kthread_create_on_node+0x140/0x140
[ 6286.808774] ---[ end trace c6cdb939184ccb4e ]---

Signed-off-by: Maurizio Lombardi <mlombard@redhat.com>
Acked-by: Chad Dupuis <chad.dupuis@qlogic.com>
Signed-off-by: Christoph Hellwig <hch@lst.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ARM: 8216/1: xscale: correct auxiliary register in suspend/resume

commit ef59a20ba375aeb97b3150a118318884743452a8 upstream.

According to the manuals I have, XScale auxiliary register should be
reached with opc_2 = 1 instead of crn = 1. cpu_xscale_proc_init
correctly uses c1, c0, 1 arguments, but cpu_xscale_do_suspend and
cpu_xscale_do_resume use c1, c1, 0. Correct suspend/resume functions to
also use c1, c0, 1.

The issue was primarily noticed thanks to qemu reporing "unsupported
instruction" on the pxa suspend path. Confirmed in PXA210/250 and PXA255
XScale Core manuals and in PXA270 and PXA320 Developers Guides.

Harware tested by me on tosa (pxa255). Robert confirmed on pxa270 board.

Tested-by: Robert Jarzmik <robert.jarzmik@free.fr>
Signed-off-by: Dmitry Eremin-Solenikov <dbaryshkov@gmail.com>
Acked-by: Robert Jarzmik <robert.jarzmik@free.fr>
Signed-off-by: Russell King <rmk+kernel@arm.linux.org.uk>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: xhci: don't start a halted endpoint before its new dequeue is set

commit c3492dbfa1050debf23a5b5cd2bc7514c5b37896 upstream.

A halted endpoint ring must first be reset, then move the ring
dequeue pointer past the problematic TRB. If we start the ring too
early after reset, but before moving the dequeue pointer we
will end up executing the same problematic TRB again.

As we always issue a set transfer dequeue command after a reset
endpoint command we can skip starting endpoint rings at reset endpoint
command completion.

Without this fix we end up trying to handle the same faulty TD for
contol endpoints. causing timeout, and failing testusb ctrl_out write
tests.

Fixes: e9df17e (USB: xhci: Correct assumptions about number of rings per endpoint.)
Tested-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Mathias Nyman <mathias.nyman@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: xhci: Reset a halted endpoint immediately when we encounter a stall.

commit 8e71a322fdb127814bcba423a512914ca5bc6cf5 upstream.

If a device is halted and reuturns a STALL, then the halted endpoint
needs to be cleared both on the host and device side. The host
side halt is cleared by issueing a xhci reset endpoint command. The device side
is cleared with a ClearFeature(ENDPOINT_HALT) request, which should
be issued by the device driver if a URB reruen -EPIPE.

Previously we cleared the host side halt after the device side was cleared.
To make sure the host side halt is cleared in time we want to issue the
reset endpoint command immedialtely when a STALL status is encountered.

Otherwise we end up not following the specs and not returning -EPIPE
several times in a row when trying to transfer data to a halted endpoint.

Fixes: bcef3fd (USB: xhci: Handle errors that cause endpoint halts.)
Tested-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Mathias Nyman <mathias.nyman@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb: xhci: rework root port wake bits if controller isn't allowed to wakeup

commit a1377e5397ab321e21b793ec8cd2b6f12bd3c718 upstream.

When system is being suspended, if host device is not allowed to do wakeup,
xhci_suspend() needs to clear all root port wake on bits. Otherwise, some
platforms may generate spurious wakeup, even if PCI PME# is disabled.

The initial commit ff8cbf250b44 ("xhci: clear root port wake on bits"),
which also got into stable, turned out to not work correctly and had to
be reverted, and is now rewritten.

Signed-off-by: Lu Baolu <baolu.lu@linux.intel.com>
Suggested-by: Alan Stern <stern@rowland.harvard.edu>
Acked-by: Alan Stern <stern@rowland.harvard.edu>
[Mathias Nyman: reword commit message]
Signed-off-by: Mathias Nyman <mathias.nyman@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
[lizf: Backported to 3.4:
 - adjust context
 - drop changes to xhci_plat_suspend()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: hda - Limit 40bit DMA for AMD HDMI controllers

commit 413cbf469a19e7662ba5025695bf5a573927105a upstream.

AMD/ATI HDMI controller chip models, we already have a filter to lower
to 32bit DMA, but the rest are supposed to be working with 64bit
although the hardware doesn't really work with 63bit but only with 40
or 48bit DMA.  In this patch, we take 40bit DMA for safety for the
AMD/ATI controllers as the graphics drivers does.

Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Benjamin Herrenschmidt <benh@kernel.crashing.org>
[lizf: Backported to 3.4:
 - adjust context
 - s/AZX_GCAP_640K/ICH6_GCAP_64OK]
Signed-off-by: Zefan Li <lizefan@huawei.com>

MIPS: Loongson: Make platform serial setup always built-in.

commit 26927f76499849e095714452b8a4e09350f6a3b9 upstream.

If SERIAL_8250 is compiled as a module, the platform specific setup
for Loongson will be a module too, and it will not work very well.
At least on Loongson 3 it will trigger a build failure,
since loongson_sysconf is not exported to modules.

Fix by making the platform specific serial code always built-in.

Signed-off-by: Aaro Koskinen <aaro.koskinen@iki.fi>
Reported-by: Ralf Baechle <ralf@linux-mips.org>
Cc: linux-mips@linux-mips.org
Cc: Huacai Chen <chenhc@lemote.com>
Cc: Markos Chandras <Markos.Chandras@imgtec.com>
Patchwork: https://patchwork.linux-mips.org/patch/8533/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb-quirks: Add reset-resume quirk for MS Wireless Laser Mouse 6000

commit 263e80b43559a6103e178a9176938ce171b23872 upstream.

This wireless mouse receiver needs a reset-resume quirk to properly come
out of reset.

BugLink: https://bugzilla.redhat.com/show_bug.cgi?id=1165206
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

Input: xpad - use proper endpoint type

commit a1f9a4072655843fc03186acbad65990cc05dd2d upstream.

The xpad wireless endpoint is not a bulk endpoint on my devices, but
rather an interrupt one, so the USB core complains when it is submitted.
I'm guessing that the author really did mean that this should be an
interrupt urb, but as there are a zillion different xpad devices out
there, let's cover out bases and handle both bulk and interrupt
endpoints just as easily.

Signed-off-by: "Pierre-Loup A. Griffais" <pgriffais@valvesoftware.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Dmitry Torokhov <dmitry.torokhov@gmail.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

powerpc/pseries: Fix endiannes issue in RTAS call from xmon

commit 3b8a3c01096925a824ed3272601082289d9c23a5 upstream.

On pseries system (LPAR) xmon failed to enter when running in LE mode,
system is hunging. Inititating xmon will lead to such an output on the
console:

SysRq : Entering xmon
cpu 0x15: Vector: 0  at [c0000003f39ffb10]
    pc: c00000000007ed7c: sysrq_handle_xmon+0x5c/0x70
    lr: c00000000007ed7c: sysrq_handle_xmon+0x5c/0x70
    sp: c0000003f39ffc70
   msr: 8000000000009033
  current = 0xc0000003fafa7180
  paca    = 0xc000000007d75e80	 softe: 0	 irq_happened: 0x01
    pid   = 14617, comm = bash
Bad kernel stack pointer fafb4b0 at eca7cc4
cpu 0x15: Vector: 300 (Data Access) at [c000000007f07d40]
    pc: 000000000eca7cc4
    lr: 000000000eca7c44
    sp: fafb4b0
   msr: 8000000000001000
   dar: 10000000
 dsisr: 42000000
  current = 0xc0000003fafa7180
  paca    = 0xc000000007d75e80	 softe: 0	 irq_happened: 0x01
    pid   = 14617, comm = bash
cpu 0x15: Exception 300 (Data Access) in xmon, returning to main loop
xmon: WARNING: bad recursive fault on cpu 0x15

The root cause is that xmon is calling RTAS to turn off the surveillance
when entering xmon, and RTAS is requiring big endian parameters.

This patch is byte swapping the RTAS arguments when running in LE mode.

Signed-off-by: Laurent Dufour <ldufour@linux.vnet.ibm.com>
Signed-off-by: Michael Ellerman <mpe@ellerman.id.au>
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/i915: Unlock panel even when LVDS is disabled

commit b0616c5306b342ceca07044dbc4f917d95c4f825 upstream.

Otherwise we'll have backtraces in assert_panel_unlocked because the
BIOS locks the register. In the reporter's case this regression was
introduced in

commit c31407a3672aaebb4acddf90944a114fa5c8af7b
Author: Chris Wilson <chris@chris-wilson.co.uk>
Date:   Thu Oct 18 21:07:01 2012 +0100

    drm/i915: Add no-lvds quirk for Supermicro X7SPA-H

Reported-by: Alexey Orishko <alexey.orishko@gmail.com>
Cc: Alexey Orishko <alexey.orishko@gmail.com>
Cc: Chris Wilson <chris@chris-wilson.co.uk>
Cc: Francois Tigeot <ftigeot@wolfpond.org>
Signed-off-by: Daniel Vetter <daniel.vetter@intel.com>
Tested-by: Alexey Orishko <alexey.orishko@gmail.com>
Signed-off-by: Jani Nikula <jani.nikula@intel.com>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

AHCI: Add DeviceIDs for Sunrise Point-LP SATA controller

commit 249cd0a187ed4ef1d0af7f74362cc2791ec5581b upstream.

This patch adds DeviceIDs for Sunrise Point-LP.

Signed-off-by: Devin Ryles <devin.ryles@intel.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

sata_fsl: fix error handling of irq_of_parse_and_map

commit aad0b624129709c94c2e19e583b6053520353fa8 upstream.

irq_of_parse_and_map() returns 0 on error (the result is unsigned int),
so testing for negative result never works.

Signed-off-by: Dmitry Torokhov <dtor@chromium.org>
Signed-off-by: Tejun Heo <tj@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/radeon: kernel panic in drm_calc_vbltimestamp_from_scanoutpos with 3.18.0-rc6

commit f5475cc43c899e33098d4db44b7c5e710f16589d upstream.

I was unable too boot 3.18.0-rc6 because of the following kernel
panic in drm_calc_vbltimestamp_from_scanoutpos():

    [drm] Initialized drm 1.1.0 20060810
    [drm] radeon kernel modesetting enabled.
    [drm] initializing kernel modesetting (RV100 0x1002:0x515E 0x15D9:0x8080).
    [drm] register mmio base: 0xC8400000
    [drm] register mmio size: 65536
    radeon 0000:0b:01.0: VRAM: 128M 0x00000000D0000000 - 0x00000000D7FFFFFF (16M used)
    radeon 0000:0b:01.0: GTT: 512M 0x00000000B0000000 - 0x00000000CFFFFFFF
    [drm] Detected VRAM RAM=128M, BAR=128M
    [drm] RAM width 16bits DDR
    [TTM] Zone  kernel: Available graphics memory: 3829346 kiB
    [TTM] Zone   dma32: Available graphics memory: 2097152 kiB
    [TTM] Initializing pool allocator
    [TTM] Initializing DMA pool allocator
    [drm] radeon: 16M of VRAM memory ready
    [drm] radeon: 512M of GTT memory ready.
    [drm] GART: num cpu pages 131072, num gpu pages 131072
    [drm] PCI GART of 512M enabled (table at 0x0000000037880000).
    radeon 0000:0b:01.0: WB disabled
    radeon 0000:0b:01.0: fence driver on ring 0 use gpu addr 0x00000000b0000000 and cpu addr 0xffff8800bbbfa000
    [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
    [drm] Driver supports precise vblank timestamp query.
    [drm] radeon: irq initialized.
    [drm] Loading R100 Microcode
    radeon 0000:0b:01.0: Direct firmware load for radeon/R100_cp.bin failed with error -2
    radeon_cp: Failed to load firmware "radeon/R100_cp.bin"
    [drm:r100_cp_init] *ERROR* Failed to load firmware!
    radeon 0000:0b:01.0: failed initializing CP (-2).
    radeon 0000:0b:01.0: Disabling GPU acceleration
    [drm] radeon: cp finalized
    BUG: unable to handle kernel NULL pointer dereference at 000000000000025c
    IP: [<ffffffff8150423b>] drm_calc_vbltimestamp_from_scanoutpos+0x4b/0x320
    PGD 0
    Oops: 0000 [#1] SMP
    Modules linked in:
    CPU: 1 PID: 1 Comm: swapper/0 Not tainted 3.18.0-rc6-4-default #2649
    Hardware name: Supermicro X7DB8/X7DB8, BIOS 6.00 07/26/2006
    task: ffff880234da2010 ti: ffff880234da4000 task.ti: ffff880234da4000
    RIP: 0010:[<ffffffff8150423b>]  [<ffffffff8150423b>] drm_calc_vbltimestamp_from_scanoutpos+0x4b/0x320
    RSP: 0000:ffff880234da7918  EFLAGS: 00010086
    RAX: ffffffff81557890 RBX: 0000000000000000 RCX: ffff880234da7a48
    RDX: ffff880234da79f4 RSI: 0000000000000000 RDI: ffff880232e15000
    RBP: ffff880234da79b8 R08: 0000000000000000 R09: 0000000000000000
    R10: 000000000000000a R11: 0000000000000001 R12: ffff880232dda1c0
    R13: ffff880232e1518c R14: 0000000000000292 R15: ffff880232e15000
    FS:  0000000000000000(0000) GS:ffff88023fc40000(0000) knlGS:0000000000000000
    CS:  0010 DS: 0000 ES: 0000 CR0: 000000008005003b
    CR2: 000000000000025c CR3: 0000000002014000 CR4: 00000000000007e0
    Stack:
     ffff880234da79d8 0000000000000286 ffff880232dcbc00 0000000000002480
     ffff880234da7958 0000000000000296 ffff880234da7998 ffffffff8151b51d
     ffff880234da7a48 0000000032dcbeb0 ffff880232dcbc00 ffff880232dcbc58
    Call Trace:
     [<ffffffff8151b51d>] ? drm_vma_offset_remove+0x1d/0x110
     [<ffffffff8152dc98>] radeon_get_vblank_timestamp_kms+0x38/0x60
     [<ffffffff8152076a>] ? ttm_bo_release_list+0xba/0x180
     [<ffffffff81503751>] drm_get_last_vbltimestamp+0x41/0x70
     [<ffffffff81503933>] vblank_disable_and_save+0x73/0x1d0
     [<ffffffff81106b2f>] ? try_to_del_timer_sync+0x4f/0x70
     [<ffffffff81505245>] drm_vblank_cleanup+0x65/0xa0
     [<ffffffff815604fa>] radeon_irq_kms_fini+0x1a/0x70
     [<ffffffff8156c07e>] r100_init+0x26e/0x410
     [<ffffffff8152ae3e>] radeon_device_init+0x7ae/0xb50
     [<ffffffff8152d57f>] radeon_driver_load_kms+0x8f/0x210
     [<ffffffff81506965>] drm_dev_register+0xb5/0x110
     [<ffffffff8150998f>] drm_get_pci_dev+0x8f/0x200
     [<ffffffff815291cd>] radeon_pci_probe+0xad/0xe0
     [<ffffffff8141a365>] local_pci_probe+0x45/0xa0
     [<ffffffff8141b741>] pci_device_probe+0xd1/0x130
     [<ffffffff81633dad>] driver_probe_device+0x12d/0x3e0
     [<ffffffff8163413b>] __driver_attach+0x9b/0xa0
     [<ffffffff816340a0>] ? __device_attach+0x40/0x40
     [<ffffffff81631cd3>] bus_for_each_dev+0x63/0xa0
     [<ffffffff8163378e>] driver_attach+0x1e/0x20
     [<ffffffff81633390>] bus_add_driver+0x180/0x240
     [<ffffffff81634914>] driver_register+0x64/0xf0
     [<ffffffff81419cac>] __pci_register_driver+0x4c/0x50
     [<ffffffff81509bf5>] drm_pci_init+0xf5/0x120
     [<ffffffff821dc871>] ? ttm_init+0x6a/0x6a
     [<ffffffff821dc908>] radeon_init+0x97/0xb5
     [<ffffffff810002fc>] do_one_initcall+0xbc/0x1f0
     [<ffffffff810e3278>] ? __wake_up+0x48/0x60
     [<ffffffff8218e256>] kernel_init_freeable+0x18a/0x215
     [<ffffffff8218d983>] ? initcall_blacklist+0xc0/0xc0
     [<ffffffff818a78f0>] ? rest_init+0x80/0x80
     [<ffffffff818a78fe>] kernel_init+0xe/0xf0
     [<ffffffff818c0c3c>] ret_from_fork+0x7c/0xb0
     [<ffffffff818a78f0>] ? rest_init+0x80/0x80
    Code: 45 ac 0f 88 a8 01 00 00 3b b7 d0 01 00 00 49 89 ff 0f 83 99 01 00 00 48 8b 47 20 48 8b 80 88 00 00 00 48 85 c0 0f 84 cd 01 00 00 <41> 8b b1 5c 02 00 00 41 8b 89 58 02 00 00 89 75 98 41 8b b1 60
    RIP  [<ffffffff8150423b>] drm_calc_vbltimestamp_from_scanoutpos+0x4b/0x320
     RSP <ffff880234da7918>
    CR2: 000000000000025c
    ---[ end trace ad2c0aadf48e2032 ]---
    Kernel panic - not syncing: Attempted to kill init! exitcode=0x00000009

It has helped me to add a NULL pointer check that was suggested at
http://lists.freedesktop.org/archives/dri-devel/2014-October/070663.html

I am not familiar with the code. But the change looks sane
and we need something fast at this stage of 3.18 development.

Suggested-by: Helge Deller <deller@gmx.de>
Signed-off-by: Petr Mladek <pmladek@suse.cz>
Tested-by: Petr Mladek <pmladek@suse.cz>
Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: fix swapoff hang after page migration and fork

commit 2022b4d18a491a578218ce7a4eca8666db895a73 upstream.

I've been seeing swapoff hangs in recent testing: it's cycling around
trying unsuccessfully to find an mm for some remaining pages of swap.

I have been exercising swap and page migration more heavily recently,
and now notice a long-standing error in copy_one_pte(): it's trying to
add dst_mm to swapoff's mmlist when it finds a swap entry, but is doing
so even when it's a migration entry or an hwpoison entry.

Which wouldn't matter much, except it adds dst_mm next to src_mm,
assuming src_mm is already on the mmlist: which may not be so.  Then if
pages are later swapped out from dst_mm, swapoff won't be able to find
where to replace them.

There's already a !non_swap_entry() test for stats: move that up before
the swap_duplicate() and the addition to mmlist.

Signed-off-by: Hugh Dickins <hughd@google.com>
Cc: Kelley Nielsen <kelleynnn@gmail.com>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ahci: disable NCQ on Samsung pci-e SSDs on macbooks

commit 67809f85d31eac600f6b28defa5386c9d2a13b1d upstream.

Samsung's pci-e SSDs with device ID 0x1600 which are found on some
macbooks time out on NCQ commands.  Blacklist NCQ on the device so
that the affected machines can at least boot.

Original-patch-by: Levente Kurusa <levex@linux.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=60731
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ahci: disable MSI instead of NCQ on Samsung pci-e SSDs on macbooks

commit 66a7cbc303f4d28f201529b06061944d51ab530c upstream.

Samsung pci-e SSDs on macbooks failed miserably on NCQ commands, so
67809f85d31e ("ahci: disable NCQ on Samsung pci-e SSDs on macbooks")
disabled NCQ on them.  It turns out that NCQ is fine as long as MSI is
not used, so let's turn off MSI and leave NCQ on.

Signed-off-by: Tejun Heo <tj@kernel.org>
Link: https://bugzilla.kernel.org/show_bug.cgi?id=60731
Tested-by: <dorin@i51.org>
Tested-by: Imre Kaloz <kaloz@openwrt.org>
Fixes: 67809f85d31e ("ahci: disable NCQ on Samsung pci-e SSDs on macbooks")
Signed-off-by: Zefan Li <lizefan@huawei.com>

ahci: disable MSI on SAMSUNG 0xa800 SSD

commit 2b21ef0aae65f22f5ba86b13c4588f6f0c2dbefb upstream.

Just like 0x1600 which got blacklisted by 66a7cbc303f4 ("ahci: disable
MSI instead of NCQ on Samsung pci-e SSDs on macbooks"), 0xa800 chokes
on NCQ commands if MSI is enabled.  Disable MSI.

Signed-off-by: Tejun Heo <tj@kernel.org>
Reported-by: Dominik Mierzejewski <dominik@greysector.net>
Link: https://bugzilla.kernel.org/show_bug.cgi?id=89171
Signed-off-by: Zefan Li <lizefan@huawei.com>

i2c: davinci: generate STP always when NACK is received

commit 9ea359f7314132cbcb5a502d2d8ef095be1f45e4 upstream.

According to I2C specification the NACK should be handled as follows:
"When SDA remains HIGH during this ninth clock pulse, this is defined as the Not
Acknowledge signal. The master can then generate either a STOP condition to
abort the transfer, or a repeated START condition to start a new transfer."
[I2C spec Rev. 6, 3.1.6: http://www.nxp.com/documents/user_manual/UM10204.pdf]

Currently the Davinci i2c driver interrupts the transfer on receipt of a
NACK but fails to send a STOP in some situations and so makes the bus
stuck until next I2C IP reset (idle/enable).

For example, the issue will happen during SMBus read transfer which
consists from two i2c messages write command/address and read data:

S Slave Address Wr A Command Code A Sr Slave Address Rd A D1..Dn A P
<--- write -----------------------> <--- read --------------------->

The I2C client device will send NACK if it can't recognize "Command Code"
and it's expected from I2C master to generate STP in this case.
But now, Davinci i2C driver will just exit with -EREMOTEIO and STP will
not be generated.

Hence, fix it by generating Stop condition (STP) always when NACK is received.

This patch fixes Davinci I2C in the same way it was done for OMAP I2C
commit cda2109a26eb ("i2c: omap: query STP always when NACK is received").

Reviewed-by: Uwe Kleine-König <u.kleine-koenig@pengutronix.de>
Reported-by: Hein Tibosch <hein_tibosch@yahoo.es>
Signed-off-by: Grygorii Strashko <grygorii.strashko@ti.com>
Signed-off-by: Wolfram Sang <wsa@the-dreams.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

eCryptfs: Force RO mount when encrypted view is enabled

commit 332b122d39c9cbff8b799007a825d94b2e7c12f2 upstream.

The ecryptfs_encrypted_view mount option greatly changes the
functionality of an eCryptfs mount. Instead of encrypting and decrypting
lower files, it provides a unified view of the encrypted files in the
lower filesystem. The presence of the ecryptfs_encrypted_view mount
option is intended to force a read-only mount and modifying files is not
supported when the feature is in use. See the following commit for more
information:

  e77a56d [PATCH] eCryptfs: Encrypted passthrough

This patch forces the mount to be read-only when the
ecryptfs_encrypted_view mount option is specified by setting the
MS_RDONLY flag on the superblock. Additionally, this patch removes some
broken logic in ecryptfs_open() that attempted to prevent modifications
of files when the encrypted view feature was in use. The check in
ecryptfs_open() was not sufficient to prevent file modifications using
system calls that do not operate on a file descriptor.

Signed-off-by: Tyler Hicks <tyhicks@canonical.com>
Reported-by: Priya Bansal <p.bansal@samsung.com>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

writeback: Move I_DIRTY_PAGES handling

commit 6290be1c1dc6589eeda213aa40946b27fa4faac8 upstream.

Instead of clearing I_DIRTY_PAGES and resetting it when we didn't succeed in
writing them all, just clear the bit only when we succeeded writing all the
pages. We also move the clearing of the bit close to other i_state handling to
separate it from writeback list handling. This is desirable because list
handling will differ for flusher thread and other writeback_single_inode()
callers in future. No filesystem plays any tricks with I_DIRTY_PAGES (like
checking it in ->writepages or ->write_inode implementation) so this movement
is safe.

Signed-off-by: Jan Kara <jack@suse.cz>
Signed-off-by: Fengguang Wu <fengguang.wu@intel.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

writeback: fix a subtle race condition in I_DIRTY clearing

commit 9c6ac78eb3521c5937b2dd8a7d1b300f41092f45 upstream.

After invoking ->dirty_inode(), __mark_inode_dirty() does smp_mb() and
tests inode->i_state locklessly to see whether it already has all the
necessary I_DIRTY bits set.  The comment above the barrier doesn't
contain any useful information - memory barriers can't ensure "changes
are seen by all cpus" by itself.

And it sure enough was broken.  Please consider the following
scenario.

 CPU 0					CPU 1
 -------------------------------------------------------------------------------

					enters __writeback_single_inode()
					grabs inode->i_lock
					tests PAGECACHE_TAG_DIRTY which is clear
 enters __set_page_dirty()
 grabs mapping->tree_lock
 sets PAGECACHE_TAG_DIRTY
 releases mapping->tree_lock
 leaves __set_page_dirty()

 enters __mark_inode_dirty()
 smp_mb()
 sees I_DIRTY_PAGES set
 leaves __mark_inode_dirty()
					clears I_DIRTY_PAGES
					releases inode->i_lock

Now @inode has dirty pages w/ I_DIRTY_PAGES clear.  This doesn't seem
to lead to an immediately critical problem because requeue_inode()
later checks PAGECACHE_TAG_DIRTY instead of I_DIRTY_PAGES when
deciding whether the inode needs to be requeued for IO and there are
enough unintentional memory barriers inbetween, so while the inode
ends up with inconsistent I_DIRTY_PAGES flag, it doesn't fall off the
IO list.

The lack of explicit barrier may also theoretically affect the other
I_DIRTY bits which deal with metadata dirtiness.  There is no
guarantee that a strong enough barrier exists between
I_DIRTY_[DATA]SYNC clearing and write_inode() writing out the dirtied
inode.  Filesystem inode writeout path likely has enough stuff which
can behave as full barrier but it's theoretically possible that the
writeout may not see all the updates from ->dirty_inode().

Fix it by adding an explicit smp_mb() after I_DIRTY clearing.  Note
that I_DIRTY_PAGES needs a special treatment as it always needs to be
cleared to be interlocked with the lockless test on
__mark_inode_dirty() side.  It's cleared unconditionally and
reinstated after smp_mb() if the mapping still has dirty pages.

Also add comments explaining how and why the barriers are paired.

Lightly tested.

Signed-off-by: Tejun Heo <tj@kernel.org>
Cc: Jan Kara <jack@suse.cz>
Cc: Mikulas Patocka <mpatocka@redhat.com>
Cc: Jens Axboe <axboe@kernel.dk>
Cc: Al Viro <viro@zeniv.linux.org.uk>
Reviewed-by: Jan Kara <jack@suse.cz>
Signed-off-by: Jens Axboe <axboe@fb.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb: renesas_usbhs: gadget: fix NULL pointer dereference in ep_disable()

commit 11432050f070810ba139d0226344eef120c3a559 upstream.

This patch fixes an issue that the NULL pointer dereference happens
when we uses g_audio driver. Since the g_audio driver will call
usb_ep_disable() in afunc_set_alt() before it calls usb_ep_enable(),
the uep->pipe of renesas usbhs driver will be NULL. So, this patch
adds a condition to avoid the oops.

Signed-off-by: Kazuya Mizuguchi <kazuya.mizuguchi.ks@renesas.com>
Signed-off-by: Takeshi Kihara <takeshi.kihara.df@renesas.com>
Signed-off-by: Yoshihiro Shimoda <yoshihiro.shimoda.uh@renesas.com>
Fixes: 2f98382dc (usb: renesas_usbhs: Add Renesas USBHS Gadget)
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

UBI: Fix invalid vfree()

commit f38aed975c0c3645bbdfc5ebe35726e64caaf588 upstream.

The logic of vfree()'ing vol->upd_buf is tied to vol->updating.
In ubi_start_update() vol->updating is set long before vmalloc()'ing
vol->upd_buf. If we encounter a write failure in ubi_start_update()
before vmalloc() the UBI device release function will try to vfree()
vol->upd_buf because vol->updating is set.
Fix this by allocating vol->upd_buf directly after setting vol->updating.

Fixes:
[   31.559338] UBI warning: vol_cdev_release: update of volume 2 not finished, volume is damaged
[   31.559340] ------------[ cut here ]------------
[   31.559343] WARNING: CPU: 1 PID: 2747 at mm/vmalloc.c:1446 __vunmap+0xe3/0x110()
[   31.559344] Trying to vfree() nonexistent vm area (ffffc90001f2b000)
[   31.559345] Modules linked in:
[   31.565620]  0000000000000bba ffff88002a0cbdb0 ffffffff818f0497 ffff88003b9ba148
[   31.566347]  ffff88002a0cbde0 ffffffff8156f515 ffff88003b9ba148 0000000000000bba
[   31.567073]  0000000000000000 0000000000000000 ffff88002a0cbe88 ffffffff8156c10a
[   31.567793] Call Trace:
[   31.568034]  [<ffffffff818f0497>] dump_stack+0x4e/0x7a
[   31.568510]  [<ffffffff8156f515>] ubi_io_write_vid_hdr+0x155/0x160
[   31.569084]  [<ffffffff8156c10a>] ubi_eba_write_leb+0x23a/0x870
[   31.569628]  [<ffffffff81569b36>] vol_cdev_write+0x226/0x380
[   31.570155]  [<ffffffff81179265>] vfs_write+0xb5/0x1f0
[   31.570627]  [<ffffffff81179f8a>] SyS_pwrite64+0x6a/0xa0
[   31.571123]  [<ffffffff818fde12>] system_call_fastpath+0x16/0x1b

Signed-off-by: Richard Weinberger <richard@nod.at>
Signed-off-by: Artem Bityutskiy <artem.bityutskiy@linux.intel.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

driver core: Fix unbalanced device reference in drivers_probe

commit bb34cb6bbd287b57e955bc5cfd42fcde6aaca279 upstream.

bus_find_device_by_name() acquires a device reference which is never
released.  This results in an object leak, which on older kernels
results in failure to release all resources of PCI devices.  libvirt
uses drivers_probe to re-attach devices to the host after assignment
and is therefore a common trigger for this leak.

Example:

 pci 0000:01:10.0: [8086:10ca] type 00 class 0x020000
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): kobject_add_internal: parent: '0000:00:01.0', set: 'devices'
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): kobject_cleanup, parent           (null)
 kobject: '0000:01:10.0' (ffff8801d79cd0a8): calling ktype release
 kobject: '0000:01:10.0': free name

[kobject freed as expected]

 pci 0000:01:10.0: [8086:10ca] type 00 class 0x020000
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): kobject_add_internal: parent: '0000:00:01.0', set: 'devices'
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): kobject_uevent_env
 kobject: '0000:01:10.0' (ffff8801d79ce0a8): fill_kobj_path: path = '/devices/pci0000:00/0000:00:01.0/0000:01:10.0'

[no free]

Signed-off-by: Alex Williamson <alex.williamson@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

drbd: merge_bvec_fn: properly remap bvm->bi_bdev

commit 3b9d35d744bb5139f9fed57f38c019bb8c7d351c upstream.

This was not noticed for many years. Affects operation if
md raid is used a backing device for DRBD.

Signed-off-by: Philipp Reisner <philipp.reisner@linbit.com>
Signed-off-by: Lars Ellenberg <lars.ellenberg@linbit.com>
Signed-off-by: Jens Axboe <axboe@fb.com>
[lizf: Backported to 3.4: s/device/mdev]
Signed-off-by: Zefan Li <lizefan@huawei.com>

PCI: Restore detection of read-only BARs

commit 36e8164882ca6d3c41cb91e6f09a3ed236841f80 upstream.

Commit 6ac665c63dca ("PCI: rewrite PCI BAR reading code") masked off
low-order bits from 'l', but not from 'sz'.  Both are passed to pci_size(),
which compares 'base == maxbase' to check for read-only BARs.  The masking
of 'l' means that comparison will never be 'true', so the check for
read-only BARs no longer works.

Resolve this by also masking off the low-order bits of 'sz' before passing
it into pci_size() as 'maxbase'.  With this change, pci_size() will once
again catch the problems that have been encountered to date:

  - AGP aperture BAR of AMD-7xx host bridges: if the AGP window is
    disabled, this BAR is read-only and read as 0x00000008 [1]

  - BARs 0-4 of ALi IDE controllers can be non-zero and read-only [1]

  - Intel Sandy Bridge - Thermal Management Controller [8086:0103];
    BAR 0 returning 0xfed98004 [2]

  - Intel Xeon E5 v3/Core i7 Power Control Unit [8086:2fc0];
    Bar 0 returning 0x00001a [3]

Link: [1] https://git.kernel.org/cgit/linux/kernel/git/tglx/history.git/commit/drivers/pci/probe.c?id=1307ef6621991f1c4bc3cec1b5a4ebd6fd3d66b9 ("PCI: probing read-only BARs" (pre-git))
Link: [2] https://bugzilla.kernel.org/show_bug.cgi?id=43331
Link: [3] https://bugzilla.kernel.org/show_bug.cgi?id=85991
Reported-by: William Unruh <unruh@physics.ubc.ca>
Reported-by: Martin Lucina <martin@lucina.net>
Signed-off-by: Myron Stowe <myron.stowe@redhat.com>
Signed-off-by: Bjorn Helgaas <bhelgaas@google.com>
CC: Matthew Wilcox <willy@linux.intel.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

scsi: correct return values for .eh_abort_handler implementations

commit b6c92b7e0af575e2b8b05bdf33633cf9e1661cbf upstream.

The .eh_abort_handler needs to return SUCCESS, FAILED, or
FAST_IO_FAIL. So fixup all callers to adhere to this requirement.

Reviewed-by: Robert Elliott <elliott@hp.com>
Signed-off-by: Hannes Reinecke <hare@suse.de>
Signed-off-by: Christoph Hellwig <hch@lst.de>
[lizf: Backported to 3.4: drop changes to esas2r_main.c]
Signed-off-by: Zefan Li <lizefan@huawei.com>

genhd: check for int overflow in disk_expand_part_tbl()

commit 5fabcb4c33fe11c7e3afdf805fde26c1a54d0953 upstream.

We can get here from blkdev_ioctl() -> blkpg_ioctl() -> add_partition()
with a user passed in partno value. If we pass in 0x7fffffff, the
new target in disk_expand_part_tbl() overflows the 'int' and we
access beyond the end of ptbl->part[] and even write to it when we
do the rcu_assign_pointer() to assign the new partition.

Reported-by: David Ramos <daramos@stanford.edu>
Signed-off-by: Jens Axboe <axboe@fb.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ASoC: sigmadsp: Refuse to load firmware files with a non-supported version

commit 50c0f21b42dd4cd02b51f82274f66912d9a7fa32 upstream.

Make sure to check the version field of the firmware header to make sure to
not accidentally try to parse a firmware file with a different layout.
Trying to do so can result in loading invalid firmware code to the device.

Signed-off-by: Lars-Peter Clausen <lars@metafoo.de>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

megaraid_sas: corrected return of wait_event from abort frame path

commit 170c238701ec38b1829321b17c70671c101bac55 upstream.

Corrected wait_event() call which was waiting for wrong completion
status (0xFF).

Signed-off-by: Sumit Saxena <sumit.saxena@avagotech.com>
Signed-off-by: Kashyap Desai <kashyap.desai@avagotech.com>
Reviewed-by: Tomas Henzl <thenzl@redhat.com>
Signed-off-by: Christoph Hellwig <hch@lst.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

cdc-acm: memory leak in error case

commit d908f8478a8d18e66c80a12adb27764920c1f1ca upstream.

If probe() fails not only the attributes need to be removed
but also the memory freed.

Reported-by: Ahmed Tamrawi <ahmedtamrawi@gmail.com>
Signed-off-by: Oliver Neukum <oneukum@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: cdc-acm: check for valid interfaces

commit 403dff4e2c94f275e24fd85f40b2732ffec268a1 upstream.

We need to check that we have both a valid data and control inteface for both
types of headers (union and not union.)

References: https://bugzilla.kernel.org/show_bug.cgi?id=83551
Reported-by: Simon Schubert <2+kernel@0x2c.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mfd: tc6393xb: Fail ohci suspend if full state restore is required

commit 1a5fb99de4850cba710d91becfa2c65653048589 upstream.

Some boards with TC6393XB chip require full state restore during system
resume thanks to chip's VCC being cut off during suspend (Sharp SL-6000
tosa is one of them). Failing to do so would result in ohci Oops on
resume due to internal memory contentes being changed. Fail ohci suspend
on tc6393xb is full state restore is required.

Recommended workaround is to unbind tmio-ohci driver before suspend and
rebind it after resume.

Signed-off-by: Dmitry Eremin-Solenikov <dbaryshkov@gmail.com>
Signed-off-by: Lee Jones <lee.jones@linaro.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

serial: samsung: wait for transfer completion before clock disable

commit 1ff383a4c3eda8893ec61b02831826e1b1f46b41 upstream.

This patch adds waiting until transmit buffer and shifter will be empty
before clock disabling.

Without this fix it's possible to have clock disabled while data was
not transmited yet, which causes unproper state of TX line and problems
in following data transfers.

Signed-off-by: Robert Baldyga <r.baldyga@samsung.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ath9k_hw: fix hardware queue allocation

commit ad8fdccf9c197a89e2d2fa78c453283dcc2c343f upstream.

The driver passes the desired hardware queue index for a WMM data queue
in qinfo->tqi_subtype. This was ignored in ath9k_hw_setuptxqueue, which
instead relied on the order in which the function is called.

Reported-by: Hubert Feurstein <h.feurstein@gmail.com>
Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ath9k: fix BE/BK queue order

commit 78063d81d353e10cbdd279c490593113b8fdae1c upstream.

Hardware queues are ordered by priority. Use queue index 0 for BK, which
has lower priority than BE.

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ath5k: fix hardware queue index assignment

commit 9e4982f6a51a2442f1bb588fee42521b44b4531c upstream.

Like with ath9k, ath5k queues also need to be ordered by priority.
queue_info->tqi_subtype already contains the correct index, so use it
instead of relying on the order of ath5k_hw_setup_tx_queue calls.

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

iommu/vt-d: Fix an off-by-one bug in __domain_mapping()

commit cc4f14aa170d895c9a43bdb56f62070c8a6da908 upstream.

There's an off-by-one bug in function __domain_mapping(), which may
trigger the BUG_ON(nr_pages < lvl_pages) when
	(nr_pages + 1) & superpage_mask == 0

The issue was introduced by commit 9051aa0268dc "intel-iommu: Combine
domain_pfn_mapping() and domain_sg_mapping()", which sets sg_res to
"nr_pages + 1" to avoid some of the 'sg_res==0' code paths.

It's safe to remove extra "+1" because sg_res is only used to calculate
page size now.

Reported-And-Tested-by: Sudeep Dutt <sudeep.dutt@intel.com>
Signed-off-by: Jiang Liu <jiang.liu@linux.intel.com>
Acked-By: David Woodhouse <David.Woodhouse@intel.com>
Signed-off-by: Joerg Roedel <jroedel@suse.de>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/vmwgfx: Don't use memory accounting for kernel-side fence objects

commit 1f563a6a46544602183e7493b6ef69769d3d76d9 upstream.

Kernel side fence objects are used when unbinding resources and may thus be
created as part of a memory reclaim operation. This might trigger recursive
memory reclaims and result in the kernel running out of stack space.

So a simple way out is to avoid accounting of these fence objects.
In principle this is OK since while user-space can trigger the creation of
such objects, it can't really hold on to them. However, their lifetime is
quite long, so some form of accounting should perhaps be implemented in the
future.

Fixes kernel crashes when running, for example viewperf11 ensight-04 test 3
with low system memory settings.

Signed-off-by: Thomas Hellstrom <thellstrom@vmware.com>
Reviewed-by: Jakob Bornecrantz <jakob@vmware.com>
Reviewed-by: Sinclair Yeh <syeh@vmware.com>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/vmwgfx: Fix fence event code

commit 89669e7a7f96be3ee8d9a22a071d7c0d3b4428fc upstream.

The commit "vmwgfx: Rework fence event action" introduced a number of bugs
that are fixed with this commit:

a) A forgotten return stateemnt.
b) An if statement with identical branches.

Reported-by: Rob Clark <robdclark@gmail.com>
Signed-off-by: Thomas Hellstrom <thellstrom@vmware.com>
Reviewed-by: Jakob Bornecrantz <jakob@vmware.com>
Reviewed-by: Sinclair Yeh <syeh@vmware.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

hp_accel: Add support for HP ZBook 15

commit 6583659e0f92e38079a8dd081e0a1181a0f37747 upstream.

HP ZBook 15 laptop needs a non-standard mapping (x_inverted).

BugLink: http://bugzilla.opensuse.org/show_bug.cgi?id=905329
Signed-off-by: Dominique Leuenberger <dimstar@opensuse.org>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Darren Hart <dvhart@linux.intel.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/radeon: check the right ring in radeon_evict_flags()

commit 5e5c21cac1001089007260c48b0c89ebaace0e71 upstream.

Check the that ring we are using for copies is functional
rather than the GFX ring.  On newer asics we use the DMA
ring for bo moves.

Reviewed-by: Christian König <christian.koenig@amd.com>
Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

can: peak_usb: fix memset() usage

commit dc50ddcd4c58a5a0226038307d6ef884bec9f8c2 upstream.

This patchs fixes a misplaced call to memset() that fills the request
buffer with 0. The problem was with sending PCAN_USBPRO_REQ_FCT
requests, the content set by the caller was thus lost.

With this patch, the memory area is zeroed only when requesting info
from the device.

Signed-off-by: Stephane Grosjean <s.grosjean@peak-system.com>
Signed-off-by: Marc Kleine-Budde <mkl@pengutronix.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

can: peak_usb: fix cleanup sequence order in case of error during init

commit af35d0f1cce7a990286e2b94c260a2c2d2a0e4b0 upstream.

This patch sets the correct reverse sequence order to the instructions
set to run, when any failure occurs during the initialization steps.
It also adds the missing unregistration call of the can device if the
failure appears after having been registered.

Signed-off-by: Stephane Grosjean <s.grosjean@peak-system.com>
Signed-off-by: Marc Kleine-Budde <mkl@pengutronix.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: usb-audio: Don't resubmit pending URBs at MIDI error recovery

commit 66139a48cee1530c91f37c145384b4ee7043f0b7 upstream.

In snd_usbmidi_error_timer(), the driver tries to resubmit MIDI input
URBs to reactivate the MIDI stream, but this causes the error when
some of URBs are still pending like:

 WARNING: CPU: 0 PID: 0 at ../drivers/usb/core/urb.c:339 usb_submit_urb+0x5f/0x70()
 URB ef705c40 submitted while active
 CPU: 0 PID: 0 Comm: swapper/0 Not tainted 3.16.6-2-desktop #1
 Hardware name: FOXCONN TPS01/TPS01, BIOS 080015  03/23/2010
  c0984bfa f4009ed4 c078deaf f4009ee4 c024c884 c09a135c f4009f00 00000000
  c0984bfa 00000153 c061ac4f c061ac4f 00000009 00000001 ef705c40 e854d1c0
  f4009eec c024c8d3 00000009 f4009ee4 c09a135c f4009f00 f4009f04 c061ac4f
 Call Trace:
  [<c0205df6>] try_stack_unwind+0x156/0x170
  [<c020482a>] dump_trace+0x5a/0x1b0
  [<c0205e56>] show_trace_log_lvl+0x46/0x50
  [<c02049d1>] show_stack_log_lvl+0x51/0xe0
  [<c0205eb7>] show_stack+0x27/0x50
  [<c078deaf>] dump_stack+0x45/0x65
  [<c024c884>] warn_slowpath_common+0x84/0xa0
  [<c024c8d3>] warn_slowpath_fmt+0x33/0x40
  [<c061ac4f>] usb_submit_urb+0x5f/0x70
  [<f7974104>] snd_usbmidi_submit_urb+0x14/0x60 [snd_usbmidi_lib]
  [<f797483a>] snd_usbmidi_error_timer+0x6a/0xa0 [snd_usbmidi_lib]
  [<c02570c0>] call_timer_fn+0x30/0x130
  [<c0257442>] run_timer_softirq+0x1c2/0x260
  [<c0251493>] __do_softirq+0xc3/0x270
  [<c0204732>] do_softirq_own_stack+0x22/0x30
  [<c025186d>] irq_exit+0x8d/0xa0
  [<c0795228>] smp_apic_timer_interrupt+0x38/0x50
  [<c0794a3c>] apic_timer_interrupt+0x34/0x3c
  [<c0673d9e>] cpuidle_enter_state+0x3e/0xd0
  [<c028bb8d>] cpu_idle_loop+0x29d/0x3e0
  [<c028bd23>] cpu_startup_entry+0x53/0x60
  [<c0bfac1e>] start_kernel+0x415/0x41a

For avoiding these errors, check the pending URBs and skip
resubmitting such ones.

Reported-and-tested-by: Stefan Seyfried <stefan.seyfried@googlemail.com>
Acked-by: Clemens Ladisch <clemens@ladisch.de>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

KEYS: Fix stale key registration at error path

commit b26bdde5bb27f3f900e25a95e33a0c476c8c2c48 upstream.

When loading encrypted-keys module, if the last check of
aes_get_sizes() in init_encrypted() fails, the driver just returns an
error without unregistering its key type.  This results in the stale
entry in the list.  In addition to memory leaks, this leads to a kernel
crash when registering a new key type later.

This patch fixes the problem by swapping the calls of aes_get_sizes()
and register_key_type(), and releasing resources properly at the error
paths.

Bugzilla: https://bugzilla.opensuse.org/show_bug.cgi?id=908163
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Mimi Zohar <zohar@linux.vnet.ibm.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

Btrfs: fix fs corruption on transaction abort if device supports discard

commit 678886bdc6378c1cbd5072da2c5a3035000214e3 upstream.

When we abort a transaction we iterate over all the ranges marked as dirty
in fs_info->freed_extents[0] and fs_info->freed_extents[1], clear them
from those trees, add them back (unpin) to the free space caches and, if
the fs was mounted with "-o discard", perform a discard on those regions.
Also, after adding the regions to the free space caches, a fitrim ioctl call
can see those ranges in a block group's free space cache and perform a discard
on the ranges, so the same issue can happen without "-o discard" as well.

This causes corruption, affecting one or multiple btree nodes (in the worst
case leaving the fs unmountable) because some of those ranges (the ones in
the fs_info->pinned_extents tree) correspond to btree nodes/leafs that are
referred by the last committed super block - breaking the rule that anything
that was committed by a transaction is untouched until the next transaction
commits successfully.

I ran into this while running in a loop (for several hours) the fstest that
I recently submitted:

  [PATCH] fstests: add btrfs test to stress chunk allocation/removal and fstrim

The corruption always happened when a transaction aborted and then fsck complained
like this:

   _check_btrfs_filesystem: filesystem on /dev/sdc is inconsistent
   *** fsck.btrfs output ***
   Check tree block failed, want=94945280, have=0
   Check tree block failed, want=94945280, have=0
   Check tree block failed, want=94945280, have=0
   Check tree block failed, want=94945280, have=0
   Check tree block failed, want=94945280, have=0
   read block failed check_tree_block
   Couldn't open file system

In this case 94945280 corresponded to the root of a tree.
Using frace what I observed was the following sequence of steps happened:

   1) transaction N started, fs_info->pinned_extents pointed to
      fs_info->freed_extents[0];

   2) node/eb 94945280 is created;

   3) eb is persisted to disk;

   4) transaction N commit starts, fs_info->pinned_extents now points to
      fs_info->freed_extents[1], and transaction N completes;

   5) transaction N + 1 starts;

   6) eb is COWed, and btrfs_free_tree_block() called for this eb;

   7) eb range (94945280 to 94945280 + 16Kb) is added to
      fs_info->pinned_extents (fs_info->freed_extents[1]);

   8) Something goes wrong in transaction N + 1, like hitting ENOSPC
      for example, and the transaction is aborted, turning the fs into
      readonly mode. The stack trace I got for example:

      [112065.253935]  [<ffffffff8140c7b6>] dump_stack+0x4d/0x66
      [112065.254271]  [<ffffffff81042984>] warn_slowpath_common+0x7f/0x98
      [112065.254567]  [<ffffffffa0325990>] ? __btrfs_abort_transaction+0x50/0x10b [btrfs]
      [112065.261674]  [<ffffffff810429e5>] warn_slowpath_fmt+0x48/0x50
      [112065.261922]  [<ffffffffa032949e>] ? btrfs_free_path+0x26/0x29 [btrfs]
      [112065.262211]  [<ffffffffa0325990>] __btrfs_abort_transaction+0x50/0x10b [btrfs]
      [112065.262545]  [<ffffffffa036b1d6>] btrfs_remove_chunk+0x537/0x58b [btrfs]
      [112065.262771]  [<ffffffffa033840f>] btrfs_delete_unused_bgs+0x1de/0x21b [btrfs]
      [112065.263105]  [<ffffffffa0343106>] cleaner_kthread+0x100/0x12f [btrfs]
      (...)
      [112065.264493] ---[ end trace dd7903a975a31a08 ]---
      [112065.264673] BTRFS: error (device sdc) in btrfs_remove_chunk:2625: errno=-28 No space left
      [112065.264997] BTRFS info (device sdc): forced readonly

   9) The clear kthread sees that the BTRFS_FS_STATE_ERROR bit is set in
      fs_info->fs_state and calls btrfs_cleanup_transaction(), which in
      turn calls btrfs_destroy_pinned_extent();

   10) Then btrfs_destroy_pinned_extent() iterates over all the ranges
       marked as dirty in fs_info->freed_extents[], and for each one
       it calls discard, if the fs was mounted with "-o discard", and
       adds the range to the free space cache of the respective block
       group;

   11) btrfs_trim_block_group(), invoked from the fitrim ioctl code path,
       sees the free space entries and performs a discard;

   12) After an umount and mount (or fsck), our eb's location on disk was full
       of zeroes, and it should have been untouched, because it was marked as
       dirty in the fs_info->pinned_extents tree, and therefore used by the
       trees that the last committed superblock points to.

Fix this by not performing a discard and not adding the ranges to the free space
caches - it's useless from this point since the fs is now in readonly mode and
we won't write free space caches to disk anymore (otherwise we would leak space)
nor any new superblock. By not adding the ranges to the free space caches, it
prevents other code paths from allocating that space and write to it as well,
therefore being safer and simpler.

This isn't a new problem, as it's been present since 2011 (git commit
acce952b0263825da32cf10489413dec78053347).

Signed-off-by: Filipe Manana <fdmanana@suse.com>
Signed-off-by: Chris Mason <clm@fb.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ncpfs: return proper error from NCP_IOC_SETROOT ioctl

commit a682e9c28cac152e6e54c39efcf046e0c8cfcf63 upstream.

If some error happens in NCP_IOC_SETROOT ioctl, the appropriate error
return value is then (in most cases) just overwritten before we return.
This can result in reporting success to userspace although error happened.

This bug was introduced by commit 2e54eb96e2c8 ("BKL: Remove BKL from
ncpfs").  Propagate the errors correctly.

Coverity id: 1226925.

Fixes: 2e54eb96e2c80 ("BKL: Remove BKL from ncpfs")
Signed-off-by: Jan Kara <jack@suse.cz>
Cc: Petr Vandrovec <petr@vandrovec.name>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86_64, switch_to(): Load TLS descriptors before switching DS and ES

commit f647d7c155f069c1a068030255c300663516420e upstream.

Otherwise, if buggy user code points DS or ES into the TLS
array, they would be corrupted after a context switch.

This also significantly improves the comments and documents some
gotchas in the code.

Before this patch, the both tests below failed.  With this
patch, the es test passes, although the gsbase test still fails.

 ----- begin es test -----

/*
 * Copyright (c) 2014 Andy Lutomirski
 * GPL v2
 */

static unsigned short GDT3(int idx)
{
	return (idx << 3) | 3;
}

static int create_tls(int idx, unsigned int base)
{
	struct user_desc desc = {
		.entry_number    = idx,
		.base_addr       = base,
		.limit           = 0xfffff,
		.seg_32bit       = 1,
		.contents        = 0, /* Data, grow-up */
		.read_exec_only  = 0,
		.limit_in_pages  = 1,
		.seg_not_present = 0,
		.useable         = 0,
	};

	if (syscall(SYS_set_thread_area, &desc) != 0)
		err(1, "set_thread_area");

	return desc.entry_number;
}

int main()
{
	int idx = create_tls(-1, 0);
	printf("Allocated GDT index %d\n", idx);

	unsigned short orig_es;
	asm volatile ("mov %%es,%0" : "=rm" (orig_es));

	int errors = 0;
	int total = 1000;
	for (int i = 0; i < total; i++) {
		asm volatile ("mov %0,%%es" : : "rm" (GDT3(idx)));
		usleep(100);

		unsigned short es;
		asm volatile ("mov %%es,%0" : "=rm" (es));
		asm volatile ("mov %0,%%es" : : "rm" (orig_es));
		if (es != GDT3(idx)) {
			if (errors == 0)
				printf("[FAIL]\tES changed from 0x%hx to 0x%hx\n",
				       GDT3(idx), es);
			errors++;
		}
	}

	if (errors) {
		printf("[FAIL]\tES was corrupted %d/%d times\n", errors, total);
		return 1;
	} else {
		printf("[OK]\tES was preserved\n");
		return 0;
	}
}

 ----- end es test -----

 ----- begin gsbase test -----

/*
 * gsbase.c, a gsbase test
 * Copyright (c) 2014 Andy Lutomirski
 * GPL v2
 */

static unsigned char *testptr, *testptr2;

static unsigned char read_gs_testvals(void)
{
	unsigned char ret;
	asm volatile ("movb %%gs:%1, %0" : "=r" (ret) : "m" (*testptr));
	return ret;
}

int main()
{
	int errors = 0;

	testptr = mmap((void *)0x200000000UL, 1, PROT_READ | PROT_WRITE,
		       MAP_PRIVATE | MAP_FIXED | MAP_ANONYMOUS, -1, 0);
	if (testptr == MAP_FAILED)
		err(1, "mmap");

	testptr2 = mmap((void *)0x300000000UL, 1, PROT_READ | PROT_WRITE,
		       MAP_PRIVATE | MAP_FIXED | MAP_ANONYMOUS, -1, 0);
	if (testptr2 == MAP_FAILED)
		err(1, "mmap");

	*testptr = 0;
	*testptr2 = 1;

	if (syscall(SYS_arch_prctl, ARCH_SET_GS,
		    (unsigned long)testptr2 - (unsigned long)testptr) != 0)
		err(1, "ARCH_SET_GS");

	usleep(100);

	if (read_gs_testvals() == 1) {
		printf("[OK]\tARCH_SET_GS worked\n");
	} else {
		printf("[FAIL]\tARCH_SET_GS failed\n");
		errors++;
	}

	asm volatile ("mov %0,%%gs" : : "r" (0));

	if (read_gs_testvals() == 0) {
		printf("[OK]\tWriting 0 to gs worked\n");
	} else {
		printf("[FAIL]\tWriting 0 to gs failed\n");
		errors++;
	}

	usleep(100);

	if (read_gs_testvals() == 0) {
		printf("[OK]\tgsbase is still zero\n");
	} else {
		printf("[FAIL]\tgsbase was corrupted\n");
		errors++;
	}

	return errors == 0 ? 0 : 1;
}

 ----- end gsbase test -----

Signed-off-by: Andy Lutomirski <luto@amacapital.net>
Cc: Andi Kleen <andi@firstfloor.org>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Link: http://lkml.kernel.org/r/509d27c9fec78217691c3dad91cec87e1006b34a.1418075657.git.luto@amacapital.net
Signed-off-by: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

genirq: Prevent proc race against freeing of irq descriptors

commit c291ee622165cb2c8d4e7af63fffd499354a23be upstream.

Since the rework of the sparse interrupt code to actually free the
unused interrupt descriptors there exists a race between the /proc
interfaces to the irq subsystem and the code which frees the interrupt
descriptor.

CPU0				CPU1
				show_interrupts()
				  desc = irq_to_desc(X);
free_desc(desc)
  remove_from_radix_tree();
  kfree(desc);
				  raw_spinlock_irq(&desc->lock);

/proc/interrupts is the only interface which can actively corrupt
kernel memory via the lock access. /proc/stat can only read from freed
memory. Extremly hard to trigger, but possible.

The interfaces in /proc/irq/N/ are not affected by this because the
removal of the proc file is serialized in procfs against concurrent
readers/writers. The removal happens before the descriptor is freed.

For architectures which have CONFIG_SPARSE_IRQ=n this is a non issue
as the descriptor is never freed. It's merely cleared out with the irq
descriptor lock held. So any concurrent proc access will either see
the old correct value or the cleared out ones.

Protect the lookup and access to the irq descriptor in
show_interrupts() with the sparse_irq_lock.

Provide kstat_irqs_usr() which is protecting the lookup and access
with sparse_irq_lock and switch /proc/stat to use it.

Document the existing kstat_irqs interfaces so it's clear that the
caller needs to take care about protection. The users of these
interfaces are either not affected due to SPARSE_IRQ=n or already
protected against removal.

Fixes: 1f5a5b87f78f "genirq: Implement a sane sparse_irq allocator"
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
[lizf: Backported to 3.4:
 - define kstat_irqs() for CONFIG_GENERIC_HARDIRQS
 - add ifdef/endif CONFIG_SPARSE_IRQ]
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86/tls: Disallow unusual TLS segments

commit 0e58af4e1d2166e9e33375a0f121e4867010d4f8 upstream.

Users have no business installing custom code segments into the
GDT, and segments that are not present but are otherwise valid
are a historical source of interesting attacks.

For completeness, block attempts to set the L bit.  (Prior to
this patch, the L bit would have been silently dropped.)

This is an ABI break.  I've checked glibc, musl, and Wine, and
none of them look like they'll have any trouble.

Note to stable maintainers: this is a hardening patch that fixes
no known bugs.  Given the possibility of ABI issues, this
probably shouldn't be backported quickly.

Signed-off-by: Andy Lutomirski <luto@amacapital.net>
Acked-by: H. Peter Anvin <hpa@zytor.com>
Cc: Konrad Rzeszutek Wilk <konrad.wilk@oracle.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: security@kernel.org <security@kernel.org>
Cc: Willy Tarreau <w@1wt.eu>
Signed-off-by: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86/tls: Don't validate lm in set_thread_area() after all

commit 3fb2f4237bb452eb4e98f6a5dbd5a445b4fed9d0 upstream.

It turns out that there's a lurking ABI issue.  GCC, when
compiling this in a 32-bit program:

struct user_desc desc = {
	.entry_number    = idx,
	.base_addr       = base,
	.limit           = 0xfffff,
	.seg_32bit       = 1,
	.contents        = 0, /* Data, grow-up */
	.read_exec_only  = 0,
	.limit_in_pages  = 1,
	.seg_not_present = 0,
	.useable         = 0,
};

will leave .lm uninitialized.  This means that anything in the
kernel that reads user_desc.lm for 32-bit tasks is unreliable.

Revert the .lm check in set_thread_area().  The value never did
anything in the first place.

Fixes: 0e58af4e1d21 ("x86/tls: Disallow unusual TLS segments")
Signed-off-by: Andy Lutomirski <luto@amacapital.net>
Acked-by: Thomas Gleixner <tglx@linutronix.de>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Link: http://lkml.kernel.org/r/d7875b60e28c512f6a6fc0baf5714d58e7eaadbb.1418856405.git.luto@amacapital.net
Signed-off-by: Ingo Molnar <mingo@kernel.org>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

storvsc: ring buffer failures may result in I/O freeze

commit e86fb5e8ab95f10ec5f2e9430119d5d35020c951 upstream.

When ring buffer returns an error indicating retry, storvsc may not
return a proper error code to SCSI when bounce buffer is not used.
This has introduced I/O freeze on RAID running atop storvsc devices.
This patch fixes it by always returning a proper error code.

Signed-off-by: Long Li <longli@microsoft.com>
Reviewed-by: K. Y. Srinivasan <kys@microsoft.com>
Signed-off-by: Christoph Hellwig <hch@lst.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

isofs: Fix infinite looping over CE entries

commit f54e18f1b831c92f6512d2eedb224cd63d607d3d upstream.

Rock Ridge extensions define so called Continuation Entries (CE) which
define where is further space with Rock Ridge data. Corrupted isofs
image can contain arbitrarily long chain of these, including a one
containing loop and thus causing kernel to end in an infinite loop when
traversing these entries.

Limit the traversal to 32 entries which should be more than enough space
to store all the Rock Ridge data.

Reported-by: P J P <ppandit@redhat.com>
Signed-off-by: Jan Kara <jack@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

iscsi-target: Fail connection on short sendmsg writes

commit 6bf6ca7515c1df06f5c03737537f5e0eb191e29e upstream.

This patch changes iscsit_do_tx_data() to fail on short writes
when kernel_sendmsg() returns a value different than requested
transfer length, returning -EPIPE and thus causing a connection
reset to occur.

This avoids a potential bug in the original code where a short
write would result in kernel_sendmsg() being called again with
the original iovec base + length.

In practice this has not been an issue because iscsit_do_tx_data()
is only used for transferring 48 byte headers + 4 byte digests,
along with seldom used control payloads from NOPIN + TEXT_RSP +
REJECT with less than 32k of data.

So following Al's audit of iovec consumers, go ahead and fail
the connection on short writes for now, and remove the bogus
logic ahead of his proper upstream fix.

Reported-by: Al Viro <viro@zeniv.linux.org.uk>
Cc: David S. Miller <davem@davemloft.net>
Signed-off-by: Nicholas Bellinger <nab@linux-iscsi.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: usb-audio: extend KEF X300A FU 10 tweak to Arcam rPAC

commit d70a1b9893f820fdbcdffac408c909c50f2e6b43 upstream.

The Arcam rPAC seems to have the same problem - whenever anything
(alsamixer, udevd, 3.9+ kernel from 60af3d037eb8c, ..) attempts to
access mixer / control interface of the card, the firmware "locks up"
the entire device, resulting in
  SNDRV_PCM_IOCTL_HW_PARAMS failed (-5): Input/output error
from alsa-lib.

Other operating systems can somehow read the mixer (there seems to be
playback volume/mute), but any manipulation is ignored by the device
(which has hardware volume controls).

Signed-off-by: Jiri Jaburek <jjaburek@redhat.com>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ocfs2: fix journal commit deadlock

commit 136f49b9171074872f2a14ad0ab10486d1ba13ca upstream.

For buffer write, page lock will be got in write_begin and released in
write_end, in ocfs2_write_end_nolock(), before it unlock the page in
ocfs2_free_write_ctxt(), it calls ocfs2_run_deallocs(), this will ask
for the read lock of journal->j_trans_barrier.  Holding page lock and
ask for journal->j_trans_barrier breaks the locking order.

This will cause a deadlock with journal commit threads, ocfs2cmt will
get write lock of journal->j_trans_barrier first, then it wakes up
kjournald2 to do the commit work, at last it waits until done.  To
commit journal, kjournald2 needs flushing data first, it needs get the
cache page lock.

Since some ocfs2 cluster locks are holding by write process, this
deadlock may hung the whole cluster.

unlock pages before ocfs2_run_deallocs() can fix the locking order, also
put unlock before ocfs2_commit_trans() to make page lock is unlocked
before j_trans_barrier to preserve unlocking order.

Signed-off-by: Junxiao Bi <junxiao.bi@oracle.com>
Reviewed-by: Wengang Wang <wen.gang.wang@oracle.com>
Reviewed-by: Mark Fasheh <mfasheh@suse.de>
Cc: Joel Becker <jlbec@evilplan.org>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

isofs: Fix unchecked printing of ER records

commit 4e2024624e678f0ebb916e6192bd23c1f9fdf696 upstream.

We didn't check length of rock ridge ER records before printing them.
Thus corrupted isofs image can cause us to access and print some memory
behind the buffer with obvious consequences.

Reported-and-tested-by: Carl Henrik Lunde <chlunde@ping.uio.no>
Signed-off-by: Jan Kara <jack@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

udf: Verify i_size when loading inode

commit e159332b9af4b04d882dbcfe1bb0117f0a6d4b58 upstream.

Verify that inode size is sane when loading inode with data stored in
ICB. Otherwise we may get confused later when working with the inode and
inode size is too big.

Reported-by: Carl Henrik Lunde <chlunde@ping.uio.no>
Signed-off-by: Jan Kara <jack@suse.cz>
[lizf: Backported to 3.4: just return on error, as there's no "out" label]
Signed-off-by: Zefan Li <lizefan@huawei.com>

udf: Verify symlink size before loading it

commit a1d47b262952a45aae62bd49cfaf33dd76c11a2c upstream.

UDF specification allows arbitrarily large symlinks. However we support
only symlinks at most one block large. Check the length of the symlink
so that we don't access memory beyond end of the symlink block.

Reported-by: Carl Henrik Lunde <chlunde@gmail.com>
Signed-off-by: Jan Kara <jack@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

udf: Check path length when reading symlink

commit 0e5cc9a40ada6046e6bc3bdfcd0c0d7e4b706b14 upstream.

Symlink reading code does not check whether the resulting path fits into
the page provided by the generic code. This isn't as easy as just
checking the symlink size because of various encoding conversions we
perform on path. So we have to check whether there is still enough space
in the buffer on the fly.

Reported-by: Carl Henrik Lunde <chlunde@ping.uio.no>
Signed-off-by: Jan Kara <jack@suse.cz>
[lizf: Backported to 3.4: udf_get_filename() is called in do_udf_readdir()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86_64, vdso: Fix the vdso address randomization algorithm

commit 394f56fe480140877304d342dec46d50dc823d46 upstream.

The theory behind vdso randomization is that it's mapped at a random
offset above the top of the stack.  To avoid wasting a page of
memory for an extra page table, the vdso isn't supposed to extend
past the lowest PMD into which it can fit.  Other than that, the
address should be a uniformly distributed address that meets all of
the alignment requirements.

The current algorithm is buggy: the vdso has about a 50% probability
of being at the very end of a PMD.  The current algorithm also has a
decent chance of failing outright due to incorrect handling of the
case where the top of the stack is near the top of its PMD.

This fixes the implementation.  The paxtest estimate of vdso
"randomisation" improves from 11 bits to 18 bits.  (Disclaimer: I
don't know what the paxtest code is actually calculating.)

It's worth noting that this algorithm is inherently biased: the vdso
is more likely to end up near the end of its PMD than near the
beginning.  Ideally we would either nix the PMD sharing requirement
or jointly randomize the vdso and the stack to reduce the bias.

In the mean time, this is a considerable improvement with basically
no risk of compatibility issues, since the allowed outputs of the
algorithm are unchanged.

As an easy test, doing this:

for i in `seq 10000`
  do grep -P vdso /proc/self/maps |cut -d- -f1
done |sort |uniq -d

used to produce lots of output (1445 lines on my most recent run).
A tiny subset looks like this:

7fffdfffe000
7fffe01fe000
7fffe05fe000
7fffe07fe000
7fffe09fe000
7fffe0bfe000
7fffe0dfe000

Note the suspicious fe000 endings.  With the fix, I get a much more
palatable 76 repeated addresses.

Reviewed-by: Kees Cook <keescook@chromium.org>
Signed-off-by: Andy Lutomirski <luto@amacapital.net>
[lizf: Backported to 3.4:
 - adjust context
 - adjust comment]
Signed-off-by: Zefan Li <lizefan@huawei.com>

udf: Check component length before reading it

commit e237ec37ec154564f8690c5bd1795339955eeef9 upstream.

Check that length specified in a component of a symlink fits in the
input buffer we are reading. Also properly ignore component length for
component types that do not use it. Otherwise we read memory after end
of buffer for corrupted udf image.

Reported-by: Carl Henrik Lunde <chlunde@ping.uio.no>
Signed-off-by: Jan Kara <jack@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

crypto: af_alg - fix backlog handling

commit 7e77bdebff5cb1e9876c561f69710b9ab8fa1f7e upstream.

If a request is backlogged, it's complete() handler will get called
twice: once with -EINPROGRESS, and once with the final error code.

af_alg's complete handler, unlike other users, does not handle the
-EINPROGRESS but instead always completes the completion that recvmsg()
is waiting on.  This can lead to a return to user space while the
request is still pending in the driver.  If userspace closes the sockets
before the requests are handled by the driver, this will lead to
use-after-frees (and potential crashes) in the kernel due to the tfm
having been freed.

The crashes can be easily reproduced (for example) by reducing the max
queue length in cryptod.c and running the following (from
http://www.chronox.de/libkcapi.html) on AES-NI capable hardware:

 $ while true; do kcapi -x 1 -e -c '__ecb-aes-aesni' \
    -k 00000000000000000000000000000000 \
    -p 00000000000000000000000000000000 >/dev/null & done

Signed-off-by: Rabin Vincent <rabin.vincent@axis.com>
Signed-off-by: Herbert Xu <herbert@gondor.apana.org.au>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: Fix stacked vlan offload features computation

commit 796f2da81bead71ffc91ef70912cd8d1827bf756 upstream.

When vlan tags are stacked, it is very likely that the outer tag is stored
in skb->vlan_tci and skb->protocol shows the inner tag's vlan_proto.
Currently netif_skb_features() first looks at skb->protocol even if there
is the outer tag in vlan_tci, thus it incorrectly retrieves the protocol
encapsulated by the inner vlan instead of the inner vlan protocol.
This allows GSO packets to be passed to HW and they end up being
corrupted.

Fixes: 58e998c6d239 ("offloading: Force software GSO for multiple vlan tags.")
Signed-off-by: Toshiaki Makita <makita.toshiaki@lab.ntt.co.jp>
Signed-off-by: David S. Miller <davem@davemloft.net>
[lizf: Backported to 3.4:
 - remove ETH_P_8021AD
 - pass protocol to harmonize_features()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

video/logo: prevent use of logos after they have been freed

commit 92b004d1aa9f367c372511ca0330f58216b25703 upstream.

If the probe of an fb driver has been deferred due to missing
dependencies, and the probe is later ran when a module is loaded, the
fbdev framework will try to find a logo to use.

However, the logos are __initdata, and have already been freed. This
causes sometimes page faults, if the logo memory is not mapped,
sometimes other random crashes as the logo data is invalid, and
sometimes nothing, if the fbdev decides to reject the logo (e.g. the
random value depicting the logo's height is too big).

This patch adds a late_initcall function to mark the logos as freed. In
reality the logos are freed later, and fbdev probe may be ran between
this late_initcall and the freeing of the logos. In that case we will
miss drawing the logo, even if it would be possible.

Signed-off-by: Tomi Valkeinen <tomi.valkeinen@ti.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: cp210x: fix ID for production CEL MeshConnect USB Stick

commit 90441b4dbe90ba0c38111ea89fa093a8c9627801 upstream.

Fixing typo for MeshConnect IDs. The original PID (0x8875) is not in
production and is not needed. Instead it has been changed to the
official production PID (0x8857).

Signed-off-by: Preston Fick <pffick@gmail.com>
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86, um: actually mark system call tables readonly

commit b485342bd79af363c77ef1a421c4a0aef2de9812 upstream.

Commit a074335a370e ("x86, um: Mark system call tables readonly") was
supposed to mark the sys_call_table in UML as RO by adding the const,
but it doesn't have the desired effect as it's nevertheless being placed
into the data section since __cacheline_aligned enforces sys_call_table
being placed into .data..cacheline_aligned instead. We need to use
the ____cacheline_aligned version instead to fix this issue.

Before:

$ nm -v arch/x86/um/sys_call_table_64.o | grep -1 "sys_call_table"
                 U sys_writev
0000000000000000 D sys_call_table
0000000000000000 D syscall_table_size

After:

$ nm -v arch/x86/um/sys_call_table_64.o | grep -1 "sys_call_table"
                 U sys_writev
0000000000000000 R sys_call_table
0000000000000000 D syscall_table_size

Fixes: a074335a370e ("x86, um: Mark system call tables readonly")
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Signed-off-by: Richard Weinberger <richard@nod.at>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: hda - Fix wrong gpio_dir & gpio_mask hint setups for IDT/STAC codecs

commit c507de88f6a336bd7296c9ec0073b2d4af8b4f5e upstream.

stac_store_hints() does utterly wrong for masking the values for
gpio_dir and gpio_data, likely due to copy&paste errors.  Fortunately,
this feature is used very rarely, so the impact must be really small.

Reported-by: Rasmus Villemoes <linux@rasmusvillemoes.dk>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

virtio: use dev_to_virtio wrapper in virtio

commit 9bffdca8c64a72ac54c47a552734ab457bc720d4 upstream.

Use dev_to_virtio wrapper in virtio to make code clearly.

Cc: Rusty Russell <rusty@rustcorp.com.au>
Cc: "Michael S. Tsirkin" <mst@redhat.com>
Signed-off-by: Wanlong Gao <gaowanlong@cn.fujitsu.com>
Signed-off-by: Rusty Russell <rusty@rustcorp.com.au>
Signed-off-by: Zefan Li <lizefan@huawei.com>

virtio_pci: defer kfree until release callback

commit 63bd62a08ca45a0c804c3c89777edc7f76a2d6da upstream.

A struct device which has just been unregistered can live on past the
point at which a driver decides to drop it's initial reference to the
kobject gained on allocation.

This implies that when releasing a virtio device, we can't free a struct
virtio_device until the underlying struct device has been released,
which might not happen immediately on device_unregister().

Unfortunately, this is exactly what virtio pci does:
it has an empty release callback, and frees memory immediately
after unregistering the device.

This causes an easy to reproduce crash if CONFIG_DEBUG_KOBJECT_RELEASE
it enabled.

To fix, free the memory only once we know the device is gone in the release
callback.

Signed-off-by: Sasha Levin <sasha.levin@oracle.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

virtio_pci: document why we defer kfree

commit a1eb03f546d651a8f39c7d0692b1f7f5b4e7e3cd upstream.

The reason we defer kfree until release function is because it's a
general rule for kobjects: kfree of the reference counter itself is only
legal in the release function.

Previous patch didn't make this clear, document this in code.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: cp210x: add IDs for CEL USB sticks and MeshWorks devices

commit 1ae78a4870989a354028cb17dabf819b595e70e3 upstream.

Added virtual com port VID/PID entries for CEL USB sticks and MeshWorks
devices.

Signed-off-by: David Peterson <david.peterson@cel.com>
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: propagate error from stack expansion even for guard page

commit fee7e49d45149fba60156f5b59014f764d3e3728 upstream.

Jay Foad reports that the address sanitizer test (asan) sometimes gets
confused by a stack pointer that ends up being outside the stack vma
that is reported by /proc/maps.

This happens due to an interaction between RLIMIT_STACK and the guard
page: when we do the guard page check, we ignore the potential error
from the stack expansion, which effectively results in a missing guard
page, since the expected stack expansion won't have been done.

And since /proc/maps explicitly ignores the guard page (commit
d7824370e263: "mm: fix up some user-visible effects of the stack guard
page"), the stack pointer ends up being outside the reported stack area.

This is the minimal patch: it just propagates the error.  It also
effectively makes the guard page part of the stack limit, which in turn
measn that the actual real stack is one page less than the stack limit.

Let's see if anybody notices.  We could teach acct_stack_growth() to
allow an extra page for a grow-up/grow-down stack in the rlimit test,
but I don't want to add more complexity if it isn't needed.

Reported-and-tested-by: Jay Foad <jay.foad@gmail.com>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

sata_dwc_460ex: fix resource leak on error path

commit 4aaa71873ddb9faf4b0c4826579e2f6d18ff9ab4 upstream.

DMA mapped IO should be unmapped on the error path in probe() and
unconditionally on remove().

Fixes: 62936009f35a ([libata] Add 460EX on-chip SATA driver, sata_dwc_460ex)
Signed-off-by: Andy Shevchenko <andriy.shevchenko@linux.intel.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

time: settimeofday: Validate the values of tv from user

commit 6ada1fc0e1c4775de0e043e1bd3ae9d065491aa5 upstream.

An unvalidated user input is multiplied by a constant, which can result in
an undefined behaviour for large values. While this is validated later,
we should avoid triggering undefined behaviour.

Cc: Thomas Gleixner <tglx@linutronix.de>
Cc: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Sasha Levin <sasha.levin@oracle.com>
[jstultz: include trivial milisecond->microsecond correction noticed
by Andy]
Signed-off-by: John Stultz <john.stultz@linaro.org>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

time: adjtimex: Validate the ADJ_FREQUENCY values

commit 5e5aeb4367b450a28f447f6d5ab57d8f2ab16a5f upstream.

Verify that the frequency value from userspace is valid and makes sense.

Unverified values can cause overflows later on.

Cc: Thomas Gleixner <tglx@linutronix.de>
Cc: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Sasha Levin <sasha.levin@oracle.com>
[jstultz: Fix up bug for negative values and drop redunent cap check]
Signed-off-by: John Stultz <john.stultz@linaro.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

Input: i8042 - reset keyboard to fix Elantech touchpad detection

commit 148e9a711e034e06310a8c36b64957934ebe30f2 upstream.

On some laptops, keyboard needs to be reset in order to successfully detect
touchpad (e.g., some Gigabyte laptop models with Elantech touchpads).
Without resettin keyboard touchpad pretends to be completely dead.

Based on the original patch by Mateusz Jończyk this version has been
expanded to include DMI based detection & application of the fix
automatically on the affected models of laptops. This has been confirmed to
fix problem by three users already on three different models of laptops.

Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=81331
Signed-off-by: Srihari Vijayaraghavan <linux.bug.reporting@gmail.com>
Acked-by: Mateusz Jończyk <mat.jonczyk@o2.pl>
Tested-by: Srihari Vijayaraghavan <linux.bug.reporting@gmail.com>
Tested by: Zakariya Dehlawi <zdehlawi@gmail.com>
Tested-by: Guillaum Bouchard <guillaum.bouchard@gmail.com>
Signed-off-by: Dmitry Torokhov <dmitry.torokhov@gmail.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

Input: I8042 - add Acer Aspire 7738 to the nomux list

commit 9333caeaeae4f831054e0e127a6ed3948b604d3e upstream.

When KBC is in active multiplexing mode the touchpad on this laptop does
not work.

Reported-by: Bilal Koc <koc.bilo@googlemail.com>
Signed-off-by: Dmitry Torokhov <dmitry.torokhov@gmail.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mac80211: fix multicast LED blinking and counter

commit d025933e29872cb1fe19fc54d80e4dfa4ee5779c upstream.

As multicast-frames can't be fragmented, "dot11MulticastReceivedFrameCount"
stopped being incremented after the use-after-free fix. Furthermore, the
RX-LED will be triggered by every multicast frame (which wouldn't happen
before) which wouldn't allow the LED to rest at all.

Fixes https://bugzilla.kernel.org/show_bug.cgi?id=89431 which also had the
patch.

Fixes: b8fff407a180 ("mac80211: fix use-after-free in defragmentation")
Signed-off-by: Andreas Müller <goo@stapelspeicher.org>
[rewrite commit message]
Signed-off-by: Johannes Berg <johannes.berg@intel.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: prevent endless growth of anon_vma hierarchy

commit 7a3ef208e662f4b63d43a23f61a64a129c525bbc upstream.

Constantly forking task causes unlimited grow of anon_vma chain.  Each
next child allocates new level of anon_vmas and links vma to all
previous levels because pages might be inherited from any level.

This patch adds heuristic which decides to reuse existing anon_vma
instead of forking new one.  It adds counter anon_vma->degree which
counts linked vmas and directly descending anon_vmas and reuses anon_vma
if counter is lower than two.  As a result each anon_vma has either vma
or at least two descending anon_vmas.  In such trees half of nodes are
leafs with alive vmas, thus count of anon_vmas is no more than two times
bigger than count of vmas.

This heuristic reuses anon_vmas as few as possible because each reuse
adds false aliasing among vmas and rmap walker ought to scan more ptes
when it searches where page is might be mapped.

Link: http://lkml.kernel.org/r/20120816024610.GA5350@evergreen.ssec.wisc.edu
Fixes: 5beb49305251 ("mm: change anon_vma linking to fix multi-process server scalability issue")
[akpm@linux-foundation.org: fix typo, per Rik]
Signed-off-by: Konstantin Khlebnikov <koct9i@gmail.com>
Reported-by: Daniel Forrest <dan.forrest@ssec.wisc.edu>
Tested-by: Michal Hocko <mhocko@suse.cz>
Tested-by: Jerome Marchand <jmarchan@redhat.com>
Reviewed-by: Michal Hocko <mhocko@suse.cz>
Reviewed-by: Rik van Riel <riel@redhat.com>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: protect set_page_dirty() from ongoing truncation

commit 2d6d7f98284648c5ed113fe22a132148950b140f upstream.

Tejun, while reviewing the code, spotted the following race condition
between the dirtying and truncation of a page:

__set_page_dirty_nobuffers()       __delete_from_page_cache()
  if (TestSetPageDirty(page))
                                     page->mapping = NULL
				     if (PageDirty())
				       dec_zone_page_state(page, NR_FILE_DIRTY);
				       dec_bdi_stat(mapping->backing_dev_info, BDI_RECLAIMABLE);
    if (page->mapping)
      account_page_dirtied(page)
        __inc_zone_page_state(page, NR_FILE_DIRTY);
	__inc_bdi_stat(mapping->backing_dev_info, BDI_RECLAIMABLE);

which results in an imbalance of NR_FILE_DIRTY and BDI_RECLAIMABLE.

Dirtiers usually lock out truncation, either by holding the page lock
directly, or in case of zap_pte_range(), by pinning the mapcount with
the page table lock held.  The notable exception to this rule, though,
is do_wp_page(), for which this race exists.  However, do_wp_page()
already waits for a locked page to unlock before setting the dirty bit,
in order to prevent a race where clear_page_dirty() misses the page bit
in the presence of dirty ptes.  Upgrade that wait to a fully locked
set_page_dirty() to also cover the situation explained above.

Afterwards, the code in set_page_dirty() dealing with a truncation race
is no longer needed.  Remove it.

Reported-by: Tejun Heo <tj@kernel.org>
Signed-off-by: Johannes Weiner <hannes@cmpxchg.org>
Acked-by: Kirill A. Shutemov <kirill.shutemov@linux.intel.com>
Reviewed-by: Jan Kara <jack@suse.cz>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
[lizf: Backported to 3.4:
 - adjust context
 - use VM_BUG_ON() instead of VM_BUG_ON_PAGE()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

HID: roccat: potential out of bounds in pyra_sysfs_write_settings()

commit 606185b20caf4c57d7e41e5a5ea4aff460aef2ab upstream.

This is a static checker fix.  We write some binary settings to the
sysfs file.  One of the settings is the "->startup_profile".  There
isn't any checking to make sure it fits into the
pyra->profile_settings[] array in the profile_activated() function.

I added a check to pyra_sysfs_write_settings() in both places because
I wasn't positive that the other callers were correct.

Signed-off-by: Dan Carpenter <dan.carpenter@oracle.com>
Signed-off-by: Jiri Kosina <jkosina@suse.cz>
[lizf: Backported to 3.4: define the variable @settings]
Signed-off-by: Zefan Li <lizefan@huawei.com>

OHCI: add a quirk for ULi M5237 blocking on reset

commit 56abcab833fafcfaeb2f5b25e0364c1dec45f53e upstream.

Commit 8dccddbc2368 ("OHCI: final fix for NVIDIA problems (I hope)")
introduced into 3.1.9 broke boot on e.g. Freescale P2020DS development
board. The code path that was previously specific to NVIDIA controllers
had then become taken for all chips.

However, the M5237 installed on the board wedges solid when accessing
its base+OHCI_FMINTERVAL register, making it impossible to boot any
kernel newer than 3.1.8 on this particular and apparently other similar
machines.

Don't readl() and writel() base+OHCI_FMINTERVAL on PCI ID 10b9:5237.

The patch is suitable for the -next tree as well as all maintained
kernels up to 3.2 inclusive.

Signed-off-by: Arseny Solokha <asolokha@kb.kras.ru>
Acked-by: Alan Stern <stern@rowland.harvard.edu>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: console: fix potential use after free

commit 32a4bf2e81ec378e5925d4e069e0677a6c86a6ad upstream.

Use tty kref to release the fake tty in usb_console_setup to avoid use
after free if the underlying serial driver has acquired a reference.

Note that using the tty destructor release_one_tty requires some more
state to be initialised.

Fixes: 4a90f09b20f4 ("tty: usb-serial krefs")
Signed-off-by: Johan Hovold <johan@kernel.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: Don't count the stack guard page towards RLIMIT_STACK

commit 690eac53daff34169a4d74fc7bfbd388c4896abb upstream.

Commit fee7e49d4514 ("mm: propagate error from stack expansion even for
guard page") made sure that we return the error properly for stack
growth conditions.  It also theorized that counting the guard page
towards the stack limit might break something, but also said "Let's see
if anybody notices".

Somebody did notice.  Apparently android-x86 sets the stack limit very
close to the limit indeed, and including the guard page in the rlimit
check causes the android 'zygote' process problems.

So this adds the (fairly trivial) code to make the stack rlimit check be
against the actual real stack size, rather than the size of the vma that
includes the guard page.

Reported-and-tested-by: Chih-Wei Huang <cwhuang@android-x86.org>
Cc: Jay Foad <jay.foad@gmail.com>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: fix corner case in anon_vma endless growing prevention

commit b800c91a0517071156e772d4fb329ad33590da62 upstream.

Fix for BUG_ON(anon_vma->degree) splashes in unlink_anon_vmas() ("kernel
BUG at mm/rmap.c:399!") caused by commit 7a3ef208e662 ("mm: prevent
endless growth of anon_vma hierarchy")

Anon_vma_clone() is usually called for a copy of source vma in
destination argument.  If source vma has anon_vma it should be already
in dst->anon_vma.  NULL in dst->anon_vma is used as a sign that it's
called from anon_vma_fork().  In this case anon_vma_clone() finds
anon_vma for reusing.

Vma_adjust() calls it differently and this breaks anon_vma reusing
logic: anon_vma_clone() links vma to old anon_vma and updates degree
counters but vma_adjust() overrides vma->anon_vma right after that.  As
a result final unlink_anon_vmas() decrements degree for wrong anon_vma.

This patch assigns ->anon_vma before calling anon_vma_clone().

Signed-off-by: Konstantin Khlebnikov <koct9i@gmail.com>
Reported-and-tested-by: Chris Clayton <chris2553@googlemail.com>
Reported-and-tested-by: Oded Gabbay <oded.gabbay@amd.com>
Reported-and-tested-by: Chih-Wei Huang <cwhuang@android-x86.org>
Acked-by: Rik van Riel <riel@redhat.com>
Acked-by: Vlastimil Babka <vbabka@suse.cz>
Cc: Daniel Forrest <dan.forrest@ssec.wisc.edu>
Cc: Michal Hocko <mhocko@suse.cz>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
[lizf: Backported to 3.4: define variable @error and return this instead
 of returning -ENOMEM]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: fix memory and reference leaks in gpiochip_add error path

commit 5539b3c938d64a60cb1fc442ac3ce9263d52de0c upstream.

Memory allocated and references taken by of_gpiochip_add and
acpi_gpiochip_add were never released on errors in gpiochip_add (e.g.
failure to find free gpio range).

Fixes: 391c970c0dd1 ("of/gpio: add default of_xlate function if device
has a node pointer")
Fixes: 664e3e5ac64c ("gpio / ACPI: register to ACPI events
automatically")

Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf: Backported to 3.4:
 - move the call to of_gpiochip_add() into the above if condition.
 - remove the call to acpi_gpiochip_remove()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ftrace/jprobes/x86: Fix conflict between jprobes and function graph tracing

commit 237d28db036e411f22c03cfd5b0f6dc2aa9bf3bc upstream.

If the function graph tracer traces a jprobe callback, the system will
crash. This can easily be demonstrated by compiling the jprobe
sample module that is in the kernel tree, loading it and running the
function graph tracer.

 # modprobe jprobe_example.ko
 # echo function_graph > /sys/kernel/debug/tracing/current_tracer
 # ls

The first two commands end up in a nice crash after the first fork.
(do_fork has a jprobe attached to it, so "ls" just triggers that fork)

The problem is caused by the jprobe_return() that all jprobe callbacks
must end with. The way jprobes works is that the function a jprobe
is attached to has a breakpoint placed at the start of it (or it uses
ftrace if fentry is supported). The breakpoint handler (or ftrace callback)
will copy the stack frame and change the ip address to return to the
jprobe handler instead of the function. The jprobe handler must end
with jprobe_return() which swaps the stack and does an int3 (breakpoint).
This breakpoint handler will then put back the saved stack frame,
simulate the instruction at the beginning of the function it added
a breakpoint to, and then continue on.

For function tracing to work, it hijakes the return address from the
stack frame, and replaces it with a hook function that will trace
the end of the call. This hook function will restore the return
address of the function call.

If the function tracer traces the jprobe handler, the hook function
for that handler will not be called, and its saved return address
will be used for the next function. This will result in a kernel crash.

To solve this, pause function tracing before the jprobe handler is called
and unpause it before it returns back to the function it probed.

Some other updates:

Used a variable "saved_sp" to hold kcb->jprobe_saved_sp. This makes the
code look a bit cleaner and easier to understand (various tries to fix
this bug required this change).

Note, if fentry is being used, jprobes will change the ip address before
the function graph tracer runs and it will not be able to trace the
function that the jprobe is probing.

Link: http://lkml.kernel.org/r/20150114154329.552437962@goodmis.org

Acked-by: Masami Hiramatsu <masami.hiramatsu.pt@hitachi.com>
Signed-off-by: Steven Rostedt <rostedt@goodmis.org>
[lizf: Backported to 3.4:
 - adjust filename
 - adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

can: dev: fix crtlmode_supported check

commit 9b1087aa5e86448fe6ad40a58964e35f3ba423d5 upstream.

When changing flags in the CAN drivers ctrlmode the provided new content has to
be checked whether the bits are allowed to be changed. The bits that are to be
changed are given as a bitfield in cm->mask. Therefore checking against
cm->flags is wrong as the content can hold any kind of values.

The iproute2 tool sets the bits in cm->mask and cm->flags depending on the
detected command line options. To be robust against bogus user space
applications additionally sanitize the provided flags with the provided mask.

Cc: Wolfgang Grandegger <wg@grandegger.com>
Signed-off-by: Oliver Hartkopp <socketcan@hartkopp.net>
Signed-off-by: Marc Kleine-Budde <mkl@pengutronix.de>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

sysfs.h: add ATTRIBUTE_GROUPS() macro

commit f2f37f58b1b933b06d6d84e80a31a1b500fb0db2 upstream.

To make it easier for driver subsystems to work with attribute groups,
create the ATTRIBUTE_GROUPS macro to remove some of the repetitive
typing for the most common use for attribute groups.

Reviewed-by: Guenter Roeck <linux@roeck-us.net>
Tested-by: Guenter Roeck <linux@roeck-us.net>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

driver core: Introduce device_create_groups

commit 39ef311204941ddd01ea2950d6220c8ccc710d15 upstream.

device_create_groups lets callers create devices as well as associated
sysfs attributes with a single call. This avoids race conditions seen
if sysfs attributes on new devices are created later.

[fixed up comment block placement and add checks for printk buffer
formats - gregkh]

Signed-off-by: Guenter Roeck <linux@roeck-us.net>
Cc: Jean Delvare <khali@linux-fr.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: sysfs: fix gpio-chip device-attribute leak

commit 121b6a79955a3a3fd7bbb9b8cb88d5b9dad6283d upstream.

The gpio-chip device attributes were never destroyed when the device was
removed.

Fix by using device_create_with_groups() to create the device attributes
of the chip class device.

Note that this also fixes the attribute-creation race with userspace.

Fixes: d8f388d8dc8d ("gpio: sysfs interface")
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpiolib: Refactor gpio_export

commit fc4e2514995d9cd7f3e1a67098ce65d72acf8ec7 upstream.

The gpio_export function uses nested if statements and the status
variable to handle the failure cases. This makes the function logic
difficult to follow. Refactor the code to abort immediately on failure
using goto. This makes the code slightly longer, but significantly
reduces the nesting and number of split lines and makes the code easier
to read.

Signed-off-by: Ryan Mallon <rmallon@gmail.com>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: sysfs: fix gpio device-attribute leak

commit 0915e6feb38de8d3601819992a5bd050201a56fa upstream.

The gpio device attributes were never destroyed when the gpio was
unexported (or on export failures).

Use device_create_with_groups() to create the default device attributes
of the gpio class device. Note that this also fixes the
attribute-creation race with userspace for these attributes.

Remove contingent attributes in export error path and on unexport.

Fixes: d8f388d8dc8d ("gpio: sysfs interface")
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf: Backported to 3.4:
 - adjust filename
 - adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: sysfs: fix gpio attribute-creation race

commit ebbeba120ab2ec6ac5f3afc1425ec6ff0b77ad6f upstream.

Fix attribute-creation race with userspace by using the default group
to create also the contingent gpio device attributes.

Fixes: d8f388d8dc8d ("gpio: sysfs interface")
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf:
 - adjust filename
 - call gpio_to_irq() instead of gpiod_to_irq]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: usb-audio: Add mic volume fix quirk for Logitech Webcam C210

libata: allow sata_sil24 to opt-out of tag ordered submission

commit 72dd299d5039a336493993dcc63413cf31d0e662 upstream.

Ronny reports: https://bugzilla.kernel.org/show_bug.cgi?id=87101
    "Since commit 8a4aeec8d "libata/ahci: accommodate tag ordered
    controllers" the access to the harddisk on the first SATA-port is
    failing on its first access. The access to the harddisk on the
    second port is working normal.

    When reverting the above commit, access to both harddisks is working
    fine again."

Maintain tag ordered submission as the default, but allow sata_sil24 to
continue with the old behavior.

Cc: Tejun Heo <tj@kernel.org>
Reported-by: Ronny Hegewald <Ronny.Hegewald@online.de>
Signed-off-by: Dan Williams <dan.j.williams@intel.com>
Signed-off-by: Tejun Heo <tj@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

scripts/recordmcount.pl: There is no -m32 gcc option on Super-H anymore

commit 1caf6aaaa47471831d77c75f094d4e00ad1ec808 upstream.

Compiling SH with gcc-4.8 fails due to the -m32 option not being
supported.

From http://buildd.debian-ports.org/status/fetch.php?pkg=linux&arch=sh4&ver=3.16.7-ckt4-1&stamp=1421425783

      CC      init/main.o
    gcc-4.8: error: unrecognized command line option '-m32'
    ld: cannot find init/.tmp_mc_main.o: No such file or directory
    objcopy: 'init/.tmp_mx_main.o': No such file
    rm: cannot remove 'init/.tmp_mx_main.o': No such file or directory
    rm: cannot remove 'init/.tmp_mc_main.o': No such file or directory

Link: http://lkml.kernel.org/r/1421537778-29001-1-git-send-email-kernel@mkarcher.dialup.fu-berlin.de
Link: http://lkml.kernel.org/r/54BCBDD4.10102@physik.fu-berlin.de

Cc: Matt Fleming <matt@console-pimps.org>
Reported-by: John Paul Adrian Glaubitz <glaubitz@physik.fu-berlin.de>
Signed-off-by: Michael Karcher <kernel@mkarcher.dialup.fu-berlin.de>
Signed-off-by: Steven Rostedt <rostedt@goodmis.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

libata: prevent HSM state change race between ISR and PIO

commit ce7514526742c0898b837d4395f515b79dfb5a12 upstream.

It is possible for ata_sff_flush_pio_task() to set ap->hsm_task_state to
HSM_ST_IDLE in between the time __ata_sff_port_intr() checks for HSM_ST_IDLE
and before it calls ata_sff_hsm_move() causing ata_sff_hsm_move() to BUG().

This problem is hard to reproduce making this patch hard to verify, but this
fix will prevent the race.

I have not been able to reproduce the problem, but here is a crash dump from
a 2.6.32 kernel.

On examining the ata port's state, its hsm_task_state field has a value of HSM_ST_IDLE:

crash> struct ata_port.hsm_task_state ffff881c1121c000
  hsm_task_state = 0

Normally, this should not be possible as ata_sff_hsm_move() was called from ata_sff_host_intr(),
which checks hsm_task_state and won't call ata_sff_hsm_move() if it has a HSM_ST_IDLE value.

PID: 11053  TASK: ffff8816e846cae0  CPU: 0   COMMAND: "sshd"
 #0 [ffff88008ba03960] machine_kexec at ffffffff81038f3b
 #1 [ffff88008ba039c0] crash_kexec at ffffffff810c5d92
 #2 [ffff88008ba03a90] oops_end at ffffffff8152b510
 #3 [ffff88008ba03ac0] die at ffffffff81010e0b
 #4 [ffff88008ba03af0] do_trap at ffffffff8152ad74
 #5 [ffff88008ba03b50] do_invalid_op at ffffffff8100cf95
 #6 [ffff88008ba03bf0] invalid_op at ffffffff8100bf9b
    [exception RIP: ata_sff_hsm_move+317]
    RIP: ffffffff813a77ad  RSP: ffff88008ba03ca0  RFLAGS: 00010097
    RAX: 0000000000000000  RBX: ffff881c1121dc60  RCX: 0000000000000000
    RDX: ffff881c1121dd10  RSI: ffff881c1121dc60  RDI: ffff881c1121c000
    RBP: ffff88008ba03d00   R8: 0000000000000000   R9: 000000000000002e
    R10: 000000000001003f  R11: 000000000000009b  R12: ffff881c1121c000
    R13: 0000000000000000  R14: 0000000000000050  R15: ffff881c1121dd78
    ORIG_RAX: ffffffffffffffff  CS: 0010  SS: 0018
 #7 [ffff88008ba03d08] ata_sff_host_intr at ffffffff813a7fbd
 #8 [ffff88008ba03d38] ata_sff_interrupt at ffffffff813a821e
 #9 [ffff88008ba03d78] handle_IRQ_event at ffffffff810e6ec0

x86, hyperv: Mark the Hyper-V clocksource as being continuous

commit 32c6590d126836a062b3140ed52d898507987017 upstream.

The Hyper-V clocksource is continuous; mark it accordingly.

Signed-off-by: K. Y. Srinivasan <kys@microsoft.com>
Acked-by: jasowang@redhat.com
Cc: gregkh@linuxfoundation.org
Cc: devel@linuxdriverproject.org
Cc: olaf@aepfle.de
Cc: apw@canonical.com
Link: http://lkml.kernel.org/r/1421108762-3331-1-git-send-email-kys@microsoft.com
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

spi: dw: Fix detecting FIFO depth

commit d297933cc7fcfbaaf2d37570baac73287bf0357d upstream.

Current code tries to find the highest valid fifo depth by checking the value
it wrote to DW_SPI_TXFLTR. There are a few problems in current code:
1) There is an off-by-one in dws->fifo_len setting because it assumes the latest
   register write fails so the latest valid value should be fifo - 1.
2) We know the depth could be from 2 to 256 from HW spec, so it is not necessary
   to test fifo == 257. In the case fifo is 257, it means the latest valid
   setting is fifo = 256. So after the for loop iteration, we should check
   fifo == 2 case instead of fifo == 257 if detecting the FIFO depth fails.
This patch fixes above issues.

Signed-off-by: Axel Lin <axel.lin@ingics.com>
Reviewed-and-tested-by: Andy Shevchenko <andriy.shevchenko@linux.intel.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

spi: dw-mid: fix FIFO size

commit 67bf9cda4b498b8cea4a40be67a470afe57d2e88 upstream.

The FIFO size is 40 accordingly to the specifications, but this means 0x40,
i.e. 64 bytes. This patch fixes the typo and enables FIFO size autodetection
for Intel MID devices.

Fixes: 7063c0d942a1 (spi/dw_spi: add DMA support)
Signed-off-by: Andy Shevchenko <andriy.shevchenko@linux.intel.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ASoC: wm8960: Fix capture sample rate from 11250 to 11025

commit 22ee76daddb87f88d2336d1b4737ef27c4f307ac upstream.

wm8960 codec can't support sample rate 11250, it must be 11025.

Signed-off-by: Zidan Wang <b50113@freescale.com>
Acked-by: Charles Keepax <ckeepax@opensource.wolfsonmicro.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

regulator: core: fix race condition in regulator_put()

commit 83b0302d347a49f951e904184afe57ac3723476e upstream.

The regulator framework maintains a list of consumer regulators
for a regulator device and protects it from concurrent access using
the regulator device's mutex lock.

In the case of regulator_put() the consumer is removed and regulator
device's parameters are updated without holding the regulator device's
mutex. This would lead to a race condition between the regulator_put()
and any function which traverses the consumer list or modifies regulator
device's parameters.
Fix this race condition by holding the regulator device's mutex in case
of regulator_put.

Signed-off-by: Ashay Jaiswal <ashayj@codeaurora.org>
Signed-off-by: Mark Brown <broonie@kernel.org>
[lizf: Backported to 3.4:
 - adjust context
 - no need to change the comment]
Signed-off-by: Zefan Li <lizefan@huawei.com>

powerpc/xmon: Fix another endiannes issue in RTAS call from xmon

commit e6eb2eba494d6f99e69ca3c3748cd37a2544ab38 upstream.

The commit 3b8a3c010969 ("powerpc/pseries: Fix endiannes issue in RTAS
call from xmon") was fixing an endianness issue in the call made from
xmon to RTAS.

However, as Michael Ellerman noticed, this fix was not complete, the
token value was not byte swapped. This lead to call an unexpected and
most of the time unexisting RTAS function, which is silently ignored by
RTAS.

This fix addresses this hole.

Reported-by: Michael Ellerman <mpe@ellerman.id.au>
Signed-off-by: Laurent Dufour <ldufour@linux.vnet.ibm.com>
Signed-off-by: Michael Ellerman <mpe@ellerman.id.au>
Signed-off-by: Zefan Li <lizefan@huawei.com>

nl80211: fix per-station group key get/del and memory leak

commit 0fa7b39131576dd1baa6ca17fca53c65d7f62249 upstream.

In case userspace attempts to obtain key information for or delete a
unicast key, this is currently erroneously rejected unless the driver
sets the WIPHY_FLAG_IBSS_RSN flag. Apparently enough drivers do so it
was never noticed.

Fix that, and while at it fix a potential memory leak: the error path
in the get_key() function was placed after allocating a message but
didn't free it - move it to a better place. Luckily admin permissions
are needed to call this operation.

Fixes: e31b82136d1ad ("cfg80211/mac80211: allow per-station GTKs")
Signed-off-by: Johannes Berg <johannes.berg@intel.com>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb-storage/SCSI: Add broken_fua blacklist flag

commit b14bf2d0c0358140041d1c1805a674376964d0e0 upstream.

Some buggy JMicron USB-ATA bridges don't know how to translate the FUA
bit in READs or WRITEs.  This patch adds an entry in unusual_devs.h
and a blacklist flag to tell the sd driver not to use FUA.

Signed-off-by: Alan Stern <stern@rowland.harvard.edu>
Reported-by: Michael Büsch <m@bues.ch>
Tested-by: Michael Büsch <m@bues.ch>
Acked-by: James Bottomley <James.Bottomley@HansenPartnership.com>
CC: Matthew Dharm <mdharm-usb@one-eyed-alien.net>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb-storage/SCSI: blacklist FUA on JMicron 152d:2566 USB-SATA controller

commit bf5c4136fa5ce471bdbf4cf59a813e32755fd014 upstream.

It looks like FUA support is broken on JMicron 152d:2566 bridge:

[223159.885704] sd 7:0:0:0: [sdc] Write Protect is off
[223159.885706] sd 7:0:0:0: [sdc] Mode Sense: 47 00 10 08
[223159.885942] sd 7:0:0:0: [sdc] Write cache: enabled, read cache: enabled, supports DPO and FUA

[223283.691677] sd 7:0:0:0: [sdc]
[223283.691680] Result: hostbyte=DID_OK driverbyte=DRIVER_SENSE
[223283.691681] sd 7:0:0:0: [sdc]
[223283.691682] Sense Key : Illegal Request [current]
[223283.691684] sd 7:0:0:0: [sdc]
[223283.691685] Add. Sense: Invalid field in cdb
[223283.691686] sd 7:0:0:0: [sdc] CDB:
[223283.691687] Write(10): 2a 08 15 d0 83 0d 00 00 01 00
[223283.691690] blk_update_request: critical target error, dev sdc, sector 2927892584

This patch adds blacklist flag so that sd will not use FUA

Signed-off-by: Dmitry Nezhevenko <dion@dion.org.ua>
Cc: Phil Dibowitz <phil@ipom.com>
Cc: Alan Stern <stern@rowland.harvard.edu>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

usb-core bInterval quirk

commit cd83ce9e6195aa3ea15ab4db92892802c20df5d0 upstream.

This patch adds a usb quirk to support devices with interupt endpoints
and bInterval values expressed as microframes. The quirk causes the
parse endpoint function to modify the reported bInterval to a standards
conforming value.

There is currently code in the endpoint parser that checks for
bIntervals that are outside of the valid range (1-16 for USB 2+ high
speed and super speed interupt endpoints). In this case, the code assumes
the bInterval is being reported in 1ms frames. As well, the correction
is only applied if the original bInterval value is out of the 1-16 range.

With this quirk applied to the device, the bInterval will be
accurately adjusted from microframes to an exponent.

Signed-off-by: James P Michels III <james.p.michels@gmail.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

USB: Add OTG PET device to TPL

commit e5dff0e80463cc3fa236e898ef1491b40be70b19 upstream.

OTG device shall support this device for allowing compliance automated testing.
The modification is derived from Pavankumar and Vijayavardhans' previous work.

Signed-off-by: Macpaul Lin <macpaul@gmail.com>
Cc: Pavankumar Kondeti <pkondeti@codeaurora.org>
Cc: Vijayavardhan Vennapusa <vvreddy@codeaurora.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

drm/i915: Only fence tiled region of object.

commit af1a7301c7cf8912dca03065d448c4437c5c239f upstream.

When creating a fence for a tiled object, only fence the area that
makes up the actual tiles.  The object may be larger than the tiled
area and if we allow those extra addresses to be fenced, they'll
get converted to addresses beyond where the object is mapped. This
opens up the possiblity of writes beyond the end of object.

To prevent this, we adjust the size of the fence to only encompass
the area that makes up the actual tiles.  The extra space is considered
un-tiled and now behaves as if it was a linear object.

Testcase: igt/gem_tiled_fence_overflow
Reported-by: Dan Hettena <danh@ghs.com>
Signed-off-by: Bob Paauwe <bob.j.paauwe@intel.com>
Reviewed-by: Daniel Vetter <daniel.vetter@ffwll.ch>
Signed-off-by: Jani Nikula <jani.nikula@intel.com>
[lizf: Backported to 3.4:
 - adjust context
 - adjust indentation
 - make the same change to both sandybridge_write_fence_reg()
   and i965_write_fence_reg()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: seq-dummy: remove deadlock-causing events on close

commit 0767e95bb96d7fdddcd590fb809e6975d93aebc5 upstream.

When the last subscriber to a "Through" port has been removed, the
subscribed destination ports might still be active, so it would be
wrong to send "all sounds off" and "reset controller" events to them.
The proper place for such a shutdown would be the closing of the actual
MIDI port (and close_substream() in rawmidi.c already can do this).

This also fixes a deadlock when dummy_unuse() tries to send events to
its own port that is already locked because it is being freed.

Reported-by: Peter Billam <peter@www.pjb.com.au>
Signed-off-by: Clemens Ladisch <clemens@ladisch.de>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: sctp: fix slab corruption from use after free on INIT collisions

commit 600ddd6825543962fb807884169e57b580dba208 upstream.

When hitting an INIT collision case during the 4WHS with AUTH enabled, as
already described in detail in commit 1be9a950c646 ("net: sctp: inherit
auth_capable on INIT collisions"), it can happen that we occasionally
still remotely trigger the following panic on server side which seems to
have been uncovered after the fix from commit 1be9a950c646 ...

[  533.876389] BUG: unable to handle kernel paging request at 00000000ffffffff
[  533.913657] IP: [<ffffffff811ac385>] __kmalloc+0x95/0x230
[  533.940559] PGD 5030f2067 PUD 0
[  533.957104] Oops: 0000 [#1] SMP
[  533.974283] Modules linked in: sctp mlx4_en [...]
[  534.939704] Call Trace:
[  534.951833]  [<ffffffff81294e30>] ? crypto_init_shash_ops+0x60/0xf0
[  534.984213]  [<ffffffff81294e30>] crypto_init_shash_ops+0x60/0xf0
[  535.015025]  [<ffffffff8128c8ed>] __crypto_alloc_tfm+0x6d/0x170
[  535.045661]  [<ffffffff8128d12c>] crypto_alloc_base+0x4c/0xb0
[  535.074593]  [<ffffffff8160bd42>] ? _raw_spin_lock_bh+0x12/0x50
[  535.105239]  [<ffffffffa0418c11>] sctp_inet_listen+0x161/0x1e0 [sctp]
[  535.138606]  [<ffffffff814e43bd>] SyS_listen+0x9d/0xb0
[  535.166848]  [<ffffffff816149a9>] system_call_fastpath+0x16/0x1b

... or depending on the the application, for example this one:

[ 1370.026490] BUG: unable to handle kernel paging request at 00000000ffffffff
[ 1370.026506] IP: [<ffffffff811ab455>] kmem_cache_alloc+0x75/0x1d0
[ 1370.054568] PGD 633c94067 PUD 0
[ 1370.070446] Oops: 0000 [#1] SMP
[ 1370.085010] Modules linked in: sctp kvm_amd kvm [...]
[ 1370.963431] Call Trace:
[ 1370.974632]  [<ffffffff8120f7cf>] ? SyS_epoll_ctl+0x53f/0x960
[ 1371.000863]  [<ffffffff8120f7cf>] SyS_epoll_ctl+0x53f/0x960
[ 1371.027154]  [<ffffffff812100d3>] ? anon_inode_getfile+0xd3/0x170
[ 1371.054679]  [<ffffffff811e3d67>] ? __alloc_fd+0xa7/0x130
[ 1371.080183]  [<ffffffff816149a9>] system_call_fastpath+0x16/0x1b

With slab debugging enabled, we can see that the poison has been overwritten:

[  669.826368] BUG kmalloc-128 (Tainted: G        W     ): Poison overwritten
[  669.826385] INFO: 0xffff880228b32e50-0xffff880228b32e50. First byte 0x6a instead of 0x6b
[  669.826414] INFO: Allocated in sctp_auth_create_key+0x23/0x50 [sctp] age=3 cpu=0 pid=18494
[  669.826424]  __slab_alloc+0x4bf/0x566
[  669.826433]  __kmalloc+0x280/0x310
[  669.826453]  sctp_auth_create_key+0x23/0x50 [sctp]
[  669.826471]  sctp_auth_asoc_create_secret+0xcb/0x1e0 [sctp]
[  669.826488]  sctp_auth_asoc_init_active_key+0x68/0xa0 [sctp]
[  669.826505]  sctp_do_sm+0x29d/0x17c0 [sctp] [...]
[  669.826629] INFO: Freed in kzfree+0x31/0x40 age=1 cpu=0 pid=18494
[  669.826635]  __slab_free+0x39/0x2a8
[  669.826643]  kfree+0x1d6/0x230
[  669.826650]  kzfree+0x31/0x40
[  669.826666]  sctp_auth_key_put+0x19/0x20 [sctp]
[  669.826681]  sctp_assoc_update+0x1ee/0x2d0 [sctp]
[  669.826695]  sctp_do_sm+0x674/0x17c0 [sctp]

Since this only triggers in some collision-cases with AUTH, the problem at
heart is that sctp_auth_key_put() on asoc->asoc_shared_key is called twice
when having refcnt 1, once directly in sctp_assoc_update() and yet again
from within sctp_auth_asoc_init_active_key() via sctp_assoc_update() on
the already kzfree'd memory, which is also consistent with the observation
of the poison decrease from 0x6b to 0x6a (note: the overwrite is detected
at a later point in time when poison is checked on new allocation).

Reference counting of auth keys revisited:

Shared keys for AUTH chunks are being stored in endpoints and associations
in endpoint_shared_keys list. On endpoint creation, a null key is being
added; on association creation, all endpoint shared keys are being cached
and thus cloned over to the association. struct sctp_shared_key only holds
a pointer to the actual key bytes, that is, struct sctp_auth_bytes which
keeps track of users internally through refcounting. Naturally, on assoc
or enpoint destruction, sctp_shared_key are being destroyed directly and
the reference on sctp_auth_bytes dropped.

User space can add keys to either list via setsockopt(2) through struct
sctp_authkey and by passing that to sctp_auth_set_key() which replaces or
adds a new auth key. There, sctp_auth_create_key() creates a new sctp_auth_bytes
with refcount 1 and in case of replacement drops the reference on the old
sctp_auth_bytes. A key can be set active from user space through setsockopt()
on the id via sctp_auth_set_active_key(), which iterates through either
endpoint_shared_keys and in case of an assoc, invokes (one of various places)
sctp_auth_asoc_init_active_key().

sctp_auth_asoc_init_active_key() computes the actual secret from local's
and peer's random, hmac and shared key parameters and returns a new key
directly as sctp_auth_bytes, that is asoc->asoc_shared_key, plus drops
the reference if there was a previous one. The secret, which where we
eventually double drop the ref comes from sctp_auth_asoc_set_secret() with
intitial refcount of 1, which also stays unchanged eventually in
sctp_assoc_update(). This key is later being used for crypto layer to
set the key for the hash in crypto_hash_setkey() from sctp_auth_calculate_hmac().

To close the loop: asoc->asoc_shared_key is freshly allocated secret
material and independant of the sctp_shared_key management keeping track
of only shared keys in endpoints and assocs. Hence, also commit 4184b2a79a76
("net: sctp: fix memory leak in auth key management") is independant of
this bug here since it concerns a different layer (though same structures
being used eventually). asoc->asoc_shared_key is reference dropped correctly
on assoc destruction in sctp_association_free() and when active keys are
being replaced in sctp_auth_asoc_init_active_key(), it always has a refcount
of 1. Hence, it's freed prematurely in sctp_assoc_update(). Simple fix is
to remove that sctp_auth_key_put() from there which fixes these panics.

Fixes: 730fc3d05cd4 ("[SCTP]: Implete SCTP-AUTH parameter processing")
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Acked-by: Vlad Yasevich <vyasevich@gmail.com>
Acked-by: Neil Horman <nhorman@tuxdriver.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ipv6: replacing a rt6_info needs to purge possible propagated rt6_infos too

commit 6e9e16e6143b725662e47026a1d0f270721cdd24 upstream.

Lubomir Rintel reported that during replacing a route the interface
reference counter isn't correctly decremented.

To quote bug <https://bugzilla.kernel.org/show_bug.cgi?id=91941>:
| [root@rhel7-5 lkundrak]# sh -x lal
| + ip link add dev0 type dummy
| + ip link set dev0 up
| + ip link add dev1 type dummy
| + ip link set dev1 up
| + ip addr add 2001:db8:8086::2/64 dev dev0
| + ip route add 2001:db8:8086::/48 dev dev0 proto static metric 20
| + ip route add 2001:db8:8088::/48 dev dev1 proto static metric 10
| + ip route replace 2001:db8:8086::/48 dev dev1 proto static metric 20
| + ip link del dev0 type dummy
| Message from syslogd@rhel7-5 at Jan 23 10:54:41 ...
|  kernel:unregister_netdevice: waiting for dev0 to become free. Usage count = 2
|
| Message from syslogd@rhel7-5 at Jan 23 10:54:51 ...
|  kernel:unregister_netdevice: waiting for dev0 to become free. Usage count = 2

During replacement of a rt6_info we must walk all parent nodes and check
if the to be replaced rt6_info got propagated. If so, replace it with
an alive one.

Fixes: 4a287eba2de3957 ("IPv6 routing, NLM_F_* flag support: REPLACE and EXCL flags support, warn about missing CREATE flag")
Reported-by: Lubomir Rintel <lkundrak@v3.sk>
Signed-off-by: Hannes Frederic Sowa <hannes@stressinduktion.org>
Tested-by: Lubomir Rintel <lkundrak@v3.sk>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

vm: add VM_FAULT_SIGSEGV handling support

commit 33692f27597fcab536d7cbbcc8f52905133e4aa7 upstream.

The core VM already knows about VM_FAULT_SIGBUS, but cannot return a
"you should SIGSEGV" error, because the SIGSEGV case was generally
handled by the caller - usually the architecture fault handler.

That results in lots of duplication - all the architecture fault
handlers end up doing very similar "look up vma, check permissions, do
retries etc" - but it generally works.  However, there are cases where
the VM actually wants to SIGSEGV, and applications _expect_ SIGSEGV.

In particular, when accessing the stack guard page, libsigsegv expects a
SIGSEGV.  And it usually got one, because the stack growth is handled by
that duplicated architecture fault handler.

However, when the generic VM layer started propagating the error return
from the stack expansion in commit fee7e49d4514 ("mm: propagate error
from stack expansion even for guard page"), that now exposed the
existing VM_FAULT_SIGBUS result to user space.  And user space really
expected SIGSEGV, not SIGBUS.

To fix that case, we need to add a VM_FAULT_SIGSEGV, and teach all those
duplicate architecture fault handlers about it.  They all already have
the code to handle SIGSEGV, so it's about just tying that new return
value to the existing code, but it's all a bit annoying.

This is the mindless minimal patch to do this.  A more extensive patch
would be to try to gather up the mostly shared fault handling logic into
one generic helper routine, and long-term we really should do that
cleanup.

Just from this patch, you can generally see that most architectures just
copied (directly or indirectly) the old x86 way of doing things, but in
the meantime that original x86 model has been improved to hold the VM
semaphore for shorter times etc and to handle VM_FAULT_RETRY and other
"newer" things, so it would be a good idea to bring all those
improvements to the generic case and teach other architectures about
them too.

Reported-and-tested-by: Takashi Iwai <tiwai@suse.de>
Tested-by: Jan Engelhardt <jengelh@inai.de>
Acked-by: Heiko Carstens <heiko.carstens@de.ibm.com> # "s390 still compiles and boots"
Cc: linux-arch@vger.kernel.org
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
[bwh: Backported to 3.2:
 - Adjust filenames, context
 - Drop arc, metag, nios2 and lustre changes
 - For sh, patch both 32-bit and 64-bit implementations to use goto bad_area
 - For s390, pass int_code and trans_exc_code as arguments to do_no_context()
   and do_sigsegv()]
Signed-off-by: Ben Hutchings <ben@decadent.org.uk>
[lizf: Backported to 3.4:
 - adjust context in arch/power/mm/fault.c
 - apply the original change in upstream commit for s390]
Signed-off-by: Zefan Li <lizefan@huawei.com>

vm: make stack guard page errors return VM_FAULT_SIGSEGV rather than SIGBUS

commit 9c145c56d0c8a0b62e48c8d71e055ad0fb2012ba upstream.

The stack guard page error case has long incorrectly caused a SIGBUS
rather than a SIGSEGV, but nobody actually noticed until commit
fee7e49d4514 ("mm: propagate error from stack expansion even for guard
page") because that error case was never actually triggered in any
normal situations.

Now that we actually report the error, people noticed the wrong signal
that resulted.  So far, only the test suite of libsigsegv seems to have
actually cared, but there are real applications that use libsigsegv, so
let's not wait for any of those to break.

Reported-and-tested-by: Takashi Iwai <tiwai@suse.de>
Tested-by: Jan Engelhardt <jengelh@inai.de>
Acked-by: Heiko Carstens <heiko.carstens@de.ibm.com> # "s390 still compiles and boots"
Cc: linux-arch@vger.kernel.org
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: sctp: fix panic on duplicate ASCONF chunks

commit b69040d8e39f20d5215a03502a8e8b4c6ab78395 upstream.

When receiving a e.g. semi-good formed connection scan in the
form of ...

  -------------- INIT[ASCONF; ASCONF_ACK] ------------->
  <----------- INIT-ACK[ASCONF; ASCONF_ACK] ------------
  -------------------- COOKIE-ECHO -------------------->
  <-------------------- COOKIE-ACK ---------------------
  ---------------- ASCONF_a; ASCONF_b ----------------->

... where ASCONF_a equals ASCONF_b chunk (at least both serials
need to be equal), we panic an SCTP server!

The problem is that good-formed ASCONF chunks that we reply with
ASCONF_ACK chunks are cached per serial. Thus, when we receive a
same ASCONF chunk twice (e.g. through a lost ASCONF_ACK), we do
not need to process them again on the server side (that was the
idea, also proposed in the RFC). Instead, we know it was cached
and we just resend the cached chunk instead. So far, so good.

Where things get nasty is in SCTP's side effect interpreter, that
is, sctp_cmd_interpreter():

While incoming ASCONF_a (chunk = event_arg) is being marked
!end_of_packet and !singleton, and we have an association context,
we do not flush the outqueue the first time after processing the
ASCONF_ACK singleton chunk via SCTP_CMD_REPLY. Instead, we keep it
queued up, although we set local_cork to 1. Commit 2e3216cd54b1
changed the precedence, so that as long as we get bundled, incoming
chunks we try possible bundling on outgoing queue as well. Before
this commit, we would just flush the output queue.

Now, while ASCONF_a's ASCONF_ACK sits in the corked outq, we
continue to process the same ASCONF_b chunk from the packet. As
we have cached the previous ASCONF_ACK, we find it, grab it and
do another SCTP_CMD_REPLY command on it. So, effectively, we rip
the chunk->list pointers and requeue the same ASCONF_ACK chunk
another time. Since we process ASCONF_b, it's correctly marked
with end_of_packet and we enforce an uncork, and thus flush, thus
crashing the kernel.

Fix it by testing if the ASCONF_ACK is currently pending and if
that is the case, do not requeue it. When flushing the output
queue we may relink the chunk for preparing an outgoing packet,
but eventually unlink it when it's copied into the skb right
before transmission.

Joint work with Vlad Yasevich.

Fixes: 2e3216cd54b1 ("sctp: Follow security requirement of responding with 1 packet")
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Signed-off-by: Vlad Yasevich <vyasevich@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: sctp: fix skb_over_panic when receiving malformed ASCONF chunks

commit 9de7922bc709eee2f609cd01d98aaedc4cf5ea74 upstream.

Commit 6f4c618ddb0 ("SCTP : Add paramters validity check for
ASCONF chunk") added basic verification of ASCONF chunks, however,
it is still possible to remotely crash a server by sending a
special crafted ASCONF chunk, even up to pre 2.6.12 kernels:

skb_over_panic: text:ffffffffa01ea1c3 len:31056 put:30768
 head:ffff88011bd81800 data:ffff88011bd81800 tail:0x7950
 end:0x440 dev:<NULL>
 ------------[ cut here ]------------
kernel BUG at net/core/skbuff.c:129!
[...]
Call Trace:
 <IRQ>
 [<ffffffff8144fb1c>] skb_put+0x5c/0x70
 [<ffffffffa01ea1c3>] sctp_addto_chunk+0x63/0xd0 [sctp]
 [<ffffffffa01eadaf>] sctp_process_asconf+0x1af/0x540 [sctp]
 [<ffffffff8152d025>] ? _read_unlock_bh+0x15/0x20
 [<ffffffffa01e0038>] sctp_sf_do_asconf+0x168/0x240 [sctp]
 [<ffffffffa01e3751>] sctp_do_sm+0x71/0x1210 [sctp]
 [<ffffffff8147645d>] ? fib_rules_lookup+0xad/0xf0
 [<ffffffffa01e6b22>] ? sctp_cmp_addr_exact+0x32/0x40 [sctp]
 [<ffffffffa01e8393>] sctp_assoc_bh_rcv+0xd3/0x180 [sctp]
 [<ffffffffa01ee986>] sctp_inq_push+0x56/0x80 [sctp]
 [<ffffffffa01fcc42>] sctp_rcv+0x982/0xa10 [sctp]
 [<ffffffffa01d5123>] ? ipt_local_in_hook+0x23/0x28 [iptable_filter]
 [<ffffffff8148bdc9>] ? nf_iterate+0x69/0xb0
 [<ffffffff81496d10>] ? ip_local_deliver_finish+0x0/0x2d0
 [<ffffffff8148bf86>] ? nf_hook_slow+0x76/0x120
 [<ffffffff81496d10>] ? ip_local_deliver_finish+0x0/0x2d0
 [<ffffffff81496ded>] ip_local_deliver_finish+0xdd/0x2d0
 [<ffffffff81497078>] ip_local_deliver+0x98/0xa0
 [<ffffffff8149653d>] ip_rcv_finish+0x12d/0x440
 [<ffffffff81496ac5>] ip_rcv+0x275/0x350
 [<ffffffff8145c88b>] __netif_receive_skb+0x4ab/0x750
 [<ffffffff81460588>] netif_receive_skb+0x58/0x60

This can be triggered e.g., through a simple scripted nmap
connection scan injecting the chunk after the handshake, for
example, ...

  -------------- INIT[ASCONF; ASCONF_ACK] ------------->
  <----------- INIT-ACK[ASCONF; ASCONF_ACK] ------------
  -------------------- COOKIE-ECHO -------------------->
  <-------------------- COOKIE-ACK ---------------------
  ------------------ ASCONF; UNKNOWN ------------------>

... where ASCONF chunk of length 280 contains 2 parameters ...

  1) Add IP address parameter (param length: 16)
  2) Add/del IP address parameter (param length: 255)

... followed by an UNKNOWN chunk of e.g. 4 bytes. Here, the
Address Parameter in the ASCONF chunk is even missing, too.
This is just an example and similarly-crafted ASCONF chunks
could be used just as well.

The ASCONF chunk passes through sctp_verify_asconf() as all
parameters passed sanity checks, and after walking, we ended
up successfully at the chunk end boundary, and thus may invoke
sctp_process_asconf(). Parameter walking is done with
WORD_ROUND() to take padding into account.

In sctp_process_asconf()'s TLV processing, we may fail in
sctp_process_asconf_param() e.g., due to removal of the IP
address that is also the source address of the packet containing
the ASCONF chunk, and thus we need to add all TLVs after the
failure to our ASCONF response to remote via helper function
sctp_add_asconf_response(), which basically invokes a
sctp_addto_chunk() adding the error parameters to the given
skb.

When walking to the next parameter this time, we proceed
with ...

  length = ntohs(asconf_param->param_hdr.length);
  asconf_param = (void *)asconf_param + length;

... instead of the WORD_ROUND()'ed length, thus resulting here
in an off-by-one that leads to reading the follow-up garbage
parameter length of 12336, and thus throwing an skb_over_panic
for the reply when trying to sctp_addto_chunk() next time,
which implicitly calls the skb_put() with that length.

Fix it by using sctp_walk_params() [ which is also used in
INIT parameter processing ] macro in the verification *and*
in ASCONF processing: it will make sure we don't spill over,
that we walk parameters WORD_ROUND()'ed. Moreover, we're being
more defensive and guard against unknown parameter types and
missized addresses.

Joint work with Vlad Yasevich.

Fixes: b896b82be4ae ("[SCTP] ADDIP: Support for processing incoming ASCONF_ACK chunks.")
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Signed-off-by: Vlad Yasevich <vyasevich@gmail.com>
Acked-by: Neil Horman <nhorman@tuxdriver.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86, mm/ASLR: Fix stack randomization on 64-bit systems

commit 4e7c22d447bb6d7e37bfe39ff658486ae78e8d77 upstream.

The issue is that the stack for processes is not properly randomized on
64 bit architectures due to an integer overflow.

The affected function is randomize_stack_top() in file
"fs/binfmt_elf.c":

  static unsigned long randomize_stack_top(unsigned long stack_top)
  {
           unsigned int random_variable = 0;

           if ((current->flags & PF_RANDOMIZE) &&
                   !(current->personality & ADDR_NO_RANDOMIZE)) {
                   random_variable = get_random_int() & STACK_RND_MASK;
                   random_variable <<= PAGE_SHIFT;
           }
           return PAGE_ALIGN(stack_top) + random_variable;
           return PAGE_ALIGN(stack_top) - random_variable;
  }

Note that, it declares the "random_variable" variable as "unsigned int".
Since the result of the shifting operation between STACK_RND_MASK (which
is 0x3fffff on x86_64, 22 bits) and PAGE_SHIFT (which is 12 on x86_64):

	  random_variable <<= PAGE_SHIFT;

then the two leftmost bits are dropped when storing the result in the
"random_variable". This variable shall be at least 34 bits long to hold
the (22+12) result.

These two dropped bits have an impact on the entropy of process stack.
Concretely, the total stack entropy is reduced by four: from 2^28 to
2^30 (One fourth of expected entropy).

This patch restores back the entropy by correcting the types involved
in the operations in the functions randomize_stack_top() and
stack_maxrandom_size().

The successful fix can be tested with:

  $ for i in `seq 1 10`; do cat /proc/self/maps | grep stack; done
  7ffeda566000-7ffeda587000 rw-p 00000000 00:00 0                          [stack]
  7fff5a332000-7fff5a353000 rw-p 00000000 00:00 0                          [stack]
  7ffcdb7a1000-7ffcdb7c2000 rw-p 00000000 00:00 0                          [stack]
  7ffd5e2c4000-7ffd5e2e5000 rw-p 00000000 00:00 0                          [stack]
  ...

Once corrected, the leading bytes should be between 7ffc and 7fff,
rather than always being 7fff.

Signed-off-by: Hector Marco-Gisbert <hecmargi@upv.es>
Signed-off-by: Ismael Ripoll <iripoll@upv.es>
[ Rebased, fixed 80 char bugs, cleaned up commit message, added test example and CVE ]
Signed-off-by: Kees Cook <keescook@chromium.org>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Andrew Morton <akpm@linux-foundation.org>
Cc: Al Viro <viro@zeniv.linux.org.uk>
Fixes: CVE-2015-1593
Link: http://lkml.kernel.org/r/20150214173350.GA18393@www.outflux.net
Signed-off-by: Borislav Petkov <bp@suse.de>
Signed-off-by: Zefan Li <lizefan@huawei.com>

MIPS: IRQ: Fix disable_irq on CPU IRQs

commit a3e6c1eff54878506b2dddcc202df9cc8180facb upstream.

If the irq_chip does not define .irq_disable, any call to disable_irq
will defer disabling the IRQ until it fires while marked as disabled.
This assumes that the handler function checks for this condition, which
handle_percpu_irq does not. In this case, calling disable_irq leads to
an IRQ storm, if the interrupt fires while disabled.

This optimization is only useful when disabling the IRQ is slow, which
is not true for the MIPS CPU IRQ.

Disable this optimization by implementing .irq_disable and .irq_enable

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Cc: linux-mips@linux-mips.org
Patchwork: https://patchwork.linux-mips.org/patch/8949/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ASoC: atmel_ssc_dai: fix start event for I2S mode

commit a43bd7e125143b875caae6d4f9938855b440faaf upstream.

According to the I2S specification information as following:
  - WS = 0, channel 1 (left)
  - WS = 1, channel 2 (right)
So, the start event should be TF/RF falling edge.

Reported-by: Songjun Wu <songjun.wu@atmel.com>
Signed-off-by: Bo Shen <voice.shen@atmel.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ALSA: ak411x: Fix stall in work callback

commit 4161b4505f1690358ac0a9ee59845a7887336b21 upstream.

When ak4114 work calls its callback and the callback invokes
ak4114_reinit(), it stalls due to flush_delayed_work().  For avoiding
this, control the reentrance by introducing a refcount.  Also
flush_delayed_work() is replaced with cancel_delayed_work_sync().

The exactly same bug is present in ak4113.c and fixed as well.

Reported-by: Pavel Hofman <pavel.hofman@ivitera.com>
Acked-by: Jaroslav Kysela <perex@perex.cz>
Tested-by: Pavel Hofman <pavel.hofman@ivitera.com>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
[lizf: Backported to 3.4: snd_ak4113_reinit() and snd_ak4114_reinit()
used flush_delayed_work_sync() instead of flush_delayed_work()]
Signed-off-by: Zefan Li <lizefan@huawei.com>

lib/checksum.c: fix carry in csum_tcpudp_nofold

commit 150ae0e94634714b23919f0c333fee28a5b199d5 upstream.

The carry from the 64->32bits folding was dropped, e.g with:
saddr=0xFFFFFFFF daddr=0xFF0000FF len=0xFFFF proto=0 sum=1,
csum_tcpudp_nofold returned 0 instead of 1.

Signed-off-by: Karl Beldan <karl.beldan@rivierawaves.com>
Cc: Al Viro <viro@ZenIV.linux.org.uk>
Cc: Eric Dumazet <eric.dumazet@gmail.com>
Cc: Arnd Bergmann <arnd@arndb.de>
Cc: Mike Frysinger <vapier@gentoo.org>
Cc: netdev@vger.kernel.org
Cc: linux-kernel@vger.kernel.org
Signed-off-by: Eric Dumazet <edumazet@google.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

caif: remove wrong dev_net_set() call

commit 8997c27ec41127bf57421cc0205413d525421ddc upstream.

src_net points to the netns where the netlink message has been received. This
netns may be different from the netns where the interface is created (because
the user may add IFLA_NET_NS_[PID|FD]). In this case, src_net is the link netns.

It seems wrong to override the netns in the newlink() handler because if it
was not already src_net, it means that the user explicitly asks to create the
netdevice in another netns.

CC: Sjur Brændeland <sjur.brandeland@stericsson.com>
CC: Dmitry Tarnyagin <dmitry.tarnyagin@lockless.no>
Fixes: 8391c4aab1aa ("caif: Bugfixes in CAIF netdevice for close and flow control")
Fixes: c41254006377 ("caif-hsi: Add rtnl support")
Signed-off-by: Nicolas Dichtel <nicolas.dichtel@6wind.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
[lizf: Backported to 3.4: drop the change to drivers/net/caif/caif_hsi.c]
Signed-off-by: Zefan Li <lizefan@huawei.com>

MIPS: Fix kernel lockup or crash after CPU offline/online

commit c7754e75100ed5e3068ac5085747f2bfc386c8d6 upstream.

As printk() invocation can cause e.g. a TLB miss, printk() cannot be
called before the exception handlers have been properly initialized.
This can happen e.g. when netconsole has been loaded as a kernel module
and the TLB table has been cleared when a CPU was offline.

Call cpu_report() in start_secondary() only after the exception handlers
have been initialized to fix this.

Without the patch the kernel will randomly either lockup or crash
after a CPU is onlined and the console driver is a module.

Signed-off-by: Hemmo Nieminen <hemmo.nieminen@iki.fi>
Signed-off-by: Aaro Koskinen <aaro.koskinen@iki.fi>
Cc: David Daney <david.daney@cavium.com>
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/8953/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
[lizf: Backported to 3.4: adjust context]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: sysfs: fix memory leak in gpiod_export_link

commit 0f303db08df0df9bd0966443ad6001e63960af16 upstream.

Fix memory leak in the gpio sysfs interface due to failure to drop
reference to device returned by class_find_device when creating a link.

Fixes: a4177ee7f1a8 ("gpiolib: allow exported GPIO nodes to be named
using sysfs links")
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

gpio: sysfs: fix memory leak in gpiod_sysfs_set_active_low

commit 49d2ca84e433dab854c7a866bc6add09cfab682d upstream.

Fix memory leak in the gpio sysfs interface due to failure to drop
reference to device returned by class_find_device when setting the
gpio-line polarity.

Fixes: 0769746183ca ("gpiolib: add support for changing value polarity
in sysfs")
Signed-off-by: Johan Hovold <johan@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
[lizf: Backported to 3.4: adjust filename]
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: sctp: fix NULL pointer dereference in af->from_addr_param on malformed packet

commit e40607cbe270a9e8360907cb1e62ddf0736e4864 upstream.

An SCTP server doing ASCONF will panic on malformed INIT ping-of-death
in the form of:

  ------------ INIT[PARAM: SET_PRIMARY_IP] ------------>

While the INIT chunk parameter verification dissects through many things
in order to detect malformed input, it misses to actually check parameters
inside of parameters. E.g. RFC5061, section 4.2.4 proposes a 'set primary
IP address' parameter in ASCONF, which has as a subparameter an address
parameter.

So an attacker may send a parameter type other than SCTP_PARAM_IPV4_ADDRESS
or SCTP_PARAM_IPV6_ADDRESS, param_type2af() will subsequently return 0
and thus sctp_get_af_specific() returns NULL, too, which we then happily
dereference unconditionally through af->from_addr_param().

The trace for the log:

BUG: unable to handle kernel NULL pointer dereference at 0000000000000078
IP: [<ffffffffa01e9c62>] sctp_process_init+0x492/0x990 [sctp]
PGD 0
Oops: 0000 [#1] SMP
[...]
Pid: 0, comm: swapper Not tainted 2.6.32-504.el6.x86_64 #1 Bochs Bochs
RIP: 0010:[<ffffffffa01e9c62>]  [<ffffffffa01e9c62>] sctp_process_init+0x492/0x990 [sctp]
[...]
Call Trace:
 <IRQ>
 [<ffffffffa01f2add>] ? sctp_bind_addr_copy+0x5d/0xe0 [sctp]
 [<ffffffffa01e1fcb>] sctp_sf_do_5_1B_init+0x21b/0x340 [sctp]
 [<ffffffffa01e3751>] sctp_do_sm+0x71/0x1210 [sctp]
 [<ffffffffa01e5c09>] ? sctp_endpoint_lookup_assoc+0xc9/0xf0 [sctp]
 [<ffffffffa01e61f6>] sctp_endpoint_bh_rcv+0x116/0x230 [sctp]
 [<ffffffffa01ee986>] sctp_inq_push+0x56/0x80 [sctp]
 [<ffffffffa01fcc42>] sctp_rcv+0x982/0xa10 [sctp]
 [<ffffffffa01d5123>] ? ipt_local_in_hook+0x23/0x28 [iptable_filter]
 [<ffffffff8148bdc9>] ? nf_iterate+0x69/0xb0
 [<ffffffff81496d10>] ? ip_local_deliver_finish+0x0/0x2d0
 [<ffffffff8148bf86>] ? nf_hook_slow+0x76/0x120
 [<ffffffff81496d10>] ? ip_local_deliver_finish+0x0/0x2d0
[...]

A minimal way to address this is to check for NULL as we do on all
other such occasions where we know sctp_get_af_specific() could
possibly return with NULL.

Fixes: d6de3097592b ("[SCTP]: Add the handling of "Set Primary IP Address" parameter to INIT")
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Cc: Vlad Yasevich <vyasevich@gmail.com>
Acked-by: Neil Horman <nhorman@tuxdriver.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: sctp: fix passing wrong parameter header to param_type2af in sctp_process_param

commit cfbf654efc6d78dc9812e030673b86f235bf677d upstream.

When making use of RFC5061, section 4.2.4. for setting the primary IP
address, we're passing a wrong parameter header to param_type2af(),
resulting always in NULL being returned.

At this point, param.p points to a sctp_addip_param struct, containing
a sctp_paramhdr (type = 0xc004, length = var), and crr_id as a correlation
id. Followed by that, as also presented in RFC5061 section 4.2.4., comes
the actual sctp_addr_param, which also contains a sctp_paramhdr, but
this time with the correct type SCTP_PARAM_IPV{4,6}_ADDRESS that
param_type2af() can make use of. Since we already hold a pointer to
addr_param from previous line, just reuse it for param_type2af().

Fixes: d6de3097592b ("[SCTP]: Add the handling of "Set Primary IP Address" parameter to INIT")
Signed-off-by: Saran Maruti Ramanara <saran.neti@telus.com>
Signed-off-by: Daniel Borkmann <dborkman@redhat.com>
Acked-by: Vlad Yasevich <vyasevich@gmail.com>
Acked-by: Neil Horman <nhorman@tuxdriver.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ASoC: sgtl5000: add delay before first I2C access

commit 58cc9c9a175885bbf6bae3acf18233d0a8229a84 upstream.

To quote from section 1.3.1 of the data sheet:
	The SGTL5000 has an internal reset that is deasserted
	8 SYS_MCLK cycles after all power rails have been brought
	up. After this time, communication can start

	...
	1.0us represents 8 SYS_MCLK cycles at the minimum 8.0 MHz SYS_MCLK.

Signed-off-by: Eric Nelson <eric.nelson@boundarydevices.com>
Reviewed-by: Fabio Estevam <fabio.estevam@freescale.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

nilfs2: fix deadlock of segment constructor over I_SYNC flag

commit 7ef3ff2fea8bf5e4a21cef47ad87710a3d0fdb52 upstream.

Nilfs2 eventually hangs in a stress test with fsstress program.  This
issue was caused by the following deadlock over I_SYNC flag between
nilfs_segctor_thread() and writeback_sb_inodes():

  nilfs_segctor_thread()
    nilfs_segctor_thread_construct()
      nilfs_segctor_unlock()
        nilfs_dispose_list()
          iput()
            iput_final()
              evict()
                inode_wait_for_writeback()  * wait for I_SYNC flag

  writeback_sb_inodes()
     * set I_SYNC flag on inode->i_state
    __writeback_single_inode()
      do_writepages()
        nilfs_writepages()
          nilfs_construct_dsync_segment()
            nilfs_segctor_sync()
               * wait for completion of segment constructor
    inode_sync_complete()
       * clear I_SYNC flag after __writeback_single_inode() completed

writeback_sb_inodes() calls do_writepages() for dirty inodes after
setting I_SYNC flag on inode->i_state.  do_writepages() in turn calls
nilfs_writepages(), which can run segment constructor and wait for its
completion.  On the other hand, segment constructor calls iput(), which
can call evict() and wait for the I_SYNC flag on
inode_wait_for_writeback().

Since segment constructor doesn't know when I_SYNC will be set, it
cannot know whether iput() will block or not unless inode->i_nlink has a
non-zero count.  We can prevent evict() from being called in iput() by
implementing sop->drop_inode(), but it's not preferable to leave inodes
with i_nlink == 0 for long periods because it even defers file
truncation and inode deallocation.  So, this instead resolves the
deadlock by calling iput() asynchronously with a workqueue for inodes
with i_nlink == 0.

Signed-off-by: Ryusuke Konishi <konishi.ryusuke@lab.ntt.co.jp>
Cc: Al Viro <viro@zeniv.linux.org.uk>
Tested-by: Ryusuke Konishi <konishi.ryusuke@lab.ntt.co.jp>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

Drivers: hv: vmbus: incorrect device name is printed when child device is unregistered

commit 84672369ffb98a51d4ddf74c20a23636da3ad615 upstream.

Whenever a device is unregistered in vmbus_device_unregister (drivers/hv/vmbus_drv.c), the device name in the log message may contain garbage as the memory has already been freed by the time pr_info is called. Log example:
 [ 3149.170475] hv_vmbus: child device àõsèè0_5 unregistered

By logging the message just before calling device_unregister, the correct device name is printed:
[ 3145.034652] hv_vmbus: child device vmbus_0_5 unregistered

Also changing register & unregister messages to debug to avoid unnecessarily cluttering the kernel log.

Signed-off-by: Fernando M Soto <fsoto@bluecatnetworks.com>
Signed-off-by: K. Y. Srinivasan <kys@microsoft.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Cc: Joseph Salisbury <joseph.salisbury@canonical.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

pagemap: do not leak physical addresses to non-privileged userspace

commit ab676b7d6fbf4b294bf198fb27ade5b0e865c7ce upstream.

As pointed by recent post[1] on exploiting DRAM physical imperfection,
/proc/PID/pagemap exposes sensitive information which can be used to do
attacks.

This disallows anybody without CAP_SYS_ADMIN to read the pagemap.

[1] http://googleprojectzero.blogspot.com/2015/03/exploiting-dram-rowhammer-bug-to-gain.html

[ Eventually we might want to do anything more finegrained, but for now
  this is the simple model.   - Linus ]

Signed-off-by: Kirill A. Shutemov <kirill.shutemov@linux.intel.com>
Acked-by: Konstantin Khlebnikov <khlebnikov@openvz.org>
Acked-by: Andy Lutomirski <luto@amacapital.net>
Cc: Pavel Emelyanov <xemul@parallels.com>
Cc: Andrew Morton <akpm@linux-foundation.org>
Cc: Mark Seaborn <mseaborn@chromium.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>
[mancha: Backported to 3.10]
Signed-off-by: mancha security <mancha1@zoho.com>

jfs: fix readdir regression

Upstream commit 44512449, "jfs: fix readdir cookie incompatibility
with NFSv4", was backported incorrectly into the stable trees which
used the filldir callback (rather than dir_emit). The position is
being incorrectly passed to filldir for the . and .. entries.

The still-maintained stable trees that need to be fixed are 3.2.y,
3.4.y and 3.10.y.

https://bugzilla.kernel.org/show_bug.cgi?id=94741

Signed-off-by: Dave Kleikamp <dave.kleikamp@oracle.com>
Cc: jfs-discussion@lists.sourceforge.net
Signed-off-by: Zefan Li <lizefan@huawei.com>

ipvs: rerouting to local clients is not needed anymore

commit 579eb62ac35845686a7c4286c0a820b4eb1f96aa upstream.

commit f5a41847acc5 ("ipvs: move ip_route_me_harder for ICMP")
from 2.6.37 introduced ip_route_me_harder() call for responses to
local clients, so that we can provide valid rt_src after SNAT.
It was used by TCP to provide valid daddr for ip_send_reply().
After commit 0a5ebb8000c5 ("ipv4: Pass explicit daddr arg to
ip_send_reply()." from 3.0 this rerouting is not needed anymore
and should be avoided, especially in LOCAL_IN.

Fixes 3.12.33 crash in xfrm reported by Florian Wiessner:
"3.12.33 - BUG xfrm_selector_match+0x25/0x2f6"

Reported-by: Smart Weblications GmbH - Florian Wiessner <f.wiessner@smart-weblications.de>
Tested-by: Smart Weblications GmbH - Florian Wiessner <f.wiessner@smart-weblications.de>
Signed-off-by: Julian Anastasov <ja@ssi.bg>
Signed-off-by: Simon Horman <horms@verge.net.au>
[Julian: Backported to 3.4]
Signed-off-by: Julian Anastasov <ja@ssi.bg>
Acked-by: Simon Horman <horms@verge.net.au>
Signed-off-by: Zefan Li <lizefan@huawei.com>

staging: comedi: cb_pcidas64: fix incorrect AI range code handling

commit be8e89087ec2d2c8a1ad1e3db64bf4efdfc3c298 upstream.

The hardware range code values and list of valid ranges for the AI
subdevice is incorrect for several supported boards.  The hardware range
code values for all boards except PCI-DAS4020/12 is determined by
calling `ai_range_bits_6xxx()` based on the maximum voltage of the range
and whether it is bipolar or unipolar, however it only returns the
correct hardware range code for the PCI-DAS60xx boards.  For
PCI-DAS6402/16 (and /12) it returns the wrong code for the unipolar
ranges.  For PCI-DAS64/Mx/16 it returns the wrong code for all the
ranges and the comedi range table is incorrect.

Change `ai_range_bits_6xxx()` to use a look-up table pointed to by new
member `ai_range_codes` of `struct pcidas64_board` to map the comedi
range table indices to the hardware range codes.  Use a new comedi range
table for the PCI-DAS64/Mx/16 boards (and the commented out variants).

Signed-off-by: Ian Abbott <abbotti@mev.co.uk>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
[Ian: Backported to 3.4]
Signed-off-by: Zefan Li <lizefan@huawei.com>

sched/rt: Reduce rq lock contention by eliminating locking of non-feasible target

commit 80e3d87b2c5582db0ab5e39610ce3707d97ba409 upstream.

This patch adds checks that prevens futile attempts to move rt tasks
to a CPU with active tasks of equal or higher priority.

This reduces run queue lock contention and improves the performance of
a well known OLTP benchmark by 0.7%.

Signed-off-by: Tim Chen <tim.c.chen@linux.intel.com>
Signed-off-by: Peter Zijlstra (Intel) <peterz@infradead.org>
Cc: Shawn Bohrer <sbohrer@rgmadvisors.com>
Cc: Suruchi Kadu <suruchi.a.kadu@intel.com>
Cc: Doug Nelson<doug.nelson@intel.com>
Cc: Steven Rostedt <rostedt@goodmis.org>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Link: http://lkml.kernel.org/r/1421430374.2399.27.camel@schen9-desk2.jf.intel.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net:socket: set msg_namelen to 0 if msg_name is passed as NULL in msghdr struct from userland.

commit 6a2a2b3ae0759843b22c929881cc184b00cc63ff upstream.

Linux manpage for recvmsg and sendmsg calls does not explicitly mention setting msg_namelen to 0 when
msg_name passed set as NULL. When developers don't set msg_namelen member in msghdr, it might contain garbage
value which will fail the validation check and sendmsg and recvmsg calls from kernel will return EINVAL. This will
break old binaries and any code for which there is no access to source code.
To fix this, we set msg_namelen to 0 when msg_name is passed as NULL from userland.

Signed-off-by: Ani Sinha <ani@arista.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Cc: Michal Marek <mmarek@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

fsnotify: next_i is freed during fsnotify_unmount_inodes.

commit 6424babfd68dd8a83d9c60a5242d27038856599f upstream.

During file system stress testing on 3.10 and 3.12 based kernels, the
umount command occasionally hung in fsnotify_unmount_inodes in the
section of code:

                spin_lock(&inode->i_lock);
                if (inode->i_state & (I_FREEING|I_WILL_FREE|I_NEW)) {
                        spin_unlock(&inode->i_lock);
                        continue;
                }

As this section of code holds the global inode_sb_list_lock, eventually
the system hangs trying to acquire the lock.

Multiple crash dumps showed:

The inode->i_state == 0x60 and i_count == 0 and i_sb_list would point
back at itself.  As this is not the value of list upon entry to the
function, the kernel never exits the loop.

To help narrow down problem, the call to list_del_init in
inode_sb_list_del was changed to list_del.  This poisons the pointers in
the i_sb_list and causes a kernel to panic if it transverse a freed
inode.

Subsequent stress testing paniced in fsnotify_unmount_inodes at the
bottom of the list_for_each_entry_safe loop showing next_i had become
free.

We believe the root cause of the problem is that next_i is being freed
during the window of time that the list_for_each_entry_safe loop
temporarily releases inode_sb_list_lock to call fsnotify and
fsnotify_inode_delete.

The code in fsnotify_unmount_inodes attempts to prevent the freeing of
inode and next_i by calling __iget.  However, the code doesn't do the
__iget call on next_i

	if i_count == 0 or
	if i_state & (I_FREEING | I_WILL_FREE)

The patch addresses this issue by advancing next_i in the above two cases
until we either find a next_i which we can __iget or we reach the end of
the list.  This makes the handling of next_i more closely match the
handling of the variable "inode."

The time to reproduce the hang is highly variable (from hours to days.) We
ran the stress test on a 3.10 kernel with the proposed patch for a week
without failure.

During list_for_each_entry_safe, next_i is becoming free causing
the loop to never terminate.  Advance next_i in those cases where
__iget is not done.

Signed-off-by: Jerry Hoemann <jerry.hoemann@hp.com>
Cc: Jeff Kirsher <jeffrey.t.kirsher@intel.com>
Cc: Ken Helias <kenhelias@firemail.de>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Jan Kara <jack@suse.cz>
Signed-off-by: Zefan Li <lizefan@huawei.com>

x86, cpu, amd: Add workaround for family 16h, erratum 793

commit 3b56496865f9f7d9bcb2f93b44c63f274f08e3b6 upstream.

This adds the workaround for erratum 793 as a precaution in case not
every BIOS implements it.  This addresses CVE-2013-6885.

Erratum text:

[Revision Guide for AMD Family 16h Models 00h-0Fh Processors,
document 51810 Rev. 3.04 November 2013]

793 Specific Combination of Writes to Write Combined Memory Types and
Locked Instructions May Cause Core Hang

Description

Under a highly specific and detailed set of internal timing
conditions, a locked instruction may trigger a timing sequence whereby
the write to a write combined memory type is not flushed, causing the
locked instruction to stall indefinitely.

Potential Effect on System

Processor core hang.

Suggested Workaround

BIOS should set MSR
C001_1020[15] = 1b.

Fix Planned

No fix planned

[ hpa: updated description, fixed typo in MSR name ]

Signed-off-by: Borislav Petkov <bp@suse.de>
Link: http://lkml.kernel.org/r/20140114230711.GS29865@pd.tnic
Tested-by: Aravind Gopalakrishnan <aravind.gopalakrishnan@amd.com>
Signed-off-by: H. Peter Anvin <hpa@linux.intel.com>
[bwh: Backported to 3.2:
 - Adjust filename
 - Venkatesh Srinivas pointed out we should use {rd,wr}msrl_safe() to
   avoid crashing on KVM.  This was fixed upstream by commit 8f86a7373a1c
   ("x86, AMD: Convert to the new bit access MSR accessors") but that's too
   much trouble to backport.  Here we must use {rd,wr}msrl_amd_safe().]
Signed-off-by: Ben Hutchings <ben@decadent.org.uk>
Cc: Moritz Muehlenhoff <jmm@debian.org>
Cc: Venkatesh Srinivas <venkateshs@google.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>

s390/3215: fix tty output containing tabs

commit e512d56c799517f33b301d81e9a5e0ebf30c2d1e upstream.

git commit 37f81fa1f63ad38e16125526bb2769ae0ea8d332
"n_tty: do O_ONLCR translation as a single write"
surfaced a bug in the 3215 device driver. In combination this
broke tab expansion for tty ouput.

The cause is an asymmetry in the behaviour of tty3215_ops->write
vs tty3215_ops->put_char. The put_char function scans for '\t'
but the write function does not.

As the driver has logic for the '\t' expansion remove XTABS
from c_oflag of the initial termios as well.

Reported-by: Stephen Powell <zlinuxman@wowway.com>
Signed-off-by: Martin Schwidefsky <schwidefsky@de.ibm.com>
Cc: Ben Hutchings <ben@decadent.org.uk>
Signed-off-by: Zefan Li <lizefan@huawei.com>

ntp: Fixup adjtimex freq validation on 32-bit systems

commit 29183a70b0b828500816bd794b3fe192fce89f73 upstream.

Additional validation of adjtimex freq values to avoid
potential multiplication overflows were added in commit
5e5aeb4367b (time: adjtimex: Validate the ADJ_FREQUENCY values)

Unfortunately the patch used LONG_MAX/MIN instead of
LLONG_MAX/MIN, which was fine on 64-bit systems, but being
much smaller on 32-bit systems caused false positives
resulting in most direct frequency adjustments to fail w/
EINVAL.

ntpd only does direct frequency adjustments at startup, so
the issue was not as easily observed there, but other time
sync applications like ptpd and chrony were more effected by
the bug.

See bugs:

  https://bugzilla.kernel.org/show_bug.cgi?id=92481
  https://bugzilla.redhat.com/show_bug.cgi?id=1188074

This patch changes the checks to use LLONG_MAX for
clarity, and additionally the checks are disabled
on 32-bit systems since LLONG_MAX/PPM_SCALE is always
larger then the 32-bit long freq value, so multiplication
overflows aren't possible there.

Reported-by: Josh Boyer <jwboyer@fedoraproject.org>
Reported-by: George Joseph <george.joseph@fairview5.com>
Tested-by: George Joseph <george.joseph@fairview5.com>
Signed-off-by: John Stultz <john.stultz@linaro.org>
Signed-off-by: Peter Zijlstra (Intel) <peterz@infradead.org>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Sasha Levin <sasha.levin@oracle.com>
Link: http://lkml.kernel.org/r/1423553436-29747-1-git-send-email-john.stultz@linaro.org
[ Prettified the changelog and the comments a bit. ]
Signed-off-by: Ingo Molnar <mingo@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

spi: dw: revisit FIFO size detection again

commit 9d239d353c319f9ff884c287ce47feb7cdf60ddc upstream.

The commit d297933cc7fc (spi: dw: Fix detecting FIFO depth) tries to fix the
logic of the FIFO detection based on the description on the comments. However,
there is a slight difference between numbers in TX Level and TX FIFO size.

So, by specification the FIFO size would be in a range 2-256 bytes. From TX
Level prospective it means we can set threshold in the range 0-(FIFO size - 1)
bytes. Hence there are currently two issues:
  a) FIFO size 2 bytes is actually skipped since TX Level is 1 bit and could be
     either 0 or 1 byte;
  b) FIFO size is incorrectly decreased by 1 which already done by meaning of
     TX Level register.

This patch fixes it eventually right.

Fixes: d297933cc7fc (spi: dw: Fix detecting FIFO depth)
Reviewed-by: Axel Lin <axel.lin@ingics.com>
Signed-off-by: Andy Shevchenko <andriy.shevchenko@linux.intel.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

nilfs2: fix deadlock of segment constructor during recovery

commit 283ee1482f349d6c0c09dfb725db5880afc56813 upstream.

According to a report from Yuxuan Shui, nilfs2 in kernel 3.19 got stuck
during recovery at mount time.  The code path that caused the deadlock was
as follows:

  nilfs_fill_super()
    load_nilfs()
      nilfs_salvage_orphan_logs()
        * Do roll-forwarding, attach segment constructor for recovery,
          and kick it.

        nilfs_segctor_thread()
          nilfs_segctor_thread_construct()
           * A lock is held with nilfs_transaction_lock()
             nilfs_segctor_do_construct()
               nilfs_segctor_drop_written_files()
                 iput()
                   iput_final()
                     write_inode_now()
                       writeback_single_inode()
                         __writeback_single_inode()
                           do_writepages()
                             nilfs_writepage()
                               nilfs_construct_dsync_segment()
                                 nilfs_transaction_lock() --> deadlock

This can happen if commit 7ef3ff2fea8b ("nilfs2: fix deadlock of segment
constructor over I_SYNC flag") is applied and roll-forward recovery was
performed at mount time.  The roll-forward recovery can happen if datasync
write is done and the file system crashes immediately after that.  For
instance, we can reproduce the issue with the following steps:

 < nilfs2 is mounted on /nilfs (device: /dev/sdb1) >
 # dd if=/dev/zero of=/nilfs/test bs=4k count=1 && sync
 # dd if=/dev/zero of=/nilfs/test conv=notrunc oflag=dsync bs=4k
 count=1 && reboot -nfh
 < the system will immediately reboot >
 # mount -t nilfs2 /dev/sdb1 /nilfs

The deadlock occurs because iput() can run segment constructor through
writeback_single_inode() if MS_ACTIVE flag is not set on sb->s_flags.  The
above commit changed segment constructor so that it calls iput()
asynchronously for inodes with i_nlink == 0, but that change was
imperfect.

This fixes the another deadlock by deferring iput() in segment constructor
even for the case that mount is not finished, that is, for the case that
MS_ACTIVE flag is not set.

Signed-off-by: Ryusuke Konishi <konishi.ryusuke@lab.ntt.co.jp>
Reported-by: Yuxuan Shui <yshuiv7@gmail.com>
Tested-by: Ryusuke Konishi <konishi.ryusuke@lab.ntt.co.jp>
Cc: Al Viro <viro@zeniv.linux.org.uk>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

net: compat: Update get_compat_msghdr() to match copy_msghdr_from_user() behaviour

commit 91edd096e224941131f896b86838b1e59553696a upstream.

Commit db31c55a6fb2 (net: clamp ->msg_namelen instead of returning an
error) introduced the clamping of msg_namelen when the unsigned value
was larger than sizeof(struct sockaddr_storage). This caused a
msg_namelen of -1 to be valid. The native code was subsequently fixed by
commit dbb490b96584 (net: socket: error on a negative msg_namelen).

In addition, the native code sets msg_namelen to 0 when msg_name is
NULL. This was done in commit (6a2a2b3ae075 net:socket: set msg_namelen
to 0 if msg_name is passed as NULL in msghdr struct from userland) and
subsequently updated by 08adb7dabd48 (fold verify_iovec() into
copy_msghdr_from_user()).

This patch brings the get_compat_msghdr() in line with
copy_msghdr_from_user().

Fixes: db31c55a6fb2 (net: clamp ->msg_namelen instead of returning an error)
Cc: David S. Miller <davem@davemloft.net>
Cc: Dan Carpenter <dan.carpenter@oracle.com>
Signed-off-by: Catalin Marinas <catalin.marinas@arm.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
[lizf: Backported to 3.4: s/uaddr/tmp1/]
Signed-off-by: Zefan Li <lizefan@huawei.com>

mm: fix anon_vma->degree underflow in anon_vma endless growing prevention

commit 3fe89b3e2a7bbf3e97657104b9b33a9d81b950b3 upstream.

I have constantly stumbled upon "kernel BUG at mm/rmap.c:399!" after
upgrading to 3.19 and had no luck with 4.0-rc1 neither.

So, after looking into new logic introduced by commit 7a3ef208e662 ("mm:
prevent endless growth of anon_vma hierarchy"), I found chances are that
unlink_anon_vmas() is called without incrementing dst->anon_vma->degree
in anon_vma_clone() due to allocation failure.  If dst->anon_vma is not
NULL in error path, its degree will be incorrectly decremented in
unlink_anon_vmas() and eventually underflow when exiting as a result of
another call to unlink_anon_vmas().  That's how "kernel BUG at
mm/rmap.c:399!" is triggered for me.

This patch fixes the underflow by dropping dst->anon_vma when allocation
fails.  It's safe to do so regardless of original value of dst->anon_vma
because dst->anon_vma doesn't have valid meaning if anon_vma_clone()
fails.  Besides, callers don't care dst->anon_vma in such case neither.

Also suggested by Michal Hocko, we can clean up vma_adjust() a bit as
anon_vma_clone() now does the work.

[akpm@linux-foundation.org: tweak comment]
Fixes: 7a3ef208e662 ("mm: prevent endless growth of anon_vma hierarchy")
Signed-off-by: Leon Yu <chianglungyu@gmail.com>
Signed-off-by: Konstantin Khlebnikov <koct9i@gmail.com>
Reviewed-by: Michal Hocko <mhocko@suse.cz>
Acked-by: Rik van Riel <riel@redhat.com>
Acked-by: David Rientjes <rientjes@google.com>
Signed-off-by: Andrew Morton <akpm@linux-foundation.org>
Signed-off-by: Linus Torvalds <torvalds@linux-foundation.org>
Signed-off-by: Zefan Li <lizefan@huawei.com>

lib/checksum.c: fix build for generic csum_tcpudp_nofold

commit 9ce357795ef208faa0d59894d9d119a7434e37f3 upstream.

Fixed commit added from64to32 under _#ifndef do_csum_ but used it
under _#ifndef csum_tcpudp_nofold_, breaking some builds (Fengguang's
robot reported TILEGX's). Move from64to32 under the latter.

Fixes: 150ae0e94634 ("lib/checksum.c: fix carry in csum_tcpudp_nofold")
Reported-by: kbuild test robot <fengguang.wu@intel.com>
Signed-off-by: Karl Beldan <karl.beldan@rivierawaves.com>
Cc: Eric Dumazet <edumazet@google.com>
Cc: David S. Miller <davem@davemloft.net>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Zefan Li <lizefan@huawei.com>

PCI: Handle read-only BARs on AMD CS553x devices

commit 06cf35f903aa6da0cc8d9f81e9bcd1f7e1b534bb upstream.

Some AMD CS553x devices have read-only BARs because of a firmware or
hardware defect.  There's a workaround in quirk_cs5536_vsa(), but it no
longer works after 36e8164882ca ("PCI: Restore detection of read-only
BARs").  Prior to 36e8164882ca, we filled in res->start; afterwards we
leave it zeroed out.  The quirk only updated the size, so the driver tried
to use a region starting at zero, which didn't work.

Expand quirk_cs5536_vsa() to read the base addresses from the BARs and
hard-code the sizes.

On Nix's system BAR 2's read-only value is 0x6200.  Prior to 36e8164882ca,
we interpret that as a 512-byte BAR based on the lowest-order bit set.  Per
datasheet sec 5.6.1, that BAR (MFGPT) requires only 64 bytes; use that to
avoid clearing any address bits if a platform uses only 64-byte alignment.

[bhelgaas: changelog, reduce BAR 2 size to 64]
Fixes: 36e8164882ca ("PCI: Restore detection of read-only BARs")
Link: https://bugzilla.kernel.org/show_bug.cgi?id=85991#c4
Link: http://support.amd.com/TechDocs/31506_cs5535_databook.pdf
Link: http://support.amd.com/TechDocs/33238G_cs5536_db.pdf
Reported-and-tested-by: Nix <nix@esperi.org.uk>
Signed-off-by: Myron Stowe <myron.stowe@redhat.com>
Signed-off-by: Bjorn Helgaas <bhelgaas@google.com>
Signed-off-by: Zefan Li <lizefan@huawei.com>
---
 Documentation/kernel-parameters.txt          |   1 +
 Makefile                                     |   2 +-
 arch/alpha/mm/fault.c                        |   2 +
 arch/arm/mm/proc-xscale.S                    |   4 +-
 arch/avr32/mm/fault.c                        |   2 +
 arch/cris/mm/fault.c                         |   2 +
 arch/frv/mm/fault.c                          |   2 +
 arch/ia64/mm/fault.c                         |   2 +
 arch/m32r/mm/fault.c                         |   2 +
 arch/m68k/mm/fault.c                         |   2 +
 arch/microblaze/mm/fault.c                   |   2 +
 arch/mips/kernel/irq_cpu.c                   |   4 +
 arch/mips/kernel/smp.c                       |   2 +-
 arch/mips/loongson/common/Makefile           |   3 +-
 arch/mips/mm/fault.c                         |   2 +
 arch/mn10300/mm/fault.c                      |   2 +
 arch/openrisc/mm/fault.c                     |   2 +
 arch/parisc/mm/fault.c                       |   2 +
 arch/powerpc/mm/fault.c                      |   6 +-
 arch/powerpc/platforms/cell/spu_fault.c      |   2 +-
 arch/powerpc/xmon/xmon.c                     |   7 +-
 arch/s390/mm/fault.c                         |   6 ++
 arch/score/mm/fault.c                        |   2 +
 arch/sh/mm/fault_32.c                        |   2 +
 arch/sh/mm/tlbflush_64.c                     |   2 +
 arch/sparc/mm/fault_32.c                     |   2 +
 arch/sparc/mm/fault_64.c                     |   2 +
 arch/tile/mm/fault.c                         |   2 +
 arch/um/kernel/trap.c                        |   2 +
 arch/x86/include/asm/ldt.h                   |   7 ++
 arch/x86/include/asm/msr-index.h             |   1 +
 arch/x86/kernel/cpu/amd.c                    |  10 ++
 arch/x86/kernel/cpu/mshyperv.c               |   1 +
 arch/x86/kernel/kprobes.c                    |  20 +++-
 arch/x86/kernel/process_64.c                 | 101 +++++++++++++-----
 arch/x86/kernel/tls.c                        |  16 +++
 arch/x86/mm/fault.c                          |   2 +
 arch/x86/mm/mmap.c                           |   6 +-
 arch/x86/um/sys_call_table_32.c              |   2 +-
 arch/x86/um/sys_call_table_64.c              |   2 +-
 arch/x86/vdso/vma.c                          |  36 +++++--
 arch/xtensa/mm/fault.c                       |   2 +
 block/genhd.c                                |  11 +-
 crypto/af_alg.c                              |   3 +
 drivers/ata/ahci.c                           |  26 +++++
 drivers/ata/libata-core.c                    |   5 +-
 drivers/ata/libata-sff.c                     |  12 +++
 drivers/ata/sata_dwc_460ex.c                 |  26 +++--
 drivers/ata/sata_fsl.c                       |   2 +-
 drivers/ata/sata_sil24.c                     |   2 +-
 drivers/base/bus.c                           |   8 +-
 drivers/base/core.c                          | 111 +++++++++++++++-----
 drivers/block/drbd/drbd_req.c                |   1 +
 drivers/gpio/gpiolib.c                       | 147 +++++++++++++++------------
 drivers/gpu/drm/i915/i915_gem.c              |  14 +++
 drivers/gpu/drm/i915/intel_lvds.c            |  24 ++---
 drivers/gpu/drm/radeon/radeon_kms.c          |   2 +
 drivers/gpu/drm/radeon/radeon_ttm.c          |   2 +-
 drivers/gpu/drm/vmwgfx/vmwgfx_fence.c        |  38 ++-----
 drivers/hid/hid-roccat-pyra.c                |   7 ++
 drivers/hv/vmbus_drv.c                       |   8 +-
 drivers/i2c/busses/i2c-davinci.c             |   8 +-
 drivers/input/joystick/xpad.c                |  16 ++-
 drivers/input/serio/i8042-x86ia64io.h        |  39 +++++++
 drivers/input/serio/i8042.c                  |  14 +++
 drivers/iommu/intel-iommu.c                  |   8 +-
 drivers/mfd/tc6393xb.c                       |  13 ++-
 drivers/mtd/ubi/upd.c                        |  10 +-
 drivers/net/can/dev.c                        |   8 +-
 drivers/net/can/usb/peak_usb/pcan_usb_core.c |  17 ++--
 drivers/net/can/usb/peak_usb/pcan_usb_pro.c  |   3 +-
 drivers/net/wireless/ath/ath5k/qcu.c         |   8 +-
 drivers/net/wireless/ath/ath9k/hw.h          |   4 +-
 drivers/net/wireless/ath/ath9k/mac.c         |   9 +-
 drivers/pci/probe.c                          |   3 +
 drivers/pci/quirks.c                         |  41 +++++++-
 drivers/platform/x86/hp_accel.c              |   1 +
 drivers/regulator/core.c                     |   2 +
 drivers/s390/char/con3215.c                  |  20 +++-
 drivers/scsi/NCR5380.c                       |  12 +--
 drivers/scsi/aha1740.c                       |   2 +-
 drivers/scsi/atari_NCR5380.c                 |   2 +-
 drivers/scsi/bnx2fc/bnx2fc_fcoe.c            |   7 ++
 drivers/scsi/megaraid.c                      |   8 +-
 drivers/scsi/megaraid/megaraid_sas_base.c    |   2 +-
 drivers/scsi/sd.c                            |   5 +-
 drivers/scsi/storvsc_drv.c                   |   7 +-
 drivers/scsi/sun3_NCR5380.c                  |  10 +-
 drivers/spi/spi-dw-mid.c                     |   1 -
 drivers/spi/spi-dw.c                         |  10 +-
 drivers/staging/comedi/drivers/cb_pcidas64.c | 123 +++++++++++++---------
 drivers/staging/iio/events.h                 |   2 +-
 drivers/target/iscsi/iscsi_target_util.c     |  26 ++---
 drivers/tty/serial/samsung.c                 |   4 +
 drivers/usb/class/cdc-acm.c                  |  10 +-
 drivers/usb/core/config.c                    |  11 ++
 drivers/usb/core/quirks.c                    |  11 ++
 drivers/usb/host/pci-quirks.c                |  18 +++-
 drivers/usb/host/xhci-pci.c                  |   2 +-
 drivers/usb/host/xhci-ring.c                 |  43 ++------
 drivers/usb/host/xhci.c                      | 102 ++++++++++---------
 drivers/usb/host/xhci.h                      |   2 +-
 drivers/usb/renesas_usbhs/mod_gadget.c       |   3 +
 drivers/usb/serial/console.c                 |  15 ++-
 drivers/usb/serial/cp210x.c                  |   3 +
 drivers/usb/serial/ftdi_sio.c                |  33 ++++++
 drivers/usb/serial/ftdi_sio_ids.h            |  39 ++++++-
 drivers/usb/serial/keyspan.c                 |  97 +++++++++++-------
 drivers/usb/serial/ssu100.c                  |  11 +-
 drivers/usb/storage/scsiglue.c               |   4 +
 drivers/usb/storage/unusual_devs.h           |  14 +++
 drivers/video/logo/logo.c                    |  17 +++-
 drivers/virtio/virtio.c                      |  19 ++--
 drivers/virtio/virtio_pci.c                  |  13 +--
 fs/binfmt_elf.c                              |   5 +-
 fs/btrfs/disk-io.c                           |   6 --
 fs/btrfs/extent-tree.c                       |  10 +-
 fs/ecryptfs/file.c                           |  12 ---
 fs/ecryptfs/main.c                           |  16 ++-
 fs/fs-writeback.c                            |  28 +++--
 fs/isofs/rock.c                              |   9 ++
 fs/jfs/jfs_dtree.c                           |   4 +-
 fs/ncpfs/ioctl.c                             |   1 -
 fs/nfsd/nfs4callback.c                       |   8 +-
 fs/nilfs2/nilfs.h                            |   2 -
 fs/nilfs2/segment.c                          |  45 +++++++-
 fs/nilfs2/segment.h                          |   5 +
 fs/notify/inode_mark.c                       |  17 ++--
 fs/ocfs2/aops.c                              |  16 ++-
 fs/proc/stat.c                               |   2 +-
 fs/proc/task_mmu.c                           |  10 ++
 fs/udf/dir.c                                 |   3 +-
 fs/udf/inode.c                               |  14 +++
 fs/udf/namei.c                               |   3 +-
 fs/udf/symlink.c                             |  57 +++++++++--
 fs/udf/udfdecl.h                             |   3 +-
 fs/udf/unicode.c                             |  28 ++---
 include/linux/device.h                       |   5 +
 include/linux/kernel_stat.h                  |   5 +
 include/linux/libata.h                       |   1 +
 include/linux/mm.h                           |   7 +-
 include/linux/rmap.h                         |  10 ++
 include/linux/sysfs.h                        |   9 ++
 include/linux/time.h                         |  13 +++
 include/linux/usb/quirks.h                   |  11 ++
 include/linux/usb_usual.h                    |   4 +-
 include/linux/virtio.h                       |   6 +-
 include/linux/writeback.h                    |   1 -
 include/net/sctp/sctp.h                      |   5 +
 include/net/sctp/sm.h                        |   6 +-
 include/scsi/scsi_device.h                   |   1 +
 include/sound/ak4113.h                       |   2 +-
 include/sound/ak4114.h                       |   2 +-
 kernel/irq/internals.h                       |   8 ++
 kernel/irq/irqdesc.c                         |  52 ++++++++++
 kernel/irq/proc.c                            |  22 +++-
 kernel/sched/rt.c                            |  17 +++-
 kernel/time.c                                |   4 +
 kernel/time/ntp.c                            |  11 ++
 lib/checksum.c                               |  12 ++-
 mm/ksm.c                                     |   2 +-
 mm/memory.c                                  |  63 +++++++-----
 mm/mmap.c                                    |  14 ++-
 mm/page-writeback.c                          |  43 +++-----
 mm/rmap.c                                    |  49 ++++++++-
 net/caif/chnl_net.c                          |   1 -
 net/compat.c                                 |   7 ++
 net/core/dev.c                               |  14 +--
 net/ipv6/ip6_fib.c                           |  45 ++++----
 net/mac80211/rx.c                            |  11 +-
 net/netfilter/ipvs/ip_vs_core.c              |  32 ++++--
 net/sctp/associola.c                         |   3 +-
 net/sctp/sm_make_chunk.c                     | 104 +++++++++++--------
 net/sctp/sm_statefuns.c                      |  18 +---
 net/socket.c                                 |   3 +
 net/sunrpc/svcsock.c                         |  27 +++--
 net/wireless/nl80211.c                       |   9 +-
 scripts/recordmcount.pl                      |   1 -
 security/keys/encrypted-keys/encrypted.c     |   5 +-
 sound/core/seq/seq_dummy.c                   |  31 ------
 sound/i2c/other/ak4113.c                     |  17 ++--
 sound/i2c/other/ak4114.c                     |  18 ++--
 sound/pci/hda/hda_intel.c                    |  14 ++-
 sound/pci/hda/patch_sigmatel.c               |   4 +-
 sound/soc/atmel/atmel_ssc_dai.c              |  18 +---
 sound/soc/codecs/sgtl5000.c                  |   3 +
 sound/soc/codecs/sigmadsp.c                  |   7 ++
 sound/soc/codecs/wm8960.c                    |   2 +-
 sound/usb/midi.c                             |   2 +
 sound/usb/mixer.c                            |   1 +
 sound/usb/mixer_maps.c                       |  15 ++-
 191 files changed, 1862 insertions(+), 881 deletions(-)

diff --git a/Documentation/kernel-parameters.txt b/Documentation/kernel-parameters.txt
index d42545c..f10244f 100644
--- a/Documentation/kernel-parameters.txt
+++ b/Documentation/kernel-parameters.txt
@@ -992,6 +992,7 @@ bytes respectively. Such letter suffixes can also be entirely omitted.
 	i8042.notimeout	[HW] Ignore timeout condition signalled by controller
 	i8042.reset	[HW] Reset the controller during init and cleanup
 	i8042.unlock	[HW] Unlock (ignore) the keylock
+	i8042.kbdreset  [HW] Reset device connected to KBD port
 
 	i810=		[HW,DRM]
 
diff --git a/Makefile b/Makefile
index 391fb89..79f1e27 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 4
-SUBLEVEL = 106
+SUBLEVEL = 107
 EXTRAVERSION =
 NAME = Saber-toothed Squirrel
 
diff --git a/arch/alpha/mm/fault.c b/arch/alpha/mm/fault.c
index 5eecab1..f153733 100644
--- a/arch/alpha/mm/fault.c
+++ b/arch/alpha/mm/fault.c
@@ -149,6 +149,8 @@ do_page_fault(unsigned long address, unsigned long mmcsr,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/arm/mm/proc-xscale.S b/arch/arm/mm/proc-xscale.S
index e766f88..08b51b7 100644
--- a/arch/arm/mm/proc-xscale.S
+++ b/arch/arm/mm/proc-xscale.S
@@ -535,7 +535,7 @@ ENTRY(cpu_xscale_do_suspend)
 	mrc	p15, 0, r5, c15, c1, 0	@ CP access reg
 	mrc	p15, 0, r6, c13, c0, 0	@ PID
 	mrc	p15, 0, r7, c3, c0, 0	@ domain ID
-	mrc	p15, 0, r8, c1, c1, 0	@ auxiliary control reg
+	mrc	p15, 0, r8, c1, c0, 1	@ auxiliary control reg
 	mrc	p15, 0, r9, c1, c0, 0	@ control reg
 	bic	r4, r4, #2		@ clear frequency change bit
 	stmia	r0, {r4 - r9}		@ store cp regs
@@ -552,7 +552,7 @@ ENTRY(cpu_xscale_do_resume)
 	mcr	p15, 0, r6, c13, c0, 0	@ PID
 	mcr	p15, 0, r7, c3, c0, 0	@ domain ID
 	mcr	p15, 0, r1, c2, c0, 0	@ translation table base addr
-	mcr	p15, 0, r8, c1, c1, 0	@ auxiliary control reg
+	mcr	p15, 0, r8, c1, c0, 1	@ auxiliary control reg
 	mov	r0, r9			@ control register
 	b	cpu_resume_mmu
 ENDPROC(cpu_xscale_do_resume)
diff --git a/arch/avr32/mm/fault.c b/arch/avr32/mm/fault.c
index f7040a1..632b649 100644
--- a/arch/avr32/mm/fault.c
+++ b/arch/avr32/mm/fault.c
@@ -136,6 +136,8 @@ asmlinkage void do_page_fault(unsigned long ecr, struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/cris/mm/fault.c b/arch/cris/mm/fault.c
index b4760d8..b07c00c 100644
--- a/arch/cris/mm/fault.c
+++ b/arch/cris/mm/fault.c
@@ -167,6 +167,8 @@ do_page_fault(unsigned long address, struct pt_regs *regs,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/frv/mm/fault.c b/arch/frv/mm/fault.c
index 331c1e2..8545496 100644
--- a/arch/frv/mm/fault.c
+++ b/arch/frv/mm/fault.c
@@ -166,6 +166,8 @@ asmlinkage void do_page_fault(int datammu, unsigned long esr0, unsigned long ear
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/ia64/mm/fault.c b/arch/ia64/mm/fault.c
index 02d29c2..3c820ea 100644
--- a/arch/ia64/mm/fault.c
+++ b/arch/ia64/mm/fault.c
@@ -162,6 +162,8 @@ ia64_do_page_fault (unsigned long address, unsigned long isr, struct pt_regs *re
 		 */
 		if (fault & VM_FAULT_OOM) {
 			goto out_of_memory;
+		} else if (fault & VM_FAULT_SIGSEGV) {
+			goto bad_area;
 		} else if (fault & VM_FAULT_SIGBUS) {
 			signal = SIGBUS;
 			goto bad_area;
diff --git a/arch/m32r/mm/fault.c b/arch/m32r/mm/fault.c
index 3cdfa9c..06827fc 100644
--- a/arch/m32r/mm/fault.c
+++ b/arch/m32r/mm/fault.c
@@ -198,6 +198,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long error_code,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/m68k/mm/fault.c b/arch/m68k/mm/fault.c
index 6b020a8..8646409 100644
--- a/arch/m68k/mm/fault.c
+++ b/arch/m68k/mm/fault.c
@@ -146,6 +146,8 @@ int do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto map_err;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto bus_err;
 		BUG();
diff --git a/arch/microblaze/mm/fault.c b/arch/microblaze/mm/fault.c
index c38a265..c7fe3da 100644
--- a/arch/microblaze/mm/fault.c
+++ b/arch/microblaze/mm/fault.c
@@ -214,6 +214,8 @@ void do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/mips/kernel/irq_cpu.c b/arch/mips/kernel/irq_cpu.c
index 972263b..0ed44be 100644
--- a/arch/mips/kernel/irq_cpu.c
+++ b/arch/mips/kernel/irq_cpu.c
@@ -55,6 +55,8 @@ static struct irq_chip mips_cpu_irq_controller = {
 	.irq_mask_ack	= mask_mips_irq,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 /*
@@ -91,6 +93,8 @@ static struct irq_chip mips_mt_cpu_irq_controller = {
 	.irq_mask_ack	= mips_mt_cpu_irq_ack,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 void __init mips_cpu_irq_init(void)
diff --git a/arch/mips/kernel/smp.c b/arch/mips/kernel/smp.c
index 41079b2..1a9bcc2 100644
--- a/arch/mips/kernel/smp.c
+++ b/arch/mips/kernel/smp.c
@@ -105,10 +105,10 @@ asmlinkage __cpuinit void start_secondary(void)
 	if ((read_c0_tcbind() & TCBIND_CURTC) == 0)
 #endif /* CONFIG_MIPS_MT_SMTC */
 	cpu_probe();
-	cpu_report();
 	per_cpu_trap_init();
 	mips_clockevent_init();
 	mp_ops->init_secondary();
+	cpu_report();
 
 	/*
 	 * XXX parity protection should be folded in here when it's converted
diff --git a/arch/mips/loongson/common/Makefile b/arch/mips/loongson/common/Makefile
index e526488..ce415f7 100644
--- a/arch/mips/loongson/common/Makefile
+++ b/arch/mips/loongson/common/Makefile
@@ -10,7 +10,8 @@ obj-$(CONFIG_GENERIC_GPIO) += gpio.o
 # Serial port support
 #
 obj-$(CONFIG_EARLY_PRINTK) += early_printk.o
-obj-$(CONFIG_SERIAL_8250) += serial.o
+loongson-serial-$(CONFIG_SERIAL_8250) := serial.o
+obj-y += $(loongson-serial-m) $(loongson-serial-y)
 obj-$(CONFIG_LOONGSON_UART_BASE) += uart_base.o
 obj-$(CONFIG_LOONGSON_MC146818) += rtc.o
 
diff --git a/arch/mips/mm/fault.c b/arch/mips/mm/fault.c
index c14f6df..5c9ba6a 100644
--- a/arch/mips/mm/fault.c
+++ b/arch/mips/mm/fault.c
@@ -155,6 +155,8 @@ asmlinkage void __kprobes do_page_fault(struct pt_regs *regs, unsigned long writ
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/mn10300/mm/fault.c b/arch/mn10300/mm/fault.c
index 90f346f..eb411b3 100644
--- a/arch/mn10300/mm/fault.c
+++ b/arch/mn10300/mm/fault.c
@@ -255,6 +255,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long fault_code,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/openrisc/mm/fault.c b/arch/openrisc/mm/fault.c
index a5dce82..162abfb 100644
--- a/arch/openrisc/mm/fault.c
+++ b/arch/openrisc/mm/fault.c
@@ -163,6 +163,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/parisc/mm/fault.c b/arch/parisc/mm/fault.c
index 18162ce..a9b765a 100644
--- a/arch/parisc/mm/fault.c
+++ b/arch/parisc/mm/fault.c
@@ -210,6 +210,8 @@ void do_page_fault(struct pt_regs *regs, unsigned long code,
 		 */
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto bad_area;
 		BUG();
diff --git a/arch/powerpc/mm/fault.c b/arch/powerpc/mm/fault.c
index 08ffcf5..3d30a4a 100644
--- a/arch/powerpc/mm/fault.c
+++ b/arch/powerpc/mm/fault.c
@@ -419,7 +419,11 @@ int __kprobes do_page_fault(struct pt_regs *regs, unsigned long address,
 	 */
 	fault = handle_mm_fault(mm, vma, address, flags);
 	if (unlikely(fault & (VM_FAULT_RETRY|VM_FAULT_ERROR))) {
-		int rc = mm_fault_error(regs, address, fault);
+		int rc;
+
+		if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
+		rc = mm_fault_error(regs, address, fault);
 		if (rc >= MM_FAULT_RETURN)
 			return rc;
 	}
diff --git a/arch/powerpc/platforms/cell/spu_fault.c b/arch/powerpc/platforms/cell/spu_fault.c
index 641e727..62f3e4e 100644
--- a/arch/powerpc/platforms/cell/spu_fault.c
+++ b/arch/powerpc/platforms/cell/spu_fault.c
@@ -75,7 +75,7 @@ int spu_handle_mm_fault(struct mm_struct *mm, unsigned long ea,
 		if (*flt & VM_FAULT_OOM) {
 			ret = -ENOMEM;
 			goto out_unlock;
-		} else if (*flt & VM_FAULT_SIGBUS) {
+		} else if (*flt & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV)) {
 			ret = -EFAULT;
 			goto out_unlock;
 		}
diff --git a/arch/powerpc/xmon/xmon.c b/arch/powerpc/xmon/xmon.c
index eab3492..7729c6c 100644
--- a/arch/powerpc/xmon/xmon.c
+++ b/arch/powerpc/xmon/xmon.c
@@ -285,10 +285,11 @@ static inline void disable_surveillance(void)
 	args.token = rtas_token("set-indicator");
 	if (args.token == RTAS_UNKNOWN_SERVICE)
 		return;
-	args.nargs = 3;
-	args.nret = 1;
+	args.token = cpu_to_be32(args.token);
+	args.nargs = cpu_to_be32(3);
+	args.nret = cpu_to_be32(1);
 	args.rets = &args.args[3];
-	args.args[0] = SURVEILLANCE_TOKEN;
+	args.args[0] = cpu_to_be32(SURVEILLANCE_TOKEN);
 	args.args[1] = 0;
 	args.args[2] = 0;
 	enter_rtas(__pa(&args));
diff --git a/arch/s390/mm/fault.c b/arch/s390/mm/fault.c
index f2b11ee..68ba1bb 100644
--- a/arch/s390/mm/fault.c
+++ b/arch/s390/mm/fault.c
@@ -237,6 +237,12 @@ static noinline void do_fault_error(struct pt_regs *regs, int fault)
 				do_no_context(regs);
 			else
 				pagefault_out_of_memory();
+		} else if (fault & VM_FAULT_SIGSEGV) {
+			/* Kernel mode? Handle exceptions or die */
+			if (!user_mode(regs))
+				do_no_context(regs);
+			else
+				do_sigsegv(regs, SEGV_MAPERR);
 		} else if (fault & VM_FAULT_SIGBUS) {
 			/* Kernel mode? Handle exceptions or die */
 			if (!(regs->psw.mask & PSW_MASK_PSTATE))
diff --git a/arch/score/mm/fault.c b/arch/score/mm/fault.c
index 47b600e..b3744ca 100644
--- a/arch/score/mm/fault.c
+++ b/arch/score/mm/fault.c
@@ -110,6 +110,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long write,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/sh/mm/fault_32.c b/arch/sh/mm/fault_32.c
index e99b104..a491963 100644
--- a/arch/sh/mm/fault_32.c
+++ b/arch/sh/mm/fault_32.c
@@ -206,6 +206,8 @@ asmlinkage void __kprobes do_page_fault(struct pt_regs *regs,
 			goto out_of_memory;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		BUG();
 	}
 	if (fault & VM_FAULT_MAJOR) {
diff --git a/arch/sh/mm/tlbflush_64.c b/arch/sh/mm/tlbflush_64.c
index 11c5a18..92f0df9 100644
--- a/arch/sh/mm/tlbflush_64.c
+++ b/arch/sh/mm/tlbflush_64.c
@@ -194,6 +194,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long writeaccess,
 			goto out_of_memory;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		BUG();
 	}
 
diff --git a/arch/sparc/mm/fault_32.c b/arch/sparc/mm/fault_32.c
index df3155a..5c6238d 100644
--- a/arch/sparc/mm/fault_32.c
+++ b/arch/sparc/mm/fault_32.c
@@ -300,6 +300,8 @@ asmlinkage void do_sparc_fault(struct pt_regs *regs, int text_fault, int write,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/sparc/mm/fault_64.c b/arch/sparc/mm/fault_64.c
index 1387aca..0dc7b90 100644
--- a/arch/sparc/mm/fault_64.c
+++ b/arch/sparc/mm/fault_64.c
@@ -443,6 +443,8 @@ asmlinkage void __kprobes do_sparc64_fault(struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/tile/mm/fault.c b/arch/tile/mm/fault.c
index 22e58f5..a362926 100644
--- a/arch/tile/mm/fault.c
+++ b/arch/tile/mm/fault.c
@@ -433,6 +433,8 @@ static int handle_page_fault(struct pt_regs *regs,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/um/kernel/trap.c b/arch/um/kernel/trap.c
index dafc947..f79ffc9 100644
--- a/arch/um/kernel/trap.c
+++ b/arch/um/kernel/trap.c
@@ -69,6 +69,8 @@ int handle_page_fault(unsigned long address, unsigned long ip,
 		if (unlikely(fault & VM_FAULT_ERROR)) {
 			if (fault & VM_FAULT_OOM) {
 				goto out_of_memory;
+			} else if (fault & VM_FAULT_SIGSEGV) {
+				goto out;
 			} else if (fault & VM_FAULT_SIGBUS) {
 				err = -EACCES;
 				goto out;
diff --git a/arch/x86/include/asm/ldt.h b/arch/x86/include/asm/ldt.h
index 46727eb..6e1aaf7 100644
--- a/arch/x86/include/asm/ldt.h
+++ b/arch/x86/include/asm/ldt.h
@@ -28,6 +28,13 @@ struct user_desc {
 	unsigned int  seg_not_present:1;
 	unsigned int  useable:1;
 #ifdef __x86_64__
+	/*
+	 * Because this bit is not present in 32-bit user code, user
+	 * programs can pass uninitialized values here.  Therefore, in
+	 * any context in which a user_desc comes from a 32-bit program,
+	 * the kernel must act as though lm == 0, regardless of the
+	 * actual value.
+	 */
 	unsigned int  lm:1;
 #endif
 };
diff --git a/arch/x86/include/asm/msr-index.h b/arch/x86/include/asm/msr-index.h
index ccb8059..e92e1e4 100644
--- a/arch/x86/include/asm/msr-index.h
+++ b/arch/x86/include/asm/msr-index.h
@@ -130,6 +130,7 @@
 #define MSR_AMD64_PATCH_LOADER		0xc0010020
 #define MSR_AMD64_OSVW_ID_LENGTH	0xc0010140
 #define MSR_AMD64_OSVW_STATUS		0xc0010141
+#define MSR_AMD64_LS_CFG		0xc0011020
 #define MSR_AMD64_DC_CFG		0xc0011022
 #define MSR_AMD64_IBSFETCHCTL		0xc0011030
 #define MSR_AMD64_IBSFETCHLINAD		0xc0011031
diff --git a/arch/x86/kernel/cpu/amd.c b/arch/x86/kernel/cpu/amd.c
index a9c8a46..5beec8a 100644
--- a/arch/x86/kernel/cpu/amd.c
+++ b/arch/x86/kernel/cpu/amd.c
@@ -417,6 +417,16 @@ static void __cpuinit early_init_amd_mc(struct cpuinfo_x86 *c)
 
 	c->x86_coreid_bits = bits;
 #endif
+
+	/* F16h erratum 793, CVE-2013-6885 */
+	if (c->x86 == 0x16 && c->x86_model <= 0xf) {
+		u64 val;
+
+		if (!rdmsrl_amd_safe(MSR_AMD64_LS_CFG, &val) &&
+		    !(val & BIT(15)))
+			wrmsrl_amd_safe(MSR_AMD64_LS_CFG, val | BIT(15));
+	}
+
 }
 
 static void __cpuinit bsp_init_amd(struct cpuinfo_x86 *c)
diff --git a/arch/x86/kernel/cpu/mshyperv.c b/arch/x86/kernel/cpu/mshyperv.c
index 646d192..c465584 100644
--- a/arch/x86/kernel/cpu/mshyperv.c
+++ b/arch/x86/kernel/cpu/mshyperv.c
@@ -55,6 +55,7 @@ static struct clocksource hyperv_cs = {
 	.rating		= 400, /* use this when running on Hyperv*/
 	.read		= read_hv_clock,
 	.mask		= CLOCKSOURCE_MASK(64),
+	.flags		= CLOCK_SOURCE_IS_CONTINUOUS,
 };
 
 static void __init ms_hyperv_init_platform(void)
diff --git a/arch/x86/kernel/kprobes.c b/arch/x86/kernel/kprobes.c
index e213fc8..15d3c45 100644
--- a/arch/x86/kernel/kprobes.c
+++ b/arch/x86/kernel/kprobes.c
@@ -1003,6 +1003,15 @@ int __kprobes setjmp_pre_handler(struct kprobe *p, struct pt_regs *regs)
 	regs->flags &= ~X86_EFLAGS_IF;
 	trace_hardirqs_off();
 	regs->ip = (unsigned long)(jp->entry);
+
+	/*
+	 * jprobes use jprobe_return() which skips the normal return
+	 * path of the function, and this messes up the accounting of the
+	 * function graph tracer to get messed up.
+	 *
+	 * Pause function graph tracing while performing the jprobe function.
+	 */
+	pause_graph_tracing();
 	return 1;
 }
 
@@ -1028,24 +1037,25 @@ int __kprobes longjmp_break_handler(struct kprobe *p, struct pt_regs *regs)
 	struct kprobe_ctlblk *kcb = get_kprobe_ctlblk();
 	u8 *addr = (u8 *) (regs->ip - 1);
 	struct jprobe *jp = container_of(p, struct jprobe, kp);
+	void *saved_sp = kcb->jprobe_saved_sp;
 
 	if ((addr > (u8 *) jprobe_return) &&
 	    (addr < (u8 *) jprobe_return_end)) {
-		if (stack_addr(regs) != kcb->jprobe_saved_sp) {
+		if (stack_addr(regs) != saved_sp) {
 			struct pt_regs *saved_regs = &kcb->jprobe_saved_regs;
 			printk(KERN_ERR
 			       "current sp %p does not match saved sp %p\n",
-			       stack_addr(regs), kcb->jprobe_saved_sp);
+			       stack_addr(regs), saved_sp);
 			printk(KERN_ERR "Saved registers for jprobe %p\n", jp);
 			show_registers(saved_regs);
 			printk(KERN_ERR "Current registers\n");
 			show_registers(regs);
 			BUG();
 		}
+		/* It's OK to start function graph tracing again */
+		unpause_graph_tracing();
 		*regs = kcb->jprobe_saved_regs;
-		memcpy((kprobe_opcode_t *)(kcb->jprobe_saved_sp),
-		       kcb->jprobes_stack,
-		       MIN_STACK_SIZE(kcb->jprobe_saved_sp));
+		memcpy(saved_sp, kcb->jprobes_stack, MIN_STACK_SIZE(saved_sp));
 		preempt_enable_no_resched();
 		return 1;
 	}
diff --git a/arch/x86/kernel/process_64.c b/arch/x86/kernel/process_64.c
index 43d8b48..bb390e1 100644
--- a/arch/x86/kernel/process_64.c
+++ b/arch/x86/kernel/process_64.c
@@ -286,24 +286,9 @@ __switch_to(struct task_struct *prev_p, struct task_struct *next_p)
 
 	fpu = switch_fpu_prepare(prev_p, next_p, cpu);
 
-	/*
-	 * Reload esp0, LDT and the page table pointer:
-	 */
+	/* Reload esp0 and ss1. */
 	load_sp0(tss, next);
 
-	/*
-	 * Switch DS and ES.
-	 * This won't pick up thread selector changes, but I guess that is ok.
-	 */
-	savesegment(es, prev->es);
-	if (unlikely(next->es | prev->es))
-		loadsegment(es, next->es);
-
-	savesegment(ds, prev->ds);
-	if (unlikely(next->ds | prev->ds))
-		loadsegment(ds, next->ds);
-
-
 	/* We must save %fs and %gs before load_TLS() because
 	 * %fs and %gs may be cleared by load_TLS().
 	 *
@@ -312,41 +297,101 @@ __switch_to(struct task_struct *prev_p, struct task_struct *next_p)
 	savesegment(fs, fsindex);
 	savesegment(gs, gsindex);
 
+	/*
+	 * Load TLS before restoring any segments so that segment loads
+	 * reference the correct GDT entries.
+	 */
 	load_TLS(next, cpu);
 
 	/*
-	 * Leave lazy mode, flushing any hypercalls made here.
-	 * This must be done before restoring TLS segments so
-	 * the GDT and LDT are properly updated, and must be
-	 * done before math_state_restore, so the TS bit is up
-	 * to date.
+	 * Leave lazy mode, flushing any hypercalls made here.  This
+	 * must be done after loading TLS entries in the GDT but before
+	 * loading segments that might reference them, and and it must
+	 * be done before math_state_restore, so the TS bit is up to
+	 * date.
 	 */
 	arch_end_context_switch(next_p);
 
+	/* Switch DS and ES.
+	 *
+	 * Reading them only returns the selectors, but writing them (if
+	 * nonzero) loads the full descriptor from the GDT or LDT.  The
+	 * LDT for next is loaded in switch_mm, and the GDT is loaded
+	 * above.
+	 *
+	 * We therefore need to write new values to the segment
+	 * registers on every context switch unless both the new and old
+	 * values are zero.
+	 *
+	 * Note that we don't need to do anything for CS and SS, as
+	 * those are saved and restored as part of pt_regs.
+	 */
+	savesegment(es, prev->es);
+	if (unlikely(next->es | prev->es))
+		loadsegment(es, next->es);
+
+	savesegment(ds, prev->ds);
+	if (unlikely(next->ds | prev->ds))
+		loadsegment(ds, next->ds);
+
 	/*
 	 * Switch FS and GS.
 	 *
-	 * Segment register != 0 always requires a reload.  Also
-	 * reload when it has changed.  When prev process used 64bit
-	 * base always reload to avoid an information leak.
+	 * These are even more complicated than FS and GS: they have
+	 * 64-bit bases are that controlled by arch_prctl.  Those bases
+	 * only differ from the values in the GDT or LDT if the selector
+	 * is 0.
+	 *
+	 * Loading the segment register resets the hidden base part of
+	 * the register to 0 or the value from the GDT / LDT.  If the
+	 * next base address zero, writing 0 to the segment register is
+	 * much faster than using wrmsr to explicitly zero the base.
+	 *
+	 * The thread_struct.fs and thread_struct.gs values are 0
+	 * if the fs and gs bases respectively are not overridden
+	 * from the values implied by fsindex and gsindex.  They
+	 * are nonzero, and store the nonzero base addresses, if
+	 * the bases are overridden.
+	 *
+	 * (fs != 0 && fsindex != 0) || (gs != 0 && gsindex != 0) should
+	 * be impossible.
+	 *
+	 * Therefore we need to reload the segment registers if either
+	 * the old or new selector is nonzero, and we need to override
+	 * the base address if next thread expects it to be overridden.
+	 *
+	 * This code is unnecessarily slow in the case where the old and
+	 * new indexes are zero and the new base is nonzero -- it will
+	 * unnecessarily write 0 to the selector before writing the new
+	 * base address.
+	 *
+	 * Note: This all depends on arch_prctl being the only way that
+	 * user code can override the segment base.  Once wrfsbase and
+	 * wrgsbase are enabled, most of this code will need to change.
 	 */
 	if (unlikely(fsindex | next->fsindex | prev->fs)) {
 		loadsegment(fs, next->fsindex);
+
 		/*
-		 * Check if the user used a selector != 0; if yes
-		 *  clear 64bit base, since overloaded base is always
-		 *  mapped to the Null selector
+		 * If user code wrote a nonzero value to FS, then it also
+		 * cleared the overridden base address.
+		 *
+		 * XXX: if user code wrote 0 to FS and cleared the base
+		 * address itself, we won't notice and we'll incorrectly
+		 * restore the prior base address next time we reschdule
+		 * the process.
 		 */
 		if (fsindex)
 			prev->fs = 0;
 	}
-	/* when next process has a 64bit base use it */
 	if (next->fs)
 		wrmsrl(MSR_FS_BASE, next->fs);
 	prev->fsindex = fsindex;
 
 	if (unlikely(gsindex | next->gsindex | prev->gs)) {
 		load_gs_index(next->gsindex);
+
+		/* This works (and fails) the same way as fsindex above. */
 		if (gsindex)
 			prev->gs = 0;
 	}
diff --git a/arch/x86/kernel/tls.c b/arch/x86/kernel/tls.c
index 9d25a6e..fe2e363 100644
--- a/arch/x86/kernel/tls.c
+++ b/arch/x86/kernel/tls.c
@@ -60,6 +60,22 @@ static bool tls_desc_okay(const struct user_desc *info)
 	if (!info->seg_32bit)
 		return false;
 
+	/* Only allow data segments in the TLS array. */
+	if (info->contents > 1)
+		return false;
+
+	/*
+	 * Non-present segments with DPL 3 present an interesting attack
+	 * surface.  The kernel should handle such segments correctly,
+	 * but TLS is very difficult to protect in a sandbox, so prevent
+	 * such segments from being created.
+	 *
+	 * If userspace needs to remove a TLS entry, it can still delete
+	 * it outright.
+	 */
+	if (info->seg_not_present)
+		return false;
+
 	return true;
 }
 
diff --git a/arch/x86/mm/fault.c b/arch/x86/mm/fault.c
index 4a0a2e8..b723f2e 100644
--- a/arch/x86/mm/fault.c
+++ b/arch/x86/mm/fault.c
@@ -887,6 +887,8 @@ mm_fault_error(struct pt_regs *regs, unsigned long error_code,
 		if (fault & (VM_FAULT_SIGBUS|VM_FAULT_HWPOISON|
 			     VM_FAULT_HWPOISON_LARGE))
 			do_sigbus(regs, error_code, address, fault);
+		else if (fault & VM_FAULT_SIGSEGV)
+			bad_area_nosemaphore(regs, error_code, address);
 		else
 			BUG();
 	}
diff --git a/arch/x86/mm/mmap.c b/arch/x86/mm/mmap.c
index 5c1ae28..75f9e5d 100644
--- a/arch/x86/mm/mmap.c
+++ b/arch/x86/mm/mmap.c
@@ -35,12 +35,12 @@ struct __read_mostly va_alignment va_align = {
 	.flags = -1,
 };
 
-static unsigned int stack_maxrandom_size(void)
+static unsigned long stack_maxrandom_size(void)
 {
-	unsigned int max = 0;
+	unsigned long max = 0;
 	if ((current->flags & PF_RANDOMIZE) &&
 		!(current->personality & ADDR_NO_RANDOMIZE)) {
-		max = ((-1U) & STACK_RND_MASK) << PAGE_SHIFT;
+		max = ((-1UL) & STACK_RND_MASK) << PAGE_SHIFT;
 	}
 
 	return max;
diff --git a/arch/x86/um/sys_call_table_32.c b/arch/x86/um/sys_call_table_32.c
index 68d1dc9..bd8b159 100644
--- a/arch/x86/um/sys_call_table_32.c
+++ b/arch/x86/um/sys_call_table_32.c
@@ -43,7 +43,7 @@ typedef asmlinkage void (*sys_call_ptr_t)(void);
 
 extern asmlinkage void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/arch/x86/um/sys_call_table_64.c b/arch/x86/um/sys_call_table_64.c
index 9924776..cbdab94 100644
--- a/arch/x86/um/sys_call_table_64.c
+++ b/arch/x86/um/sys_call_table_64.c
@@ -48,7 +48,7 @@ typedef void (*sys_call_ptr_t)(void);
 
 extern void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/arch/x86/vdso/vma.c b/arch/x86/vdso/vma.c
index 00aaf04..47aa108 100644
--- a/arch/x86/vdso/vma.c
+++ b/arch/x86/vdso/vma.c
@@ -117,23 +117,39 @@ subsys_initcall(init_vdso);
 
 struct linux_binprm;
 
-/* Put the vdso above the (randomized) stack with another randomized offset.
-   This way there is no hole in the middle of address space.
-   To save memory make sure it is still in the same PTE as the stack top.
-   This doesn't give that many random bits */
+/*
+ * Put the vdso above the (randomized) stack with another randomized
+ * offset.  This way there is no hole in the middle of address space.
+ * To save memory make sure it is still in the same PTE as the stack
+ * top.  This doesn't give that many random bits.
+ *
+ * Note that this algorithm is imperfect: the distribution of the vdso
+ * start address within a PMD is biased toward the end.
+ *
+ */
 static unsigned long vdso_addr(unsigned long start, unsigned len)
 {
 	unsigned long addr, end;
 	unsigned offset;
-	end = (start + PMD_SIZE - 1) & PMD_MASK;
+
+	/*
+	 * Round up the start address.  It can start out unaligned as a result
+	 * of stack start randomization.
+	 */
+	start = PAGE_ALIGN(start);
+
+	/* Round the lowest possible end address up to a PMD boundary. */
+	end = (start + len + PMD_SIZE - 1) & PMD_MASK;
 	if (end >= TASK_SIZE_MAX)
 		end = TASK_SIZE_MAX;
 	end -= len;
-	/* This loses some more bits than a modulo, but is cheaper */
-	offset = get_random_int() & (PTRS_PER_PTE - 1);
-	addr = start + (offset << PAGE_SHIFT);
-	if (addr >= end)
-		addr = end;
+
+	if (end > start) {
+		offset = get_random_int() % (((end - start) >> PAGE_SHIFT) + 1);
+		addr = start + (offset << PAGE_SHIFT);
+	} else {
+		addr = start;
+	}
 
 	/*
 	 * page-align it here so that get_unmapped_area doesn't
diff --git a/arch/xtensa/mm/fault.c b/arch/xtensa/mm/fault.c
index b17885a..b3877be 100644
--- a/arch/xtensa/mm/fault.c
+++ b/arch/xtensa/mm/fault.c
@@ -108,6 +108,8 @@ void do_page_fault(struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/block/genhd.c b/block/genhd.c
index da61520..6542b9b 100644
--- a/block/genhd.c
+++ b/block/genhd.c
@@ -1069,9 +1069,16 @@ int disk_expand_part_tbl(struct gendisk *disk, int partno)
 	struct disk_part_tbl *old_ptbl = disk->part_tbl;
 	struct disk_part_tbl *new_ptbl;
 	int len = old_ptbl ? old_ptbl->len : 0;
-	int target = partno + 1;
+	int i, target;
 	size_t size;
-	int i;
+
+	/*
+	 * check for int overflow, since we can get here from blkpg_ioctl()
+	 * with a user passed 'partno'.
+	 */
+	target = partno + 1;
+	if (target < 0)
+		return -EINVAL;
 
 	/* disk_max_parts() is zero during initialization, ignore if so */
 	if (disk_max_parts(disk) && target > disk_max_parts(disk))
diff --git a/crypto/af_alg.c b/crypto/af_alg.c
index bf948e1..6ef6e2a 100644
--- a/crypto/af_alg.c
+++ b/crypto/af_alg.c
@@ -449,6 +449,9 @@ void af_alg_complete(struct crypto_async_request *req, int err)
 {
 	struct af_alg_completion *completion = req->data;
 
+	if (err == -EINPROGRESS)
+		return;
+
 	completion->err = err;
 	complete(&completion->completion);
 }
diff --git a/drivers/ata/ahci.c b/drivers/ata/ahci.c
index ca9a287..6fc61eb 100644
--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -61,6 +61,8 @@ enum board_ids {
 	/* board IDs by feature in alphabetical order */
 	board_ahci,
 	board_ahci_ign_iferr,
+	board_ahci_nomsi,
+	board_ahci_noncq,
 	board_ahci_nosntf,
 	board_ahci_yes_fbs,
 
@@ -121,6 +123,20 @@ static const struct ata_port_info ahci_port_info[] = {
 		.udma_mask	= ATA_UDMA6,
 		.port_ops	= &ahci_ops,
 	},
+	[board_ahci_nomsi] = {
+		AHCI_HFLAGS	(AHCI_HFLAG_NO_MSI),
+		.flags		= AHCI_FLAG_COMMON,
+		.pio_mask	= ATA_PIO4,
+		.udma_mask	= ATA_UDMA6,
+		.port_ops	= &ahci_ops,
+	},
+	[board_ahci_noncq] = {
+		AHCI_HFLAGS	(AHCI_HFLAG_NO_NCQ),
+		.flags		= AHCI_FLAG_COMMON,
+		.pio_mask	= ATA_PIO4,
+		.udma_mask	= ATA_UDMA6,
+		.port_ops	= &ahci_ops,
+	},
 	[board_ahci_nosntf] =
 	{
 		AHCI_HFLAGS	(AHCI_HFLAG_NO_SNTF),
@@ -313,6 +329,9 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(INTEL, 0x8c87), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8e), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8f), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d03), board_ahci }, /* Sunrise Point-LP AHCI */
+	{ PCI_VDEVICE(INTEL, 0x9d05), board_ahci }, /* Sunrise Point-LP RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d07), board_ahci }, /* Sunrise Point-LP RAID */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H AHCI */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H RAID */
 	{ PCI_VDEVICE(INTEL, 0xa105), board_ahci }, /* Sunrise Point-H RAID */
@@ -469,6 +488,13 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(ASMEDIA, 0x0611), board_ahci },	/* ASM1061 */
 	{ PCI_VDEVICE(ASMEDIA, 0x0612), board_ahci },	/* ASM1062 */
 
+	/*
+	 * Samsung SSDs found on some macbooks.  NCQ times out if MSI is
+	 * enabled.  https://bugzilla.kernel.org/show_bug.cgi?id=60731
+	 */
+	{ PCI_VDEVICE(SAMSUNG, 0x1600), board_ahci_nomsi },
+	{ PCI_VDEVICE(SAMSUNG, 0xa800), board_ahci_nomsi },
+
 	/* Enmotus */
 	{ PCI_DEVICE(0x1c44, 0x8000), board_ahci },
 
diff --git a/drivers/ata/libata-core.c b/drivers/ata/libata-core.c
index 6b92236..adaf994 100644
--- a/drivers/ata/libata-core.c
+++ b/drivers/ata/libata-core.c
@@ -4712,7 +4712,10 @@ static struct ata_queued_cmd *ata_qc_new(struct ata_port *ap)
 		return NULL;
 
 	for (i = 0, tag = ap->last_tag + 1; i < max_queue; i++, tag++) {
-		tag = tag < max_queue ? tag : 0;
+		if (ap->flags & ATA_FLAG_LOWTAG)
+			tag = i;
+		else
+			tag = tag < max_queue ? tag : 0;
 
 		/* the last tag is reserved for internal command. */
 		if (tag == ATA_TAG_INTERNAL)
diff --git a/drivers/ata/libata-sff.c b/drivers/ata/libata-sff.c
index 3723e5e..fad2734 100644
--- a/drivers/ata/libata-sff.c
+++ b/drivers/ata/libata-sff.c
@@ -1333,7 +1333,19 @@ void ata_sff_flush_pio_task(struct ata_port *ap)
 	DPRINTK("ENTER\n");
 
 	cancel_delayed_work_sync(&ap->sff_pio_task);
+
+	/*
+	 * We wanna reset the HSM state to IDLE.  If we do so without
+	 * grabbing the port lock, critical sections protected by it which
+	 * expect the HSM state to stay stable may get surprised.  For
+	 * example, we may set IDLE in between the time
+	 * __ata_sff_port_intr() checks for HSM_ST_IDLE and before it calls
+	 * ata_sff_hsm_move() causing ata_sff_hsm_move() to BUG().
+	 */
+	spin_lock_irq(ap->lock);
 	ap->hsm_task_state = HSM_ST_IDLE;
+	spin_unlock_irq(ap->lock);
+
 	ap->sff_pio_task_link = NULL;
 
 	if (ata_msg_ctl(ap))
diff --git a/drivers/ata/sata_dwc_460ex.c b/drivers/ata/sata_dwc_460ex.c
index 69f7cde..9d6eb14 100644
--- a/drivers/ata/sata_dwc_460ex.c
+++ b/drivers/ata/sata_dwc_460ex.c
@@ -791,7 +791,7 @@ static int dma_dwc_init(struct sata_dwc_device *hsdev, int irq)
 	if (err) {
 		dev_err(host_pvt.dwc_dev, "%s: dma_request_interrupts returns"
 			" %d\n", __func__, err);
-		goto error_out;
+		return err;
 	}
 
 	/* Enabe DMA */
@@ -802,11 +802,6 @@ static int dma_dwc_init(struct sata_dwc_device *hsdev, int irq)
 		sata_dma_regs);
 
 	return 0;
-
-error_out:
-	dma_dwc_exit(hsdev);
-
-	return err;
 }
 
 static int sata_dwc_scr_read(struct ata_link *link, unsigned int scr, u32 *val)
@@ -1634,7 +1629,7 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	char *ver = (char *)&versionr;
 	u8 *base = NULL;
 	int err = 0;
-	int irq, rc;
+	int irq;
 	struct ata_host *host;
 	struct ata_port_info pi = sata_dwc_port_info[0];
 	const struct ata_port_info *ppi[] = { &pi, NULL };
@@ -1688,7 +1683,7 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	if (irq == NO_IRQ) {
 		dev_err(&ofdev->dev, "no SATA DMA irq\n");
 		err = -ENODEV;
-		goto error_out;
+		goto error_iomap;
 	}
 
 	/* Get physical SATA DMA register base address */
@@ -1697,14 +1692,16 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 		dev_err(&ofdev->dev, "ioremap failed for AHBDMA register"
 			" address\n");
 		err = -ENODEV;
-		goto error_out;
+		goto error_iomap;
 	}
 
 	/* Save dev for later use in dev_xxx() routines */
 	host_pvt.dwc_dev = &ofdev->dev;
 
 	/* Initialize AHB DMAC */
-	dma_dwc_init(hsdev, irq);
+	err = dma_dwc_init(hsdev, irq);
+	if (err)
+		goto error_dma_iomap;
 
 	/* Enable SATA Interrupts */
 	sata_dwc_enable_interrupts(hsdev);
@@ -1722,9 +1719,8 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	 * device discovery process, invoking our port_start() handler &
 	 * error_handler() to execute a dummy Softreset EH session
 	 */
-	rc = ata_host_activate(host, irq, sata_dwc_isr, 0, &sata_dwc_sht);
-
-	if (rc != 0)
+	err = ata_host_activate(host, irq, sata_dwc_isr, 0, &sata_dwc_sht);
+	if (err)
 		dev_err(&ofdev->dev, "failed to activate host");
 
 	dev_set_drvdata(&ofdev->dev, host);
@@ -1733,7 +1729,8 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 error_out:
 	/* Free SATA DMA resources */
 	dma_dwc_exit(hsdev);
-
+error_dma_iomap:
+	iounmap((void __iomem *)host_pvt.sata_dma_regs);
 error_iomap:
 	iounmap(base);
 error_kmalloc:
@@ -1754,6 +1751,7 @@ static int sata_dwc_remove(struct platform_device *ofdev)
 	/* Free SATA DMA resources */
 	dma_dwc_exit(hsdev);
 
+	iounmap((void __iomem *)host_pvt.sata_dma_regs);
 	iounmap(hsdev->reg_base);
 	kfree(hsdev);
 	kfree(host);
diff --git a/drivers/ata/sata_fsl.c b/drivers/ata/sata_fsl.c
index d6577b9..3d3b59a 100644
--- a/drivers/ata/sata_fsl.c
+++ b/drivers/ata/sata_fsl.c
@@ -1426,7 +1426,7 @@ static int sata_fsl_probe(struct platform_device *ofdev)
 	host_priv->csr_base = csr_base;
 
 	irq = irq_of_parse_and_map(ofdev->dev.of_node, 0);
-	if (irq < 0) {
+	if (!irq) {
 		dev_err(&ofdev->dev, "invalid irq from platform\n");
 		goto error_exit_with_cleanup;
 	}
diff --git a/drivers/ata/sata_sil24.c b/drivers/ata/sata_sil24.c
index e7e610a..cb68aa3 100644
--- a/drivers/ata/sata_sil24.c
+++ b/drivers/ata/sata_sil24.c
@@ -246,7 +246,7 @@ enum {
 	/* host flags */
 	SIL24_COMMON_FLAGS	= ATA_FLAG_SATA | ATA_FLAG_PIO_DMA |
 				  ATA_FLAG_NCQ | ATA_FLAG_ACPI_SATA |
-				  ATA_FLAG_AN | ATA_FLAG_PMP,
+				  ATA_FLAG_AN | ATA_FLAG_PMP | ATA_FLAG_LOWTAG,
 	SIL24_FLAG_PCIX_IRQ_WOC	= (1 << 24), /* IRQ loss errata on PCI-X */
 
 	IRQ_STAT_4PORTS		= 0xf,
diff --git a/drivers/base/bus.c b/drivers/base/bus.c
index feb30c1..b23bb9c 100644
--- a/drivers/base/bus.c
+++ b/drivers/base/bus.c
@@ -245,13 +245,15 @@ static ssize_t store_drivers_probe(struct bus_type *bus,
 				   const char *buf, size_t count)
 {
 	struct device *dev;
+	int err = -EINVAL;
 
 	dev = bus_find_device_by_name(bus, NULL, buf);
 	if (!dev)
 		return -ENODEV;
-	if (bus_rescan_devices_helper(dev, NULL) != 0)
-		return -EINVAL;
-	return count;
+	if (bus_rescan_devices_helper(dev, NULL) == 0)
+		err = count;
+	put_device(dev);
+	return err;
 }
 #endif
 
diff --git a/drivers/base/core.c b/drivers/base/core.c
index 32e86d6..aeaf0e1 100644
--- a/drivers/base/core.c
+++ b/drivers/base/core.c
@@ -1494,34 +1494,11 @@ static void device_create_release(struct device *dev)
 	kfree(dev);
 }
 
-/**
- * device_create_vargs - creates a device and registers it with sysfs
- * @class: pointer to the struct class that this device should be registered to
- * @parent: pointer to the parent struct device of this new device, if any
- * @devt: the dev_t for the char device to be added
- * @drvdata: the data to be added to the device for callbacks
- * @fmt: string for the device's name
- * @args: va_list for the device's name
- *
- * This function can be used by char device classes.  A struct device
- * will be created in sysfs, registered to the specified class.
- *
- * A "dev" file will be created, showing the dev_t for the device, if
- * the dev_t is not 0,0.
- * If a pointer to a parent struct device is passed in, the newly created
- * struct device will be a child of that device in sysfs.
- * The pointer to the struct device will be returned from the call.
- * Any further sysfs files that might be required can be created using this
- * pointer.
- *
- * Returns &struct device pointer on success, or ERR_PTR() on error.
- *
- * Note: the struct class passed to this function must have previously
- * been created with a call to class_create().
- */
-struct device *device_create_vargs(struct class *class, struct device *parent,
-				   dev_t devt, void *drvdata, const char *fmt,
-				   va_list args)
+static struct device *
+device_create_groups_vargs(struct class *class, struct device *parent,
+			   dev_t devt, void *drvdata,
+			   const struct attribute_group **groups,
+			   const char *fmt, va_list args)
 {
 	struct device *dev = NULL;
 	int retval = -ENODEV;
@@ -1538,6 +1515,7 @@ struct device *device_create_vargs(struct class *class, struct device *parent,
 	dev->devt = devt;
 	dev->class = class;
 	dev->parent = parent;
+	dev->groups = groups;
 	dev->release = device_create_release;
 	dev_set_drvdata(dev, drvdata);
 
@@ -1555,6 +1533,39 @@ struct device *device_create_vargs(struct class *class, struct device *parent,
 	put_device(dev);
 	return ERR_PTR(retval);
 }
+
+/**
+ * device_create_vargs - creates a device and registers it with sysfs
+ * @class: pointer to the struct class that this device should be registered to
+ * @parent: pointer to the parent struct device of this new device, if any
+ * @devt: the dev_t for the char device to be added
+ * @drvdata: the data to be added to the device for callbacks
+ * @fmt: string for the device's name
+ * @args: va_list for the device's name
+ *
+ * This function can be used by char device classes.  A struct device
+ * will be created in sysfs, registered to the specified class.
+ *
+ * A "dev" file will be created, showing the dev_t for the device, if
+ * the dev_t is not 0,0.
+ * If a pointer to a parent struct device is passed in, the newly created
+ * struct device will be a child of that device in sysfs.
+ * The pointer to the struct device will be returned from the call.
+ * Any further sysfs files that might be required can be created using this
+ * pointer.
+ *
+ * Returns &struct device pointer on success, or ERR_PTR() on error.
+ *
+ * Note: the struct class passed to this function must have previously
+ * been created with a call to class_create().
+ */
+struct device *device_create_vargs(struct class *class, struct device *parent,
+				   dev_t devt, void *drvdata, const char *fmt,
+				   va_list args)
+{
+	return device_create_groups_vargs(class, parent, devt, drvdata, NULL,
+					  fmt, args);
+}
 EXPORT_SYMBOL_GPL(device_create_vargs);
 
 /**
@@ -1594,6 +1605,50 @@ struct device *device_create(struct class *class, struct device *parent,
 }
 EXPORT_SYMBOL_GPL(device_create);
 
+/**
+ * device_create_with_groups - creates a device and registers it with sysfs
+ * @class: pointer to the struct class that this device should be registered to
+ * @parent: pointer to the parent struct device of this new device, if any
+ * @devt: the dev_t for the char device to be added
+ * @drvdata: the data to be added to the device for callbacks
+ * @groups: NULL-terminated list of attribute groups to be created
+ * @fmt: string for the device's name
+ *
+ * This function can be used by char device classes.  A struct device
+ * will be created in sysfs, registered to the specified class.
+ * Additional attributes specified in the groups parameter will also
+ * be created automatically.
+ *
+ * A "dev" file will be created, showing the dev_t for the device, if
+ * the dev_t is not 0,0.
+ * If a pointer to a parent struct device is passed in, the newly created
+ * struct device will be a child of that device in sysfs.
+ * The pointer to the struct device will be returned from the call.
+ * Any further sysfs files that might be required can be created using this
+ * pointer.
+ *
+ * Returns &struct device pointer on success, or ERR_PTR() on error.
+ *
+ * Note: the struct class passed to this function must have previously
+ * been created with a call to class_create().
+ */
+struct device *device_create_with_groups(struct class *class,
+					 struct device *parent, dev_t devt,
+					 void *drvdata,
+					 const struct attribute_group **groups,
+					 const char *fmt, ...)
+{
+	va_list vargs;
+	struct device *dev;
+
+	va_start(vargs, fmt);
+	dev = device_create_groups_vargs(class, parent, devt, drvdata, groups,
+					 fmt, vargs);
+	va_end(vargs);
+	return dev;
+}
+EXPORT_SYMBOL_GPL(device_create_with_groups);
+
 static int __match_devt(struct device *dev, void *data)
 {
 	dev_t *devt = data;
diff --git a/drivers/block/drbd/drbd_req.c b/drivers/block/drbd/drbd_req.c
index be984e0..43da226 100644
--- a/drivers/block/drbd/drbd_req.c
+++ b/drivers/block/drbd/drbd_req.c
@@ -1184,6 +1184,7 @@ int drbd_merge_bvec(struct request_queue *q, struct bvec_merge_data *bvm, struct
 		struct request_queue * const b =
 			mdev->ldev->backing_bdev->bd_disk->queue;
 		if (b->merge_bvec_fn) {
+			bvm->bi_bdev = mdev->ldev->backing_bdev;
 			backing_limit = b->merge_bvec_fn(b, bvm, bvec);
 			limit = min(limit, backing_limit);
 		}
diff --git a/drivers/gpio/gpiolib.c b/drivers/gpio/gpiolib.c
index 234cb1e..06d916b 100644
--- a/drivers/gpio/gpiolib.c
+++ b/drivers/gpio/gpiolib.c
@@ -60,6 +60,7 @@ struct gpio_desc {
 #define FLAG_ACTIVE_LOW	7	/* sysfs value has active low */
 #define FLAG_OPEN_DRAIN	8	/* Gpio is open drain type */
 #define FLAG_OPEN_SOURCE 9	/* Gpio is open source type */
+#define FLAG_SYSFS_DIR	10	/* show sysfs direction attribute */
 
 #define ID_SHIFT	16	/* add new flags before this one */
 
@@ -319,7 +320,7 @@ static ssize_t gpio_value_store(struct device *dev,
 	return status;
 }
 
-static const DEVICE_ATTR(value, 0644,
+static DEVICE_ATTR(value, 0644,
 		gpio_value_show, gpio_value_store);
 
 static irqreturn_t gpio_sysfs_irq(int irq, void *priv)
@@ -542,17 +543,47 @@ static ssize_t gpio_active_low_store(struct device *dev,
 	return status ? : size;
 }
 
-static const DEVICE_ATTR(active_low, 0644,
+static DEVICE_ATTR(active_low, 0644,
 		gpio_active_low_show, gpio_active_low_store);
 
-static const struct attribute *gpio_attrs[] = {
+static umode_t gpio_is_visible(struct kobject *kobj, struct attribute *attr,
+			       int n)
+{
+	struct device *dev = container_of(kobj, struct device, kobj);
+	struct gpio_desc *desc = dev_get_drvdata(dev);
+	unsigned gpio = desc - gpio_desc;
+	umode_t mode = attr->mode;
+	bool show_direction = test_bit(FLAG_SYSFS_DIR, &desc->flags);
+
+	if (attr == &dev_attr_direction.attr) {
+		if (!show_direction)
+			mode = 0;
+	} else if (attr == &dev_attr_edge.attr) {
+		if (gpio_to_irq(gpio) < 0)
+			mode = 0;
+		if (!show_direction && test_bit(FLAG_IS_OUT, &desc->flags))
+			mode = 0;
+	}
+
+	return mode;
+}
+
+static struct attribute *gpio_attrs[] = {
+	&dev_attr_direction.attr,
+	&dev_attr_edge.attr,
 	&dev_attr_value.attr,
 	&dev_attr_active_low.attr,
 	NULL,
 };
 
-static const struct attribute_group gpio_attr_group = {
-	.attrs = (struct attribute **) gpio_attrs,
+static const struct attribute_group gpio_group = {
+	.attrs = gpio_attrs,
+	.is_visible = gpio_is_visible,
+};
+
+static const struct attribute_group *gpio_groups[] = {
+	&gpio_group,
+	NULL
 };
 
 /*
@@ -589,16 +620,13 @@ static ssize_t chip_ngpio_show(struct device *dev,
 }
 static DEVICE_ATTR(ngpio, 0444, chip_ngpio_show, NULL);
 
-static const struct attribute *gpiochip_attrs[] = {
+static struct attribute *gpiochip_attrs[] = {
 	&dev_attr_base.attr,
 	&dev_attr_label.attr,
 	&dev_attr_ngpio.attr,
 	NULL,
 };
-
-static const struct attribute_group gpiochip_attr_group = {
-	.attrs = (struct attribute **) gpiochip_attrs,
-};
+ATTRIBUTE_GROUPS(gpiochip);
 
 /*
  * /sys/class/gpio/export ... write-only
@@ -704,8 +732,9 @@ int gpio_export(unsigned gpio, bool direction_may_change)
 {
 	unsigned long		flags;
 	struct gpio_desc	*desc;
-	int			status = -EINVAL;
+	int			status;
 	const char		*ioname = NULL;
+	struct device		*dev;
 
 	/* can't export until sysfs is available ... */
 	if (!gpio_class.p) {
@@ -713,59 +742,50 @@ int gpio_export(unsigned gpio, bool direction_may_change)
 		return -ENOENT;
 	}
 
-	if (!gpio_is_valid(gpio))
-		goto done;
+	if (!gpio_is_valid(gpio)) {
+		pr_debug("%s: gpio %d is not valid\n", __func__, gpio);
+		return -EINVAL;
+	}
 
 	mutex_lock(&sysfs_lock);
 
 	spin_lock_irqsave(&gpio_lock, flags);
 	desc = &gpio_desc[gpio];
-	if (test_bit(FLAG_REQUESTED, &desc->flags)
-			&& !test_bit(FLAG_EXPORT, &desc->flags)) {
-		status = 0;
-		if (!desc->chip->direction_input
-				|| !desc->chip->direction_output)
-			direction_may_change = false;
+	if (!test_bit(FLAG_REQUESTED, &desc->flags) ||
+	     test_bit(FLAG_EXPORT, &desc->flags)) {
+		spin_unlock_irqrestore(&gpio_lock, flags);
+		pr_debug("%s: gpio %d unavailable (requested=%d, exported=%d)\n",
+				__func__, gpio,
+				test_bit(FLAG_REQUESTED, &desc->flags),
+				test_bit(FLAG_EXPORT, &desc->flags));
+		return -EPERM;
+	}
+
+	if (desc->chip->direction_input && desc->chip->direction_output &&
+			direction_may_change) {
+		set_bit(FLAG_SYSFS_DIR, &desc->flags);
 	}
+
 	spin_unlock_irqrestore(&gpio_lock, flags);
 
 	if (desc->chip->names && desc->chip->names[gpio - desc->chip->base])
 		ioname = desc->chip->names[gpio - desc->chip->base];
 
-	if (status == 0) {
-		struct device	*dev;
-
-		dev = device_create(&gpio_class, desc->chip->dev, MKDEV(0, 0),
-				desc, ioname ? ioname : "gpio%u", gpio);
-		if (!IS_ERR(dev)) {
-			status = sysfs_create_group(&dev->kobj,
-						&gpio_attr_group);
-
-			if (!status && direction_may_change)
-				status = device_create_file(dev,
-						&dev_attr_direction);
-
-			if (!status && gpio_to_irq(gpio) >= 0
-					&& (direction_may_change
-						|| !test_bit(FLAG_IS_OUT,
-							&desc->flags)))
-				status = device_create_file(dev,
-						&dev_attr_edge);
-
-			if (status != 0)
-				device_unregister(dev);
-		} else
-			status = PTR_ERR(dev);
-		if (status == 0)
-			set_bit(FLAG_EXPORT, &desc->flags);
+	dev = device_create_with_groups(&gpio_class, desc->chip->dev,
+					MKDEV(0, 0), desc, gpio_groups,
+					ioname ? ioname : "gpio%u", gpio);
+	if (IS_ERR(dev)) {
+		status = PTR_ERR(dev);
+		goto fail_unlock;
 	}
 
+	set_bit(FLAG_EXPORT, &desc->flags);
 	mutex_unlock(&sysfs_lock);
+	return 0;
 
-done:
-	if (status)
-		pr_debug("%s: gpio%d status %d\n", __func__, gpio, status);
-
+fail_unlock:
+	mutex_unlock(&sysfs_lock);
+	pr_debug("%s: gpio%d status %d\n", __func__, gpio, status);
 	return status;
 }
 EXPORT_SYMBOL_GPL(gpio_export);
@@ -805,6 +825,7 @@ int gpio_export_link(struct device *dev, const char *name, unsigned gpio)
 		if (tdev != NULL) {
 			status = sysfs_create_link(&dev->kobj, &tdev->kobj,
 						name);
+			put_device(tdev);
 		} else {
 			status = -ENODEV;
 		}
@@ -855,7 +876,7 @@ int gpio_sysfs_set_active_low(unsigned gpio, int value)
 	}
 
 	status = sysfs_set_active_low(desc, dev, value);
-
+	put_device(dev);
 unlock:
 	mutex_unlock(&sysfs_lock);
 
@@ -893,6 +914,7 @@ void gpio_unexport(unsigned gpio)
 		dev = class_find_device(&gpio_class, NULL, desc, match_export);
 		if (dev) {
 			gpio_setup_irq(desc, dev, 0);
+			clear_bit(FLAG_SYSFS_DIR, &desc->flags);
 			clear_bit(FLAG_EXPORT, &desc->flags);
 		} else
 			status = -ENODEV;
@@ -924,13 +946,13 @@ static int gpiochip_export(struct gpio_chip *chip)
 
 	/* use chip->base for the ID; it's already known to be unique */
 	mutex_lock(&sysfs_lock);
-	dev = device_create(&gpio_class, chip->dev, MKDEV(0, 0), chip,
-				"gpiochip%d", chip->base);
-	if (!IS_ERR(dev)) {
-		status = sysfs_create_group(&dev->kobj,
-				&gpiochip_attr_group);
-	} else
+	dev = device_create_with_groups(&gpio_class, chip->dev, MKDEV(0, 0),
+					chip, gpiochip_groups,
+					"gpiochip%d", chip->base);
+	if (IS_ERR(dev))
 		status = PTR_ERR(dev);
+	else
+		status = 0;
 	chip->exported = (status == 0);
 	mutex_unlock(&sysfs_lock);
 
@@ -1081,23 +1103,22 @@ int gpiochip_add(struct gpio_chip *chip)
 				? (1 << FLAG_IS_OUT)
 				: 0;
 		}
-	}
 
 #ifdef CONFIG_PINCTRL
 	INIT_LIST_HEAD(&chip->pin_ranges);
 #endif
-
-	of_gpiochip_add(chip);
+	
+		of_gpiochip_add(chip);
+	}
 
 unlock:
 	spin_unlock_irqrestore(&gpio_lock, flags);
 
-	if (status)
-		goto fail;
-
 	status = gpiochip_export(chip);
-	if (status)
+	if (status) {
+		of_gpiochip_remove(chip);
 		goto fail;
+	}
 
 	pr_info("gpiochip_add: registered GPIOs %d to %d on device: %s\n",
 		chip->base, chip->base + chip->ngpio - 1,
diff --git a/drivers/gpu/drm/i915/i915_gem.c b/drivers/gpu/drm/i915/i915_gem.c
index 2ac4ded..b1f1d10 100644
--- a/drivers/gpu/drm/i915/i915_gem.c
+++ b/drivers/gpu/drm/i915/i915_gem.c
@@ -2193,6 +2193,13 @@ static int sandybridge_write_fence_reg(struct drm_i915_gem_object *obj,
 	int regnum = obj->fence_reg;
 	uint64_t val;
 
+	/* Adjust fence size to match tiled area */
+	if (obj->tiling_mode != I915_TILING_NONE) {
+		uint32_t row_size = obj->stride *
+			(obj->tiling_mode == I915_TILING_Y ? 32 : 8);
+		size = (size / row_size) * row_size;
+	}
+
 	val = (uint64_t)((obj->gtt_offset + size - 4096) &
 			 0xfffff000) << 32;
 	val |= obj->gtt_offset & 0xfffff000;
@@ -2230,6 +2237,13 @@ static int i965_write_fence_reg(struct drm_i915_gem_object *obj,
 	int regnum = obj->fence_reg;
 	uint64_t val;
 
+	/* Adjust fence size to match tiled area */
+	if (obj->tiling_mode != I915_TILING_NONE) {
+		uint32_t row_size = obj->stride *
+			(obj->tiling_mode == I915_TILING_Y ? 32 : 8);
+		size = (size / row_size) * row_size;
+	}
+
 	val = (uint64_t)((obj->gtt_offset + size - 4096) &
 		    0xfffff000) << 32;
 	val |= obj->gtt_offset & 0xfffff000;
diff --git a/drivers/gpu/drm/i915/intel_lvds.c b/drivers/gpu/drm/i915/intel_lvds.c
index 77190cc..3febe29 100644
--- a/drivers/gpu/drm/i915/intel_lvds.c
+++ b/drivers/gpu/drm/i915/intel_lvds.c
@@ -932,6 +932,17 @@ bool intel_lvds_init(struct drm_device *dev)
 	int pipe;
 	u8 pin;
 
+	/*
+	 * Unlock registers and just leave them unlocked. Do this before
+	 * checking quirk lists to avoid bogus WARNINGs.
+	 */
+	if (HAS_PCH_SPLIT(dev)) {
+		I915_WRITE(PCH_PP_CONTROL,
+			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
+	} else {
+		I915_WRITE(PP_CONTROL,
+			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
+	}
 	if (!intel_lvds_supported(dev))
 		return false;
 
@@ -1109,19 +1120,6 @@ bool intel_lvds_init(struct drm_device *dev)
 		pwm = I915_READ(BLC_PWM_PCH_CTL1);
 		pwm |= PWM_PCH_ENABLE;
 		I915_WRITE(BLC_PWM_PCH_CTL1, pwm);
-		/*
-		 * Unlock registers and just
-		 * leave them unlocked
-		 */
-		I915_WRITE(PCH_PP_CONTROL,
-			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
-	} else {
-		/*
-		 * Unlock registers and just
-		 * leave them unlocked
-		 */
-		I915_WRITE(PP_CONTROL,
-			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
 	}
 	dev_priv->lid_notifier.notifier_call = intel_lid_notify;
 	if (acpi_lid_notifier_register(&dev_priv->lid_notifier)) {
diff --git a/drivers/gpu/drm/radeon/radeon_kms.c b/drivers/gpu/drm/radeon/radeon_kms.c
index 9b46238..b731686 100644
--- a/drivers/gpu/drm/radeon/radeon_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_kms.c
@@ -428,6 +428,8 @@ int radeon_get_vblank_timestamp_kms(struct drm_device *dev, int crtc,
 
 	/* Get associated drm_crtc: */
 	drmcrtc = &rdev->mode_info.crtcs[crtc]->base;
+	if (!drmcrtc)
+		return -EINVAL;
 
 	/* Helper routine in DRM core does all the work: */
 	return drm_calc_vbltimestamp_from_scanoutpos(dev, crtc, max_error,
diff --git a/drivers/gpu/drm/radeon/radeon_ttm.c b/drivers/gpu/drm/radeon/radeon_ttm.c
index 49b55ed..15042d0 100644
--- a/drivers/gpu/drm/radeon/radeon_ttm.c
+++ b/drivers/gpu/drm/radeon/radeon_ttm.c
@@ -188,7 +188,7 @@ static void radeon_evict_flags(struct ttm_buffer_object *bo,
 	rbo = container_of(bo, struct radeon_bo, tbo);
 	switch (bo->mem.mem_type) {
 	case TTM_PL_VRAM:
-		if (rbo->rdev->ring[RADEON_RING_TYPE_GFX_INDEX].ready == false)
+		if (rbo->rdev->ring[radeon_copy_ring_index(rbo->rdev)].ready == false)
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_CPU);
 		else
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_GTT);
diff --git a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
index 7e07433..992b46b 100644
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
@@ -485,14 +485,7 @@ void vmw_fence_obj_flush(struct vmw_fence_obj *fence)
 
 static void vmw_fence_destroy(struct vmw_fence_obj *fence)
 {
-	struct vmw_fence_manager *fman = fence->fman;
-
 	kfree(fence);
-	/*
-	 * Free kernel space accounting.
-	 */
-	ttm_mem_global_free(vmw_mem_glob(fman->dev_priv),
-			    fman->fence_size);
 }
 
 int vmw_fence_create(struct vmw_fence_manager *fman,
@@ -500,20 +493,12 @@ int vmw_fence_create(struct vmw_fence_manager *fman,
 		     uint32_t mask,
 		     struct vmw_fence_obj **p_fence)
 {
-	struct ttm_mem_global *mem_glob = vmw_mem_glob(fman->dev_priv);
 	struct vmw_fence_obj *fence;
 	int ret;
 
-	ret = ttm_mem_global_alloc(mem_glob, fman->fence_size,
-				   false, false);
-	if (unlikely(ret != 0))
-		return ret;
-
 	fence = kzalloc(sizeof(*fence), GFP_KERNEL);
-	if (unlikely(fence == NULL)) {
-		ret = -ENOMEM;
-		goto out_no_object;
-	}
+	if (unlikely(fence == NULL))
+		return -ENOMEM;
 
 	ret = vmw_fence_obj_init(fman, fence, seqno, mask,
 				 vmw_fence_destroy);
@@ -525,8 +510,6 @@ int vmw_fence_create(struct vmw_fence_manager *fman,
 
 out_err_init:
 	kfree(fence);
-out_no_object:
-	ttm_mem_global_free(mem_glob, fman->fence_size);
 	return ret;
 }
 
@@ -1049,6 +1032,8 @@ int vmw_event_fence_action_create(struct drm_file *file_priv,
 	if (ret != 0)
 		goto out_no_queue;
 
+	return 0;
+
 out_no_queue:
 	event->base.destroy(&event->base);
 out_no_event:
@@ -1123,17 +1108,10 @@ int vmw_fence_event_ioctl(struct drm_device *dev, void *data,
 
 	BUG_ON(fence == NULL);
 
-	if (arg->flags & DRM_VMW_FE_FLAG_REQ_TIME)
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-	else
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-
+	ret = vmw_event_fence_action_create(file_priv, fence,
+					    arg->flags,
+					    arg->user_data,
+					    true);
 	if (unlikely(ret != 0)) {
 		if (ret != -ERESTARTSYS)
 			DRM_ERROR("Failed to attach event to fence.\n");
diff --git a/drivers/hid/hid-roccat-pyra.c b/drivers/hid/hid-roccat-pyra.c
index df05c1b..5346647 100644
--- a/drivers/hid/hid-roccat-pyra.c
+++ b/drivers/hid/hid-roccat-pyra.c
@@ -35,6 +35,8 @@ static struct class *pyra_class;
 static void profile_activated(struct pyra_device *pyra,
 		unsigned int new_profile)
 {
+	if (new_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return;
 	pyra->actual_profile = new_profile;
 	pyra->actual_cpi = pyra->profile_settings[pyra->actual_profile].y_cpi;
 }
@@ -299,10 +301,15 @@ static ssize_t pyra_sysfs_write_settings(struct file *fp,
 	int retval = 0;
 	int difference;
 	struct pyra_roccat_report roccat_report;
+	struct pyra_settings const *settings;
 
 	if (off != 0 || count != sizeof(struct pyra_settings))
 		return -EINVAL;
 
+	settings = (struct pyra_settings const *)buf;
+	if (settings->startup_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return -EINVAL;
+
 	mutex_lock(&pyra->pyra_lock);
 	difference = memcmp(buf, &pyra->settings, sizeof(struct pyra_settings));
 	if (difference) {
diff --git a/drivers/hv/vmbus_drv.c b/drivers/hv/vmbus_drv.c
index 10619b3..1ec309d 100644
--- a/drivers/hv/vmbus_drv.c
+++ b/drivers/hv/vmbus_drv.c
@@ -681,7 +681,7 @@ int vmbus_device_register(struct hv_device *child_device_obj)
 	if (ret)
 		pr_err("Unable to register child device\n");
 	else
-		pr_info("child device %s registered\n",
+		pr_debug("child device %s registered\n",
 			dev_name(&child_device_obj->device));
 
 	return ret;
@@ -693,14 +693,14 @@ int vmbus_device_register(struct hv_device *child_device_obj)
  */
 void vmbus_device_unregister(struct hv_device *device_obj)
 {
+	pr_debug("child device %s unregistered\n",
+		dev_name(&device_obj->device));
+
 	/*
 	 * Kick off the process of unregistering the device.
 	 * This will call vmbus_remove() and eventually vmbus_device_release()
 	 */
 	device_unregister(&device_obj->device);
-
-	pr_info("child device %s unregistered\n",
-		dev_name(&device_obj->device));
 }
 
 
diff --git a/drivers/i2c/busses/i2c-davinci.c b/drivers/i2c/busses/i2c-davinci.c
index 79b4bcb..1837fe6 100644
--- a/drivers/i2c/busses/i2c-davinci.c
+++ b/drivers/i2c/busses/i2c-davinci.c
@@ -416,11 +416,9 @@ i2c_davinci_xfer_msg(struct i2c_adapter *adap, struct i2c_msg *msg, int stop)
 	if (dev->cmd_err & DAVINCI_I2C_STR_NACK) {
 		if (msg->flags & I2C_M_IGNORE_NAK)
 			return msg->len;
-		if (stop) {
-			w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
-			w |= DAVINCI_I2C_MDR_STP;
-			davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
-		}
+		w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
+		w |= DAVINCI_I2C_MDR_STP;
+		davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
 		return -EREMOTEIO;
 	}
 	return -EIO;
diff --git a/drivers/input/joystick/xpad.c b/drivers/input/joystick/xpad.c
index 42f7b25..b4e8db8 100644
--- a/drivers/input/joystick/xpad.c
+++ b/drivers/input/joystick/xpad.c
@@ -979,9 +979,19 @@ static int xpad_probe(struct usb_interface *intf, const struct usb_device_id *id
 		}
 
 		ep_irq_in = &intf->cur_altsetting->endpoint[1].desc;
-		usb_fill_bulk_urb(xpad->bulk_out, udev,
-				usb_sndbulkpipe(udev, ep_irq_in->bEndpointAddress),
-				xpad->bdata, XPAD_PKT_LEN, xpad_bulk_out, xpad);
+		if (usb_endpoint_is_bulk_out(ep_irq_in)) {
+			usb_fill_bulk_urb(xpad->bulk_out, udev,
+					  usb_sndbulkpipe(udev,
+							  ep_irq_in->bEndpointAddress),
+					  xpad->bdata, XPAD_PKT_LEN,
+					  xpad_bulk_out, xpad);
+		} else {
+			usb_fill_int_urb(xpad->bulk_out, udev,
+					 usb_sndintpipe(udev,
+							ep_irq_in->bEndpointAddress),
+					 xpad->bdata, XPAD_PKT_LEN,
+					 xpad_bulk_out, xpad, 0);
+		}
 
 		/*
 		 * Submit the int URB immediately rather than waiting for open
diff --git a/drivers/input/serio/i8042-x86ia64io.h b/drivers/input/serio/i8042-x86ia64io.h
index ce715b1..78227f3 100644
--- a/drivers/input/serio/i8042-x86ia64io.h
+++ b/drivers/input/serio/i8042-x86ia64io.h
@@ -408,6 +408,13 @@ static const struct dmi_system_id __initconst i8042_dmi_nomux_table[] = {
 		},
 	},
 	{
+		/* Acer Aspire 7738 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "Acer"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "Aspire 7738"),
+		},
+	},
+	{
 		/* Gericom Bellagio */
 		.matches = {
 			DMI_MATCH(DMI_SYS_VENDOR, "Gericom"),
@@ -721,6 +728,35 @@ static const struct dmi_system_id __initconst i8042_dmi_dritek_table[] = {
 	{ }
 };
 
+/*
+ * Some laptops need keyboard reset before probing for the trackpad to get
+ * it detected, initialised & finally work.
+ */
+static const struct dmi_system_id __initconst i8042_dmi_kbdreset_table[] = {
+	{
+		/* Gigabyte P35 v2 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P35V2"),
+		},
+	},
+		{
+		/* Aorus branded Gigabyte X3 Plus - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "X3"),
+		},
+	},
+	{
+		/* Gigabyte P34 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P34"),
+		},
+	},
+	{ }
+};
+
 #endif /* CONFIG_X86 */
 
 #ifdef CONFIG_PNP
@@ -1001,6 +1037,9 @@ static int __init i8042_platform_init(void)
 	if (dmi_check_system(i8042_dmi_dritek_table))
 		i8042_dritek = true;
 
+	if (dmi_check_system(i8042_dmi_kbdreset_table))
+		i8042_kbdreset = true;
+
 	/*
 	 * A20 was already enabled during early kernel init. But some buggy
 	 * BIOSes (in MSI Laptops) require A20 to be enabled using 8042 to
diff --git a/drivers/input/serio/i8042.c b/drivers/input/serio/i8042.c
index 8656441..178e75d 100644
--- a/drivers/input/serio/i8042.c
+++ b/drivers/input/serio/i8042.c
@@ -67,6 +67,10 @@ static bool i8042_notimeout;
 module_param_named(notimeout, i8042_notimeout, bool, 0);
 MODULE_PARM_DESC(notimeout, "Ignore timeouts signalled by i8042");
 
+static bool i8042_kbdreset;
+module_param_named(kbdreset, i8042_kbdreset, bool, 0);
+MODULE_PARM_DESC(kbdreset, "Reset device connected to KBD port");
+
 #ifdef CONFIG_X86
 static bool i8042_dritek;
 module_param_named(dritek, i8042_dritek, bool, 0);
@@ -783,6 +787,16 @@ static int __init i8042_check_aux(void)
 		return -1;
 
 /*
+ * Reset keyboard (needed on some laptops to successfully detect
+ * touchpad, e.g., some Gigabyte laptop models with Elantech
+ * touchpads).
+ */
+	if (i8042_kbdreset) {
+		pr_warn("Attempting to reset device connected to KBD port\n");
+		i8042_kbd_write(NULL, (unsigned char) 0xff);
+	}
+
+/*
  * Test AUX IRQ delivery to make sure BIOS did not grab the IRQ and
  * used it for a PCI card or somethig else.
  */
diff --git a/drivers/iommu/intel-iommu.c b/drivers/iommu/intel-iommu.c
index a5f4359..2e48b22 100644
--- a/drivers/iommu/intel-iommu.c
+++ b/drivers/iommu/intel-iommu.c
@@ -1792,7 +1792,7 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 	struct dma_pte *first_pte = NULL, *pte = NULL;
 	phys_addr_t uninitialized_var(pteval);
 	int addr_width = agaw_to_width(domain->agaw) - VTD_PAGE_SHIFT;
-	unsigned long sg_res;
+	unsigned long sg_res = 0;
 	unsigned int largepage_lvl = 0;
 	unsigned long lvl_pages = 0;
 
@@ -1803,10 +1803,8 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 
 	prot &= DMA_PTE_READ | DMA_PTE_WRITE | DMA_PTE_SNP;
 
-	if (sg)
-		sg_res = 0;
-	else {
-		sg_res = nr_pages + 1;
+	if (!sg) {
+		sg_res = nr_pages;
 		pteval = ((phys_addr_t)phys_pfn << VTD_PAGE_SHIFT) | prot;
 	}
 
diff --git a/drivers/mfd/tc6393xb.c b/drivers/mfd/tc6393xb.c
index 9612264..b69d91b 100644
--- a/drivers/mfd/tc6393xb.c
+++ b/drivers/mfd/tc6393xb.c
@@ -263,6 +263,17 @@ static int tc6393xb_ohci_disable(struct platform_device *dev)
 	return 0;
 }
 
+static int tc6393xb_ohci_suspend(struct platform_device *dev)
+{
+	struct tc6393xb_platform_data *tcpd = dev_get_platdata(dev->dev.parent);
+
+	/* We can't properly store/restore OHCI state, so fail here */
+	if (tcpd->resume_restore)
+		return -EBUSY;
+
+	return tc6393xb_ohci_disable(dev);
+}
+
 static int tc6393xb_fb_enable(struct platform_device *dev)
 {
 	struct tc6393xb *tc6393xb = dev_get_drvdata(dev->dev.parent);
@@ -403,7 +414,7 @@ static struct mfd_cell __devinitdata tc6393xb_cells[] = {
 		.num_resources = ARRAY_SIZE(tc6393xb_ohci_resources),
 		.resources = tc6393xb_ohci_resources,
 		.enable = tc6393xb_ohci_enable,
-		.suspend = tc6393xb_ohci_disable,
+		.suspend = tc6393xb_ohci_suspend,
 		.resume = tc6393xb_ohci_enable,
 		.disable = tc6393xb_ohci_disable,
 	},
diff --git a/drivers/mtd/ubi/upd.c b/drivers/mtd/ubi/upd.c
index 425bf5a..068a246 100644
--- a/drivers/mtd/ubi/upd.c
+++ b/drivers/mtd/ubi/upd.c
@@ -135,6 +135,10 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 	ubi_assert(!vol->updating && !vol->changing_leb);
 	vol->updating = 1;
 
+	vol->upd_buf = vmalloc(ubi->leb_size);
+	if (!vol->upd_buf)
+		return -ENOMEM;
+
 	err = set_update_marker(ubi, vol);
 	if (err)
 		return err;
@@ -154,14 +158,12 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 		err = clear_update_marker(ubi, vol, 0);
 		if (err)
 			return err;
+
+		vfree(vol->upd_buf);
 		vol->updating = 0;
 		return 0;
 	}
 
-	vol->upd_buf = vmalloc(ubi->leb_size);
-	if (!vol->upd_buf)
-		return -ENOMEM;
-
 	vol->upd_ebs = div_u64(bytes + vol->usable_leb_size - 1,
 			       vol->usable_leb_size);
 	vol->upd_bytes = bytes;
diff --git a/drivers/net/can/dev.c b/drivers/net/can/dev.c
index d4f7f95..88c39e4 100644
--- a/drivers/net/can/dev.c
+++ b/drivers/net/can/dev.c
@@ -612,10 +612,14 @@ static int can_changelink(struct net_device *dev,
 		if (dev->flags & IFF_UP)
 			return -EBUSY;
 		cm = nla_data(data[IFLA_CAN_CTRLMODE]);
-		if (cm->flags & ~priv->ctrlmode_supported)
+
+		/* check whether changed bits are allowed to be modified */
+		if (cm->mask & ~priv->ctrlmode_supported)
 			return -EOPNOTSUPP;
+
+		/* clear bits to be modified and copy the flag values */
 		priv->ctrlmode &= ~cm->mask;
-		priv->ctrlmode |= cm->flags;
+		priv->ctrlmode |= (cm->flags & cm->mask);
 	}
 
 	if (data[IFLA_CAN_BITTIMING]) {
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_core.c b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
index d2f91f7..925c7e1 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_core.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
@@ -737,7 +737,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 		dev_err(&intf->dev, "%s: couldn't alloc cmd buffer\n",
 			PCAN_USB_DRIVER_NAME);
 		err = -ENOMEM;
-		goto lbl_set_intf_data;
+		goto lbl_free_candev;
 	}
 
 	dev->udev = usb_dev;
@@ -776,7 +776,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	err = register_candev(netdev);
 	if (err) {
 		dev_err(&intf->dev, "couldn't register CAN device: %d\n", err);
-		goto lbl_free_cmd_buf;
+		goto lbl_restore_intf_data;
 	}
 
 	if (dev->prev_siblings)
@@ -789,14 +789,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	if (dev->adapter->dev_init) {
 		err = dev->adapter->dev_init(dev);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* set bus off */
 	if (dev->adapter->dev_set_bus) {
 		err = dev->adapter->dev_set_bus(dev, 0);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* get device number early */
@@ -808,11 +808,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 
 	return 0;
 
-lbl_free_cmd_buf:
-	kfree(dev->cmd_buf);
+lbl_unregister_candev:
+	unregister_candev(netdev);
 
-lbl_set_intf_data:
+lbl_restore_intf_data:
 	usb_set_intfdata(intf, dev->prev_siblings);
+	kfree(dev->cmd_buf);
+
+lbl_free_candev:
 	free_candev(netdev);
 
 	return err;
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
index c95913a..5fe28be 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
@@ -333,8 +333,6 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	if (!(dev->state & PCAN_USB_STATE_CONNECTED))
 		return 0;
 
-	memset(req_addr, '\0', req_size);
-
 	req_type = USB_TYPE_VENDOR | USB_RECIP_OTHER;
 
 	switch (req_id) {
@@ -345,6 +343,7 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	default:
 		p = usb_rcvctrlpipe(dev->udev, 0);
 		req_type |= USB_DIR_IN;
+		memset(req_addr, '\0', req_size);
 		break;
 	}
 
diff --git a/drivers/net/wireless/ath/ath5k/qcu.c b/drivers/net/wireless/ath/ath5k/qcu.c
index 30b50f9..19ba204 100644
--- a/drivers/net/wireless/ath/ath5k/qcu.c
+++ b/drivers/net/wireless/ath/ath5k/qcu.c
@@ -223,13 +223,7 @@ ath5k_hw_setup_tx_queue(struct ath5k_hw *ah, enum ath5k_tx_queue queue_type,
 	} else {
 		switch (queue_type) {
 		case AR5K_TX_QUEUE_DATA:
-			for (queue = AR5K_TX_QUEUE_ID_DATA_MIN;
-				ah->ah_txq[queue].tqi_type !=
-				AR5K_TX_QUEUE_INACTIVE; queue++) {
-
-				if (queue > AR5K_TX_QUEUE_ID_DATA_MAX)
-					return -EINVAL;
-			}
+			queue = queue_info->tqi_subtype;
 			break;
 		case AR5K_TX_QUEUE_UAPSD:
 			queue = AR5K_TX_QUEUE_ID_UAPSD;
diff --git a/drivers/net/wireless/ath/ath9k/hw.h b/drivers/net/wireless/ath/ath9k/hw.h
index f49be96..d4f09b4 100644
--- a/drivers/net/wireless/ath/ath9k/hw.h
+++ b/drivers/net/wireless/ath/ath9k/hw.h
@@ -181,8 +181,8 @@
 #define PAPRD_IDEAL_AGC2_PWR_RANGE	0xe0
 
 enum ath_hw_txq_subtype {
-	ATH_TXQ_AC_BE = 0,
-	ATH_TXQ_AC_BK = 1,
+	ATH_TXQ_AC_BK = 0,
+	ATH_TXQ_AC_BE = 1,
 	ATH_TXQ_AC_VI = 2,
 	ATH_TXQ_AC_VO = 3,
 };
diff --git a/drivers/net/wireless/ath/ath9k/mac.c b/drivers/net/wireless/ath/ath9k/mac.c
index f7bd253..2d628f9 100644
--- a/drivers/net/wireless/ath/ath9k/mac.c
+++ b/drivers/net/wireless/ath/ath9k/mac.c
@@ -303,14 +303,7 @@ int ath9k_hw_setuptxqueue(struct ath_hw *ah, enum ath9k_tx_queue type,
 		q = ATH9K_NUM_TX_QUEUES - 3;
 		break;
 	case ATH9K_TX_QUEUE_DATA:
-		for (q = 0; q < ATH9K_NUM_TX_QUEUES; q++)
-			if (ah->txq[q].tqi_type ==
-			    ATH9K_TX_QUEUE_INACTIVE)
-				break;
-		if (q == ATH9K_NUM_TX_QUEUES) {
-			ath_err(common, "No available TX queue\n");
-			return -1;
-		}
+		q = qinfo->tqi_subtype;
 		break;
 	default:
 		ath_err(common, "Invalid TX queue type: %u\n", type);
diff --git a/drivers/pci/probe.c b/drivers/pci/probe.c
index 63e0199..d62ad0b 100644
--- a/drivers/pci/probe.c
+++ b/drivers/pci/probe.c
@@ -254,14 +254,17 @@ int __pci_read_base(struct pci_dev *dev, enum pci_bar_type type,
 		res->flags |= IORESOURCE_SIZEALIGN;
 		if (res->flags & IORESOURCE_IO) {
 			l &= PCI_BASE_ADDRESS_IO_MASK;
+			sz &= PCI_BASE_ADDRESS_IO_MASK;
 			mask = PCI_BASE_ADDRESS_IO_MASK & (u32) IO_SPACE_LIMIT;
 		} else {
 			l &= PCI_BASE_ADDRESS_MEM_MASK;
+			sz &= PCI_BASE_ADDRESS_MEM_MASK;
 			mask = (u32)PCI_BASE_ADDRESS_MEM_MASK;
 		}
 	} else {
 		res->flags |= (l & IORESOURCE_ROM_ENABLE);
 		l &= PCI_ROM_ADDRESS_MASK;
+		sz &= PCI_ROM_ADDRESS_MASK;
 		mask = (u32)PCI_ROM_ADDRESS_MASK;
 	}
 
diff --git a/drivers/pci/quirks.c b/drivers/pci/quirks.c
index e587d00..ffde183 100644
--- a/drivers/pci/quirks.c
+++ b/drivers/pci/quirks.c
@@ -327,19 +327,52 @@ static void __devinit quirk_s3_64M(struct pci_dev *dev)
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_S3,	PCI_DEVICE_ID_S3_868,		quirk_s3_64M);
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_S3,	PCI_DEVICE_ID_S3_968,		quirk_s3_64M);
 
+static void quirk_io(struct pci_dev *dev, int pos, unsigned size,
+		     const char *name)
+{
+	u32 region;
+	struct pci_bus_region bus_region;
+	struct resource *res = dev->resource + pos;
+
+	pci_read_config_dword(dev, PCI_BASE_ADDRESS_0 + (pos << 2), &region);
+
+	if (!region)
+		return;
+
+	res->name = pci_name(dev);
+	res->flags = region & ~PCI_BASE_ADDRESS_IO_MASK;
+	res->flags |=
+		(IORESOURCE_IO | IORESOURCE_PCI_FIXED | IORESOURCE_SIZEALIGN);
+	region &= ~(size - 1);
+
+	/* Convert from PCI bus to resource space */
+	bus_region.start = region;
+	bus_region.end = region + size - 1;
+	pcibios_bus_to_resource(dev->bus, res, &bus_region);
+
+	dev_info(&dev->dev, FW_BUG "%s quirk: reg 0x%x: %pR\n",
+		 name, PCI_BASE_ADDRESS_0 + (pos << 2), res);
+}
+
 /*
  * Some CS5536 BIOSes (for example, the Soekris NET5501 board w/ comBIOS
  * ver. 1.33  20070103) don't set the correct ISA PCI region header info.
  * BAR0 should be 8 bytes; instead, it may be set to something like 8k
  * (which conflicts w/ BAR1's memory range).
+ *
+ * CS553x's ISA PCI BARs may also be read-only (ref:
+ * https://bugzilla.kernel.org/show_bug.cgi?id=85991 - Comment #4 forward).
  */
 static void __devinit quirk_cs5536_vsa(struct pci_dev *dev)
 {
+	static char *name = "CS5536 ISA bridge";
+
 	if (pci_resource_len(dev, 0) != 8) {
-		struct resource *res = &dev->resource[0];
-		res->end = res->start + 8 - 1;
-		dev_info(&dev->dev, "CS5536 ISA bridge bug detected "
-				"(incorrect header); workaround applied.\n");
+		quirk_io(dev, 0,   8, name);	/* SMB */
+		quirk_io(dev, 1, 256, name);	/* GPIO */
+		quirk_io(dev, 2,  64, name);	/* MFGPT */
+		dev_info(&dev->dev, "%s bug detected (incorrect header); workaround applied\n",
+			 name);
 	}
 }
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_AMD, PCI_DEVICE_ID_AMD_CS5536_ISA, quirk_cs5536_vsa);
diff --git a/drivers/platform/x86/hp_accel.c b/drivers/platform/x86/hp_accel.c
index 0076fea..be6b648 100644
--- a/drivers/platform/x86/hp_accel.c
+++ b/drivers/platform/x86/hp_accel.c
@@ -237,6 +237,7 @@ static struct dmi_system_id lis3lv02d_dmi_ids[] = {
 	AXIS_DMI_MATCH("HPB64xx", "HP ProBook 64", xy_swap),
 	AXIS_DMI_MATCH("HPB64xx", "HP EliteBook 84", xy_swap),
 	AXIS_DMI_MATCH("HPB65xx", "HP ProBook 65", x_inverted),
+	AXIS_DMI_MATCH("HPZBook15", "HP ZBook 15", x_inverted),
 	{ NULL, }
 /* Laptop models without axis info (yet):
  * "NC6910" "HP Compaq 6910"
diff --git a/drivers/regulator/core.c b/drivers/regulator/core.c
index c45c2dc..98ccd6a 100644
--- a/drivers/regulator/core.c
+++ b/drivers/regulator/core.c
@@ -1427,12 +1427,14 @@ void regulator_put(struct regulator *regulator)
 		device_remove_file(regulator->dev, &regulator->dev_attr);
 		kfree(regulator->dev_attr.attr.name);
 	}
+	mutex_lock(&rdev->mutex);
 	kfree(regulator->supply_name);
 	list_del(&regulator->list);
 	kfree(regulator);
 
 	rdev->open_count--;
 	rdev->exclusive = 0;
+	mutex_unlock(&rdev->mutex);
 
 	module_put(rdev->owner);
 	mutex_unlock(&regulator_list_mutex);
diff --git a/drivers/s390/char/con3215.c b/drivers/s390/char/con3215.c
index 4f9f1dc..fa47d8d 100644
--- a/drivers/s390/char/con3215.c
+++ b/drivers/s390/char/con3215.c
@@ -997,12 +997,26 @@ static int tty3215_write(struct tty_struct * tty,
 			 const unsigned char *buf, int count)
 {
 	struct raw3215_info *raw;
+	int i, written;
 
 	if (!tty)
 		return 0;
 	raw = (struct raw3215_info *) tty->driver_data;
-	raw3215_write(raw, buf, count);
-	return count;
+	written = count;
+	while (count > 0) {
+		for (i = 0; i < count; i++)
+			if (buf[i] == '\t' || buf[i] == '\n')
+				break;
+		raw3215_write(raw, buf, i);
+		count -= i;
+		buf += i;
+		if (count > 0) {
+			raw3215_putchar(raw, *buf);
+			count--;
+			buf++;
+		}
+	}
+	return written;
 }
 
 /*
@@ -1149,7 +1163,7 @@ static int __init tty3215_init(void)
 	driver->subtype = SYSTEM_TYPE_TTY;
 	driver->init_termios = tty_std_termios;
 	driver->init_termios.c_iflag = IGNBRK | IGNPAR;
-	driver->init_termios.c_oflag = ONLCR | XTABS;
+	driver->init_termios.c_oflag = ONLCR;
 	driver->init_termios.c_lflag = ISIG;
 	driver->flags = TTY_DRIVER_REAL_RAW;
 	tty_set_operations(driver, &tty3215_ops);
diff --git a/drivers/scsi/NCR5380.c b/drivers/scsi/NCR5380.c
index 165e4dd86..a57f85a 100644
--- a/drivers/scsi/NCR5380.c
+++ b/drivers/scsi/NCR5380.c
@@ -2662,14 +2662,14 @@ static void NCR5380_dma_complete(NCR5380_instance * instance) {
  *
  * Purpose : abort a command
  *
- * Inputs : cmd - the Scsi_Cmnd to abort, code - code to set the 
- *      host byte of the result field to, if zero DID_ABORTED is 
+ * Inputs : cmd - the Scsi_Cmnd to abort, code - code to set the
+ *      host byte of the result field to, if zero DID_ABORTED is
  *      used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
- *	XXX - there is no way to abort the command that is currently 
- *	connected, you have to wait for it to complete.  If this is 
+ *	XXX - there is no way to abort the command that is currently
+ *	connected, you have to wait for it to complete.  If this is
  *	a problem, we could implement longjmp() / setjmp(), setjmp()
  *	called where the loop started in NCR5380_main().
  *
@@ -2719,7 +2719,7 @@ static int NCR5380_abort(Scsi_Cmnd * cmd) {
  * aborted flag and get back into our main loop.
  */
 
-		return 0;
+		return SUCCESS;
 	}
 #endif
 
diff --git a/drivers/scsi/aha1740.c b/drivers/scsi/aha1740.c
index a3e6ed3..d0fa3e7 100644
--- a/drivers/scsi/aha1740.c
+++ b/drivers/scsi/aha1740.c
@@ -550,7 +550,7 @@ static int aha1740_eh_abort_handler (Scsi_Cmnd *dummy)
  * quiet as possible...
  */
 
-	return 0;
+	return SUCCESS;
 }
 
 static struct scsi_host_template aha1740_template = {
diff --git a/drivers/scsi/atari_NCR5380.c b/drivers/scsi/atari_NCR5380.c
index 2db79b4..589c2a3 100644
--- a/drivers/scsi/atari_NCR5380.c
+++ b/drivers/scsi/atari_NCR5380.c
@@ -2638,7 +2638,7 @@ static void NCR5380_reselect(struct Scsi_Host *instance)
  *	host byte of the result field to, if zero DID_ABORTED is
  *	used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
  * XXX - there is no way to abort the command that is currently
  *	 connected, you have to wait for it to complete.  If this is
diff --git a/drivers/scsi/bnx2fc/bnx2fc_fcoe.c b/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
index c1c6a92..cabfbf3 100644
--- a/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
+++ b/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
@@ -406,6 +406,7 @@ static int bnx2fc_rcv(struct sk_buff *skb, struct net_device *dev,
 	struct fc_frame_header *fh;
 	struct fcoe_rcv_info *fr;
 	struct fcoe_percpu_s *bg;
+	struct sk_buff *tmp_skb;
 	unsigned short oxid;
 
 	interface = container_of(ptype, struct bnx2fc_interface,
@@ -417,6 +418,12 @@ static int bnx2fc_rcv(struct sk_buff *skb, struct net_device *dev,
 		goto err;
 	}
 
+	tmp_skb = skb_share_check(skb, GFP_ATOMIC);
+	if (!tmp_skb)
+		goto err;
+
+	skb = tmp_skb;
+
 	if (unlikely(eth_hdr(skb)->h_proto != htons(ETH_P_FCOE))) {
 		printk(KERN_ERR PFX "bnx2fc_rcv: Wrong FC type frame\n");
 		goto err;
diff --git a/drivers/scsi/megaraid.c b/drivers/scsi/megaraid.c
index 4d39a9f..152fe62 100644
--- a/drivers/scsi/megaraid.c
+++ b/drivers/scsi/megaraid.c
@@ -1967,7 +1967,7 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 	     cmd->device->id, cmd->device->lun);
 
 	if(list_empty(&adapter->pending_list))
-		return FALSE;
+		return FAILED;
 
 	list_for_each_safe(pos, next, &adapter->pending_list) {
 
@@ -1990,7 +1990,7 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 					(aor==SCB_ABORT) ? "ABORTING":"RESET",
 					scb->idx);
 
-				return FALSE;
+				return FAILED;
 			}
 			else {
 
@@ -2015,12 +2015,12 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 				list_add_tail(SCSI_LIST(cmd),
 						&adapter->completed_list);
 
-				return TRUE;
+				return SUCCESS;
 			}
 		}
 	}
 
-	return FALSE;
+	return FAILED;
 }
 
 static inline int
diff --git a/drivers/scsi/megaraid/megaraid_sas_base.c b/drivers/scsi/megaraid/megaraid_sas_base.c
index 6188700..bacd344 100644
--- a/drivers/scsi/megaraid/megaraid_sas_base.c
+++ b/drivers/scsi/megaraid/megaraid_sas_base.c
@@ -919,7 +919,7 @@ megasas_issue_blocked_abort_cmd(struct megasas_instance *instance,
 	abort_fr->abort_mfi_phys_addr_hi = 0;
 
 	cmd->sync_cmd = 1;
-	cmd->cmd_status = 0xFF;
+	cmd->cmd_status = ENODATA;
 
 	instance->instancet->issue_dcmd(instance, cmd);
 
diff --git a/drivers/scsi/sd.c b/drivers/scsi/sd.c
index 71459d5..e127ceb 100644
--- a/drivers/scsi/sd.c
+++ b/drivers/scsi/sd.c
@@ -2227,7 +2227,10 @@ sd_read_cache_type(struct scsi_disk *sdkp, unsigned char *buffer)
 		}
 
 		sdkp->DPOFUA = (data.device_specific & 0x10) != 0;
-		if (sdkp->DPOFUA && !sdkp->device->use_10_for_rw) {
+		if (sdp->broken_fua) {
+			sd_printk(KERN_NOTICE, sdkp, "Disabling FUA\n");
+			sdkp->DPOFUA = 0;
+		} else if (sdkp->DPOFUA && !sdkp->device->use_10_for_rw) {
 			sd_printk(KERN_NOTICE, sdkp,
 				  "Uses READ/WRITE(6), disabling FUA\n");
 			sdkp->DPOFUA = 0;
diff --git a/drivers/scsi/storvsc_drv.c b/drivers/scsi/storvsc_drv.c
index 446c023..a0df0fb 100644
--- a/drivers/scsi/storvsc_drv.c
+++ b/drivers/scsi/storvsc_drv.c
@@ -1359,13 +1359,12 @@ static int storvsc_queuecommand(struct Scsi_Host *host, struct scsi_cmnd *scmnd)
 	if (ret == -EAGAIN) {
 		/* no more space */
 
-		if (cmd_request->bounce_sgl_count) {
+		if (cmd_request->bounce_sgl_count)
 			destroy_bounce_buffer(cmd_request->bounce_sgl,
 					cmd_request->bounce_sgl_count);
 
-			ret = SCSI_MLQUEUE_DEVICE_BUSY;
-			goto queue_error;
-		}
+		ret = SCSI_MLQUEUE_DEVICE_BUSY;
+		goto queue_error;
 	}
 
 	return 0;
diff --git a/drivers/scsi/sun3_NCR5380.c b/drivers/scsi/sun3_NCR5380.c
index 7e12a2e..9aaf084 100644
--- a/drivers/scsi/sun3_NCR5380.c
+++ b/drivers/scsi/sun3_NCR5380.c
@@ -2624,15 +2624,15 @@ static void NCR5380_reselect (struct Scsi_Host *instance)
  * Purpose : abort a command
  *
  * Inputs : cmd - the struct scsi_cmnd to abort, code - code to set the
- * 	host byte of the result field to, if zero DID_ABORTED is 
+ *	host byte of the result field to, if zero DID_ABORTED is
  *	used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
- * XXX - there is no way to abort the command that is currently 
- * 	 connected, you have to wait for it to complete.  If this is 
+ * XXX - there is no way to abort the command that is currently
+ *	 connected, you have to wait for it to complete.  If this is
  *	 a problem, we could implement longjmp() / setjmp(), setjmp()
- * 	 called where the loop started in NCR5380_main().
+ *	 called where the loop started in NCR5380_main().
  */
 
 static int NCR5380_abort(struct scsi_cmnd *cmd)
diff --git a/drivers/spi/spi-dw-mid.c b/drivers/spi/spi-dw-mid.c
index efc494a..f15f624 100644
--- a/drivers/spi/spi-dw-mid.c
+++ b/drivers/spi/spi-dw-mid.c
@@ -219,7 +219,6 @@ int dw_spi_mid_init(struct dw_spi *dws)
 	iounmap(clk_reg);
 
 	dws->num_cs = 16;
-	dws->fifo_len = 40;	/* FIFO has 40 words buffer */
 
 #ifdef CONFIG_SPI_DW_MID_DMA
 	dws->dma_priv = kzalloc(sizeof(struct mid_dma), GFP_KERNEL);
diff --git a/drivers/spi/spi-dw.c b/drivers/spi/spi-dw.c
index d1a495f..cce2d7b 100644
--- a/drivers/spi/spi-dw.c
+++ b/drivers/spi/spi-dw.c
@@ -394,9 +394,6 @@ static void pump_transfers(unsigned long data)
 	chip = dws->cur_chip;
 	spi = message->spi;
 
-	if (unlikely(!chip->clk_div))
-		chip->clk_div = dws->max_freq / chip->speed_hz;
-
 	if (message->state == ERROR_STATE) {
 		message->status = -EIO;
 		goto early_exit;
@@ -438,7 +435,7 @@ static void pump_transfers(unsigned long data)
 	if (transfer->speed_hz) {
 		speed = chip->speed_hz;
 
-		if (transfer->speed_hz != speed) {
+		if ((transfer->speed_hz != speed) || (!chip->clk_div)) {
 			speed = transfer->speed_hz;
 			if (speed > dws->max_freq) {
 				printk(KERN_ERR "MRST SPI0: unsupported"
@@ -677,7 +674,6 @@ static int dw_spi_setup(struct spi_device *spi)
 		dev_err(&spi->dev, "No max speed HZ parameter\n");
 		return -EINVAL;
 	}
-	chip->speed_hz = spi->max_speed_hz;
 
 	chip->tmode = 0; /* Tx & Rx */
 	/* Default SPI mode is SCPOL = 0, SCPH = 0 */
@@ -784,13 +780,13 @@ static void spi_hw_init(struct dw_spi *dws)
 	 */
 	if (!dws->fifo_len) {
 		u32 fifo;
-		for (fifo = 2; fifo <= 257; fifo++) {
+		for (fifo = 1; fifo < 256; fifo++) {
 			dw_writew(dws, DW_SPI_TXFLTR, fifo);
 			if (fifo != dw_readw(dws, DW_SPI_TXFLTR))
 				break;
 		}
 
-		dws->fifo_len = (fifo == 257) ? 0 : fifo;
+		dws->fifo_len = (fifo == 1) ? 0 : fifo;
 		dw_writew(dws, DW_SPI_TXFLTR, 0);
 	}
 }
diff --git a/drivers/staging/comedi/drivers/cb_pcidas64.c b/drivers/staging/comedi/drivers/cb_pcidas64.c
index 915157d..6f743df 100644
--- a/drivers/staging/comedi/drivers/cb_pcidas64.c
+++ b/drivers/staging/comedi/drivers/cb_pcidas64.c
@@ -423,6 +423,29 @@ static const struct comedi_lrange ai_ranges_64xx = {
 	 }
 };
 
+static const uint8_t ai_range_code_64xx[8] = {
+	0x0, 0x1, 0x2, 0x3,	/* bipolar 10, 5, 2,5, 1.25 */
+	0x8, 0x9, 0xa, 0xb	/* unipolar 10, 5, 2.5, 1.25 */
+};
+
+/* analog input ranges for 64-Mx boards */
+static const struct comedi_lrange ai_ranges_64_mx = {
+	7, {
+		BIP_RANGE(5),
+		BIP_RANGE(2.5),
+		BIP_RANGE(1.25),
+		BIP_RANGE(0.625),
+		UNI_RANGE(5),
+		UNI_RANGE(2.5),
+		UNI_RANGE(1.25)
+	}
+};
+
+static const uint8_t ai_range_code_64_mx[7] = {
+	0x0, 0x1, 0x2, 0x3,	/* bipolar 5, 2.5, 1.25, 0.625 */
+	0x9, 0xa, 0xb		/* unipolar 5, 2.5, 1.25 */
+};
+
 /* analog input ranges for 60xx boards */
 static const struct comedi_lrange ai_ranges_60xx = {
 	4,
@@ -434,6 +457,10 @@ static const struct comedi_lrange ai_ranges_60xx = {
 	 }
 };
 
+static const uint8_t ai_range_code_60xx[4] = {
+	0x0, 0x1, 0x4, 0x7	/* bipolar 10, 5, 0.5, 0.05 */
+};
+
 /* analog input ranges for 6030, etc boards */
 static const struct comedi_lrange ai_ranges_6030 = {
 	14,
@@ -455,6 +482,11 @@ static const struct comedi_lrange ai_ranges_6030 = {
 	 }
 };
 
+static const uint8_t ai_range_code_6030[14] = {
+	0x0, 0x1, 0x2, 0x3, 0x4, 0x5, 0x6, /* bip 10, 5, 2, 1, 0.5, 0.2, 0.1 */
+	0x9, 0xa, 0xb, 0xc, 0xd, 0xe, 0xf  /* uni 10, 5, 2, 1, 0.5, 0.2, 0.1 */
+};
+
 /* analog input ranges for 6052, etc boards */
 static const struct comedi_lrange ai_ranges_6052 = {
 	15,
@@ -477,6 +509,11 @@ static const struct comedi_lrange ai_ranges_6052 = {
 	 }
 };
 
+static const uint8_t ai_range_code_6052[15] = {
+	0x0, 0x1, 0x2, 0x3, 0x4, 0x5, 0x6, 0x7,	/* bipolar 10 ... 0.05 */
+	0x9, 0xa, 0xb, 0xc, 0xd, 0xe, 0xf	/* unipolar 10 ... 0.1 */
+};
+
 /* analog input ranges for 4020 board */
 static const struct comedi_lrange ai_ranges_4020 = {
 	2,
@@ -561,6 +598,7 @@ struct pcidas64_board {
 	int ai_bits;		/*  analog input resolution */
 	int ai_speed;		/*  fastest conversion period in ns */
 	const struct comedi_lrange *ai_range_table;
+	const uint8_t *ai_range_code;
 	int ao_nchan;		/*  number of analog out channels */
 	int ao_bits;		/*  analog output resolution */
 	int ao_scan_speed;	/*  analog output speed (for a scan, not conversion) */
@@ -619,6 +657,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -635,6 +674,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -650,7 +690,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -666,7 +707,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -682,7 +724,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -698,6 +741,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -714,6 +758,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -729,6 +774,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -745,6 +791,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -761,6 +808,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -777,6 +825,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -791,6 +840,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -803,6 +853,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -816,6 +867,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -830,6 +882,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -846,6 +899,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -862,6 +916,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -878,6 +933,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 3333,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -894,6 +950,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -910,6 +967,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -942,6 +1000,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -954,7 +1013,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -967,7 +1027,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -980,7 +1041,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -993,7 +1055,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1006,7 +1069,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1019,7 +1083,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1257,45 +1322,7 @@ module_exit(driver_cb_pcidas_cleanup_module);
 static unsigned int ai_range_bits_6xxx(const struct comedi_device *dev,
 				       unsigned int range_index)
 {
-	const struct comedi_krange *range =
-	    &board(dev)->ai_range_table->range[range_index];
-	unsigned int bits = 0;
-
-	switch (range->max) {
-	case 10000000:
-		bits = 0x000;
-		break;
-	case 5000000:
-		bits = 0x100;
-		break;
-	case 2000000:
-	case 2500000:
-		bits = 0x200;
-		break;
-	case 1000000:
-	case 1250000:
-		bits = 0x300;
-		break;
-	case 500000:
-		bits = 0x400;
-		break;
-	case 200000:
-	case 250000:
-		bits = 0x500;
-		break;
-	case 100000:
-		bits = 0x600;
-		break;
-	case 50000:
-		bits = 0x700;
-		break;
-	default:
-		comedi_error(dev, "bug! in ai_range_bits_6xxx");
-		break;
-	}
-	if (range->min == 0)
-		bits += 0x900;
-	return bits;
+	return board(dev)->ai_range_code[range_index] << 8;
 }
 
 static unsigned int hw_revision(const struct comedi_device *dev,
diff --git a/drivers/staging/iio/events.h b/drivers/staging/iio/events.h
index c25f0e3..a6f999c 100644
--- a/drivers/staging/iio/events.h
+++ b/drivers/staging/iio/events.h
@@ -90,7 +90,7 @@ enum iio_event_direction {
 
 #define IIO_EVENT_CODE_EXTRACT_TYPE(mask) ((mask >> 56) & 0xFF)
 
-#define IIO_EVENT_CODE_EXTRACT_DIR(mask) ((mask >> 48) & 0xCF)
+#define IIO_EVENT_CODE_EXTRACT_DIR(mask) ((mask >> 48) & 0x7F)
 
 #define IIO_EVENT_CODE_EXTRACT_CHAN_TYPE(mask) ((mask >> 32) & 0xFF)
 
diff --git a/drivers/target/iscsi/iscsi_target_util.c b/drivers/target/iscsi/iscsi_target_util.c
index 4c05ed6..8d57ab3 100644
--- a/drivers/target/iscsi/iscsi_target_util.c
+++ b/drivers/target/iscsi/iscsi_target_util.c
@@ -1480,15 +1480,15 @@ static int iscsit_do_tx_data(
 	struct iscsi_conn *conn,
 	struct iscsi_data_count *count)
 {
-	int data = count->data_length, total_tx = 0, tx_loop = 0, iov_len;
+	int ret, iov_len;
 	struct kvec *iov_p;
 	struct msghdr msg;
 
 	if (!conn || !conn->sock || !conn->conn_ops)
 		return -1;
 
-	if (data <= 0) {
-		pr_err("Data length is: %d\n", data);
+	if (count->data_length <= 0) {
+		pr_err("Data length is: %d\n", count->data_length);
 		return -1;
 	}
 
@@ -1497,20 +1497,16 @@ static int iscsit_do_tx_data(
 	iov_p = count->iov;
 	iov_len = count->iov_count;
 
-	while (total_tx < data) {
-		tx_loop = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
-					(data - total_tx));
-		if (tx_loop <= 0) {
-			pr_debug("tx_loop: %d total_tx %d\n",
-				tx_loop, total_tx);
-			return tx_loop;
-		}
-		total_tx += tx_loop;
-		pr_debug("tx_loop: %d, total_tx: %d, data: %d\n",
-					tx_loop, total_tx, data);
+	ret = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
+			     count->data_length);
+	if (ret != count->data_length) {
+		pr_err("Unexpected ret: %d send data %d\n",
+		       ret, count->data_length);
+		return -EPIPE;
 	}
+	pr_debug("ret: %d, sent data: %d\n", ret, count->data_length);
 
-	return total_tx;
+	return ret;
 }
 
 int rx_data(
diff --git a/drivers/tty/serial/samsung.c b/drivers/tty/serial/samsung.c
index c49f3bf..8b409d4 100644
--- a/drivers/tty/serial/samsung.c
+++ b/drivers/tty/serial/samsung.c
@@ -528,11 +528,15 @@ static void s3c24xx_serial_pm(struct uart_port *port, unsigned int level,
 			      unsigned int old)
 {
 	struct s3c24xx_uart_port *ourport = to_ourport(port);
+	int timeout = 10000;
 
 	ourport->pm_level = level;
 
 	switch (level) {
 	case 3:
+		while (--timeout && !s3c24xx_serial_txempty_nofifo(port))
+			udelay(100);
+
 		if (!IS_ERR(ourport->baudclk) && ourport->baudclk != NULL)
 			clk_disable(ourport->baudclk);
 
diff --git a/drivers/usb/class/cdc-acm.c b/drivers/usb/class/cdc-acm.c
index 8f4a628..0532577 100644
--- a/drivers/usb/class/cdc-acm.c
+++ b/drivers/usb/class/cdc-acm.c
@@ -1108,10 +1108,11 @@ static int acm_probe(struct usb_interface *intf,
 	} else {
 		control_interface = usb_ifnum_to_if(usb_dev, union_header->bMasterInterface0);
 		data_interface = usb_ifnum_to_if(usb_dev, (data_interface_num = union_header->bSlaveInterface0));
-		if (!control_interface || !data_interface) {
-			dev_dbg(&intf->dev, "no interfaces\n");
-			return -ENODEV;
-		}
+	}
+
+	if (!control_interface || !data_interface) {
+		dev_dbg(&intf->dev, "no interfaces\n");
+		return -ENODEV;
 	}
 
 	if (data_interface_num != call_interface_num)
@@ -1429,6 +1430,7 @@ static void acm_disconnect(struct usb_interface *intf)
 				&dev_attr_wCountryCodes);
 		device_remove_file(&acm->control->dev,
 				&dev_attr_iCountryCodeRelDate);
+		kfree(acm->country_codes);
 	}
 	device_remove_file(&acm->control->dev, &dev_attr_bmCapabilities);
 	usb_set_intfdata(acm->control, NULL);
diff --git a/drivers/usb/core/config.c b/drivers/usb/core/config.c
index 6ed7e7c..cc1004a 100644
--- a/drivers/usb/core/config.c
+++ b/drivers/usb/core/config.c
@@ -201,6 +201,17 @@ static int usb_parse_endpoint(struct device *ddev, int cfgno, int inum,
 			if (n == 0)
 				n = 9;	/* 32 ms = 2^(9-1) uframes */
 			j = 16;
+
+			/*
+			 * Adjust bInterval for quirked devices.
+			 * This quirk fixes bIntervals reported in
+			 * linear microframes.
+			 */
+			if (to_usb_device(ddev)->quirks &
+				USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL) {
+				n = clamp(fls(d->bInterval), i, j);
+				i = j = n;
+			}
 			break;
 		default:		/* USB_SPEED_FULL or _LOW */
 			/* For low-speed, 10 ms is the official minimum.
diff --git a/drivers/usb/core/quirks.c b/drivers/usb/core/quirks.c
index d482141..95f60d0 100644
--- a/drivers/usb/core/quirks.c
+++ b/drivers/usb/core/quirks.c
@@ -38,6 +38,9 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* Creative SB Audigy 2 NX */
 	{ USB_DEVICE(0x041e, 0x3020), .driver_info = USB_QUIRK_RESET_RESUME },
 
+	/* Microsoft Wireless Laser Mouse 6000 Receiver */
+	{ USB_DEVICE(0x045e, 0x00e1), .driver_info = USB_QUIRK_RESET_RESUME },
+
 	/* Microsoft LifeCam-VX700 v2.0 */
 	{ USB_DEVICE(0x045e, 0x0770), .driver_info = USB_QUIRK_RESET_RESUME },
 
@@ -174,6 +177,10 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* SKYMEDI USB_DRIVE */
 	{ USB_DEVICE(0x1516, 0x8628), .driver_info = USB_QUIRK_RESET_RESUME },
 
+	/* Razer - Razer Blade Keyboard */
+	{ USB_DEVICE(0x1532, 0x0116), .driver_info =
+			USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL },
+
 	/* BUILDWIN Photo Frame */
 	{ USB_DEVICE(0x1908, 0x1315), .driver_info =
 			USB_QUIRK_HONOR_BNUMINTERFACES },
@@ -184,6 +191,10 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* Protocol and OTG Electrical Test Device */
 	{ USB_DEVICE(0x1a0a, 0x0200), .driver_info = USB_QUIRK_OTG_PET },
 
+	/* Protocol and OTG Electrical Test Device */
+	{ USB_DEVICE(0x1a0a, 0x0200), .driver_info =
+			USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL },
+
 	{ }  /* terminating entry must be last */
 };
 
diff --git a/drivers/usb/host/pci-quirks.c b/drivers/usb/host/pci-quirks.c
index 90dcf54..1f230ed 100644
--- a/drivers/usb/host/pci-quirks.c
+++ b/drivers/usb/host/pci-quirks.c
@@ -470,7 +470,8 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 {
 	void __iomem *base;
 	u32 control;
-	u32 fminterval;
+	u32 fminterval = 0;
+	bool no_fminterval = false;
 	int cnt;
 
 	if (!mmio_resource_enabled(pdev, 0))
@@ -480,6 +481,13 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	if (base == NULL)
 		return;
 
+	/*
+	 * ULi M5237 OHCI controller locks the whole system when accessing
+	 * the OHCI_FMINTERVAL offset.
+	 */
+	if (pdev->vendor == PCI_VENDOR_ID_AL && pdev->device == 0x5237)
+		no_fminterval = true;
+
 	control = readl(base + OHCI_CONTROL);
 
 /* On PA-RISC, PDC can leave IR set incorrectly; ignore it there. */
@@ -518,7 +526,9 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	}
 
 	/* software reset of the controller, preserving HcFmInterval */
-	fminterval = readl(base + OHCI_FMINTERVAL);
+	if (!no_fminterval)
+		fminterval = readl(base + OHCI_FMINTERVAL);
+
 	writel(OHCI_HCR, base + OHCI_CMDSTATUS);
 
 	/* reset requires max 10 us delay */
@@ -527,7 +537,9 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 			break;
 		udelay(1);
 	}
-	writel(fminterval, base + OHCI_FMINTERVAL);
+
+	if (!no_fminterval)
+		writel(fminterval, base + OHCI_FMINTERVAL);
 
 	/* Now the controller is safely in SUSPEND and nothing can wake it up */
 	iounmap(base);
diff --git a/drivers/usb/host/xhci-pci.c b/drivers/usb/host/xhci-pci.c
index 0e1f1f0..7d1a99d 100644
--- a/drivers/usb/host/xhci-pci.c
+++ b/drivers/usb/host/xhci-pci.c
@@ -222,7 +222,7 @@ static int xhci_pci_suspend(struct usb_hcd *hcd, bool do_wakeup)
 			xhci->shared_hcd->state != HC_STATE_SUSPENDED)
 		return -EINVAL;
 
-	retval = xhci_suspend(xhci);
+	retval = xhci_suspend(xhci, do_wakeup);
 
 	return retval;
 }
diff --git a/drivers/usb/host/xhci-ring.c b/drivers/usb/host/xhci-ring.c
index 5cdb965..7a10a49 100644
--- a/drivers/usb/host/xhci-ring.c
+++ b/drivers/usb/host/xhci-ring.c
@@ -1182,9 +1182,8 @@ static void handle_reset_ep_completion(struct xhci_hcd *xhci,
 				false);
 		xhci_ring_cmd_db(xhci);
 	} else {
-		/* Clear our internal halted state and restart the ring(s) */
+		/* Clear our internal halted state */
 		xhci->devs[slot_id]->eps[ep_index].ep_state &= ~EP_HALTED;
-		ring_doorbell_for_active_rings(xhci, slot_id, ep_index);
 	}
 }
 
@@ -1922,23 +1921,12 @@ static int finish_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		ep->stopped_trb = event_trb;
 		return 0;
 	} else {
-		if (trb_comp_code == COMP_STALL) {
-			/* The transfer is completed from the driver's
-			 * perspective, but we need to issue a set dequeue
-			 * command for this stalled endpoint to move the dequeue
-			 * pointer past the TD.  We can't do that here because
-			 * the halt condition must be cleared first.  Let the
-			 * USB class driver clear the stall later.
-			 */
-			ep->stopped_td = td;
-			ep->stopped_trb = event_trb;
-			ep->stopped_stream = ep_ring->stream_id;
-		} else if (xhci_requires_manual_halt_cleanup(xhci,
-					ep_ctx, trb_comp_code)) {
-			/* Other types of errors halt the endpoint, but the
-			 * class driver doesn't call usb_reset_endpoint() unless
-			 * the error is -EPIPE.  Clear the halted status in the
-			 * xHCI hardware manually.
+		if (trb_comp_code == COMP_STALL ||
+		    xhci_requires_manual_halt_cleanup(xhci, ep_ctx,
+						      trb_comp_code)) {
+			/* Issue a reset endpoint command to clear the host side			 * halt, followed by a set dequeue command to move the
+			 * dequeue pointer past the TD.
+			 * The class driver clears the device side halt later.
 			 */
 			xhci_cleanup_halted_endpoint(xhci,
 					slot_id, ep_index, ep_ring->stream_id,
@@ -2058,9 +2046,7 @@ static int process_ctrl_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		else
 			td->urb->actual_length = 0;
 
-		xhci_cleanup_halted_endpoint(xhci,
-			slot_id, ep_index, 0, td, event_trb);
-		return finish_td(xhci, td, event_trb, event, ep, status, true);
+		return finish_td(xhci, td, event_trb, event, ep, status, false);
 	}
 	/*
 	 * Did we transfer any data, despite the errors that might have
@@ -2612,17 +2598,8 @@ static int handle_tx_event(struct xhci_hcd *xhci,
 		if (ret) {
 			urb = td->urb;
 			urb_priv = urb->hcpriv;
-			/* Leave the TD around for the reset endpoint function
-			 * to use(but only if it's not a control endpoint,
-			 * since we already queued the Set TR dequeue pointer
-			 * command for stalled control endpoints).
-			 */
-			if (usb_endpoint_xfer_control(&urb->ep->desc) ||
-				(trb_comp_code != COMP_STALL &&
-					trb_comp_code != COMP_BABBLE))
-				xhci_urb_free_priv(xhci, urb_priv);
-			else
-				kfree(urb_priv);
+
+			xhci_urb_free_priv(xhci, urb_priv);
 
 			usb_hcd_unlink_urb_from_ep(bus_to_hcd(urb->dev->bus), urb);
 			if ((urb->actual_length != urb->transfer_buffer_length &&
diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index 1bef534..b20962d 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -33,6 +33,8 @@
 #define DRIVER_AUTHOR "Sarah Sharp"
 #define DRIVER_DESC "'eXtensible' Host Controller (xHC) Driver"
 
+#define	PORT_WAKE_BITS	(PORT_WKOC_E | PORT_WKDISC_E | PORT_WKCONN_E)
+
 /* Some 0.95 hardware can't handle the chain bit on a Link TRB being cleared */
 static int link_quirk;
 module_param(link_quirk, int, S_IRUGO | S_IWUSR);
@@ -887,18 +889,56 @@ static void xhci_clear_command_ring(struct xhci_hcd *xhci)
 	xhci_set_cmd_ring_deq(xhci);
 }
 
+static void xhci_disable_port_wake_on_bits(struct xhci_hcd *xhci)
+{
+	int port_index;
+	__le32 __iomem **port_array;
+	unsigned long flags;
+	u32 t1, t2;
+
+	spin_lock_irqsave(&xhci->lock, flags);
+
+	/* disble usb3 ports Wake bits*/
+	port_index = xhci->num_usb3_ports;
+	port_array = xhci->usb3_ports;
+	while (port_index--) {
+		t1 = readl(port_array[port_index]);
+		t1 = xhci_port_state_to_neutral(t1);
+		t2 = t1 & ~PORT_WAKE_BITS;
+		if (t1 != t2)
+			writel(t2, port_array[port_index]);
+	}
+
+	/* disble usb2 ports Wake bits*/
+	port_index = xhci->num_usb2_ports;
+	port_array = xhci->usb2_ports;
+	while (port_index--) {
+		t1 = readl(port_array[port_index]);
+		t1 = xhci_port_state_to_neutral(t1);
+		t2 = t1 & ~PORT_WAKE_BITS;
+		if (t1 != t2)
+			writel(t2, port_array[port_index]);
+	}
+
+	spin_unlock_irqrestore(&xhci->lock, flags);
+}
+
 /*
  * Stop HC (not bus-specific)
  *
  * This is called when the machine transition into S3/S4 mode.
  *
  */
-int xhci_suspend(struct xhci_hcd *xhci)
+int xhci_suspend(struct xhci_hcd *xhci, bool do_wakeup)
 {
 	int			rc = 0;
 	struct usb_hcd		*hcd = xhci_to_hcd(xhci);
 	u32			command;
 
+	/* Clear root port wake on bits if wakeup not allowed. */
+	if (!do_wakeup)
+		xhci_disable_port_wake_on_bits(xhci);
+
 	/* Don't poll the roothubs on bus suspend. */
 	xhci_dbg(xhci, "%s: stopping port polling.\n", __func__);
 	clear_bit(HCD_FLAG_POLL_RH, &hcd->flags);
@@ -2851,61 +2891,31 @@ void xhci_cleanup_stalled_ring(struct xhci_hcd *xhci,
 	}
 }
 
-/* Deal with stalled endpoints.  The core should have sent the control message
- * to clear the halt condition.  However, we need to make the xHCI hardware
- * reset its sequence number, since a device will expect a sequence number of
- * zero after the halt condition is cleared.
+/* Called when clearing halted device. The core should have sent the control
+ * message to clear the device halt condition. The host side of the halt should
+ * already be cleared with a reset endpoint command issued when the STALL tx
+ * event was received.
+ *
  * Context: in_interrupt
  */
+
 void xhci_endpoint_reset(struct usb_hcd *hcd,
 		struct usb_host_endpoint *ep)
 {
 	struct xhci_hcd *xhci;
-	struct usb_device *udev;
-	unsigned int ep_index;
-	unsigned long flags;
-	int ret;
-	struct xhci_virt_ep *virt_ep;
 
 	xhci = hcd_to_xhci(hcd);
-	udev = (struct usb_device *) ep->hcpriv;
-	/* Called with a root hub endpoint (or an endpoint that wasn't added
-	 * with xhci_add_endpoint()
-	 */
-	if (!ep->hcpriv)
-		return;
-	ep_index = xhci_get_endpoint_index(&ep->desc);
-	virt_ep = &xhci->devs[udev->slot_id]->eps[ep_index];
-	if (!virt_ep->stopped_td) {
-		xhci_dbg(xhci, "Endpoint 0x%x not halted, refusing to reset.\n",
-				ep->desc.bEndpointAddress);
-		return;
-	}
-	if (usb_endpoint_xfer_control(&ep->desc)) {
-		xhci_dbg(xhci, "Control endpoint stall already handled.\n");
-		return;
-	}
-
-	xhci_dbg(xhci, "Queueing reset endpoint command\n");
-	spin_lock_irqsave(&xhci->lock, flags);
-	ret = xhci_queue_reset_ep(xhci, udev->slot_id, ep_index);
 	/*
-	 * Can't change the ring dequeue pointer until it's transitioned to the
-	 * stopped state, which is only upon a successful reset endpoint
-	 * command.  Better hope that last command worked!
+	 * We might need to implement the config ep cmd in xhci 4.8.1 note:
+	 * The Reset Endpoint Command may only be issued to endpoints in the
+	 * Halted state. If software wishes reset the Data Toggle or Sequence
+	 * Number of an endpoint that isn't in the Halted state, then software
+	 * may issue a Configure Endpoint Command with the Drop and Add bits set
+	 * for the target endpoint. that is in the Stopped state.
 	 */
-	if (!ret) {
-		xhci_cleanup_stalled_ring(xhci, udev, ep_index);
-		kfree(virt_ep->stopped_td);
-		xhci_ring_cmd_db(xhci);
-	}
-	virt_ep->stopped_td = NULL;
-	virt_ep->stopped_trb = NULL;
-	virt_ep->stopped_stream = 0;
-	spin_unlock_irqrestore(&xhci->lock, flags);
-
-	if (ret)
-		xhci_warn(xhci, "FIXME allocate a new ring segment\n");
+	/* For now just print debug to follow the situation */
+	xhci_dbg(xhci, "Endpoint 0x%x ep reset callback called\n",
+		 ep->desc.bEndpointAddress);
 }
 
 static int xhci_check_streams_endpoint(struct xhci_hcd *xhci,
diff --git a/drivers/usb/host/xhci.h b/drivers/usb/host/xhci.h
index d643c1a..16cc569 100644
--- a/drivers/usb/host/xhci.h
+++ b/drivers/usb/host/xhci.h
@@ -1755,7 +1755,7 @@ void xhci_shutdown(struct usb_hcd *hcd);
 int xhci_gen_setup(struct usb_hcd *hcd, xhci_get_quirks_t get_quirks);
 
 #ifdef	CONFIG_PM
-int xhci_suspend(struct xhci_hcd *xhci);
+int xhci_suspend(struct xhci_hcd *xhci, bool do_wakeup);
 int xhci_resume(struct xhci_hcd *xhci, bool hibernated);
 #else
 #define	xhci_suspend	NULL
diff --git a/drivers/usb/renesas_usbhs/mod_gadget.c b/drivers/usb/renesas_usbhs/mod_gadget.c
index 00bd2a5..056dc6e 100644
--- a/drivers/usb/renesas_usbhs/mod_gadget.c
+++ b/drivers/usb/renesas_usbhs/mod_gadget.c
@@ -672,6 +672,9 @@ static int __usbhsg_ep_set_halt_wedge(struct usb_ep *ep, int halt, int wedge)
 	struct device *dev = usbhsg_gpriv_to_dev(gpriv);
 	unsigned long flags;
 
+	if (!pipe)
+		return -EINVAL;
+
 	usbhsg_pipe_disable(uep);
 
 	dev_dbg(dev, "set halt %d (pipe %d)\n",
diff --git a/drivers/usb/serial/console.c b/drivers/usb/serial/console.c
index 1ee6b2a..87302dd 100644
--- a/drivers/usb/serial/console.c
+++ b/drivers/usb/serial/console.c
@@ -47,6 +47,8 @@ static struct console usbcons;
  * ------------------------------------------------------------
  */
 
+static const struct tty_operations usb_console_fake_tty_ops = {
+};
 
 /*
  * The parsing of the command line works exactly like the
@@ -141,14 +143,17 @@ static int usb_console_setup(struct console *co, char *options)
 				goto reset_open_count;
 			}
 			kref_init(&tty->kref);
-			tty_port_tty_set(&port->port, tty);
 			tty->driver = usb_serial_tty_driver;
 			tty->index = co->index;
+			INIT_LIST_HEAD(&tty->tty_files);
+			kref_get(&tty->driver->kref);
+			tty->ops = &usb_console_fake_tty_ops;
 			if (tty_init_termios(tty)) {
 				retval = -ENOMEM;
 				err("no more memory");
-				goto free_tty;
+				goto put_tty;
 			}
+			tty_port_tty_set(&port->port, tty);
 		}
 
 		/* only call the device specific open if this
@@ -170,7 +175,7 @@ static int usb_console_setup(struct console *co, char *options)
 			serial->type->set_termios(tty, port, &dummy);
 
 			tty_port_tty_set(&port->port, NULL);
-			kfree(tty);
+			tty_kref_put(tty);
 		}
 		set_bit(ASYNCB_INITIALIZED, &port->port.flags);
 	}
@@ -186,8 +191,8 @@ static int usb_console_setup(struct console *co, char *options)
 
  fail:
 	tty_port_tty_set(&port->port, NULL);
- free_tty:
-	kfree(tty);
+ put_tty:
+	tty_kref_put(tty);
  reset_open_count:
 	port->port.count = 0;
 	usb_autopm_put_interface(serial->interface);
diff --git a/drivers/usb/serial/cp210x.c b/drivers/usb/serial/cp210x.c
index 19074db..8137937 100644
--- a/drivers/usb/serial/cp210x.c
+++ b/drivers/usb/serial/cp210x.c
@@ -126,9 +126,12 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(0x10C4, 0x85F8) }, /* Virtenio Preon32 */
 	{ USB_DEVICE(0x10C4, 0x8664) }, /* AC-Services CAN-IF */
 	{ USB_DEVICE(0x10C4, 0x8665) }, /* AC-Services OBD-IF */
+	{ USB_DEVICE(0x10C4, 0x8856) },	/* CEL EM357 ZigBee USB Stick - LR */
+	{ USB_DEVICE(0x10C4, 0x8857) },	/* CEL EM357 ZigBee USB Stick */
 	{ USB_DEVICE(0x10C4, 0x88A4) }, /* MMB Networks ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x88A5) }, /* Planet Innovation Ingeni ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x8946) }, /* Ketra N1 Wireless Interface */
+	{ USB_DEVICE(0x10C4, 0x8977) },	/* CEL MeshWorks DevKit Device */
 	{ USB_DEVICE(0x10C4, 0xEA60) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA61) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA70) }, /* Silicon Labs factory default */
diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index a89433b..4bfcfa7 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -494,6 +494,39 @@ static struct usb_device_id id_table_combined [] = {
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FD_PID) },
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FE_PID) },
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FF_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_4701_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9300_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9301_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9302_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9303_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9304_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9305_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9306_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9307_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9308_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9309_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930A_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930B_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930C_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930D_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930E_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930F_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9310_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9311_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9312_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9313_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9314_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9315_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9316_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9317_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9318_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9319_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931A_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931B_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931C_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931D_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931E_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931F_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_PERLE_ULTRAPORT_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_PIEGROUP_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_TNC_X_PID) },
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index 64ee791..ecb4dee 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -920,8 +920,8 @@
 #define BAYER_CONTOUR_CABLE_PID        0x6001
 
 /*
- * The following are the values for the Matrix Orbital FTDI Range
- * Anything in this range will use an FT232RL.
+ * Matrix Orbital Intelligent USB displays.
+ * http://www.matrixorbital.com
  */
 #define MTXORB_VID			0x1B3D
 #define MTXORB_FTDI_RANGE_0100_PID	0x0100
@@ -1180,8 +1180,39 @@
 #define MTXORB_FTDI_RANGE_01FD_PID	0x01FD
 #define MTXORB_FTDI_RANGE_01FE_PID	0x01FE
 #define MTXORB_FTDI_RANGE_01FF_PID	0x01FF
-
-
+#define MTXORB_FTDI_RANGE_4701_PID	0x4701
+#define MTXORB_FTDI_RANGE_9300_PID	0x9300
+#define MTXORB_FTDI_RANGE_9301_PID	0x9301
+#define MTXORB_FTDI_RANGE_9302_PID	0x9302
+#define MTXORB_FTDI_RANGE_9303_PID	0x9303
+#define MTXORB_FTDI_RANGE_9304_PID	0x9304
+#define MTXORB_FTDI_RANGE_9305_PID	0x9305
+#define MTXORB_FTDI_RANGE_9306_PID	0x9306
+#define MTXORB_FTDI_RANGE_9307_PID	0x9307
+#define MTXORB_FTDI_RANGE_9308_PID	0x9308
+#define MTXORB_FTDI_RANGE_9309_PID	0x9309
+#define MTXORB_FTDI_RANGE_930A_PID	0x930A
+#define MTXORB_FTDI_RANGE_930B_PID	0x930B
+#define MTXORB_FTDI_RANGE_930C_PID	0x930C
+#define MTXORB_FTDI_RANGE_930D_PID	0x930D
+#define MTXORB_FTDI_RANGE_930E_PID	0x930E
+#define MTXORB_FTDI_RANGE_930F_PID	0x930F
+#define MTXORB_FTDI_RANGE_9310_PID	0x9310
+#define MTXORB_FTDI_RANGE_9311_PID	0x9311
+#define MTXORB_FTDI_RANGE_9312_PID	0x9312
+#define MTXORB_FTDI_RANGE_9313_PID	0x9313
+#define MTXORB_FTDI_RANGE_9314_PID	0x9314
+#define MTXORB_FTDI_RANGE_9315_PID	0x9315
+#define MTXORB_FTDI_RANGE_9316_PID	0x9316
+#define MTXORB_FTDI_RANGE_9317_PID	0x9317
+#define MTXORB_FTDI_RANGE_9318_PID	0x9318
+#define MTXORB_FTDI_RANGE_9319_PID	0x9319
+#define MTXORB_FTDI_RANGE_931A_PID	0x931A
+#define MTXORB_FTDI_RANGE_931B_PID	0x931B
+#define MTXORB_FTDI_RANGE_931C_PID	0x931C
+#define MTXORB_FTDI_RANGE_931D_PID	0x931D
+#define MTXORB_FTDI_RANGE_931E_PID	0x931E
+#define MTXORB_FTDI_RANGE_931F_PID	0x931F
 
 /*
  * The Mobility Lab (TML)
diff --git a/drivers/usb/serial/keyspan.c b/drivers/usb/serial/keyspan.c
index 66d806e..0879ac7 100644
--- a/drivers/usb/serial/keyspan.c
+++ b/drivers/usb/serial/keyspan.c
@@ -323,24 +323,28 @@ static void	usa26_indat_callback(struct urb *urb)
 		if ((data[0] & 0x80) == 0) {
 			/* no errors on individual bytes, only
 			   possible overrun err */
-			if (data[0] & RXERROR_OVERRUN)
-				err = TTY_OVERRUN;
-			else
-				err = 0;
+			if (data[0] & RXERROR_OVERRUN) {
+				tty_insert_flip_char(tty, 0, TTY_OVERRUN);
+			}
 			for (i = 1; i < urb->actual_length ; ++i)
-				tty_insert_flip_char(tty, data[i], err);
+				tty_insert_flip_char(tty, data[i], TTY_NORMAL);
 		} else {
 			/* some bytes had errors, every byte has status */
 			dbg("%s - RX error!!!!", __func__);
 			for (i = 0; i + 1 < urb->actual_length; i += 2) {
-				int stat = data[i], flag = 0;
-				if (stat & RXERROR_OVERRUN)
-					flag |= TTY_OVERRUN;
-				if (stat & RXERROR_FRAMING)
-					flag |= TTY_FRAME;
-				if (stat & RXERROR_PARITY)
-					flag |= TTY_PARITY;
+				int stat = data[i];
+				int flag = TTY_NORMAL;
+
+				if (stat & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				/* XXX should handle break (0x10) */
+				if (stat & RXERROR_PARITY)
+					flag = TTY_PARITY;
+				else if (stat & RXERROR_FRAMING)
+					flag = TTY_FRAME;
+
 				tty_insert_flip_char(tty, data[i+1], flag);
 			}
 		}
@@ -712,14 +716,19 @@ static void	usa49_indat_callback(struct urb *urb)
 		} else {
 			/* some bytes had errors, every byte has status */
 			for (i = 0; i + 1 < urb->actual_length; i += 2) {
-				int stat = data[i], flag = 0;
-				if (stat & RXERROR_OVERRUN)
-					flag |= TTY_OVERRUN;
-				if (stat & RXERROR_FRAMING)
-					flag |= TTY_FRAME;
-				if (stat & RXERROR_PARITY)
-					flag |= TTY_PARITY;
+				int stat = data[i];
+				int flag = TTY_NORMAL;
+
+				if (stat & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				/* XXX should handle break (0x10) */
+				if (stat & RXERROR_PARITY)
+					flag = TTY_PARITY;
+				else if (stat & RXERROR_FRAMING)
+					flag = TTY_FRAME;
+
 				tty_insert_flip_char(tty, data[i+1], flag);
 			}
 		}
@@ -779,14 +788,19 @@ static void usa49wg_indat_callback(struct urb *urb)
 				 * some bytes had errors, every byte has status
 				 */
 				for (x = 0; x + 1 < len; x += 2) {
-					int stat = data[i], flag = 0;
-					if (stat & RXERROR_OVERRUN)
-						flag |= TTY_OVERRUN;
-					if (stat & RXERROR_FRAMING)
-						flag |= TTY_FRAME;
-					if (stat & RXERROR_PARITY)
-						flag |= TTY_PARITY;
+					int stat = data[i];
+					int flag = TTY_NORMAL;
+
+					if (stat & RXERROR_OVERRUN) {
+						tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+					}
 					/* XXX should handle break (0x10) */
+					if (stat & RXERROR_PARITY)
+						flag = TTY_PARITY;
+					else if (stat & RXERROR_FRAMING)
+						flag = TTY_FRAME;
+
 					tty_insert_flip_char(tty,
 							data[i+1], flag);
 					i += 2;
@@ -844,25 +858,32 @@ static void usa90_indat_callback(struct urb *urb)
 			if ((data[0] & 0x80) == 0) {
 				/* no errors on individual bytes, only
 				   possible overrun err*/
-				if (data[0] & RXERROR_OVERRUN)
-					err = TTY_OVERRUN;
-				else
-					err = 0;
+				if (data[0] & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				for (i = 1; i < urb->actual_length ; ++i)
 					tty_insert_flip_char(tty, data[i],
-									err);
+								TTY_NORMAL);
 			}  else {
 			/* some bytes had errors, every byte has status */
 				dbg("%s - RX error!!!!", __func__);
 				for (i = 0; i + 1 < urb->actual_length; i += 2) {
-					int stat = data[i], flag = 0;
-					if (stat & RXERROR_OVERRUN)
-						flag |= TTY_OVERRUN;
-					if (stat & RXERROR_FRAMING)
-						flag |= TTY_FRAME;
-					if (stat & RXERROR_PARITY)
-						flag |= TTY_PARITY;
+					int stat = data[i];
+					int flag = TTY_NORMAL;
+
+					if (stat & RXERROR_OVERRUN) {
+						tty_insert_flip_char(
+								tty, 0,
+								TTY_OVERRUN);
+					}
+
 					/* XXX should handle break (0x10) */
+					if (stat & RXERROR_PARITY)
+						flag = TTY_PARITY;
+					else if (stat & RXERROR_FRAMING)
+						flag = TTY_FRAME;
+
 					tty_insert_flip_char(tty, data[i+1],
 									flag);
 				}
diff --git a/drivers/usb/serial/ssu100.c b/drivers/usb/serial/ssu100.c
index d19fa6a..f425507 100644
--- a/drivers/usb/serial/ssu100.c
+++ b/drivers/usb/serial/ssu100.c
@@ -598,10 +598,10 @@ static void ssu100_update_lsr(struct usb_serial_port *port, u8 lsr,
 			if (*tty_flag == TTY_NORMAL)
 				*tty_flag = TTY_FRAME;
 		}
-		if (lsr & UART_LSR_OE){
+		if (lsr & UART_LSR_OE) {
 			priv->icount.overrun++;
-			if (*tty_flag == TTY_NORMAL)
-				*tty_flag = TTY_OVERRUN;
+			tty_insert_flip_char(tty_port_tty_get(&port->port),
+					0, TTY_OVERRUN);
 		}
 	}
 
@@ -622,11 +622,8 @@ static int ssu100_process_packet(struct urb *urb,
 	if ((len >= 4) &&
 	    (packet[0] == 0x1b) && (packet[1] == 0x1b) &&
 	    ((packet[2] == 0x00) || (packet[2] == 0x01))) {
-		if (packet[2] == 0x00) {
+		if (packet[2] == 0x00)
 			ssu100_update_lsr(port, packet[3], &flag);
-			if (flag == TTY_OVERRUN)
-				tty_insert_flip_char(tty, 0, TTY_OVERRUN);
-		}
 		if (packet[2] == 0x01)
 			ssu100_update_msr(port, packet[3]);
 
diff --git a/drivers/usb/storage/scsiglue.c b/drivers/usb/storage/scsiglue.c
index a4f033b..b987c53 100644
--- a/drivers/usb/storage/scsiglue.c
+++ b/drivers/usb/storage/scsiglue.c
@@ -247,6 +247,10 @@ static int slave_configure(struct scsi_device *sdev)
 			sdev->use_rpm_auto = 1;
 			sdev->autosuspend_delay = us->sdev_autosuspend_delay;
 		}
+		
+		/* A few buggy USB-ATA bridges don't understand FUA */
+		if (us->fflags & US_FL_BROKEN_FUA)
+			sdev->broken_fua = 1;
 	} else {
 
 		/* Non-disk-type devices don't need to blacklist any pages
diff --git a/drivers/usb/storage/unusual_devs.h b/drivers/usb/storage/unusual_devs.h
index a280945..25174be 100644
--- a/drivers/usb/storage/unusual_devs.h
+++ b/drivers/usb/storage/unusual_devs.h
@@ -1940,6 +1940,13 @@ UNUSUAL_DEV(  0x14cd, 0x6600, 0x0201, 0x0201,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_IGNORE_RESIDUE ),
 
+/* Reported by Michael Büsch <m@bues.ch> */
+UNUSUAL_DEV(  0x152d, 0x0567, 0x0114, 0x0114,
+		"JMicron",
+		"USB to ATA/ATAPI Bridge",
+		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
+		US_FL_BROKEN_FUA ),
+
 /* Reported by Alexandre Oliva <oliva@lsd.ic.unicamp.br>
  * JMicron responds to USN and several other SCSI ioctls with a
  * residue that causes subsequent I/O requests to fail.  */
@@ -1949,6 +1956,13 @@ UNUSUAL_DEV(  0x152d, 0x2329, 0x0100, 0x0100,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_IGNORE_RESIDUE | US_FL_SANE_SENSE ),
 
+/* Reported by Dmitry Nezhevenko <dion@dion.org.ua> */
+UNUSUAL_DEV(  0x152d, 0x2566, 0x0114, 0x0114,
+		"JMicron",
+		"USB to ATA/ATAPI Bridge",
+		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
+		US_FL_BROKEN_FUA ),
+
 /* Entrega Technologies U1-SC25 (later Xircom PortGear PGSCSI)
  * and Mac USB Dock USB-SCSI */
 UNUSUAL_DEV(  0x1645, 0x0007, 0x0100, 0x0133,
diff --git a/drivers/video/logo/logo.c b/drivers/video/logo/logo.c
index 080c35b..cc5dbb5 100644
--- a/drivers/video/logo/logo.c
+++ b/drivers/video/logo/logo.c
@@ -25,6 +25,21 @@ static bool nologo;
 module_param(nologo, bool, 0);
 MODULE_PARM_DESC(nologo, "Disables startup logo");
 
+/*
+ * Logos are located in the initdata, and will be freed in kernel_init.
+ * Use late_init to mark the logos as freed to prevent any further use.
+ */
+
+static bool logos_freed;
+
+static int __init fb_logo_late_init(void)
+{
+	logos_freed = true;
+	return 0;
+}
+
+late_initcall(fb_logo_late_init);
+
 /* logo's are marked __initdata. Use __init_refok to tell
  * modpost that it is intended that this function uses data
  * marked __initdata.
@@ -33,7 +48,7 @@ const struct linux_logo * __init_refok fb_find_logo(int depth)
 {
 	const struct linux_logo *logo = NULL;
 
-	if (nologo)
+	if (nologo || logos_freed)
 		return NULL;
 
 	if (depth >= 1) {
diff --git a/drivers/virtio/virtio.c b/drivers/virtio/virtio.c
index 984c501..cc02a9b 100644
--- a/drivers/virtio/virtio.c
+++ b/drivers/virtio/virtio.c
@@ -9,33 +9,32 @@ static unsigned int dev_index;
 static ssize_t device_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%04x\n", dev->id.device);
 }
 static ssize_t vendor_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%04x\n", dev->id.vendor);
 }
 static ssize_t status_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%08x\n", dev->config->get_status(dev));
 }
 static ssize_t modalias_show(struct device *_d,
 			     struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
-
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "virtio:d%08Xv%08X\n",
 		       dev->id.device, dev->id.vendor);
 }
 static ssize_t features_show(struct device *_d,
 			     struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d, struct virtio_device, dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	unsigned int i;
 	ssize_t len = 0;
 
@@ -70,7 +69,7 @@ static inline int virtio_id_match(const struct virtio_device *dev,
 static int virtio_dev_match(struct device *_dv, struct device_driver *_dr)
 {
 	unsigned int i;
-	struct virtio_device *dev = container_of(_dv,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_dv);
 	const struct virtio_device_id *ids;
 
 	ids = container_of(_dr, struct virtio_driver, driver)->id_table;
@@ -82,7 +81,7 @@ static int virtio_dev_match(struct device *_dv, struct device_driver *_dr)
 
 static int virtio_uevent(struct device *_dv, struct kobj_uevent_env *env)
 {
-	struct virtio_device *dev = container_of(_dv,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_dv);
 
 	return add_uevent_var(env, "MODALIAS=virtio:d%08Xv%08X",
 			      dev->id.device, dev->id.vendor);
@@ -110,7 +109,7 @@ EXPORT_SYMBOL_GPL(virtio_check_driver_offered_feature);
 static int virtio_dev_probe(struct device *_d)
 {
 	int err, i;
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	struct virtio_driver *drv = container_of(dev->dev.driver,
 						 struct virtio_driver, driver);
 	u32 device_features;
@@ -148,7 +147,7 @@ static int virtio_dev_probe(struct device *_d)
 
 static int virtio_dev_remove(struct device *_d)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	struct virtio_driver *drv = container_of(dev->dev.driver,
 						 struct virtio_driver, driver);
 
diff --git a/drivers/virtio/virtio_pci.c b/drivers/virtio/virtio_pci.c
index a41f264..cc56763 100644
--- a/drivers/virtio/virtio_pci.c
+++ b/drivers/virtio/virtio_pci.c
@@ -624,11 +624,13 @@ static struct virtio_config_ops virtio_pci_config_ops = {
 
 static void virtio_pci_release_dev(struct device *_d)
 {
-	/*
-	 * No need for a release method as we allocate/free
-	 * all devices together with the pci devices.
-	 * Provide an empty one to avoid getting a warning from core.
-	 */
+	struct virtio_device *vdev = dev_to_virtio(_d);
+	struct virtio_pci_device *vp_dev = to_vp_device(vdev);
+
+	/* As struct device is a kobject, it's not safe to
+	 * free the memory (including the reference counter itself)
+	 * until it's release callback. */
+	kfree(vp_dev);
 }
 
 /* the PCI probing function */
@@ -716,7 +718,6 @@ static void __devexit virtio_pci_remove(struct pci_dev *pci_dev)
 	pci_iounmap(pci_dev, vp_dev->ioaddr);
 	pci_release_regions(pci_dev);
 	pci_disable_device(pci_dev);
-	kfree(vp_dev);
 }
 
 #ifdef CONFIG_PM
diff --git a/fs/binfmt_elf.c b/fs/binfmt_elf.c
index cb815f9..78f5082 100644
--- a/fs/binfmt_elf.c
+++ b/fs/binfmt_elf.c
@@ -539,11 +539,12 @@ static unsigned long load_elf_interp(struct elfhdr *interp_elf_ex,
 
 static unsigned long randomize_stack_top(unsigned long stack_top)
 {
-	unsigned int random_variable = 0;
+	unsigned long random_variable = 0;
 
 	if ((current->flags & PF_RANDOMIZE) &&
 		!(current->personality & ADDR_NO_RANDOMIZE)) {
-		random_variable = get_random_int() & STACK_RND_MASK;
+		random_variable = (unsigned long) get_random_int();
+		random_variable &= STACK_RND_MASK;
 		random_variable <<= PAGE_SHIFT;
 	}
 #ifdef CONFIG_STACK_GROWSUP
diff --git a/fs/btrfs/disk-io.c b/fs/btrfs/disk-io.c
index a7ffc88..7c23cd9 100644
--- a/fs/btrfs/disk-io.c
+++ b/fs/btrfs/disk-io.c
@@ -3556,12 +3556,6 @@ static int btrfs_destroy_pinned_extent(struct btrfs_root *root,
 		if (ret)
 			break;
 
-		/* opt_discard */
-		if (btrfs_test_opt(root, DISCARD))
-			ret = btrfs_error_discard_extent(root, start,
-							 end + 1 - start,
-							 NULL);
-
 		clear_extent_dirty(unpin, start, end, GFP_NOFS);
 		btrfs_error_unpin_extent_range(root, start, end);
 		cond_resched();
diff --git a/fs/btrfs/extent-tree.c b/fs/btrfs/extent-tree.c
index 224ce21..cf6e7f4 100644
--- a/fs/btrfs/extent-tree.c
+++ b/fs/btrfs/extent-tree.c
@@ -4892,7 +4892,8 @@ void btrfs_prepare_extent_commit(struct btrfs_trans_handle *trans,
 	update_global_block_rsv(fs_info);
 }
 
-static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
+static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end,
+			      const bool return_free_space)
 {
 	struct btrfs_fs_info *fs_info = root->fs_info;
 	struct btrfs_block_group_cache *cache = NULL;
@@ -4912,7 +4913,8 @@ static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
 
 		if (start < cache->last_byte_to_unpin) {
 			len = min(len, cache->last_byte_to_unpin - start);
-			btrfs_add_free_space(cache, start, len);
+			if (return_free_space)
+				btrfs_add_free_space(cache, start, len);
 		}
 
 		start += len;
@@ -4960,7 +4962,7 @@ int btrfs_finish_extent_commit(struct btrfs_trans_handle *trans,
 						   end + 1 - start, NULL);
 
 		clear_extent_dirty(unpin, start, end, GFP_NOFS);
-		unpin_extent_range(root, start, end);
+		unpin_extent_range(root, start, end, true);
 		cond_resched();
 	}
 
@@ -8008,7 +8010,7 @@ int btrfs_init_space_info(struct btrfs_fs_info *fs_info)
 
 int btrfs_error_unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
 {
-	return unpin_extent_range(root, start, end);
+	return unpin_extent_range(root, start, end, false);
 }
 
 int btrfs_error_discard_extent(struct btrfs_root *root, u64 bytenr,
diff --git a/fs/ecryptfs/file.c b/fs/ecryptfs/file.c
index d45ba45..f04aa33 100644
--- a/fs/ecryptfs/file.c
+++ b/fs/ecryptfs/file.c
@@ -195,24 +195,12 @@ static int ecryptfs_open(struct inode *inode, struct file *file)
 {
 	int rc = 0;
 	struct ecryptfs_crypt_stat *crypt_stat = NULL;
-	struct ecryptfs_mount_crypt_stat *mount_crypt_stat;
 	struct dentry *ecryptfs_dentry = file->f_path.dentry;
 	/* Private value of ecryptfs_dentry allocated in
 	 * ecryptfs_lookup() */
 	struct dentry *lower_dentry;
 	struct ecryptfs_file_info *file_info;
 
-	mount_crypt_stat = &ecryptfs_superblock_to_private(
-		ecryptfs_dentry->d_sb)->mount_crypt_stat;
-	if ((mount_crypt_stat->flags & ECRYPTFS_ENCRYPTED_VIEW_ENABLED)
-	    && ((file->f_flags & O_WRONLY) || (file->f_flags & O_RDWR)
-		|| (file->f_flags & O_CREAT) || (file->f_flags & O_TRUNC)
-		|| (file->f_flags & O_APPEND))) {
-		printk(KERN_WARNING "Mount has encrypted view enabled; "
-		       "files may only be read\n");
-		rc = -EPERM;
-		goto out;
-	}
 	/* Released in ecryptfs_release or end of function if failure */
 	file_info = kmem_cache_zalloc(ecryptfs_file_info_cache, GFP_KERNEL);
 	ecryptfs_set_file_private(file, file_info);
diff --git a/fs/ecryptfs/main.c b/fs/ecryptfs/main.c
index 240832e..93b7bec 100644
--- a/fs/ecryptfs/main.c
+++ b/fs/ecryptfs/main.c
@@ -494,6 +494,7 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 {
 	struct super_block *s;
 	struct ecryptfs_sb_info *sbi;
+	struct ecryptfs_mount_crypt_stat *mount_crypt_stat;
 	struct ecryptfs_dentry_info *root_info;
 	const char *err = "Getting sb failed";
 	struct inode *inode;
@@ -512,6 +513,7 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 		err = "Error parsing options";
 		goto out;
 	}
+	mount_crypt_stat = &sbi->mount_crypt_stat;
 
 	s = sget(fs_type, NULL, set_anon_super, NULL);
 	if (IS_ERR(s)) {
@@ -557,11 +559,19 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 
 	/**
 	 * Set the POSIX ACL flag based on whether they're enabled in the lower
-	 * mount. Force a read-only eCryptfs mount if the lower mount is ro.
-	 * Allow a ro eCryptfs mount even when the lower mount is rw.
+	 * mount.
 	 */
 	s->s_flags = flags & ~MS_POSIXACL;
-	s->s_flags |= path.dentry->d_sb->s_flags & (MS_RDONLY | MS_POSIXACL);
+	s->s_flags |= path.dentry->d_sb->s_flags & MS_POSIXACL;
+
+	/**
+	 * Force a read-only eCryptfs mount when:
+	 *   1) The lower mount is ro
+	 *   2) The ecryptfs_encrypted_view mount option is specified
+	 */
+	if (path.dentry->d_sb->s_flags & MS_RDONLY ||
+	    mount_crypt_stat->flags & ECRYPTFS_ENCRYPTED_VIEW_ENABLED)
+		s->s_flags |= MS_RDONLY;
 
 	s->s_maxbytes = path.dentry->d_sb->s_maxbytes;
 	s->s_blocksize = path.dentry->d_sb->s_blocksize;
diff --git a/fs/fs-writeback.c b/fs/fs-writeback.c
index 5f0d26b..5189ad1 100644
--- a/fs/fs-writeback.c
+++ b/fs/fs-writeback.c
@@ -403,7 +403,6 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 
 	/* Set I_SYNC, reset I_DIRTY_PAGES */
 	inode->i_state |= I_SYNC;
-	inode->i_state &= ~I_DIRTY_PAGES;
 	spin_unlock(&inode->i_lock);
 	spin_unlock(&wb->list_lock);
 
@@ -428,9 +427,28 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 	 * write_inode()
 	 */
 	spin_lock(&inode->i_lock);
+
 	dirty = inode->i_state & I_DIRTY;
-	inode->i_state &= ~(I_DIRTY_SYNC | I_DIRTY_DATASYNC);
+	inode->i_state &= ~I_DIRTY;
+
+	/*
+	 * Paired with smp_mb() in __mark_inode_dirty().  This allows
+	 * __mark_inode_dirty() to test i_state without grabbing i_lock -
+	 * either they see the I_DIRTY bits cleared or we see the dirtied
+	 * inode.
+	 *
+	 * I_DIRTY_PAGES is always cleared together above even if @mapping
+	 * still has dirty pages.  The flag is reinstated after smp_mb() if
+	 * necessary.  This guarantees that either __mark_inode_dirty()
+	 * sees clear I_DIRTY_PAGES or we see PAGECACHE_TAG_DIRTY.
+	 */
+	smp_mb();
+
+	if (mapping_tagged(mapping, PAGECACHE_TAG_DIRTY))
+		inode->i_state |= I_DIRTY_PAGES;
+
 	spin_unlock(&inode->i_lock);
+
 	/* Don't write the inode if only I_DIRTY_PAGES was set */
 	if (dirty & (I_DIRTY_SYNC | I_DIRTY_DATASYNC)) {
 		int err = write_inode(inode, wbc);
@@ -456,7 +474,6 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 			 * We didn't write back all the pages.  nfs_writepages()
 			 * sometimes bales out without doing anything.
 			 */
-			inode->i_state |= I_DIRTY_PAGES;
 			if (wbc->nr_to_write <= 0) {
 				/*
 				 * slice used up: queue for next turn
@@ -1074,12 +1091,11 @@ void __mark_inode_dirty(struct inode *inode, int flags)
 	}
 
 	/*
-	 * make sure that changes are seen by all cpus before we test i_state
-	 * -- mikulas
+	 * Paired with smp_mb() in __writeback_single_inode() for the
+	 * following lockless i_state test.  See there for details.
 	 */
 	smp_mb();
 
-	/* avoid the locking if we can */
 	if ((inode->i_state & flags) == flags)
 		return;
 
diff --git a/fs/isofs/rock.c b/fs/isofs/rock.c
index ee62cc0..1780949 100644
--- a/fs/isofs/rock.c
+++ b/fs/isofs/rock.c
@@ -30,6 +30,7 @@ struct rock_state {
 	int cont_size;
 	int cont_extent;
 	int cont_offset;
+	int cont_loops;
 	struct inode *inode;
 };
 
@@ -73,6 +74,9 @@ static void init_rock_state(struct rock_state *rs, struct inode *inode)
 	rs->inode = inode;
 }
 
+/* Maximum number of Rock Ridge continuation entries */
+#define RR_MAX_CE_ENTRIES 32
+
 /*
  * Returns 0 if the caller should continue scanning, 1 if the scan must end
  * and -ve on error.
@@ -105,6 +109,8 @@ static int rock_continue(struct rock_state *rs)
 			goto out;
 		}
 		ret = -EIO;
+		if (++rs->cont_loops >= RR_MAX_CE_ENTRIES)
+			goto out;
 		bh = sb_bread(rs->inode->i_sb, rs->cont_extent);
 		if (bh) {
 			memcpy(rs->buffer, bh->b_data + rs->cont_offset,
@@ -356,6 +362,9 @@ parse_rock_ridge_inode_internal(struct iso_directory_record *de,
 			rs.cont_size = isonum_733(rr->u.CE.size);
 			break;
 		case SIG('E', 'R'):
+			/* Invalid length of ER tag id? */
+			if (rr->u.ER.len_id + offsetof(struct rock_ridge, u.ER.data) > rr->len)
+				goto out;
 			ISOFS_SB(inode->i_sb)->s_rock = 1;
 			printk(KERN_DEBUG "ISO 9660 Extensions: ");
 			{
diff --git a/fs/jfs/jfs_dtree.c b/fs/jfs/jfs_dtree.c
index b6f17c0..33c8624 100644
--- a/fs/jfs/jfs_dtree.c
+++ b/fs/jfs/jfs_dtree.c
@@ -3103,7 +3103,7 @@ int jfs_readdir(struct file *filp, void *dirent, filldir_t filldir)
 				 * self "."
 				 */
 				filp->f_pos = 1;
-				if (filldir(dirent, ".", 1, 0, ip->i_ino,
+				if (filldir(dirent, ".", 1, 1, ip->i_ino,
 					    DT_DIR))
 					return 0;
 			}
@@ -3111,7 +3111,7 @@ int jfs_readdir(struct file *filp, void *dirent, filldir_t filldir)
 			 * parent ".."
 			 */
 			filp->f_pos = 2;
-			if (filldir(dirent, "..", 2, 1, PARENT(ip), DT_DIR))
+			if (filldir(dirent, "..", 2, 2, PARENT(ip), DT_DIR))
 				return 0;
 
 			/*
diff --git a/fs/ncpfs/ioctl.c b/fs/ncpfs/ioctl.c
index 6958adf..0a76def 100644
--- a/fs/ncpfs/ioctl.c
+++ b/fs/ncpfs/ioctl.c
@@ -445,7 +445,6 @@ static long __ncp_ioctl(struct inode *inode, unsigned int cmd, unsigned long arg
 						result = -EIO;
 					}
 				}
-				result = 0;
 			}
 			mutex_unlock(&server->root_setup_lock);
 
diff --git a/fs/nfsd/nfs4callback.c b/fs/nfsd/nfs4callback.c
index c8e9f63..ebf3f59 100644
--- a/fs/nfsd/nfs4callback.c
+++ b/fs/nfsd/nfs4callback.c
@@ -784,8 +784,12 @@ static bool nfsd41_cb_get_slot(struct nfs4_client *clp, struct rpc_task *task)
 {
 	if (test_and_set_bit(0, &clp->cl_cb_slot_busy) != 0) {
 		rpc_sleep_on(&clp->cl_cb_waitq, task, NULL);
-		dprintk("%s slot is busy\n", __func__);
-		return false;
+		/* Race breaker */
+		if (test_and_set_bit(0, &clp->cl_cb_slot_busy) != 0) {
+			dprintk("%s slot is busy\n", __func__);
+			return false;
+		}
+		rpc_wake_up_queued_task(&clp->cl_cb_waitq, task);
 	}
 	return true;
 }
diff --git a/fs/nilfs2/nilfs.h b/fs/nilfs2/nilfs.h
index 250add8..161a10c 100644
--- a/fs/nilfs2/nilfs.h
+++ b/fs/nilfs2/nilfs.h
@@ -128,7 +128,6 @@ enum {
  * @ti_save: Backup of journal_info field of task_struct
  * @ti_flags: Flags
  * @ti_count: Nest level
- * @ti_garbage:	List of inode to be put when releasing semaphore
  */
 struct nilfs_transaction_info {
 	u32			ti_magic;
@@ -137,7 +136,6 @@ struct nilfs_transaction_info {
 				   one of other filesystems has a bug. */
 	unsigned short		ti_flags;
 	unsigned short		ti_count;
-	struct list_head	ti_garbage;
 };
 
 /* ti_magic */
diff --git a/fs/nilfs2/segment.c b/fs/nilfs2/segment.c
index e0a5a18..7bb866c 100644
--- a/fs/nilfs2/segment.c
+++ b/fs/nilfs2/segment.c
@@ -302,7 +302,6 @@ static void nilfs_transaction_lock(struct super_block *sb,
 	ti->ti_count = 0;
 	ti->ti_save = cur_ti;
 	ti->ti_magic = NILFS_TI_MAGIC;
-	INIT_LIST_HEAD(&ti->ti_garbage);
 	current->journal_info = ti;
 
 	for (;;) {
@@ -329,8 +328,6 @@ static void nilfs_transaction_unlock(struct super_block *sb)
 
 	up_write(&nilfs->ns_segctor_sem);
 	current->journal_info = ti->ti_save;
-	if (!list_empty(&ti->ti_garbage))
-		nilfs_dispose_list(nilfs, &ti->ti_garbage, 0);
 }
 
 static void *nilfs_segctor_map_segsum_entry(struct nilfs_sc_info *sci,
@@ -743,6 +740,15 @@ static void nilfs_dispose_list(struct the_nilfs *nilfs,
 	}
 }
 
+static void nilfs_iput_work_func(struct work_struct *work)
+{
+	struct nilfs_sc_info *sci = container_of(work, struct nilfs_sc_info,
+						 sc_iput_work);
+	struct the_nilfs *nilfs = sci->sc_super->s_fs_info;
+
+	nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 0);
+}
+
 static int nilfs_test_metadata_dirty(struct the_nilfs *nilfs,
 				     struct nilfs_root *root)
 {
@@ -1896,8 +1902,9 @@ static int nilfs_segctor_collect_dirty_files(struct nilfs_sc_info *sci,
 static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 					     struct the_nilfs *nilfs)
 {
-	struct nilfs_transaction_info *ti = current->journal_info;
 	struct nilfs_inode_info *ii, *n;
+	int during_mount = !(sci->sc_super->s_flags & MS_ACTIVE);
+	int defer_iput = false;
 
 	spin_lock(&nilfs->ns_inode_lock);
 	list_for_each_entry_safe(ii, n, &sci->sc_dirty_files, i_dirty) {
@@ -1908,9 +1915,24 @@ static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 		clear_bit(NILFS_I_BUSY, &ii->i_state);
 		brelse(ii->i_bh);
 		ii->i_bh = NULL;
-		list_move_tail(&ii->i_dirty, &ti->ti_garbage);
+		list_del_init(&ii->i_dirty);
+		if (!ii->vfs_inode.i_nlink || during_mount) {
+			/*
+			 * Defer calling iput() to avoid deadlocks if
+			 * i_nlink == 0 or mount is not yet finished.
+			 */
+			list_add_tail(&ii->i_dirty, &sci->sc_iput_queue);
+			defer_iput = true;
+		} else {
+			spin_unlock(&nilfs->ns_inode_lock);
+			iput(&ii->vfs_inode);
+			spin_lock(&nilfs->ns_inode_lock);
+		}
 	}
 	spin_unlock(&nilfs->ns_inode_lock);
+
+	if (defer_iput)
+		schedule_work(&sci->sc_iput_work);
 }
 
 /*
@@ -2577,6 +2599,8 @@ static struct nilfs_sc_info *nilfs_segctor_new(struct super_block *sb,
 	INIT_LIST_HEAD(&sci->sc_segbufs);
 	INIT_LIST_HEAD(&sci->sc_write_logs);
 	INIT_LIST_HEAD(&sci->sc_gc_inodes);
+	INIT_LIST_HEAD(&sci->sc_iput_queue);
+	INIT_WORK(&sci->sc_iput_work, nilfs_iput_work_func);
 	init_timer(&sci->sc_timer);
 
 	sci->sc_interval = HZ * NILFS_SC_DEFAULT_TIMEOUT;
@@ -2603,6 +2627,8 @@ static void nilfs_segctor_write_out(struct nilfs_sc_info *sci)
 		ret = nilfs_segctor_construct(sci, SC_LSEG_SR);
 		nilfs_transaction_unlock(sci->sc_super);
 
+		flush_work(&sci->sc_iput_work);
+
 	} while (ret && retrycount-- > 0);
 }
 
@@ -2627,6 +2653,9 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		|| sci->sc_seq_request != sci->sc_seq_done);
 	spin_unlock(&sci->sc_state_lock);
 
+	if (flush_work(&sci->sc_iput_work))
+		flag = true;
+
 	if (flag || !nilfs_segctor_confirm(sci))
 		nilfs_segctor_write_out(sci);
 
@@ -2636,6 +2665,12 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		nilfs_dispose_list(nilfs, &sci->sc_dirty_files, 1);
 	}
 
+	if (!list_empty(&sci->sc_iput_queue)) {
+		nilfs_warning(sci->sc_super, __func__,
+			      "iput queue is not empty\n");
+		nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 1);
+	}
+
 	WARN_ON(!list_empty(&sci->sc_segbufs));
 	WARN_ON(!list_empty(&sci->sc_write_logs));
 
diff --git a/fs/nilfs2/segment.h b/fs/nilfs2/segment.h
index 38a1d00..a48d6de 100644
--- a/fs/nilfs2/segment.h
+++ b/fs/nilfs2/segment.h
@@ -26,6 +26,7 @@
 #include <linux/types.h>
 #include <linux/fs.h>
 #include <linux/buffer_head.h>
+#include <linux/workqueue.h>
 #include <linux/nilfs2_fs.h>
 #include "nilfs.h"
 
@@ -92,6 +93,8 @@ struct nilfs_segsum_pointer {
  * @sc_nblk_inc: Block count of current generation
  * @sc_dirty_files: List of files to be written
  * @sc_gc_inodes: List of GC inodes having blocks to be written
+ * @sc_iput_queue: list of inodes for which iput should be done
+ * @sc_iput_work: work struct to defer iput call
  * @sc_freesegs: array of segment numbers to be freed
  * @sc_nfreesegs: number of segments on @sc_freesegs
  * @sc_dsync_inode: inode whose data pages are written for a sync operation
@@ -135,6 +138,8 @@ struct nilfs_sc_info {
 
 	struct list_head	sc_dirty_files;
 	struct list_head	sc_gc_inodes;
+	struct list_head	sc_iput_queue;
+	struct work_struct	sc_iput_work;
 
 	__u64		       *sc_freesegs;
 	size_t			sc_nfreesegs;
diff --git a/fs/notify/inode_mark.c b/fs/notify/inode_mark.c
index b13c00a..df6dacc 100644
--- a/fs/notify/inode_mark.c
+++ b/fs/notify/inode_mark.c
@@ -282,20 +282,25 @@ void fsnotify_unmount_inodes(struct list_head *list)
 		spin_unlock(&inode->i_lock);
 
 		/* In case the dropping of a reference would nuke next_i. */
-		if ((&next_i->i_sb_list != list) &&
-		    atomic_read(&next_i->i_count)) {
+		while (&next_i->i_sb_list != list) {
 			spin_lock(&next_i->i_lock);
-			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE))) {
+			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE)) &&
+						atomic_read(&next_i->i_count)) {
 				__iget(next_i);
 				need_iput = next_i;
+				spin_unlock(&next_i->i_lock);
+				break;
 			}
 			spin_unlock(&next_i->i_lock);
+			next_i = list_entry(next_i->i_sb_list.next,
+						struct inode, i_sb_list);
 		}
 
 		/*
-		 * We can safely drop inode_sb_list_lock here because we hold
-		 * references on both inode and next_i.  Also no new inodes
-		 * will be added since the umount has begun.
+		 * We can safely drop inode_sb_list_lock here because either
+		 * we actually hold references on both inode and next_i or
+		 * end of list.  Also no new inodes will be added since the
+		 * umount has begun.
 		 */
 		spin_unlock(&inode_sb_list_lock);
 
diff --git a/fs/ocfs2/aops.c b/fs/ocfs2/aops.c
index 340bd02..e9829ca 100644
--- a/fs/ocfs2/aops.c
+++ b/fs/ocfs2/aops.c
@@ -917,7 +917,7 @@ void ocfs2_unlock_and_free_pages(struct page **pages, int num_pages)
 	}
 }
 
-static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+static void ocfs2_unlock_pages(struct ocfs2_write_ctxt *wc)
 {
 	int i;
 
@@ -938,7 +938,11 @@ static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
 		page_cache_release(wc->w_target_page);
 	}
 	ocfs2_unlock_and_free_pages(wc->w_pages, wc->w_num_pages);
+}
 
+static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+{
+	ocfs2_unlock_pages(wc);
 	brelse(wc->w_di_bh);
 	kfree(wc);
 }
@@ -2059,11 +2063,19 @@ int ocfs2_write_end_nolock(struct address_space *mapping,
 	di->i_mtime_nsec = di->i_ctime_nsec = cpu_to_le32(inode->i_mtime.tv_nsec);
 	ocfs2_journal_dirty(handle, wc->w_di_bh);
 
+	/* unlock pages before dealloc since it needs acquiring j_trans_barrier
+	 * lock, or it will cause a deadlock since journal commit threads holds
+	 * this lock and will ask for the page lock when flushing the data.
+	 * put it here to preserve the unlock order.
+	 */
+	ocfs2_unlock_pages(wc);
+
 	ocfs2_commit_trans(osb, handle);
 
 	ocfs2_run_deallocs(osb, &wc->w_dealloc);
 
-	ocfs2_free_write_ctxt(wc);
+	brelse(wc->w_di_bh);
+	kfree(wc);
 
 	return copied;
 }
diff --git a/fs/proc/stat.c b/fs/proc/stat.c
index a1ca9bc..95f2e25 100644
--- a/fs/proc/stat.c
+++ b/fs/proc/stat.c
@@ -159,7 +159,7 @@ static int show_stat(struct seq_file *p, void *v)
 
 	/* sum again ? it could be updated? */
 	for_each_irq_nr(j)
-		seq_put_decimal_ull(p, ' ', kstat_irqs(j));
+		seq_put_decimal_ull(p, ' ', kstat_irqs_usr(j));
 
 	seq_printf(p,
 		"\nctxt %llu\n"
diff --git a/fs/proc/task_mmu.c b/fs/proc/task_mmu.c
index e4e423a..324eb57 100644
--- a/fs/proc/task_mmu.c
+++ b/fs/proc/task_mmu.c
@@ -1054,9 +1054,19 @@ static ssize_t pagemap_read(struct file *file, char __user *buf,
 	return ret;
 }
 
+static int pagemap_open(struct inode *inode, struct file *file)
+{
+	/* do not disclose physical addresses to unprivileged
+	   userspace (closes a rowhammer attack vector) */
+	if (!capable(CAP_SYS_ADMIN))
+		return -EPERM;
+	return 0;
+}
+
 const struct file_operations proc_pagemap_operations = {
 	.llseek		= mem_lseek, /* borrow this */
 	.read		= pagemap_read,
+	.open		= pagemap_open,
 };
 #endif /* CONFIG_PROC_PAGE_MONITOR */
 
diff --git a/fs/udf/dir.c b/fs/udf/dir.c
index eb8bfe2..56341af 100644
--- a/fs/udf/dir.c
+++ b/fs/udf/dir.c
@@ -163,7 +163,8 @@ static int do_udf_readdir(struct inode *dir, struct file *filp,
 			struct kernel_lb_addr tloc = lelb_to_cpu(cfi.icb.extLocation);
 
 			iblock = udf_get_lb_pblock(dir->i_sb, &tloc, 0);
-			flen = udf_get_filename(dir->i_sb, nameptr, fname, lfi);
+			flen = udf_get_filename(dir->i_sb, nameptr, lfi, fname,
+						UDF_NAME_LEN);
 			dt_type = DT_UNKNOWN;
 		}
 
diff --git a/fs/udf/inode.c b/fs/udf/inode.c
index aa70035..8053ee7 100644
--- a/fs/udf/inode.c
+++ b/fs/udf/inode.c
@@ -1392,6 +1392,20 @@ static void udf_fill_inode(struct inode *inode, struct buffer_head *bh)
 							iinfo->i_lenEAttr;
 	}
 
+	/* Sanity checks for files in ICB so that we don't get confused later */
+	if (iinfo->i_alloc_type == ICBTAG_FLAG_AD_IN_ICB) {
+		/*
+		 * For file in ICB data is stored in allocation descriptor
+		 * so sizes should match
+		 */
+		if (iinfo->i_lenAlloc != inode->i_size)
+			return;
+		/* File in ICB has to fit in there... */
+		if (inode->i_size > inode->i_sb->s_blocksize -
+					udf_file_entry_alloc_offset(inode))
+			return;
+	}
+
 	switch (fe->icbTag.fileType) {
 	case ICBTAG_FILE_TYPE_DIRECTORY:
 		inode->i_op = &udf_dir_inode_operations;
diff --git a/fs/udf/namei.c b/fs/udf/namei.c
index 78bff11..407c129 100644
--- a/fs/udf/namei.c
+++ b/fs/udf/namei.c
@@ -233,7 +233,8 @@ static struct fileIdentDesc *udf_find_entry(struct inode *dir,
 		if (!lfi)
 			continue;
 
-		flen = udf_get_filename(dir->i_sb, nameptr, fname, lfi);
+		flen = udf_get_filename(dir->i_sb, nameptr, lfi, fname,
+					UDF_NAME_LEN);
 		if (flen && udf_match(flen, fname, child->len, child->name))
 			goto out_ok;
 	}
diff --git a/fs/udf/symlink.c b/fs/udf/symlink.c
index d7c6dbe..0422b7b 100644
--- a/fs/udf/symlink.c
+++ b/fs/udf/symlink.c
@@ -30,49 +30,73 @@
 #include <linux/buffer_head.h>
 #include "udf_i.h"
 
-static void udf_pc_to_char(struct super_block *sb, unsigned char *from,
-			   int fromlen, unsigned char *to)
+static int udf_pc_to_char(struct super_block *sb, unsigned char *from,
+			  int fromlen, unsigned char *to, int tolen)
 {
 	struct pathComponent *pc;
 	int elen = 0;
+	int comp_len;
 	unsigned char *p = to;
 
+	/* Reserve one byte for terminating \0 */
+	tolen--;
 	while (elen < fromlen) {
 		pc = (struct pathComponent *)(from + elen);
+		elen += sizeof(struct pathComponent);
 		switch (pc->componentType) {
 		case 1:
 			/*
 			 * Symlink points to some place which should be agreed
  			 * upon between originator and receiver of the media. Ignore.
 			 */
-			if (pc->lengthComponentIdent > 0)
+			if (pc->lengthComponentIdent > 0) {
+				elen += pc->lengthComponentIdent;
 				break;
+			}
 			/* Fall through */
 		case 2:
+			if (tolen == 0)
+				return -ENAMETOOLONG;
 			p = to;
 			*p++ = '/';
+			tolen--;
 			break;
 		case 3:
+			if (tolen < 3)
+				return -ENAMETOOLONG;
 			memcpy(p, "../", 3);
 			p += 3;
+			tolen -= 3;
 			break;
 		case 4:
+			if (tolen < 2)
+				return -ENAMETOOLONG;
 			memcpy(p, "./", 2);
 			p += 2;
+			tolen -= 2;
 			/* that would be . - just ignore */
 			break;
 		case 5:
-			p += udf_get_filename(sb, pc->componentIdent, p,
-					      pc->lengthComponentIdent);
+			elen += pc->lengthComponentIdent;
+			if (elen > fromlen)
+				return -EIO;
+			comp_len = udf_get_filename(sb, pc->componentIdent,
+						    pc->lengthComponentIdent,
+						    p, tolen);
+			p += comp_len;
+			tolen -= comp_len;
+			if (tolen == 0)
+				return -ENAMETOOLONG;
 			*p++ = '/';
+			tolen--;
 			break;
 		}
-		elen += sizeof(struct pathComponent) + pc->lengthComponentIdent;
 	}
 	if (p > to + 1)
 		p[-1] = '\0';
 	else
 		p[0] = '\0';
+	return 0;
 }
 
 static int udf_symlink_filler(struct file *file, struct page *page)
@@ -80,11 +104,17 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	struct inode *inode = page->mapping->host;
 	struct buffer_head *bh = NULL;
 	unsigned char *symlink;
-	int err = -EIO;
+	int err;
 	unsigned char *p = kmap(page);
 	struct udf_inode_info *iinfo;
 	uint32_t pos;
 
+	/* We don't support symlinks longer than one block */
+	if (inode->i_size > inode->i_sb->s_blocksize) {
+		err = -ENAMETOOLONG;
+		goto out_unmap;
+	}
+
 	iinfo = UDF_I(inode);
 	pos = udf_block_map(inode, 0);
 
@@ -94,14 +124,18 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	} else {
 		bh = sb_bread(inode->i_sb, pos);
 
-		if (!bh)
-			goto out;
+		if (!bh) {
+			err = -EIO;
+			goto out_unlock_inode;
+		}
 
 		symlink = bh->b_data;
 	}
 
-	udf_pc_to_char(inode->i_sb, symlink, inode->i_size, p);
+	err = udf_pc_to_char(inode->i_sb, symlink, inode->i_size, p, PAGE_SIZE);
 	brelse(bh);
+	if (err)
+		goto out_unlock_inode;
 
 	up_read(&iinfo->i_data_sem);
 	SetPageUptodate(page);
@@ -109,9 +143,10 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	unlock_page(page);
 	return 0;
 
-out:
+out_unlock_inode:
 	up_read(&iinfo->i_data_sem);
 	SetPageError(page);
+out_unmap:
 	kunmap(page);
 	unlock_page(page);
 	return err;
diff --git a/fs/udf/udfdecl.h b/fs/udf/udfdecl.h
index ebe1031..375f648 100644
--- a/fs/udf/udfdecl.h
+++ b/fs/udf/udfdecl.h
@@ -207,7 +207,8 @@ udf_get_lb_pblock(struct super_block *sb, struct kernel_lb_addr *loc,
 }
 
 /* unicode.c */
-extern int udf_get_filename(struct super_block *, uint8_t *, uint8_t *, int);
+extern int udf_get_filename(struct super_block *, uint8_t *, int, uint8_t *,
+			    int);
 extern int udf_put_filename(struct super_block *, const uint8_t *, uint8_t *,
 			    int);
 extern int udf_build_ustr(struct ustr *, dstring *, int);
diff --git a/fs/udf/unicode.c b/fs/udf/unicode.c
index 44b815e..d29c06f 100644
--- a/fs/udf/unicode.c
+++ b/fs/udf/unicode.c
@@ -28,7 +28,8 @@
 
 #include "udf_sb.h"
 
-static int udf_translate_to_linux(uint8_t *, uint8_t *, int, uint8_t *, int);
+static int udf_translate_to_linux(uint8_t *, int, uint8_t *, int, uint8_t *,
+				  int);
 
 static int udf_char_to_ustr(struct ustr *dest, const uint8_t *src, int strlen)
 {
@@ -333,8 +334,8 @@ static int udf_NLStoCS0(struct nls_table *nls, dstring *ocu, struct ustr *uni,
 	return u_len + 1;
 }
 
-int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
-		     int flen)
+int udf_get_filename(struct super_block *sb, uint8_t *sname, int slen,
+		     uint8_t *dname, int dlen)
 {
 	struct ustr *filename, *unifilename;
 	int len = 0;
@@ -347,7 +348,7 @@ int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
 	if (!unifilename)
 		goto out1;
 
-	if (udf_build_ustr_exact(unifilename, sname, flen))
+	if (udf_build_ustr_exact(unifilename, sname, slen))
 		goto out2;
 
 	if (UDF_QUERY_FLAG(sb, UDF_FLAG_UTF8)) {
@@ -366,7 +367,8 @@ int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
 	} else
 		goto out2;
 
-	len = udf_translate_to_linux(dname, filename->u_name, filename->u_len,
+	len = udf_translate_to_linux(dname, dlen,
+				     filename->u_name, filename->u_len,
 				     unifilename->u_name, unifilename->u_len);
 out2:
 	kfree(unifilename);
@@ -403,10 +405,12 @@ int udf_put_filename(struct super_block *sb, const uint8_t *sname,
 #define EXT_MARK		'.'
 #define CRC_MARK		'#'
 #define EXT_SIZE 		5
+/* Number of chars we need to store generated CRC to make filename unique */
+#define CRC_LEN			5
 
-static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
-				  int udfLen, uint8_t *fidName,
-				  int fidNameLen)
+static int udf_translate_to_linux(uint8_t *newName, int newLen,
+				  uint8_t *udfName, int udfLen,
+				  uint8_t *fidName, int fidNameLen)
 {
 	int index, newIndex = 0, needsCRC = 0;
 	int extIndex = 0, newExtIndex = 0, hasExt = 0;
@@ -440,7 +444,7 @@ static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
 					newExtIndex = newIndex;
 				}
 			}
-			if (newIndex < 256)
+			if (newIndex < newLen)
 				newName[newIndex++] = curr;
 			else
 				needsCRC = 1;
@@ -468,13 +472,13 @@ static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
 				}
 				ext[localExtIndex++] = curr;
 			}
-			maxFilenameLen = 250 - localExtIndex;
+			maxFilenameLen = newLen - CRC_LEN - localExtIndex;
 			if (newIndex > maxFilenameLen)
 				newIndex = maxFilenameLen;
 			else
 				newIndex = newExtIndex;
-		} else if (newIndex > 250)
-			newIndex = 250;
+		} else if (newIndex > newLen - CRC_LEN)
+			newIndex = newLen - CRC_LEN;
 		newName[newIndex++] = CRC_MARK;
 		valueCRC = crc_itu_t(0, fidName, fidNameLen);
 		newName[newIndex++] = hexChar[(valueCRC & 0xf000) >> 12];
diff --git a/include/linux/device.h b/include/linux/device.h
index c297f25..5bf8909 100644
--- a/include/linux/device.h
+++ b/include/linux/device.h
@@ -849,6 +849,11 @@ extern __printf(5, 6)
 struct device *device_create(struct class *cls, struct device *parent,
 			     dev_t devt, void *drvdata,
 			     const char *fmt, ...);
+extern __printf(6, 7)
+struct device *device_create_with_groups(struct class *cls,
+			     struct device *parent, dev_t devt, void *drvdata,
+			     const struct attribute_group **groups,
+			     const char *fmt, ...);
 extern void device_destroy(struct class *cls, dev_t devt);
 
 /*
diff --git a/include/linux/kernel_stat.h b/include/linux/kernel_stat.h
index 2fbd905..8e62498 100644
--- a/include/linux/kernel_stat.h
+++ b/include/linux/kernel_stat.h
@@ -104,8 +104,13 @@ static inline unsigned int kstat_irqs(unsigned int irq)
 
 	return sum;
 }
+static inline unsigned int kstat_irqs_usr(unsigned int irq)
+{
+	return kstat_irqs(irq);
+}
 #else
 extern unsigned int kstat_irqs(unsigned int irq);
+extern unsigned int kstat_irqs_usr(unsigned int irq);
 #endif
 
 /*
diff --git a/include/linux/libata.h b/include/linux/libata.h
index dd16deb..764cd54 100644
--- a/include/linux/libata.h
+++ b/include/linux/libata.h
@@ -207,6 +207,7 @@ enum {
 	ATA_FLAG_SW_ACTIVITY	= (1 << 22), /* driver supports sw activity
 					      * led */
 	ATA_FLAG_NO_DIPM	= (1 << 23), /* host not happy with DIPM */
+	ATA_FLAG_LOWTAG		= (1 << 24), /* host wants lowest available tag */
 
 	/* bits 24:31 of ap->flags are reserved for LLD specific flags */
 
diff --git a/include/linux/mm.h b/include/linux/mm.h
index 337627e..076349e 100644
--- a/include/linux/mm.h
+++ b/include/linux/mm.h
@@ -869,6 +869,7 @@ static inline int page_mapped(struct page *page)
 #define VM_FAULT_WRITE	0x0008	/* Special case for get_user_pages */
 #define VM_FAULT_HWPOISON 0x0010	/* Hit poisoned small page */
 #define VM_FAULT_HWPOISON_LARGE 0x0020  /* Hit poisoned large page. Index encoded in upper bits */
+#define VM_FAULT_SIGSEGV 0x0040
 
 #define VM_FAULT_NOPAGE	0x0100	/* ->fault installed the pte, not return page */
 #define VM_FAULT_LOCKED	0x0200	/* ->fault locked the returned page */
@@ -876,8 +877,8 @@ static inline int page_mapped(struct page *page)
 
 #define VM_FAULT_HWPOISON_LARGE_MASK 0xf000 /* encodes hpage index for large hwpoison */
 
-#define VM_FAULT_ERROR	(VM_FAULT_OOM | VM_FAULT_SIGBUS | VM_FAULT_HWPOISON | \
-			 VM_FAULT_HWPOISON_LARGE)
+#define VM_FAULT_ERROR	(VM_FAULT_OOM | VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV | \
+			 VM_FAULT_HWPOISON | VM_FAULT_HWPOISON_LARGE)
 
 /* Encode hstate index for a hwpoisoned large page */
 #define VM_FAULT_SET_HINDEX(x) ((x) << 12)
@@ -1490,7 +1491,7 @@ extern int expand_downwards(struct vm_area_struct *vma,
 #if VM_GROWSUP
 extern int expand_upwards(struct vm_area_struct *vma, unsigned long address);
 #else
-  #define expand_upwards(vma, address) do { } while (0)
+  #define expand_upwards(vma, address) (0)
 #endif
 
 /* Look up the first VMA which satisfies  addr < vm_end,  NULL if none. */
diff --git a/include/linux/rmap.h b/include/linux/rmap.h
index a5ddc60..2f69ff4 100644
--- a/include/linux/rmap.h
+++ b/include/linux/rmap.h
@@ -37,6 +37,16 @@ struct anon_vma {
 	atomic_t refcount;
 
 	/*
+	 * Count of child anon_vmas and VMAs which points to this anon_vma.
+	 *
+	 * This counter is used for making decision about reusing anon_vma
+	 * instead of forking new one. See comments in function anon_vma_clone.
+	 */
+	unsigned degree;
+
+	struct anon_vma *parent;	/* Parent of this anon_vma */
+
+	/*
 	 * NOTE: the LSB of the head.next is set by
 	 * mm_take_all_locks() _after_ taking the above lock. So the
 	 * head must only be read/written after taking the above lock
diff --git a/include/linux/sysfs.h b/include/linux/sysfs.h
index 0010009..caf2e56 100644
--- a/include/linux/sysfs.h
+++ b/include/linux/sysfs.h
@@ -80,6 +80,15 @@ struct attribute_group {
 
 #define __ATTR_NULL { .attr = { .name = NULL } }
 
+#define ATTRIBUTE_GROUPS(name)					\
+static const struct attribute_group name##_group = {		\
+	.attrs = name##_attrs,					\
+};								\
+static const struct attribute_group *name##_groups[] = {	\
+	&name##_group,						\
+	NULL,							\
+}
+
 #define attr_name(_attr) (_attr).attr.name
 
 struct file;
diff --git a/include/linux/time.h b/include/linux/time.h
index 64ec8a1..6e7c65e 100644
--- a/include/linux/time.h
+++ b/include/linux/time.h
@@ -202,6 +202,19 @@ extern void getboottime(struct timespec *ts);
 extern void monotonic_to_bootbased(struct timespec *ts);
 extern void get_monotonic_boottime(struct timespec *ts);
 
+static inline bool timeval_valid(const struct timeval *tv)
+{
+	/* Dates before 1970 are bogus */
+	if (tv->tv_sec < 0)
+		return false;
+
+	/* Can't have more microseconds then a second */
+	if (tv->tv_usec < 0 || tv->tv_usec >= USEC_PER_SEC)
+		return false;
+
+	return true;
+}
+
 extern struct timespec timespec_trunc(struct timespec t, unsigned gran);
 extern int timekeeping_valid_for_hres(void);
 extern u64 timekeeping_max_deferment(void);
diff --git a/include/linux/usb/quirks.h b/include/linux/usb/quirks.h
index b1a7654..4bfff7a 100644
--- a/include/linux/usb/quirks.h
+++ b/include/linux/usb/quirks.h
@@ -35,4 +35,15 @@
 /* device can't handle device_qualifier descriptor requests */
 #define USB_QUIRK_DEVICE_QUALIFIER	0x00000100
 
+/*
+ * For high speed and super speed interupt endpoints, the USB 2.0 and
+ * USB 3.0 spec require the interval in microframes
+ * (1 microframe = 125 microseconds) to be calculated as
+ * interval = 2 ^ (bInterval-1).
+ *
+ * Devices with this quirk report their bInterval as the result of this
+ * calculation instead of the exponent variable used in the calculation.
+ */
+#define USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL	0x00000080
+
 #endif /* __LINUX_USB_QUIRKS_H */
diff --git a/include/linux/usb_usual.h b/include/linux/usb_usual.h
index 17df360..f2000e9 100644
--- a/include/linux/usb_usual.h
+++ b/include/linux/usb_usual.h
@@ -64,7 +64,9 @@
 	US_FLAG(NO_READ_CAPACITY_16,	0x00080000)		\
 		/* cannot handle READ_CAPACITY_16 */		\
 	US_FLAG(INITIAL_READ10,	0x00100000)			\
-		/* Initial READ(10) (and others) must be retried */
+		/* Initial READ(10) (and others) must be retried */	\
+	US_FLAG(BROKEN_FUA,	0x01000000)			\
+		/* Cannot handle FUA in WRITE or READ CDBs */	\
 
 #define US_FLAG(name, value)	US_FL_##name = value ,
 enum { US_DO_ALL_FLAGS };
diff --git a/include/linux/virtio.h b/include/linux/virtio.h
index c2814ab..eba97bf 100644
--- a/include/linux/virtio.h
+++ b/include/linux/virtio.h
@@ -280,7 +280,11 @@ struct virtio_device {
 	void *priv;
 };
 
-#define dev_to_virtio(dev) container_of(dev, struct virtio_device, dev)
+static inline struct virtio_device *dev_to_virtio(struct device *_dev)
+{
+	return container_of(_dev, struct virtio_device, dev);
+}
+
 int register_virtio_device(struct virtio_device *dev);
 void unregister_virtio_device(struct virtio_device *dev);
 
diff --git a/include/linux/writeback.h b/include/linux/writeback.h
index 57b3695..4c5950c 100644
--- a/include/linux/writeback.h
+++ b/include/linux/writeback.h
@@ -187,7 +187,6 @@ int write_cache_pages(struct address_space *mapping,
 		      struct writeback_control *wbc, writepage_t writepage,
 		      void *data);
 int do_writepages(struct address_space *mapping, struct writeback_control *wbc);
-void set_page_dirty_balance(struct page *page, int page_mkwrite);
 void writeback_set_ratelimit(void);
 void tag_pages_for_writeback(struct address_space *mapping,
 			     pgoff_t start, pgoff_t end);
diff --git a/include/net/sctp/sctp.h b/include/net/sctp/sctp.h
index a2ef814..43c8bbc 100644
--- a/include/net/sctp/sctp.h
+++ b/include/net/sctp/sctp.h
@@ -524,6 +524,11 @@ static inline void sctp_assoc_pending_pmtu(struct sctp_association *asoc)
 	asoc->pmtu_pending = 0;
 }
 
+static inline bool sctp_chunk_pending(const struct sctp_chunk *chunk)
+{
+	return !list_empty(&chunk->list);
+}
+
 /* Walk through a list of TLV parameters.  Don't trust the
  * individual parameter lengths and instead depend on
  * the chunk length to indicate when to stop.  Make sure
diff --git a/include/net/sctp/sm.h b/include/net/sctp/sm.h
index 9148632..4d1be75 100644
--- a/include/net/sctp/sm.h
+++ b/include/net/sctp/sm.h
@@ -251,9 +251,9 @@ struct sctp_chunk *sctp_make_asconf_update_ip(struct sctp_association *,
 					      int, __be16);
 struct sctp_chunk *sctp_make_asconf_set_prim(struct sctp_association *asoc,
 					     union sctp_addr *addr);
-int sctp_verify_asconf(const struct sctp_association *asoc,
-		       struct sctp_paramhdr *param_hdr, void *chunk_end,
-		       struct sctp_paramhdr **errp);
+bool sctp_verify_asconf(const struct sctp_association *asoc,
+			struct sctp_chunk *chunk, bool addr_param_needed,
+			struct sctp_paramhdr **errp);
 struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 				       struct sctp_chunk *asconf);
 int sctp_process_asconf_ack(struct sctp_association *asoc,
diff --git a/include/scsi/scsi_device.h b/include/scsi/scsi_device.h
index 0564655..ef54805 100644
--- a/include/scsi/scsi_device.h
+++ b/include/scsi/scsi_device.h
@@ -154,6 +154,7 @@ struct scsi_device {
 	unsigned try_rc_10_first:1;	/* Try READ_CAPACACITY_10 first */
 	unsigned is_visible:1;	/* is the device visible in sysfs */
 	unsigned use_rpm_auto:1; /* Enable runtime PM auto suspend */
+	unsigned broken_fua:1;		/* Don't set FUA bit */
 
 #define SCSI_DEFAULT_AUTOSUSPEND_DELAY  -1
 	int autosuspend_delay;
diff --git a/include/sound/ak4113.h b/include/sound/ak4113.h
index 2609048..3a34f6e 100644
--- a/include/sound/ak4113.h
+++ b/include/sound/ak4113.h
@@ -286,7 +286,7 @@ struct ak4113 {
 	ak4113_write_t *write;
 	ak4113_read_t *read;
 	void *private_data;
-	unsigned int init:1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[AK4113_WRITABLE_REGS];
 	struct snd_kcontrol *kctls[AK4113_CONTROLS];
diff --git a/include/sound/ak4114.h b/include/sound/ak4114.h
index 3ce69fd..6944116 100644
--- a/include/sound/ak4114.h
+++ b/include/sound/ak4114.h
@@ -168,7 +168,7 @@ struct ak4114 {
 	ak4114_write_t * write;
 	ak4114_read_t * read;
 	void * private_data;
-	unsigned int init: 1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[7];
 	unsigned char txcsb[5];
diff --git a/kernel/irq/internals.h b/kernel/irq/internals.h
index 001fa5b..8a160e8 100644
--- a/kernel/irq/internals.h
+++ b/kernel/irq/internals.h
@@ -74,6 +74,14 @@ extern void irq_percpu_disable(struct irq_desc *desc, unsigned int cpu);
 extern void mask_irq(struct irq_desc *desc);
 extern void unmask_irq(struct irq_desc *desc);
 
+#ifdef CONFIG_SPARSE_IRQ
+extern void irq_lock_sparse(void);
+extern void irq_unlock_sparse(void);
+#else
+static inline void irq_lock_sparse(void) { }
+static inline void irq_unlock_sparse(void) { }
+#endif
+
 extern void init_kstat_irqs(struct irq_desc *desc, int node, int nr);
 
 irqreturn_t handle_irq_event_percpu(struct irq_desc *desc, struct irqaction *action);
diff --git a/kernel/irq/irqdesc.c b/kernel/irq/irqdesc.c
index 8ab8e93..07d4551 100644
--- a/kernel/irq/irqdesc.c
+++ b/kernel/irq/irqdesc.c
@@ -131,6 +131,16 @@ static void free_masks(struct irq_desc *desc)
 static inline void free_masks(struct irq_desc *desc) { }
 #endif
 
+void irq_lock_sparse(void)
+{
+	mutex_lock(&sparse_irq_lock);
+}
+
+void irq_unlock_sparse(void)
+{
+	mutex_unlock(&sparse_irq_lock);
+}
+
 static struct irq_desc *alloc_desc(int irq, int node, struct module *owner)
 {
 	struct irq_desc *desc;
@@ -167,6 +177,12 @@ static void free_desc(unsigned int irq)
 
 	unregister_irq_proc(irq, desc);
 
+	/*
+	 * sparse_irq_lock protects also show_interrupts() and
+	 * kstat_irq_usr(). Once we deleted the descriptor from the
+	 * sparse tree we can free it. Access in proc will fail to
+	 * lookup the descriptor.
+	 */
 	mutex_lock(&sparse_irq_lock);
 	delete_irq_desc(irq);
 	mutex_unlock(&sparse_irq_lock);
@@ -489,6 +505,15 @@ void dynamic_irq_cleanup(unsigned int irq)
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
 }
 
+/**
+ * kstat_irqs_cpu - Get the statistics for an interrupt on a cpu
+ * @irq:	The interrupt number
+ * @cpu:	The cpu number
+ *
+ * Returns the sum of interrupt counts on @cpu since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -497,6 +522,14 @@ unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 			*per_cpu_ptr(desc->kstat_irqs, cpu) : 0;
 }
 
+/**
+ * kstat_irqs - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs(unsigned int irq)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -509,3 +542,22 @@ unsigned int kstat_irqs(unsigned int irq)
 		sum += *per_cpu_ptr(desc->kstat_irqs, cpu);
 	return sum;
 }
+
+/**
+ * kstat_irqs_usr - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. Contrary to kstat_irqs() this can be called from any
+ * preemptible context. It's protected against concurrent removal of
+ * an interrupt descriptor when sparse irqs are enabled.
+ */
+unsigned int kstat_irqs_usr(unsigned int irq)
+{
+	int sum;
+
+	irq_lock_sparse();
+	sum = kstat_irqs(irq);
+	irq_unlock_sparse();
+	return sum;
+}
diff --git a/kernel/irq/proc.c b/kernel/irq/proc.c
index 4bd4faa..fb655f5 100644
--- a/kernel/irq/proc.c
+++ b/kernel/irq/proc.c
@@ -15,6 +15,23 @@
 
 #include "internals.h"
 
+/*
+ * Access rules:
+ *
+ * procfs protects read/write of /proc/irq/N/ files against a
+ * concurrent free of the interrupt descriptor. remove_proc_entry()
+ * immediately prevents new read/writes to happen and waits for
+ * already running read/write functions to complete.
+ *
+ * We remove the proc entries first and then delete the interrupt
+ * descriptor from the radix tree and free it. So it is guaranteed
+ * that irq_to_desc(N) is valid as long as the read/writes are
+ * permitted by procfs.
+ *
+ * The read from /proc/interrupts is a different problem because there
+ * is no protection. So the lookup and the access to irqdesc
+ * information must be protected by sparse_irq_lock.
+ */
 static struct proc_dir_entry *root_irq_dir;
 
 #ifdef CONFIG_SMP
@@ -441,9 +458,10 @@ int show_interrupts(struct seq_file *p, void *v)
 		seq_putc(p, '\n');
 	}
 
+	irq_lock_sparse();
 	desc = irq_to_desc(i);
 	if (!desc)
-		return 0;
+		goto outsparse;
 
 	raw_spin_lock_irqsave(&desc->lock, flags);
 	for_each_online_cpu(j)
@@ -481,6 +499,8 @@ int show_interrupts(struct seq_file *p, void *v)
 	seq_putc(p, '\n');
 out:
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
+outsparse:
+	irq_unlock_sparse();
 	return 0;
 }
 #endif
diff --git a/kernel/sched/rt.c b/kernel/sched/rt.c
index c9fb92e..4ffa3bd 100644
--- a/kernel/sched/rt.c
+++ b/kernel/sched/rt.c
@@ -1293,7 +1293,12 @@ select_task_rq_rt(struct task_struct *p, int sd_flag, int flags)
 	    (p->rt.nr_cpus_allowed > 1)) {
 		int target = find_lowest_rq(p);
 
-		if (target != -1)
+		/*
+		 * Don't bother moving it if the destination CPU is
+		 * not running a lower priority task.
+		 */
+		if (target != -1 &&
+		    p->prio < cpu_rq(target)->rt.highest_prio.curr)
 			cpu = target;
 	}
 	rcu_read_unlock();
@@ -1579,6 +1584,16 @@ static struct rq *find_lock_lowest_rq(struct task_struct *task, struct rq *rq)
 
 		lowest_rq = cpu_rq(cpu);
 
+		if (lowest_rq->rt.highest_prio.curr <= task->prio) {
+			/*
+			 * Target rq has tasks of equal or higher priority,
+			 * retrying does not release any lock and is unlikely
+			 * to yield a different result.
+			 */
+			lowest_rq = NULL;
+			break;
+		}
+
 		/* if the prio of this runqueue changed, try again */
 		if (double_lock_balance(rq, lowest_rq)) {
 			/*
diff --git a/kernel/time.c b/kernel/time.c
index a095290..0864d70 100644
--- a/kernel/time.c
+++ b/kernel/time.c
@@ -186,6 +186,10 @@ SYSCALL_DEFINE2(settimeofday, struct timeval __user *, tv,
 	if (tv) {
 		if (copy_from_user(&user_tv, tv, sizeof(*tv)))
 			return -EFAULT;
+
+		if (!timeval_valid(&user_tv))
+			return -EINVAL;
+
 		new_ts.tv_sec = user_tv.tv_sec;
 		new_ts.tv_nsec = user_tv.tv_usec * NSEC_PER_USEC;
 	}
diff --git a/kernel/time/ntp.c b/kernel/time/ntp.c
index 8b70710..e32587e 100644
--- a/kernel/time/ntp.c
+++ b/kernel/time/ntp.c
@@ -660,6 +660,17 @@ int do_adjtimex(struct timex *txc)
 			return result;
 	}
 
+	/*
+	 * Check for potential multiplication overflows that can
+	 * only happen on 64-bit systems:
+	 */
+	if ((txc->modes & ADJ_FREQUENCY) && (BITS_PER_LONG == 64)) {
+		if (LLONG_MIN / PPM_SCALE > txc->freq)
+			return -EINVAL;
+		if (LLONG_MAX / PPM_SCALE < txc->freq)
+			return -EINVAL;
+	}
+
 	getnstimeofday(&ts);
 
 	spin_lock_irq(&ntp_lock);
diff --git a/lib/checksum.c b/lib/checksum.c
index 12dceb2..33f29f0 100644
--- a/lib/checksum.c
+++ b/lib/checksum.c
@@ -179,6 +179,15 @@ csum_partial_copy(const void *src, void *dst, int len, __wsum sum)
 EXPORT_SYMBOL(csum_partial_copy);
 
 #ifndef csum_tcpudp_nofold
+static inline u32 from64to32(u64 x)
+{
+	/* add up 32-bit and 32-bit for 32+c bit */
+	x = (x & 0xffffffff) + (x >> 32);
+	/* add up carry.. */
+	x = (x & 0xffffffff) + (x >> 32);
+	return (u32)x;
+}
+
 __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 			unsigned short len,
 			unsigned short proto,
@@ -193,8 +202,7 @@ __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 #else
 	s += (proto + len) << 8;
 #endif
-	s += (s >> 32);
-	return (__force __wsum)s;
+	return (__force __wsum)from64to32(s);
 }
 EXPORT_SYMBOL(csum_tcpudp_nofold);
 #endif
diff --git a/mm/ksm.c b/mm/ksm.c
index fca9dc5..f945af8 100644
--- a/mm/ksm.c
+++ b/mm/ksm.c
@@ -339,7 +339,7 @@ static int break_ksm(struct vm_area_struct *vma, unsigned long addr)
 		else
 			ret = VM_FAULT_WRITE;
 		put_page(page);
-	} while (!(ret & (VM_FAULT_WRITE | VM_FAULT_SIGBUS | VM_FAULT_OOM)));
+	} while (!(ret & (VM_FAULT_WRITE | VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV | VM_FAULT_OOM)));
 	/*
 	 * We must loop because handle_mm_fault() may back out if there's
 	 * any difficulty e.g. if pte accessed bit gets updated concurrently.
diff --git a/mm/memory.c b/mm/memory.c
index 6d5e635..0e4c5fe 100644
--- a/mm/memory.c
+++ b/mm/memory.c
@@ -852,20 +852,20 @@ copy_one_pte(struct mm_struct *dst_mm, struct mm_struct *src_mm,
 		if (!pte_file(pte)) {
 			swp_entry_t entry = pte_to_swp_entry(pte);
 
-			if (swap_duplicate(entry) < 0)
-				return entry.val;
-
-			/* make sure dst_mm is on swapoff's mmlist. */
-			if (unlikely(list_empty(&dst_mm->mmlist))) {
-				spin_lock(&mmlist_lock);
-				if (list_empty(&dst_mm->mmlist))
-					list_add(&dst_mm->mmlist,
-						 &src_mm->mmlist);
-				spin_unlock(&mmlist_lock);
-			}
-			if (likely(!non_swap_entry(entry)))
+			if (likely(!non_swap_entry(entry))) {
+				if (swap_duplicate(entry) < 0)
+					return entry.val;
+
+				/* make sure dst_mm is on swapoff's mmlist. */
+				if (unlikely(list_empty(&dst_mm->mmlist))) {
+					spin_lock(&mmlist_lock);
+					if (list_empty(&dst_mm->mmlist))
+						list_add(&dst_mm->mmlist,
+							 &src_mm->mmlist);
+					spin_unlock(&mmlist_lock);
+				}
 				rss[MM_SWAPENTS]++;
-			else if (is_migration_entry(entry)) {
+			} else if (is_migration_entry(entry)) {
 				page = migration_entry_to_page(entry);
 
 				if (PageAnon(page))
@@ -1805,7 +1805,7 @@ int __get_user_pages(struct task_struct *tsk, struct mm_struct *mm,
 						else
 							return -EFAULT;
 					}
-					if (ret & VM_FAULT_SIGBUS)
+					if (ret & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV))
 						return i ? i : -EFAULT;
 					BUG();
 				}
@@ -1909,7 +1909,7 @@ int fixup_user_fault(struct task_struct *tsk, struct mm_struct *mm,
 			return -ENOMEM;
 		if (ret & (VM_FAULT_HWPOISON | VM_FAULT_HWPOISON_LARGE))
 			return -EHWPOISON;
-		if (ret & VM_FAULT_SIGBUS)
+		if (ret & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV))
 			return -EFAULT;
 		BUG();
 	}
@@ -2699,18 +2699,25 @@ static int do_wp_page(struct mm_struct *mm, struct vm_area_struct *vma,
 		if (!dirty_page)
 			return ret;
 
-		/*
-		 * Yes, Virginia, this is actually required to prevent a race
-		 * with clear_page_dirty_for_io() from clearing the page dirty
-		 * bit after it clear all dirty ptes, but before a racing
-		 * do_wp_page installs a dirty pte.
-		 *
-		 * __do_fault is protected similarly.
-		 */
 		if (!page_mkwrite) {
-			wait_on_page_locked(dirty_page);
-			set_page_dirty_balance(dirty_page, page_mkwrite);
+			struct address_space *mapping;
+			int dirtied;
+
+			lock_page(dirty_page);
+			dirtied = set_page_dirty(dirty_page);
+			VM_BUG_ON(dirty_page);
+			mapping = dirty_page->mapping;
+			unlock_page(dirty_page);
+
+			if (dirtied && mapping) {
+				/*
+				 * Some device drivers do not set page.mapping
+				 * but still dirty their pages
+				 */
+				balance_dirty_pages_ratelimited(mapping);
+			}
 		}
+
 		put_page(dirty_page);
 		if (page_mkwrite) {
 			struct address_space *mapping = dirty_page->mapping;
@@ -3165,7 +3172,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (prev && prev->vm_end == address)
 			return prev->vm_flags & VM_GROWSDOWN ? 0 : -ENOMEM;
 
-		expand_downwards(vma, address - PAGE_SIZE);
+		return expand_downwards(vma, address - PAGE_SIZE);
 	}
 	if ((vma->vm_flags & VM_GROWSUP) && address + PAGE_SIZE == vma->vm_end) {
 		struct vm_area_struct *next = vma->vm_next;
@@ -3174,7 +3181,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (next && next->vm_start == address + PAGE_SIZE)
 			return next->vm_flags & VM_GROWSUP ? 0 : -ENOMEM;
 
-		expand_upwards(vma, address + PAGE_SIZE);
+		return expand_upwards(vma, address + PAGE_SIZE);
 	}
 	return 0;
 }
@@ -3196,7 +3203,7 @@ static int do_anonymous_page(struct mm_struct *mm, struct vm_area_struct *vma,
 
 	/* Check if we need to add a guard page to the stack */
 	if (check_stack_guard_page(vma, address) < 0)
-		return VM_FAULT_SIGBUS;
+		return VM_FAULT_SIGSEGV;
 
 	/* Use the zero-page for reads */
 	if (!(flags & FAULT_FLAG_WRITE)) {
diff --git a/mm/mmap.c b/mm/mmap.c
index eadef99..4cef37e 100644
--- a/mm/mmap.c
+++ b/mm/mmap.c
@@ -567,9 +567,12 @@ again:			remove_next = 1 + (end > next->vm_end);
 		 * shrinking vma had, to cover any anon pages imported.
 		 */
 		if (exporter && exporter->anon_vma && !importer->anon_vma) {
-			if (anon_vma_clone(importer, exporter))
-				return -ENOMEM;
+			int error;
+
 			importer->anon_vma = exporter->anon_vma;
+			error = anon_vma_clone(importer, exporter);
+			if (error)
+				return error;
 		}
 	}
 
@@ -1734,14 +1737,17 @@ static int acct_stack_growth(struct vm_area_struct *vma, unsigned long size, uns
 {
 	struct mm_struct *mm = vma->vm_mm;
 	struct rlimit *rlim = current->signal->rlim;
-	unsigned long new_start;
+	unsigned long new_start, actual_size;
 
 	/* address space limit tests */
 	if (!may_expand_vm(mm, grow))
 		return -ENOMEM;
 
 	/* Stack limit test */
-	if (size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
+	actual_size = size;
+	if (size && (vma->vm_flags & (VM_GROWSUP | VM_GROWSDOWN)))
+		actual_size -= PAGE_SIZE;
+	if (actual_size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
 		return -ENOMEM;
 
 	/* mlock limit tests */
diff --git a/mm/page-writeback.c b/mm/page-writeback.c
index fea1aec..7308710 100644
--- a/mm/page-writeback.c
+++ b/mm/page-writeback.c
@@ -1397,16 +1397,6 @@ static void balance_dirty_pages(struct address_space *mapping,
 		bdi_start_background_writeback(bdi);
 }
 
-void set_page_dirty_balance(struct page *page, int page_mkwrite)
-{
-	if (set_page_dirty(page) || page_mkwrite) {
-		struct address_space *mapping = page_mapping(page);
-
-		if (mapping)
-			balance_dirty_pages_ratelimited(mapping);
-	}
-}
-
 static DEFINE_PER_CPU(int, bdp_ratelimits);
 
 /*
@@ -1992,32 +1982,25 @@ EXPORT_SYMBOL(account_page_writeback);
  * page dirty in that case, but not all the buffers.  This is a "bottom-up"
  * dirtying, whereas __set_page_dirty_buffers() is a "top-down" dirtying.
  *
- * Most callers have locked the page, which pins the address_space in memory.
- * But zap_pte_range() does not lock the page, however in that case the
- * mapping is pinned by the vma's ->vm_file reference.
- *
- * We take care to handle the case where the page was truncated from the
- * mapping by re-checking page_mapping() inside tree_lock.
+ * The caller must ensure this doesn't race with truncation.  Most will simply
+ * hold the page lock, but e.g. zap_pte_range() calls with the page mapped and
+ * the pte lock held, which also locks out truncat
  */
 int __set_page_dirty_nobuffers(struct page *page)
 {
 	if (!TestSetPageDirty(page)) {
 		struct address_space *mapping = page_mapping(page);
-		struct address_space *mapping2;
 		unsigned long flags;
 
 		if (!mapping)
 			return 1;
 
 		spin_lock_irqsave(&mapping->tree_lock, flags);
-		mapping2 = page_mapping(page);
-		if (mapping2) { /* Race with truncate? */
-			BUG_ON(mapping2 != mapping);
-			WARN_ON_ONCE(!PagePrivate(page) && !PageUptodate(page));
-			account_page_dirtied(page, mapping);
-			radix_tree_tag_set(&mapping->page_tree,
-				page_index(page), PAGECACHE_TAG_DIRTY);
-		}
+		BUG_ON(page_mapping(page) != mapping);
+		WARN_ON_ONCE(!PagePrivate(page) && !PageUptodate(page));
+		account_page_dirtied(page, mapping);
+		radix_tree_tag_set(&mapping->page_tree, page_index(page),
+				   PAGECACHE_TAG_DIRTY);
 		spin_unlock_irqrestore(&mapping->tree_lock, flags);
 		if (mapping->host) {
 			/* !PageAnon && !swapper_space */
@@ -2174,12 +2157,10 @@ int clear_page_dirty_for_io(struct page *page)
 		/*
 		 * We carefully synchronise fault handlers against
 		 * installing a dirty pte and marking the page dirty
-		 * at this point. We do this by having them hold the
-		 * page lock at some point after installing their
-		 * pte, but before marking the page dirty.
-		 * Pages are always locked coming in here, so we get
-		 * the desired exclusion. See mm/memory.c:do_wp_page()
-		 * for more comments.
+		 * at this point.  We do this by having them hold the
+		 * page lock while dirtying the page, and pages are
+		 * always locked coming in here, so we get the desired
+		 * exclusion.
 		 */
 		if (TestClearPageDirty(page)) {
 			dec_zone_page_state(page, NR_FILE_DIRTY);
diff --git a/mm/rmap.c b/mm/rmap.c
index ecce3ec..46dfc4e 100644
--- a/mm/rmap.c
+++ b/mm/rmap.c
@@ -72,6 +72,8 @@ static inline struct anon_vma *anon_vma_alloc(void)
 	anon_vma = kmem_cache_alloc(anon_vma_cachep, GFP_KERNEL);
 	if (anon_vma) {
 		atomic_set(&anon_vma->refcount, 1);
+		anon_vma->degree = 1;	/* Reference for first vma */
+		anon_vma->parent = anon_vma;
 		/*
 		 * Initialise the anon_vma root to point to itself. If called
 		 * from fork, the root will be reset to the parents anon_vma.
@@ -193,6 +195,8 @@ int anon_vma_prepare(struct vm_area_struct *vma)
 		if (likely(!vma->anon_vma)) {
 			vma->anon_vma = anon_vma;
 			anon_vma_chain_link(vma, avc, anon_vma);
+			/* vma reference or self-parent link for new root */
+			anon_vma->degree++;
 			allocated = NULL;
 			avc = NULL;
 		}
@@ -241,6 +245,14 @@ static inline void unlock_anon_vma_root(struct anon_vma *root)
 /*
  * Attach the anon_vmas from src to dst.
  * Returns 0 on success, -ENOMEM on failure.
+ *
+ * If dst->anon_vma is NULL this function tries to find and reuse existing
+ * anon_vma which has no vmas and only one child anon_vma. This prevents
+ * degradation of anon_vma hierarchy to endless linear chain in case of
+ * constantly forking task. On the other hand, an anon_vma with more than one
+ * child isn't reused even if there was no alive vma, thus rmap walker has a
+ * good chance of avoiding scanning the whole hierarchy when it searches where
+ * page is mapped.
  */
 int anon_vma_clone(struct vm_area_struct *dst, struct vm_area_struct *src)
 {
@@ -261,11 +273,32 @@ int anon_vma_clone(struct vm_area_struct *dst, struct vm_area_struct *src)
 		anon_vma = pavc->anon_vma;
 		root = lock_anon_vma_root(root, anon_vma);
 		anon_vma_chain_link(dst, avc, anon_vma);
+
+		/*
+		 * Reuse existing anon_vma if its degree lower than two,
+		 * that means it has no vma and only one anon_vma child.
+		 *
+		 * Do not chose parent anon_vma, otherwise first child
+		 * will always reuse it. Root anon_vma is never reused:
+		 * it has self-parent reference and at least one child.
+		 */
+		if (!dst->anon_vma && anon_vma != src->anon_vma &&
+				anon_vma->degree < 2)
+			dst->anon_vma = anon_vma;
 	}
+	if (dst->anon_vma)
+		dst->anon_vma->degree++;
 	unlock_anon_vma_root(root);
 	return 0;
 
  enomem_failure:
+	/*
+	 * dst->anon_vma is dropped here otherwise its degree can be incorrectly
+	 * decremented in unlink_anon_vmas().
+	 * We can safely do this because callers of anon_vma_clone() don't care
+	 * about dst->anon_vma if anon_vma_clone() failed.
+	 */
+	dst->anon_vma = NULL;
 	unlink_anon_vmas(dst);
 	return -ENOMEM;
 }
@@ -329,6 +362,9 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	if (!pvma->anon_vma)
 		return 0;
 
+	/* Drop inherited anon_vma, we'll reuse existing or allocate new. */
+	vma->anon_vma = NULL;
+
 	/*
 	 * First, attach the new VMA to the parent VMA's anon_vmas,
 	 * so rmap can find non-COWed pages in child processes.
@@ -336,6 +372,10 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	if (anon_vma_clone(vma, pvma))
 		return -ENOMEM;
 
+	/* An existing anon_vma has been reused, all done then. */
+	if (vma->anon_vma)
+		return 0;
+
 	/* Then add our own anon_vma. */
 	anon_vma = anon_vma_alloc();
 	if (!anon_vma)
@@ -349,6 +389,7 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	 * lock any of the anon_vmas in this anon_vma tree.
 	 */
 	anon_vma->root = pvma->anon_vma->root;
+	anon_vma->parent = pvma->anon_vma;
 	/*
 	 * With refcounts, an anon_vma can stay around longer than the
 	 * process it belongs to. The root anon_vma needs to be pinned until
@@ -359,6 +400,7 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	vma->anon_vma = anon_vma;
 	anon_vma_lock(anon_vma);
 	anon_vma_chain_link(vma, avc, anon_vma);
+	anon_vma->parent->degree++;
 	anon_vma_unlock(anon_vma);
 
 	return 0;
@@ -389,12 +431,16 @@ void unlink_anon_vmas(struct vm_area_struct *vma)
 		 * Leave empty anon_vmas on the list - we'll need
 		 * to free them outside the lock.
 		 */
-		if (list_empty(&anon_vma->head))
+		if (list_empty(&anon_vma->head)) {
+			anon_vma->parent->degree--;
 			continue;
+		}
 
 		list_del(&avc->same_vma);
 		anon_vma_chain_free(avc);
 	}
+	if (vma->anon_vma)
+		vma->anon_vma->degree--;
 	unlock_anon_vma_root(root);
 
 	/*
@@ -405,6 +451,7 @@ void unlink_anon_vmas(struct vm_area_struct *vma)
 	list_for_each_entry_safe(avc, next, &vma->anon_vma_chain, same_vma) {
 		struct anon_vma *anon_vma = avc->anon_vma;
 
+		BUG_ON(anon_vma->degree);
 		put_anon_vma(anon_vma);
 
 		list_del(&avc->same_vma);
diff --git a/net/caif/chnl_net.c b/net/caif/chnl_net.c
index d09340e..b8d9403 100644
--- a/net/caif/chnl_net.c
+++ b/net/caif/chnl_net.c
@@ -467,7 +467,6 @@ static int ipcaif_newlink(struct net *src_net, struct net_device *dev,
 	ASSERT_RTNL();
 	caifdev = netdev_priv(dev);
 	caif_netlink_parms(data, &caifdev->conn_req);
-	dev_net_set(caifdev->netdev, src_net);
 
 	ret = register_netdevice(dev);
 	if (ret)
diff --git a/net/compat.c b/net/compat.c
index f7f82ba..618ad24 100644
--- a/net/compat.c
+++ b/net/compat.c
@@ -71,6 +71,13 @@ int get_compat_msghdr(struct msghdr *kmsg, struct compat_msghdr __user *umsg)
 	    __get_user(kmsg->msg_controllen, &umsg->msg_controllen) ||
 	    __get_user(kmsg->msg_flags, &umsg->msg_flags))
 		return -EFAULT;
+
+	if (!tmp1)
+		kmsg->msg_namelen = 0;
+
+	if (kmsg->msg_namelen < 0)
+		return -EINVAL;
+
 	if (kmsg->msg_namelen > sizeof(struct sockaddr_storage))
 		kmsg->msg_namelen = sizeof(struct sockaddr_storage);
 	kmsg->msg_name = compat_ptr(tmp1);
diff --git a/net/core/dev.c b/net/core/dev.c
index 634f56d..06ea934 100644
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -2143,12 +2143,14 @@ netdev_features_t netif_skb_features(struct sk_buff *skb)
 	if (skb_shinfo(skb)->gso_segs > skb->dev->gso_max_segs)
 		features &= ~NETIF_F_GSO_MASK;
 
-	if (protocol == htons(ETH_P_8021Q)) {
-		struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
-		protocol = veh->h_vlan_encapsulated_proto;
-	} else if (!vlan_tx_tag_present(skb)) {
-		return harmonize_features(skb, protocol, features);
-	}
+	if (!vlan_tx_tag_present(skb)) {
+		if (unlikely(protocol == htons(ETH_P_8021Q))) {
+			struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
+			protocol = veh->h_vlan_encapsulated_proto;
+		} else {
+			return harmonize_features(skb, protocol, features);
+		}
+        }
 
 	features &= (skb->dev->vlan_features | NETIF_F_HW_VLAN_TX);
 
diff --git a/net/ipv6/ip6_fib.c b/net/ipv6/ip6_fib.c
index 5bb77a6..2cfcfb7 100644
--- a/net/ipv6/ip6_fib.c
+++ b/net/ipv6/ip6_fib.c
@@ -633,6 +633,29 @@ static struct fib6_node * fib6_add_1(struct fib6_node *root, void *addr,
 	return ln;
 }
 
+static void fib6_purge_rt(struct rt6_info *rt, struct fib6_node *fn,
+			  struct net *net)
+{
+	if (atomic_read(&rt->rt6i_ref) != 1) {
+		/* This route is used as dummy address holder in some split
+		 * nodes. It is not leaked, but it still holds other resources,
+		 * which must be released in time. So, scan ascendant nodes
+		 * and replace dummy references to this route with references
+		 * to still alive ones.
+		 */
+		while (fn) {
+			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
+				fn->leaf = fib6_find_prefix(net, fn);
+				atomic_inc(&fn->leaf->rt6i_ref);
+				rt6_release(rt);
+			}
+			fn = fn->parent;
+		}
+		/* No more references are possible at this point. */
+		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
+	}
+}
+
 /*
  *	Insert routing information in a node.
  */
@@ -723,11 +746,12 @@ static int fib6_add_rt2node(struct fib6_node *fn, struct rt6_info *rt,
 		rt->dst.rt6_next = iter->dst.rt6_next;
 		atomic_inc(&rt->rt6i_ref);
 		inet6_rt_notify(RTM_NEWROUTE, rt, info);
-		rt6_release(iter);
 		if (!(fn->fn_flags & RTN_RTINFO)) {
 			info->nl_net->ipv6.rt6_stats->fib_route_nodes++;
 			fn->fn_flags |= RTN_RTINFO;
 		}
+		fib6_purge_rt(iter, fn, info->nl_net);
+		rt6_release(iter);
 	}
 
 	return 0;
@@ -1229,24 +1253,7 @@ static void fib6_del_route(struct fib6_node *fn, struct rt6_info **rtp,
 		fn = fib6_repair_tree(net, fn);
 	}
 
-	if (atomic_read(&rt->rt6i_ref) != 1) {
-		/* This route is used as dummy address holder in some split
-		 * nodes. It is not leaked, but it still holds other resources,
-		 * which must be released in time. So, scan ascendant nodes
-		 * and replace dummy references to this route with references
-		 * to still alive ones.
-		 */
-		while (fn) {
-			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
-				fn->leaf = fib6_find_prefix(net, fn);
-				atomic_inc(&fn->leaf->rt6i_ref);
-				rt6_release(rt);
-			}
-			fn = fn->parent;
-		}
-		/* No more references are possible at this point. */
-		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
-	}
+	fib6_purge_rt(rt, fn, net);
 
 	inet6_rt_notify(RTM_DELROUTE, rt, info);
 	rt6_release(rt);
diff --git a/net/mac80211/rx.c b/net/mac80211/rx.c
index 32929b0..24f2a41 100644
--- a/net/mac80211/rx.c
+++ b/net/mac80211/rx.c
@@ -1486,14 +1486,14 @@ ieee80211_rx_h_defragment(struct ieee80211_rx_data *rx)
 	sc = le16_to_cpu(hdr->seq_ctrl);
 	frag = sc & IEEE80211_SCTL_FRAG;
 
-	if (likely(!ieee80211_has_morefrags(fc) && frag == 0))
-		goto out;
-
 	if (is_multicast_ether_addr(hdr->addr1)) {
 		rx->local->dot11MulticastReceivedFrameCount++;
-		goto out;
+		goto out_no_led;
 	}
 
+	if (likely(!ieee80211_has_morefrags(fc) && frag == 0))
+		goto out;
+
 	I802_DEBUG_INC(rx->local->rx_handlers_fragments);
 
 	if (skb_linearize(rx->skb))
@@ -1584,9 +1584,10 @@ ieee80211_rx_h_defragment(struct ieee80211_rx_data *rx)
 	status->rx_flags |= IEEE80211_RX_FRAGMENTED;
 
  out:
+	ieee80211_led_rx(rx->local);
+ out_no_led:
 	if (rx->sta)
 		rx->sta->rx_packets++;
-	ieee80211_led_rx(rx->local);
 	return RX_CONTINUE;
 }
 
diff --git a/net/netfilter/ipvs/ip_vs_core.c b/net/netfilter/ipvs/ip_vs_core.c
index 00bdb1d..abdb475 100644
--- a/net/netfilter/ipvs/ip_vs_core.c
+++ b/net/netfilter/ipvs/ip_vs_core.c
@@ -662,16 +662,24 @@ static inline int ip_vs_gather_frags_v6(struct sk_buff *skb, u_int32_t user)
 }
 #endif
 
-static int ip_vs_route_me_harder(int af, struct sk_buff *skb)
+static int ip_vs_route_me_harder(int af, struct sk_buff *skb,
+				 unsigned int hooknum)
 {
+	if (!sysctl_snat_reroute(skb))
+		return 0;
+	/* Reroute replies only to remote clients (FORWARD and LOCAL_OUT) */
+	if (NF_INET_LOCAL_IN == hooknum)
+		return 0;
 #ifdef CONFIG_IP_VS_IPV6
 	if (af == AF_INET6) {
-		if (sysctl_snat_reroute(skb) && ip6_route_me_harder(skb) != 0)
+		struct dst_entry *dst = skb_dst(skb);
+
+		if (dst->dev && !(dst->dev->flags & IFF_LOOPBACK) &&
+		    ip6_route_me_harder(skb) != 0)
 			return 1;
 	} else
 #endif
-		if ((sysctl_snat_reroute(skb) ||
-		     skb_rtable(skb)->rt_flags & RTCF_LOCAL) &&
+		if (!(skb_rtable(skb)->rt_flags & RTCF_LOCAL) &&
 		    ip_route_me_harder(skb, RTN_LOCAL) != 0)
 			return 1;
 
@@ -782,7 +790,8 @@ static int handle_response_icmp(int af, struct sk_buff *skb,
 				union nf_inet_addr *snet,
 				__u8 protocol, struct ip_vs_conn *cp,
 				struct ip_vs_protocol *pp,
-				unsigned int offset, unsigned int ihl)
+				unsigned int offset, unsigned int ihl,
+				unsigned int hooknum)
 {
 	unsigned int verdict = NF_DROP;
 
@@ -812,7 +821,7 @@ static int handle_response_icmp(int af, struct sk_buff *skb,
 #endif
 		ip_vs_nat_icmp(skb, pp, cp, 1);
 
-	if (ip_vs_route_me_harder(af, skb))
+	if (ip_vs_route_me_harder(af, skb, hooknum))
 		goto out;
 
 	/* do the statistics and put it back */
@@ -908,7 +917,7 @@ static int ip_vs_out_icmp(struct sk_buff *skb, int *related,
 
 	snet.ip = iph->saddr;
 	return handle_response_icmp(AF_INET, skb, &snet, cih->protocol, cp,
-				    pp, offset, ihl);
+				    pp, offset, ihl, hooknum);
 }
 
 #ifdef CONFIG_IP_VS_IPV6
@@ -985,7 +994,8 @@ static int ip_vs_out_icmp_v6(struct sk_buff *skb, int *related,
 
 	snet.in6 = iph->saddr;
 	return handle_response_icmp(AF_INET6, skb, &snet, cih->nexthdr, cp,
-				    pp, offset, sizeof(struct ipv6hdr));
+				    pp, offset, sizeof(struct ipv6hdr),
+				    hooknum);
 }
 #endif
 
@@ -1018,7 +1028,7 @@ static inline int is_tcp_reset(const struct sk_buff *skb, int nh_len)
  */
 static unsigned int
 handle_response(int af, struct sk_buff *skb, struct ip_vs_proto_data *pd,
-		struct ip_vs_conn *cp, int ihl)
+		struct ip_vs_conn *cp, int ihl, unsigned int hooknum)
 {
 	struct ip_vs_protocol *pp = pd->pp;
 
@@ -1056,7 +1066,7 @@ handle_response(int af, struct sk_buff *skb, struct ip_vs_proto_data *pd,
 	 * if it came from this machine itself.  So re-compute
 	 * the routing information.
 	 */
-	if (ip_vs_route_me_harder(af, skb))
+	if (ip_vs_route_me_harder(af, skb, hooknum))
 		goto drop;
 
 	IP_VS_DBG_PKT(10, af, pp, skb, 0, "After SNAT");
@@ -1169,7 +1179,7 @@ ip_vs_out(unsigned int hooknum, struct sk_buff *skb, int af)
 	cp = pp->conn_out_get(af, skb, &iph, iph.len, 0);
 
 	if (likely(cp))
-		return handle_response(af, skb, pd, cp, iph.len);
+		return handle_response(af, skb, pd, cp, iph.len, hooknum);
 	if (sysctl_nat_icmp_send(net) &&
 	    (pp->protocol == IPPROTO_TCP ||
 	     pp->protocol == IPPROTO_UDP ||
diff --git a/net/sctp/associola.c b/net/sctp/associola.c
index da54d29..d014b05 100644
--- a/net/sctp/associola.c
+++ b/net/sctp/associola.c
@@ -1272,7 +1272,6 @@ void sctp_assoc_update(struct sctp_association *asoc,
 	asoc->peer.peer_hmacs = new->peer.peer_hmacs;
 	new->peer.peer_hmacs = NULL;
 
-	sctp_auth_key_put(asoc->asoc_shared_key);
 	sctp_auth_asoc_init_active_key(asoc, GFP_ATOMIC);
 }
 
@@ -1638,6 +1637,8 @@ struct sctp_chunk *sctp_assoc_lookup_asconf_ack(
 	 * ack chunk whose serial number matches that of the request.
 	 */
 	list_for_each_entry(ack, &asoc->asconf_ack_list, transmitted_list) {
+		if (sctp_chunk_pending(ack))
+			continue;
 		if (ack->subh.addip_hdr->serial == serial) {
 			sctp_chunk_hold(ack);
 			return ack;
diff --git a/net/sctp/sm_make_chunk.c b/net/sctp/sm_make_chunk.c
index adb0287..f1249b3 100644
--- a/net/sctp/sm_make_chunk.c
+++ b/net/sctp/sm_make_chunk.c
@@ -2569,7 +2569,10 @@ static int sctp_process_param(struct sctp_association *asoc,
 
 		addr_param = param.v + sizeof(sctp_addip_param_t);
 
-		af = sctp_get_af_specific(param_type2af(param.p->type));
+		af = sctp_get_af_specific(param_type2af(addr_param->p.type));
+		if (af == NULL)
+			break;
+
 		af->from_addr_param(&addr, addr_param,
 				    htons(asoc->peer.port), 0);
 
@@ -3068,50 +3071,63 @@ static __be16 sctp_process_asconf_param(struct sctp_association *asoc,
 	return SCTP_ERROR_NO_ERROR;
 }
 
-/* Verify the ASCONF packet before we process it.  */
-int sctp_verify_asconf(const struct sctp_association *asoc,
-		       struct sctp_paramhdr *param_hdr, void *chunk_end,
-		       struct sctp_paramhdr **errp) {
-	sctp_addip_param_t *asconf_param;
+/* Verify the ASCONF packet before we process it. */
+bool sctp_verify_asconf(const struct sctp_association *asoc,
+			struct sctp_chunk *chunk, bool addr_param_needed,
+			struct sctp_paramhdr **errp)
+{
+	sctp_addip_chunk_t *addip = (sctp_addip_chunk_t *) chunk->chunk_hdr;
 	union sctp_params param;
-	int length, plen;
+	bool addr_param_seen = false;
 
-	param.v = (sctp_paramhdr_t *) param_hdr;
-	while (param.v <= chunk_end - sizeof(sctp_paramhdr_t)) {
-		length = ntohs(param.p->length);
-		*errp = param.p;
-
-		if (param.v > chunk_end - length ||
-		    length < sizeof(sctp_paramhdr_t))
-			return 0;
+	sctp_walk_params(param, addip, addip_hdr.params) {
+		size_t length = ntohs(param.p->length);
 
+		*errp = param.p;
 		switch (param.p->type) {
+		case SCTP_PARAM_ERR_CAUSE:
+			break;
+		case SCTP_PARAM_IPV4_ADDRESS:
+			if (length != sizeof(sctp_ipv4addr_param_t))
+				return false;
+			addr_param_seen = true;
+			break;
+		case SCTP_PARAM_IPV6_ADDRESS:
+			if (length != sizeof(sctp_ipv6addr_param_t))
+				return false;
+			addr_param_seen = true;
+			break;
 		case SCTP_PARAM_ADD_IP:
 		case SCTP_PARAM_DEL_IP:
 		case SCTP_PARAM_SET_PRIMARY:
-			asconf_param = (sctp_addip_param_t *)param.v;
-			plen = ntohs(asconf_param->param_hdr.length);
-			if (plen < sizeof(sctp_addip_param_t) +
-			    sizeof(sctp_paramhdr_t))
-				return 0;
+			/* In ASCONF chunks, these need to be first. */
+			if (addr_param_needed && !addr_param_seen)
+				return false;
+			length = ntohs(param.addip->param_hdr.length);
+			if (length < sizeof(sctp_addip_param_t) +
+				     sizeof(sctp_paramhdr_t))
+				return false;
 			break;
 		case SCTP_PARAM_SUCCESS_REPORT:
 		case SCTP_PARAM_ADAPTATION_LAYER_IND:
 			if (length != sizeof(sctp_addip_param_t))
-				return 0;
-
+				return false;
 			break;
 		default:
-			break;
+			/* This is unkown to us, reject! */
+			return false;
 		}
-
-		param.v += WORD_ROUND(length);
 	}
 
-	if (param.v != chunk_end)
-		return 0;
+	/* Remaining sanity checks. */
+	if (addr_param_needed && !addr_param_seen)
+		return false;
+	if (!addr_param_needed && addr_param_seen)
+		return false;
+	if (param.v != chunk->chunk_end)
+		return false;
 
-	return 1;
+	return true;
 }
 
 /* Process an incoming ASCONF chunk with the next expected serial no. and
@@ -3120,16 +3136,17 @@ int sctp_verify_asconf(const struct sctp_association *asoc,
 struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 				       struct sctp_chunk *asconf)
 {
+	sctp_addip_chunk_t *addip = (sctp_addip_chunk_t *) asconf->chunk_hdr;
+	bool all_param_pass = true;
+	union sctp_params param;
 	sctp_addiphdr_t		*hdr;
 	union sctp_addr_param	*addr_param;
 	sctp_addip_param_t	*asconf_param;
 	struct sctp_chunk	*asconf_ack;
-
 	__be16	err_code;
 	int	length = 0;
 	int	chunk_len;
 	__u32	serial;
-	int	all_param_pass = 1;
 
 	chunk_len = ntohs(asconf->chunk_hdr->length) - sizeof(sctp_chunkhdr_t);
 	hdr = (sctp_addiphdr_t *)asconf->skb->data;
@@ -3157,9 +3174,14 @@ struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 		goto done;
 
 	/* Process the TLVs contained within the ASCONF chunk. */
-	while (chunk_len > 0) {
+	sctp_walk_params(param, addip, addip_hdr.params) {
+		/* Skip preceeding address parameters. */
+		if (param.p->type == SCTP_PARAM_IPV4_ADDRESS ||
+		    param.p->type == SCTP_PARAM_IPV6_ADDRESS)
+			continue;
+
 		err_code = sctp_process_asconf_param(asoc, asconf,
-						     asconf_param);
+						     param.addip);
 		/* ADDIP 4.1 A7)
 		 * If an error response is received for a TLV parameter,
 		 * all TLVs with no response before the failed TLV are
@@ -3167,28 +3189,20 @@ struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 		 * the failed response are considered unsuccessful unless
 		 * a specific success indication is present for the parameter.
 		 */
-		if (SCTP_ERROR_NO_ERROR != err_code)
-			all_param_pass = 0;
-
+		if (err_code != SCTP_ERROR_NO_ERROR)
+			all_param_pass = false;
 		if (!all_param_pass)
-			sctp_add_asconf_response(asconf_ack,
-						 asconf_param->crr_id, err_code,
-						 asconf_param);
+			sctp_add_asconf_response(asconf_ack, param.addip->crr_id,
+						 err_code, param.addip);
 
 		/* ADDIP 4.3 D11) When an endpoint receiving an ASCONF to add
 		 * an IP address sends an 'Out of Resource' in its response, it
 		 * MUST also fail any subsequent add or delete requests bundled
 		 * in the ASCONF.
 		 */
-		if (SCTP_ERROR_RSRC_LOW == err_code)
+		if (err_code == SCTP_ERROR_RSRC_LOW)
 			goto done;
-
-		/* Move to the next ASCONF param. */
-		length = ntohs(asconf_param->param_hdr.length);
-		asconf_param = (void *)asconf_param + length;
-		chunk_len -= length;
 	}
-
 done:
 	asoc->peer.addip_serial++;
 
diff --git a/net/sctp/sm_statefuns.c b/net/sctp/sm_statefuns.c
index 5ac33b6..a6a3006 100644
--- a/net/sctp/sm_statefuns.c
+++ b/net/sctp/sm_statefuns.c
@@ -3516,9 +3516,7 @@ sctp_disposition_t sctp_sf_do_asconf(const struct sctp_endpoint *ep,
 	struct sctp_chunk	*asconf_ack = NULL;
 	struct sctp_paramhdr	*err_param = NULL;
 	sctp_addiphdr_t		*hdr;
-	union sctp_addr_param	*addr_param;
 	__u32			serial;
-	int			length;
 
 	if (!sctp_vtag_verify(chunk, asoc)) {
 		sctp_add_cmd_sf(commands, SCTP_CMD_REPORT_BAD_TAG,
@@ -3543,17 +3541,8 @@ sctp_disposition_t sctp_sf_do_asconf(const struct sctp_endpoint *ep,
 	hdr = (sctp_addiphdr_t *)chunk->skb->data;
 	serial = ntohl(hdr->serial);
 
-	addr_param = (union sctp_addr_param *)hdr->params;
-	length = ntohs(addr_param->p.length);
-	if (length < sizeof(sctp_paramhdr_t))
-		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
-			   (void *)addr_param, commands);
-
 	/* Verify the ASCONF chunk before processing it. */
-	if (!sctp_verify_asconf(asoc,
-			    (sctp_paramhdr_t *)((void *)addr_param + length),
-			    (void *)chunk->chunk_end,
-			    &err_param))
+	if (!sctp_verify_asconf(asoc, chunk, true, &err_param))
 		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
 						  (void *)err_param, commands);
 
@@ -3670,10 +3659,7 @@ sctp_disposition_t sctp_sf_do_asconf_ack(const struct sctp_endpoint *ep,
 	rcvd_serial = ntohl(addip_hdr->serial);
 
 	/* Verify the ASCONF-ACK chunk before processing it. */
-	if (!sctp_verify_asconf(asoc,
-	    (sctp_paramhdr_t *)addip_hdr->params,
-	    (void *)asconf_ack->chunk_end,
-	    &err_param))
+	if (!sctp_verify_asconf(asoc, asconf_ack, false, &err_param))
 		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
 			   (void *)err_param, commands);
 
diff --git a/net/socket.c b/net/socket.c
index 24a6d15..ee74d1c 100644
--- a/net/socket.c
+++ b/net/socket.c
@@ -1929,6 +1929,9 @@ static int copy_msghdr_from_user(struct msghdr *kmsg,
 	if (copy_from_user(kmsg, umsg, sizeof(struct msghdr)))
 		return -EFAULT;
 
+	if (kmsg->msg_name == NULL)
+		kmsg->msg_namelen = 0;
+
 	if (kmsg->msg_namelen < 0)
 		return -EINVAL;
 
diff --git a/net/sunrpc/svcsock.c b/net/sunrpc/svcsock.c
index 4c23cfc..a0769e1 100644
--- a/net/sunrpc/svcsock.c
+++ b/net/sunrpc/svcsock.c
@@ -1055,17 +1055,12 @@ static int receive_cb_reply(struct svc_sock *svsk, struct svc_rqst *rqstp)
 	xid = *p++;
 	calldir = *p;
 
-	if (bc_xprt)
-		req = xprt_lookup_rqst(bc_xprt, xid);
-
-	if (!req) {
-		printk(KERN_NOTICE
-			"%s: Got unrecognized reply: "
-			"calldir 0x%x xpt_bc_xprt %p xid %08x\n",
-			__func__, ntohl(calldir),
-			bc_xprt, xid);
+	if (!bc_xprt)
 		return -EAGAIN;
-	}
+	spin_lock_bh(&bc_xprt->transport_lock);
+	req = xprt_lookup_rqst(bc_xprt, xid);
+	if (!req)
+		goto unlock_notfound;
 
 	memcpy(&req->rq_private_buf, &req->rq_rcv_buf, sizeof(struct xdr_buf));
 	/*
@@ -1076,11 +1071,21 @@ static int receive_cb_reply(struct svc_sock *svsk, struct svc_rqst *rqstp)
 	dst = &req->rq_private_buf.head[0];
 	src = &rqstp->rq_arg.head[0];
 	if (dst->iov_len < src->iov_len)
-		return -EAGAIN; /* whatever; just giving up. */
+		goto unlock_eagain; /* whatever; just giving up. */
 	memcpy(dst->iov_base, src->iov_base, src->iov_len);
 	xprt_complete_rqst(req->rq_task, svsk->sk_reclen);
 	rqstp->rq_arg.len = 0;
+	spin_unlock_bh(&bc_xprt->transport_lock);
 	return 0;
+unlock_notfound:
+	printk(KERN_NOTICE
+		"%s: Got unrecognized reply: "
+		"calldir 0x%x xpt_bc_xprt %p xid %08x\n",
+		__func__, ntohl(calldir),
+		bc_xprt, ntohl(xid));
+unlock_eagain:
+	spin_unlock_bh(&bc_xprt->transport_lock);
+	return -EAGAIN;
 }
 
 static int copy_pages_to_kvecs(struct kvec *vec, struct page **pages, int len)
diff --git a/net/wireless/nl80211.c b/net/wireless/nl80211.c
index be8244d..1bab426 100644
--- a/net/wireless/nl80211.c
+++ b/net/wireless/nl80211.c
@@ -1957,6 +1957,9 @@ static int nl80211_get_key(struct sk_buff *skb, struct genl_info *info)
 	if (!rdev->ops->get_key)
 		return -EOPNOTSUPP;
 
+	if (!pairwise && mac_addr && !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
+		return -ENOENT;
+
 	msg = nlmsg_new(NLMSG_DEFAULT_SIZE, GFP_KERNEL);
 	if (!msg)
 		return -ENOMEM;
@@ -1974,10 +1977,6 @@ static int nl80211_get_key(struct sk_buff *skb, struct genl_info *info)
 	if (mac_addr)
 		NLA_PUT(msg, NL80211_ATTR_MAC, ETH_ALEN, mac_addr);
 
-	if (pairwise && mac_addr &&
-	    !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
-		return -ENOENT;
-
 	err = rdev->ops->get_key(&rdev->wiphy, dev, key_idx, pairwise,
 				 mac_addr, &cookie, get_key_callback);
 
@@ -2149,7 +2148,7 @@ static int nl80211_del_key(struct sk_buff *skb, struct genl_info *info)
 	wdev_lock(dev->ieee80211_ptr);
 	err = nl80211_key_allowed(dev->ieee80211_ptr);
 
-	if (key.type == NL80211_KEYTYPE_PAIRWISE && mac_addr &&
+	if (key.type == NL80211_KEYTYPE_GROUP && mac_addr &&
 	    !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
 		err = -ENOENT;
 
diff --git a/scripts/recordmcount.pl b/scripts/recordmcount.pl
index 858966a..679218b 100755
--- a/scripts/recordmcount.pl
+++ b/scripts/recordmcount.pl
@@ -262,7 +262,6 @@ sub check_objcopy
     # force flags for this arch
     $ld .= " -m shlelf_linux";
     $objcopy .= " -O elf32-sh-linux";
-    $cc .= " -m32";
 
 } elsif ($arch eq "powerpc") {
     $local_regex = "^[0-9a-fA-F]+\\s+t\\s+(\\.?\\S+)";
diff --git a/security/keys/encrypted-keys/encrypted.c b/security/keys/encrypted-keys/encrypted.c
index 2d1bb8a..a02f923 100644
--- a/security/keys/encrypted-keys/encrypted.c
+++ b/security/keys/encrypted-keys/encrypted.c
@@ -1016,10 +1016,13 @@ static int __init init_encrypted(void)
 	ret = encrypted_shash_alloc();
 	if (ret < 0)
 		return ret;
+	ret = aes_get_sizes();
+	if (ret < 0)
+		goto out;
 	ret = register_key_type(&key_type_encrypted);
 	if (ret < 0)
 		goto out;
-	return aes_get_sizes();
+	return 0;
 out:
 	encrypted_shash_release();
 	return ret;
diff --git a/sound/core/seq/seq_dummy.c b/sound/core/seq/seq_dummy.c
index dbc5507..f60d814 100644
--- a/sound/core/seq/seq_dummy.c
+++ b/sound/core/seq/seq_dummy.c
@@ -82,36 +82,6 @@ struct snd_seq_dummy_port {
 static int my_client = -1;
 
 /*
- * unuse callback - send ALL_SOUNDS_OFF and RESET_CONTROLLERS events
- * to subscribers.
- * Note: this callback is called only after all subscribers are removed.
- */
-static int
-dummy_unuse(void *private_data, struct snd_seq_port_subscribe *info)
-{
-	struct snd_seq_dummy_port *p;
-	int i;
-	struct snd_seq_event ev;
-
-	p = private_data;
-	memset(&ev, 0, sizeof(ev));
-	if (p->duplex)
-		ev.source.port = p->connect;
-	else
-		ev.source.port = p->port;
-	ev.dest.client = SNDRV_SEQ_ADDRESS_SUBSCRIBERS;
-	ev.type = SNDRV_SEQ_EVENT_CONTROLLER;
-	for (i = 0; i < 16; i++) {
-		ev.data.control.channel = i;
-		ev.data.control.param = MIDI_CTL_ALL_SOUNDS_OFF;
-		snd_seq_kernel_client_dispatch(p->client, &ev, 0, 0);
-		ev.data.control.param = MIDI_CTL_RESET_CONTROLLERS;
-		snd_seq_kernel_client_dispatch(p->client, &ev, 0, 0);
-	}
-	return 0;
-}
-
-/*
  * event input callback - just redirect events to subscribers
  */
 static int
@@ -175,7 +145,6 @@ create_port(int idx, int type)
 		| SNDRV_SEQ_PORT_TYPE_PORT;
 	memset(&pcb, 0, sizeof(pcb));
 	pcb.owner = THIS_MODULE;
-	pcb.unuse = dummy_unuse;
 	pcb.event_input = dummy_input;
 	pcb.private_free = dummy_free;
 	pcb.private_data = rec;
diff --git a/sound/i2c/other/ak4113.c b/sound/i2c/other/ak4113.c
index dde5c9c..e1ab3ad 100644
--- a/sound/i2c/other/ak4113.c
+++ b/sound/i2c/other/ak4113.c
@@ -56,8 +56,7 @@ static inline unsigned char reg_read(struct ak4113 *ak4113, unsigned char reg)
 
 static void snd_ak4113_free(struct ak4113 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -89,6 +88,7 @@ int snd_ak4113_create(struct snd_card *card, ak4113_read_t *read,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4113_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < AK4113_WRITABLE_REGS ; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -139,13 +139,11 @@ static void ak4113_init_regs(struct ak4113 *chip)
 
 void snd_ak4113_reinit(struct ak4113 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work_sync(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4113_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 EXPORT_SYMBOL_GPL(snd_ak4113_reinit);
@@ -632,8 +630,9 @@ static void ak4113_stats(struct work_struct *work)
 {
 	struct ak4113 *chip = container_of(work, struct ak4113, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4113_check_rate_and_errors(chip, chip->check_flags);
 
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
diff --git a/sound/i2c/other/ak4114.c b/sound/i2c/other/ak4114.c
index fdf3c1b..4c6b379 100644
--- a/sound/i2c/other/ak4114.c
+++ b/sound/i2c/other/ak4114.c
@@ -66,8 +66,7 @@ static void reg_dump(struct ak4114 *ak4114)
 
 static void snd_ak4114_free(struct ak4114 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -100,6 +99,7 @@ int snd_ak4114_create(struct snd_card *card,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4114_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < 7; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -152,13 +152,11 @@ static void ak4114_init_regs(struct ak4114 *chip)
 
 void snd_ak4114_reinit(struct ak4114 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work_sync(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4114_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
@@ -612,10 +610,10 @@ static void ak4114_stats(struct work_struct *work)
 {
 	struct ak4114 *chip = container_of(work, struct ak4114, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4114_check_rate_and_errors(chip, chip->check_flags);
-
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
 EXPORT_SYMBOL(snd_ak4114_create);
diff --git a/sound/pci/hda/hda_intel.c b/sound/pci/hda/hda_intel.c
index 33e538f..f461737 100644
--- a/sound/pci/hda/hda_intel.c
+++ b/sound/pci/hda/hda_intel.c
@@ -2685,6 +2685,7 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	struct azx *chip;
 	int i, err;
 	unsigned short gcap;
+	unsigned int dma_bits = 64;
 	static struct snd_device_ops ops = {
 		.dev_free = azx_dev_free,
 	};
@@ -2780,9 +2781,14 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	gcap = azx_readw(chip, GCAP);
 	snd_printdd(SFX "chipset global capabilities = 0x%x\n", gcap);
 
+	/* AMD devices support 40 or 48bit DMA, take the safe one */
+	if (chip->pci->vendor == PCI_VENDOR_ID_AMD)
+		dma_bits = 40;
+
 	/* disable SB600 64bit support for safety */
 	if (chip->pci->vendor == PCI_VENDOR_ID_ATI) {
 		struct pci_dev *p_smbus;
+		dma_bits = 40;
 		p_smbus = pci_get_device(PCI_VENDOR_ID_ATI,
 					 PCI_DEVICE_ID_ATI_SBX00_SMBUS,
 					 NULL);
@@ -2812,9 +2818,11 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	}
 
 	/* allow 64bit DMA address if supported by H/W */
-	if ((gcap & ICH6_GCAP_64OK) && !pci_set_dma_mask(pci, DMA_BIT_MASK(64)))
-		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(64));
-	else {
+	if (!(gcap & ICH6_GCAP_64OK))
+		dma_bits = 32;
+	if (!pci_set_dma_mask(pci, DMA_BIT_MASK(dma_bits))) {
+		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(dma_bits));
+	} else {
 		pci_set_dma_mask(pci, DMA_BIT_MASK(32));
 		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(32));
 	}
diff --git a/sound/pci/hda/patch_sigmatel.c b/sound/pci/hda/patch_sigmatel.c
index 137b67f..606f87a 100644
--- a/sound/pci/hda/patch_sigmatel.c
+++ b/sound/pci/hda/patch_sigmatel.c
@@ -4246,9 +4246,9 @@ static void stac_store_hints(struct hda_codec *codec)
 			spec->gpio_mask;
 	}
 	if (get_int_hint(codec, "gpio_dir", &spec->gpio_dir))
-		spec->gpio_mask &= spec->gpio_mask;
-	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
 		spec->gpio_dir &= spec->gpio_mask;
+	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
+		spec->gpio_data &= spec->gpio_mask;
 	if (get_int_hint(codec, "eapd_mask", &spec->eapd_mask))
 		spec->eapd_mask &= spec->gpio_mask;
 	if (get_int_hint(codec, "gpio_mute", &spec->gpio_mute))
diff --git a/sound/soc/atmel/atmel_ssc_dai.c b/sound/soc/atmel/atmel_ssc_dai.c
index 354341e..8d7d29c 100644
--- a/sound/soc/atmel/atmel_ssc_dai.c
+++ b/sound/soc/atmel/atmel_ssc_dai.c
@@ -341,7 +341,6 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 	struct atmel_pcm_dma_params *dma_params;
 	int dir, channels, bits;
 	u32 tfmr, rfmr, tcmr, rcmr;
-	int start_event;
 	int ret;
 
 	/*
@@ -460,19 +459,10 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		 * The SSC transmit clock is obtained from the BCLK signal on
 		 * on the TK line, and the SSC receive clock is
 		 * generated from the transmit clock.
-		 *
-		 *  For single channel data, one sample is transferred
-		 * on the falling edge of the LRC clock.
-		 * For two channel data, one sample is
-		 * transferred on both edges of the LRC clock.
 		 */
-		start_event = ((channels == 1)
-				? SSC_START_FALLING_RF
-				: SSC_START_EDGE_RF);
-
 		rcmr =	  SSC_BF(RCMR_PERIOD, 0)
 			| SSC_BF(RCMR_STTDLY, START_DELAY)
-			| SSC_BF(RCMR_START, start_event)
+			| SSC_BF(RCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(RCMR_CKI, SSC_CKI_RISING)
 			| SSC_BF(RCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(RCMR_CKS, SSC_CKS_CLOCK);
@@ -480,14 +470,14 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		rfmr =	  SSC_BF(RFMR_FSEDGE, SSC_FSEDGE_POSITIVE)
 			| SSC_BF(RFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(RFMR_FSLEN, 0)
-			| SSC_BF(RFMR_DATNB, 0)
+			| SSC_BF(RFMR_DATNB, (channels - 1))
 			| SSC_BIT(RFMR_MSBF)
 			| SSC_BF(RFMR_LOOP, 0)
 			| SSC_BF(RFMR_DATLEN, (bits - 1));
 
 		tcmr =	  SSC_BF(TCMR_PERIOD, 0)
 			| SSC_BF(TCMR_STTDLY, START_DELAY)
-			| SSC_BF(TCMR_START, start_event)
+			| SSC_BF(TCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(TCMR_CKI, SSC_CKI_FALLING)
 			| SSC_BF(TCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(TCMR_CKS, SSC_CKS_PIN);
@@ -496,7 +486,7 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 			| SSC_BF(TFMR_FSDEN, 0)
 			| SSC_BF(TFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(TFMR_FSLEN, 0)
-			| SSC_BF(TFMR_DATNB, 0)
+			| SSC_BF(TFMR_DATNB, (channels - 1))
 			| SSC_BIT(TFMR_MSBF)
 			| SSC_BF(TFMR_DATDEF, 0)
 			| SSC_BF(TFMR_DATLEN, (bits - 1));
diff --git a/sound/soc/codecs/sgtl5000.c b/sound/soc/codecs/sgtl5000.c
index c40b7ca..87cbf14 100644
--- a/sound/soc/codecs/sgtl5000.c
+++ b/sound/soc/codecs/sgtl5000.c
@@ -1238,6 +1238,9 @@ static int sgtl5000_enable_regulators(struct snd_soc_codec *codec)
 	/* wait for all power rails bring up */
 	udelay(10);
 
+	/* Need 8 clocks before I2C accesses */
+	udelay(1);
+
 	/* read chip information */
 	reg = snd_soc_read(codec, SGTL5000_CHIP_ID);
 	if (((reg & SGTL5000_PARTID_MASK) >> SGTL5000_PARTID_SHIFT) !=
diff --git a/sound/soc/codecs/sigmadsp.c b/sound/soc/codecs/sigmadsp.c
index 4068f24..bb3878c 100644
--- a/sound/soc/codecs/sigmadsp.c
+++ b/sound/soc/codecs/sigmadsp.c
@@ -176,6 +176,13 @@ static int _process_sigma_firmware(struct device *dev,
 		goto done;
 	}
 
+	if (ssfw_head->version != 1) {
+		dev_err(dev,
+			"Failed to load firmware: Invalid version %d. Supported firmware versions: 1\n",
+			ssfw_head->version);
+		goto done;
+	}
+
 	crc = crc32(0, fw->data + sizeof(*ssfw_head),
 			fw->size - sizeof(*ssfw_head));
 	pr_debug("%s: crc=%x\n", __func__, crc);
diff --git a/sound/soc/codecs/wm8960.c b/sound/soc/codecs/wm8960.c
index ddb0d90..a09d7eb 100644
--- a/sound/soc/codecs/wm8960.c
+++ b/sound/soc/codecs/wm8960.c
@@ -496,7 +496,7 @@ static struct {
 	{ 22050, 2 },
 	{ 24000, 2 },
 	{ 16000, 3 },
-	{ 11250, 4 },
+	{ 11025, 4 },
 	{ 12000, 4 },
 	{  8000, 5 },
 };
diff --git a/sound/usb/midi.c b/sound/usb/midi.c
index 2778815..c6ded49 100644
--- a/sound/usb/midi.c
+++ b/sound/usb/midi.c
@@ -365,6 +365,8 @@ static void snd_usbmidi_error_timer(unsigned long data)
 		if (in && in->error_resubmit) {
 			in->error_resubmit = 0;
 			for (j = 0; j < INPUT_URBS; ++j) {
+				if (atomic_read(&in->urbs[j]->use_count))
+					continue;
 				in->urbs[j]->dev = umidi->dev;
 				snd_usbmidi_submit_urb(in->urbs[j], GFP_ATOMIC);
 			}
diff --git a/sound/usb/mixer.c b/sound/usb/mixer.c
index 460e2048..5f6b1a6 100644
--- a/sound/usb/mixer.c
+++ b/sound/usb/mixer.c
@@ -909,6 +909,7 @@ static void volume_control_quirks(struct usb_mixer_elem_info *cval,
 	case USB_ID(0x046d, 0x0807): /* Logitech Webcam C500 */
 	case USB_ID(0x046d, 0x0808):
 	case USB_ID(0x046d, 0x0809):
+	case USB_ID(0x046d, 0x0819): /* Logitech Webcam C210 */
 	case USB_ID(0x046d, 0x081d): /* HD Webcam c510 */
 	case USB_ID(0x046d, 0x0991):
 	/* Most audio usb devices lie about volume resolution.
diff --git a/sound/usb/mixer_maps.c b/sound/usb/mixer_maps.c
index d1d72ff..621bc9e 100644
--- a/sound/usb/mixer_maps.c
+++ b/sound/usb/mixer_maps.c
@@ -328,8 +328,11 @@ static struct usbmix_name_map gamecom780_map[] = {
 	{}
 };
 
-static const struct usbmix_name_map kef_x300a_map[] = {
-	{ 10, NULL }, /* firmware locks up (?) when we try to access this FU */
+/* some (all?) SCMS USB3318 devices are affected by a firmware lock up
+ * when anything attempts to access FU 10 (control)
+ */
+static const struct usbmix_name_map scms_usb3318_map[] = {
+	{ 10, NULL },
 	{ 0 }
 };
 
@@ -425,8 +428,14 @@ static struct usbmix_ctl_map usbmix_ctl_maps[] = {
 		.map = ebox44_map,
 	},
 	{
+		/* KEF X300A */
 		.id = USB_ID(0x27ac, 0x1000),
-		.map = kef_x300a_map,
+		.map = scms_usb3318_map,
+	},
+	{
+		/* Arcam rPAC */
+		.id = USB_ID(0x25c4, 0x0003),
+		.map = scms_usb3318_map,
 	},
 	{ 0 } /* terminator */
 };
