From e6a48b3e560b2e046d4dd5b8a8805caf00044aa6 Mon Sep 17 00:00:00 2001
From: Tad <tad@spotco.us>
Date: Wed, 28 Oct 2015 10:31:20 -0400
Subject: [PATCH] Linux 3.4.109 -> 3.4.110

---
 Documentation/networking/pktgen.txt               | 77 +++++++++++++--------
 Makefile                                          |  2 +-
 arch/arm/net/bpf_jit_32.c                         |  2 +-
 arch/s390/crypto/ghash_s390.c                     |  2 +-
 arch/x86/include/asm/kvm_host.h                   |  2 +-
 arch/x86/kvm/i8254.c                              |  2 +-
 arch/x86/kvm/lapic.c                              |  5 +-
 arch/x86/pci/acpi.c                               | 11 +++
 drivers/acpi/acpica/utxface.c                     | 10 +--
 drivers/base/regmap/regmap.c                      |  2 +-
 drivers/char/agp/intel-gtt.c                      |  2 +-
 drivers/crypto/talitos.c                          |  1 +
 drivers/dma/mv_xor.c                              | 72 ++++++++++++--------
 drivers/dma/mv_xor.h                              |  1 +
 drivers/gpu/drm/i915/i915_gem.c                   |  3 +
 drivers/gpu/drm/radeon/evergreen.c                |  2 +-
 drivers/gpu/drm/radeon/ni.c                       |  2 +-
 drivers/gpu/drm/radeon/r600.c                     |  2 +-
 drivers/gpu/drm/radeon/radeon_cs.c                |  4 +-
 drivers/gpu/drm/radeon/radeon_irq_kms.c           |  2 +
 drivers/gpu/drm/radeon/rv770.c                    |  2 +-
 drivers/gpu/drm/radeon/si.c                       |  2 +-
 drivers/infiniband/hw/qib/qib.h                   |  4 ++
 drivers/infiniband/hw/qib/qib_keys.c              |  4 ++
 drivers/infiniband/hw/qib/qib_verbs.c             | 14 ++--
 drivers/infiniband/hw/qib/qib_verbs.h             |  2 +
 drivers/mtd/maps/dc21285.c                        |  4 +-
 drivers/mtd/mtd_blkdevs.c                         |  5 ++
 drivers/net/ethernet/stmicro/stmmac/descs.h       |  2 +
 drivers/net/ethernet/stmicro/stmmac/enh_desc.c    |  4 +-
 drivers/net/ethernet/stmicro/stmmac/norm_desc.c   |  4 +-
 drivers/net/ethernet/stmicro/stmmac/stmmac_main.c | 18 +++--
 drivers/net/wireless/ath/ath9k/main.c             | 13 ++--
 drivers/net/wireless/rndis_wlan.c                 |  6 +-
 drivers/pcmcia/topic.h                            | 16 +++++
 drivers/platform/x86/dell-laptop.c                |  8 +--
 drivers/platform/x86/ideapad-laptop.c             |  3 +-
 drivers/regulator/core.c                          |  2 +-
 drivers/scsi/ipr.h                                |  2 +-
 drivers/staging/rtl8712/rtl8712_recv.c            |  3 +-
 drivers/tty/serial/atmel_serial.c                 | 11 +--
 drivers/usb/core/hub.c                            | 81 +++++++++--------------
 drivers/watchdog/omap_wdt.c                       |  7 ++
 fs/dcache.c                                       | 10 +++
 fs/ext4/indirect.c                                |  2 +-
 fs/ext4/inode.c                                   | 22 +++++-
 fs/ext4/super.c                                   |  1 +
 fs/fuse/inode.c                                   |  2 +-
 fs/jbd2/checkpoint.c                              | 46 ++++++++++---
 fs/jbd2/commit.c                                  |  2 +-
 fs/jbd2/journal.c                                 | 49 +++++++++++---
 fs/namei.c                                        | 29 +++++++-
 fs/nfs/nfs3xdr.c                                  |  2 +-
 fs/nfs/nfs4state.c                                |  2 +
 include/acpi/actypes.h                            |  1 +
 include/linux/jbd2.h                              |  7 +-
 include/linux/nfs_xdr.h                           |  2 +-
 include/net/sctp/structs.h                        |  5 ++
 kernel/hrtimer.c                                  | 12 +++-
 kernel/rcutiny.c                                  |  5 ++
 kernel/trace/trace_events_filter.c                | 10 ++-
 lib/bitmap.c                                      | 17 ++---
 mm/kmemleak.c                                     | 19 +++++-
 net/9p/client.c                                   |  3 +-
 net/bridge/br_ioctl.c                             |  2 -
 net/bridge/br_multicast.c                         |  5 ++
 net/bridge/br_stp_if.c                            |  4 +-
 net/ceph/osdmap.c                                 |  2 +-
 net/core/pktgen.c                                 |  2 +-
 net/packet/af_packet.c                            | 20 +-----
 net/sctp/socket.c                                 | 43 +++++++++---
 net/sunrpc/backchannel_rqst.c                     |  2 +-
 sound/soc/codecs/wm8737.c                         |  6 +-
 sound/soc/codecs/wm8903.h                         |  2 +-
 sound/soc/codecs/wm8955.c                         |  2 +-
 sound/soc/codecs/wm8960.c                         |  2 +-
 76 files changed, 511 insertions(+), 252 deletions(-)

diff --git a/Documentation/networking/pktgen.txt b/Documentation/networking/pktgen.txt
index 75e4fd7..a03239c 100644
--- a/Documentation/networking/pktgen.txt
+++ b/Documentation/networking/pktgen.txt
@@ -24,17 +24,33 @@ For monitoring and control pktgen creates:
         /proc/net/pktgen/ethX
 
 
-Viewing threads
-===============
-/proc/net/pktgen/kpktgend_0 
-Name: kpktgend_0  max_before_softirq: 10000
-Running: 
-Stopped: eth1 
-Result: OK: max_before_softirq=10000
+Kernel threads
+==============
+Pktgen creates a thread for each CPU with affinity to that CPU.
+Which is controlled through procfile /proc/net/pktgen/kpktgend_X.
+
+Example: /proc/net/pktgen/kpktgend_0
+
+ Running:
+ Stopped: eth4@0
+ Result: OK: add_device=eth4@0
+
+Most important are the devices assigned to the thread.
 
-Most important the devices assigned to thread. Note! A device can only belong 
-to one thread.
+The two basic thread commands are:
+ * add_device DEVICE@NAME -- adds a single device
+ * rem_device_all         -- remove all associated devices
 
+When adding a device to a thread, a corrosponding procfile is created
+which is used for configuring this device. Thus, device names need to
+be unique.
+
+To support adding the same device to multiple threads, which is useful
+with multi queue NICs, a the device naming scheme is extended with "@":
+ device@something
+
+The part after "@" can be anything, but it is custom to use the thread
+number.
 
 Viewing devices
 ===============
@@ -42,29 +58,32 @@ Viewing devices
 Parm section holds configured info. Current hold running stats. 
 Result is printed after run or after interruption. Example:
 
-/proc/net/pktgen/eth1       
+/proc/net/pktgen/eth4@0
 
-Params: count 10000000  min_pkt_size: 60  max_pkt_size: 60
-     frags: 0  delay: 0  clone_skb: 1000000  ifname: eth1
+ Params: count 100000  min_pkt_size: 60  max_pkt_size: 60
+     frags: 0  delay: 0  clone_skb: 64  ifname: eth4@0
      flows: 0 flowlen: 0
-     dst_min: 10.10.11.2  dst_max: 
-     src_min:   src_max: 
-     src_mac: 00:00:00:00:00:00  dst_mac: 00:04:23:AC:FD:82
-     udp_src_min: 9  udp_src_max: 9  udp_dst_min: 9  udp_dst_max: 9
-     src_mac_count: 0  dst_mac_count: 0 
-     Flags: 
-Current:
-     pkts-sofar: 10000000  errors: 39664
-     started: 1103053986245187us  stopped: 1103053999346329us idle: 880401us
-     seq_num: 10000011  cur_dst_mac_offset: 0  cur_src_mac_offset: 0
-     cur_saddr: 0x10a0a0a  cur_daddr: 0x20b0a0a
-     cur_udp_dst: 9  cur_udp_src: 9
+     queue_map_min: 0  queue_map_max: 0
+     dst_min: 192.168.81.2  dst_max:
+     src_min:   src_max:
+     src_mac: 90:e2:ba:0a:56:b4 dst_mac: 00:1b:21:3c:9d:f8
+     udp_src_min: 9  udp_src_max: 109  udp_dst_min: 9  udp_dst_max: 9
+     src_mac_count: 0  dst_mac_count: 0
+     Flags: UDPSRC_RND  NO_TIMESTAMP  QUEUE_MAP_CPU
+ Current:
+     pkts-sofar: 100000  errors: 0
+     started: 623913381008us  stopped: 623913396439us idle: 25us
+     seq_num: 100001  cur_dst_mac_offset: 0  cur_src_mac_offset: 0
+     cur_saddr: 192.168.8.3  cur_daddr: 192.168.81.2
+     cur_udp_dst: 9  cur_udp_src: 42
+     cur_queue_map: 
      flows: 0
-Result: OK: 13101142(c12220741+d880401) usec, 10000000 (60byte,0frags)
-  763292pps 390Mb/sec (390805504bps) errors: 39664
+ Result: OK: 15430(c15405d25) usec, 100000 (60byte,0frags)
+  6480562pps 3110Mb/sec (3110669760bps) errors: 0
 
-Configuring threads and devices
-================================
+
+Configuring devices
+===================
 This is done via the /proc interface easiest done via pgset in the scripts
 
 Examples:
@@ -177,6 +196,8 @@ Note when adding devices to a specific CPU there good idea to also assign
 /proc/irq/XX/smp_affinity so the TX-interrupts gets bound to the same CPU.
 as this reduces cache bouncing when freeing skb's.
 
+Plus using the device flag QUEUE_MAP_CPU, which maps the SKBs TX queue
+to the running threads CPU (directly from smp_processor_id()).
 
 Current commands and configuration options
 ==========================================
diff --git a/Makefile b/Makefile
index ad126daa..45ff15e 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 4
-SUBLEVEL = 109
+SUBLEVEL = 110
 EXTRAVERSION =
 NAME = Saber-toothed Squirrel
 
diff --git a/arch/arm/net/bpf_jit_32.c b/arch/arm/net/bpf_jit_32.c
index ad94145..77026415 100644
--- a/arch/arm/net/bpf_jit_32.c
+++ b/arch/arm/net/bpf_jit_32.c
@@ -899,7 +899,7 @@ void bpf_jit_compile(struct sk_filter *fp)
 		if (ctx.imm_count)
 			kfree(ctx.imms);
 #endif
-		bpf_jit_binary_free(header);
+		module_free(NULL, ctx.target);
 		goto out;
 	}
 	build_epilogue(&ctx);
diff --git a/arch/s390/crypto/ghash_s390.c b/arch/s390/crypto/ghash_s390.c
index c2dac2e..69b5a4b 100644
--- a/arch/s390/crypto/ghash_s390.c
+++ b/arch/s390/crypto/ghash_s390.c
@@ -115,7 +115,7 @@ static int ghash_final(struct shash_desc *desc, u8 *dst)
 	struct ghash_desc_ctx *dctx = shash_desc_ctx(desc);
 
 	ghash_flush(dctx);
-	memcpy(dst, dtx->icv, GHASH_BLOCK_SIZE);
+	memcpy(dst, dctx->icv, GHASH_BLOCK_SIZE);
 
 	return 0;
 }
diff --git a/arch/x86/include/asm/kvm_host.h b/arch/x86/include/asm/kvm_host.h
index 4f78757..d60facb 100644
--- a/arch/x86/include/asm/kvm_host.h
+++ b/arch/x86/include/asm/kvm_host.h
@@ -509,7 +509,7 @@ struct kvm_arch {
 	struct kvm_pic *vpic;
 	struct kvm_ioapic *vioapic;
 	struct kvm_pit *vpit;
-	int vapics_in_nmi_mode;
+	atomic_t vapics_in_nmi_mode;
 
 	unsigned int tss_addr;
 	struct page *apic_access_page;
diff --git a/arch/x86/kvm/i8254.c b/arch/x86/kvm/i8254.c
index db336f9..eaad49a 100644
--- a/arch/x86/kvm/i8254.c
+++ b/arch/x86/kvm/i8254.c
@@ -317,7 +317,7 @@ static void pit_do_work(struct work_struct *work)
 		 * LVT0 to NMI delivery. Other PIC interrupts are just sent to
 		 * VCPU0, and only if its LVT0 is in EXTINT mode.
 		 */
-		if (kvm->arch.vapics_in_nmi_mode > 0)
+		if (atomic_read(&kvm->arch.vapics_in_nmi_mode) > 0)
 			kvm_for_each_vcpu(i, vcpu, kvm)
 				kvm_apic_nmi_wd_deliver(vcpu);
 	}
diff --git a/arch/x86/kvm/lapic.c b/arch/x86/kvm/lapic.c
index 578613d..53454a6 100644
--- a/arch/x86/kvm/lapic.c
+++ b/arch/x86/kvm/lapic.c
@@ -761,10 +761,10 @@ static void apic_manage_nmi_watchdog(struct kvm_lapic *apic, u32 lvt0_val)
 		if (!nmi_wd_enabled) {
 			apic_debug("Receive NMI setting on APIC_LVT0 "
 				   "for cpu %d\n", apic->vcpu->vcpu_id);
-			apic->vcpu->kvm->arch.vapics_in_nmi_mode++;
+			atomic_inc(&apic->vcpu->kvm->arch.vapics_in_nmi_mode);
 		}
 	} else if (nmi_wd_enabled)
-		apic->vcpu->kvm->arch.vapics_in_nmi_mode--;
+		atomic_dec(&apic->vcpu->kvm->arch.vapics_in_nmi_mode);
 }
 
 static int apic_reg_write(struct kvm_lapic *apic, u32 reg, u32 val)
@@ -1257,6 +1257,7 @@ void kvm_apic_post_state_restore(struct kvm_vcpu *vcpu)
 
 	apic_update_ppr(apic);
 	hrtimer_cancel(&apic->lapic_timer.timer);
+	apic_manage_nmi_watchdog(apic, apic_get_reg(apic, APIC_LVT0));
 	update_divide_count(apic);
 	start_apic_timer(apic);
 	apic->irr_pending = true;
diff --git a/arch/x86/pci/acpi.c b/arch/x86/pci/acpi.c
index ed2835e..65cf4f2 100644
--- a/arch/x86/pci/acpi.c
+++ b/arch/x86/pci/acpi.c
@@ -70,6 +70,17 @@ static const struct dmi_system_id pci_use_crs_table[] __initconst = {
 			DMI_MATCH(DMI_BIOS_VENDOR, "Phoenix Technologies, LTD"),
 		},
 	},
+	/* https://bugs.launchpad.net/ubuntu/+source/alsa-driver/+bug/931368 */
+	/* https://bugs.launchpad.net/ubuntu/+source/alsa-driver/+bug/1033299 */
+	{
+		.callback = set_use_crs,
+		.ident = "Foxconn K8M890-8237A",
+		.matches = {
+			DMI_MATCH(DMI_BOARD_VENDOR, "Foxconn"),
+			DMI_MATCH(DMI_BOARD_NAME, "K8M890-8237A"),
+			DMI_MATCH(DMI_BIOS_VENDOR, "Phoenix Technologies, LTD"),
+		},
+	},
 
 	/* Now for the blacklist.. */
 
diff --git a/drivers/acpi/acpica/utxface.c b/drivers/acpi/acpica/utxface.c
index afa94f5..0985ab7 100644
--- a/drivers/acpi/acpica/utxface.c
+++ b/drivers/acpi/acpica/utxface.c
@@ -166,10 +166,12 @@ acpi_status acpi_enable_subsystem(u32 flags)
 	 * Obtain a permanent mapping for the FACS. This is required for the
 	 * Global Lock and the Firmware Waking Vector
 	 */
-	status = acpi_tb_initialize_facs();
-	if (ACPI_FAILURE(status)) {
-		ACPI_WARNING((AE_INFO, "Could not map the FACS table"));
-		return_ACPI_STATUS(status);
+	if (!(flags & ACPI_NO_FACS_INIT)) {
+		status = acpi_tb_initialize_facs();
+		if (ACPI_FAILURE(status)) {
+			ACPI_WARNING((AE_INFO, "Could not map the FACS table"));
+			return_ACPI_STATUS(status);
+		}
 	}
 #endif				/* !ACPI_REDUCED_HARDWARE */
 
diff --git a/drivers/base/regmap/regmap.c b/drivers/base/regmap/regmap.c
index 8e81f85..0ac67ac 100644
--- a/drivers/base/regmap/regmap.c
+++ b/drivers/base/regmap/regmap.c
@@ -784,7 +784,7 @@ int regmap_bulk_read(struct regmap *map, unsigned int reg, void *val,
 			ret = regmap_read(map, reg + i, &ival);
 			if (ret != 0)
 				return ret;
-			memcpy(val + (i * val_bytes), &ival, val_bytes);
+			map->format.format_val(val + (i * val_bytes), ival);
 		}
 	}
 
diff --git a/drivers/char/agp/intel-gtt.c b/drivers/char/agp/intel-gtt.c
index 7f025fb..4e985cd 100644
--- a/drivers/char/agp/intel-gtt.c
+++ b/drivers/char/agp/intel-gtt.c
@@ -1194,7 +1194,7 @@ static inline int needs_idle_maps(void)
 	/* Query intel_iommu to see if we need the workaround. Presumably that
 	 * was loaded first.
 	 */
-	if ((gpu_devid == PCI_DEVICE_ID_INTEL_IRONLAKE_M_HB ||
+	if ((gpu_devid == PCI_DEVICE_ID_INTEL_IRONLAKE_D_IG ||
 	     gpu_devid == PCI_DEVICE_ID_INTEL_IRONLAKE_M_IG) &&
 	     intel_iommu_gfx_mapped)
 		return 1;
diff --git a/drivers/crypto/talitos.c b/drivers/crypto/talitos.c
index 921039e..a759fdc 100644
--- a/drivers/crypto/talitos.c
+++ b/drivers/crypto/talitos.c
@@ -2653,6 +2653,7 @@ static struct talitos_crypto_alg *talitos_alg_alloc(struct device *dev,
 		break;
 	default:
 		dev_err(dev, "unknown algorithm type %d\n", t_alg->algt.type);
+		kfree(t_alg);
 		return ERR_PTR(-EINVAL);
 	}
 
diff --git a/drivers/dma/mv_xor.c b/drivers/dma/mv_xor.c
index fa5d55f..c8fecbc 100644
--- a/drivers/dma/mv_xor.c
+++ b/drivers/dma/mv_xor.c
@@ -390,7 +390,8 @@ static void __mv_xor_slot_cleanup(struct mv_xor_chan *mv_chan)
 	dma_cookie_t cookie = 0;
 	int busy = mv_chan_is_busy(mv_chan);
 	u32 current_desc = mv_chan_get_current_desc(mv_chan);
-	int seen_current = 0;
+	int current_cleaned = 0;
+	struct mv_xor_desc *hw_desc;
 
 	dev_dbg(mv_chan->device->common.dev, "%s %d\n", __func__, __LINE__);
 	dev_dbg(mv_chan->device->common.dev, "current_desc %x\n", current_desc);
@@ -402,38 +403,57 @@ static void __mv_xor_slot_cleanup(struct mv_xor_chan *mv_chan)
 
 	list_for_each_entry_safe(iter, _iter, &mv_chan->chain,
 					chain_node) {
-		prefetch(_iter);
-		prefetch(&_iter->async_tx);
 
-		/* do not advance past the current descriptor loaded into the
-		 * hardware channel, subsequent descriptors are either in
-		 * process or have not been submitted
-		 */
-		if (seen_current)
-			break;
+		/* clean finished descriptors */
+		hw_desc = iter->hw_desc;
+		if (hw_desc->status & XOR_DESC_SUCCESS) {
+			cookie = mv_xor_run_tx_complete_actions(iter, mv_chan,
+								cookie);
 
-		/* stop the search if we reach the current descriptor and the
-		 * channel is busy
-		 */
-		if (iter->async_tx.phys == current_desc) {
-			seen_current = 1;
-			if (busy)
+			/* done processing desc, clean slot */
+			mv_xor_clean_slot(iter, mv_chan);
+
+			/* break if we did cleaned the current */
+			if (iter->async_tx.phys == current_desc) {
+				current_cleaned = 1;
+				break;
+			}
+		} else {
+			if (iter->async_tx.phys == current_desc) {
+				current_cleaned = 0;
 				break;
+			}
 		}
-
-		cookie = mv_xor_run_tx_complete_actions(iter, mv_chan, cookie);
-
-		if (mv_xor_clean_slot(iter, mv_chan))
-			break;
 	}
 
 	if ((busy == 0) && !list_empty(&mv_chan->chain)) {
-		struct mv_xor_desc_slot *chain_head;
-		chain_head = list_entry(mv_chan->chain.next,
-					struct mv_xor_desc_slot,
-					chain_node);
-
-		mv_xor_start_new_chain(mv_chan, chain_head);
+		if (current_cleaned) {
+			/*
+			 * current descriptor cleaned and removed, run
+			 * from list head
+			 */
+			iter = list_entry(mv_chan->chain.next,
+					  struct mv_xor_desc_slot,
+					  chain_node);
+			mv_xor_start_new_chain(mv_chan, iter);
+		} else {
+			if (!list_is_last(&iter->chain_node, &mv_chan->chain)) {
+				/*
+				 * descriptors are still waiting after
+				 * current, trigger them
+				 */
+				iter = list_entry(iter->chain_node.next,
+						  struct mv_xor_desc_slot,
+						  chain_node);
+				mv_xor_start_new_chain(mv_chan, iter);
+			} else {
+				/*
+				 * some descriptors are still waiting
+				 * to be cleaned
+				 */
+				tasklet_schedule(&mv_chan->irq_tasklet);
+			}
+		}
 	}
 
 	if (cookie > 0)
diff --git a/drivers/dma/mv_xor.h b/drivers/dma/mv_xor.h
index 654876b..0af0377 100644
--- a/drivers/dma/mv_xor.h
+++ b/drivers/dma/mv_xor.h
@@ -30,6 +30,7 @@
 #define XOR_OPERATION_MODE_XOR		0
 #define XOR_OPERATION_MODE_MEMCPY	2
 #define XOR_OPERATION_MODE_MEMSET	4
+#define XOR_DESC_SUCCESS		0x40000000
 
 #define XOR_CURR_DESC(chan)	(chan->mmr_base + 0x210 + (chan->idx * 4))
 #define XOR_NEXT_DESC(chan)	(chan->mmr_base + 0x200 + (chan->idx * 4))
diff --git a/drivers/gpu/drm/i915/i915_gem.c b/drivers/gpu/drm/i915/i915_gem.c
index e1c744d..b1f1d10 100644
--- a/drivers/gpu/drm/i915/i915_gem.c
+++ b/drivers/gpu/drm/i915/i915_gem.c
@@ -1779,6 +1779,9 @@ i915_gem_retire_requests_ring(struct intel_ring_buffer *ring)
 	uint32_t seqno;
 	int i;
 
+	if (list_empty(&ring->request_list))
+		return;
+
 	WARN_ON(i915_verify_lists(ring->dev));
 
 	seqno = ring->get_seqno(ring);
diff --git a/drivers/gpu/drm/radeon/evergreen.c b/drivers/gpu/drm/radeon/evergreen.c
index db4df97..c5fe79e 100644
--- a/drivers/gpu/drm/radeon/evergreen.c
+++ b/drivers/gpu/drm/radeon/evergreen.c
@@ -1079,7 +1079,7 @@ int evergreen_pcie_gart_enable(struct radeon_device *rdev)
 	WREG32(MC_VM_MB_L1_TLB2_CNTL, tmp);
 	WREG32(MC_VM_MB_L1_TLB3_CNTL, tmp);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_START_ADDR, rdev->mc.gtt_start >> 12);
-	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, (rdev->mc.gtt_end >> 12) - 1);
+	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, rdev->mc.gtt_end >> 12);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_BASE_ADDR, rdev->gart.table_addr >> 12);
 	WREG32(VM_CONTEXT0_CNTL, ENABLE_CONTEXT | PAGE_TABLE_DEPTH(0) |
 				RANGE_PROTECTION_FAULT_ENABLE_DEFAULT);
diff --git a/drivers/gpu/drm/radeon/ni.c b/drivers/gpu/drm/radeon/ni.c
index 1f45179..461262e 100644
--- a/drivers/gpu/drm/radeon/ni.c
+++ b/drivers/gpu/drm/radeon/ni.c
@@ -1075,7 +1075,7 @@ int cayman_pcie_gart_enable(struct radeon_device *rdev)
 	       L2_CACHE_BIGK_FRAGMENT_SIZE(6));
 	/* setup context0 */
 	WREG32(VM_CONTEXT0_PAGE_TABLE_START_ADDR, rdev->mc.gtt_start >> 12);
-	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, (rdev->mc.gtt_end >> 12) - 1);
+	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, rdev->mc.gtt_end >> 12);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_BASE_ADDR, rdev->gart.table_addr >> 12);
 	WREG32(VM_CONTEXT0_PROTECTION_FAULT_DEFAULT_ADDR,
 			(u32)(rdev->dummy_page.addr >> 12));
diff --git a/drivers/gpu/drm/radeon/r600.c b/drivers/gpu/drm/radeon/r600.c
index d441aed..9c7062d 100644
--- a/drivers/gpu/drm/radeon/r600.c
+++ b/drivers/gpu/drm/radeon/r600.c
@@ -930,7 +930,7 @@ int r600_pcie_gart_enable(struct radeon_device *rdev)
 	WREG32(MC_VM_L1_TLB_MCB_RD_SEM_CNTL, tmp | ENABLE_SEMAPHORE_MODE);
 	WREG32(MC_VM_L1_TLB_MCB_WR_SEM_CNTL, tmp | ENABLE_SEMAPHORE_MODE);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_START_ADDR, rdev->mc.gtt_start >> 12);
-	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, (rdev->mc.gtt_end >> 12) - 1);
+	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, rdev->mc.gtt_end >> 12);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_BASE_ADDR, rdev->gart.table_addr >> 12);
 	WREG32(VM_CONTEXT0_CNTL, ENABLE_CONTEXT | PAGE_TABLE_DEPTH(0) |
 				RANGE_PROTECTION_FAULT_ENABLE_DEFAULT);
diff --git a/drivers/gpu/drm/radeon/radeon_cs.c b/drivers/gpu/drm/radeon/radeon_cs.c
index d66d2cd..f3ee360 100644
--- a/drivers/gpu/drm/radeon/radeon_cs.c
+++ b/drivers/gpu/drm/radeon/radeon_cs.c
@@ -49,7 +49,7 @@ int radeon_cs_parser_relocs(struct radeon_cs_parser *p)
 	if (p->relocs_ptr == NULL) {
 		return -ENOMEM;
 	}
-	p->relocs = drm_calloc_large(p->nrelocs, sizeof(struct radeon_bo_list));
+	p->relocs = kcalloc(p->nrelocs, sizeof(struct radeon_cs_reloc), GFP_KERNEL);
 	if (p->relocs == NULL) {
 		return -ENOMEM;
 	}
@@ -324,7 +324,7 @@ static void radeon_cs_parser_fini(struct radeon_cs_parser *parser, int error)
 		}
 	}
 	kfree(parser->track);
-	drm_free_large(parser->relocs);
+	kfree(parser->relocs);
 	kfree(parser->relocs_ptr);
 	for (i = 0; i < parser->nchunks; i++) {
 		kfree(parser->chunks[i].kdata);
diff --git a/drivers/gpu/drm/radeon/radeon_irq_kms.c b/drivers/gpu/drm/radeon/radeon_irq_kms.c
index 645dcbf..77c456d 100644
--- a/drivers/gpu/drm/radeon/radeon_irq_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_irq_kms.c
@@ -51,10 +51,12 @@ static void radeon_hotplug_work_func(struct work_struct *work)
 	struct drm_mode_config *mode_config = &dev->mode_config;
 	struct drm_connector *connector;
 
+	mutex_lock(&mode_config->mutex);
 	if (mode_config->num_connector) {
 		list_for_each_entry(connector, &mode_config->connector_list, head)
 			radeon_connector_hotplug(connector);
 	}
+	mutex_unlock(&mode_config->mutex);
 	/* Just fire off a uevent and let userspace tell us what to do */
 	drm_helper_hpd_irq_event(dev);
 }
diff --git a/drivers/gpu/drm/radeon/rv770.c b/drivers/gpu/drm/radeon/rv770.c
index 3358730..1ec1255 100644
--- a/drivers/gpu/drm/radeon/rv770.c
+++ b/drivers/gpu/drm/radeon/rv770.c
@@ -158,7 +158,7 @@ int rv770_pcie_gart_enable(struct radeon_device *rdev)
 	WREG32(MC_VM_MB_L1_TLB2_CNTL, tmp);
 	WREG32(MC_VM_MB_L1_TLB3_CNTL, tmp);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_START_ADDR, rdev->mc.gtt_start >> 12);
-	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, (rdev->mc.gtt_end >> 12) - 1);
+	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, rdev->mc.gtt_end >> 12);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_BASE_ADDR, rdev->gart.table_addr >> 12);
 	WREG32(VM_CONTEXT0_CNTL, ENABLE_CONTEXT | PAGE_TABLE_DEPTH(0) |
 				RANGE_PROTECTION_FAULT_ENABLE_DEFAULT);
diff --git a/drivers/gpu/drm/radeon/si.c b/drivers/gpu/drm/radeon/si.c
index 3b6e641..6609a23 100644
--- a/drivers/gpu/drm/radeon/si.c
+++ b/drivers/gpu/drm/radeon/si.c
@@ -2537,7 +2537,7 @@ int si_pcie_gart_enable(struct radeon_device *rdev)
 	       L2_CACHE_BIGK_FRAGMENT_SIZE(0));
 	/* setup context0 */
 	WREG32(VM_CONTEXT0_PAGE_TABLE_START_ADDR, rdev->mc.gtt_start >> 12);
-	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, (rdev->mc.gtt_end >> 12) - 1);
+	WREG32(VM_CONTEXT0_PAGE_TABLE_END_ADDR, rdev->mc.gtt_end >> 12);
 	WREG32(VM_CONTEXT0_PAGE_TABLE_BASE_ADDR, rdev->gart.table_addr >> 12);
 	WREG32(VM_CONTEXT0_PROTECTION_FAULT_DEFAULT_ADDR,
 			(u32)(rdev->dummy_page.addr >> 12));
diff --git a/drivers/infiniband/hw/qib/qib.h b/drivers/infiniband/hw/qib/qib.h
index c7d4ef1..dcff64f 100644
--- a/drivers/infiniband/hw/qib/qib.h
+++ b/drivers/infiniband/hw/qib/qib.h
@@ -1429,6 +1429,10 @@ extern struct mutex qib_mutex;
 			qib_get_unit_name((dd)->unit), ##__VA_ARGS__); \
 	} while (0)
 
+#define qib_dev_warn(dd, fmt, ...) \
+	dev_warn(&(dd)->pcidev->dev, "%s: " fmt, \
+		qib_get_unit_name((dd)->unit), ##__VA_ARGS__)
+
 #define qib_dev_porterr(dd, port, fmt, ...) \
 	do { \
 		dev_err(&(dd)->pcidev->dev, "%s: IB%u:%u " fmt, \
diff --git a/drivers/infiniband/hw/qib/qib_keys.c b/drivers/infiniband/hw/qib/qib_keys.c
index 8fd19a4..ca6e6cf 100644
--- a/drivers/infiniband/hw/qib/qib_keys.c
+++ b/drivers/infiniband/hw/qib/qib_keys.c
@@ -69,6 +69,10 @@ int qib_alloc_lkey(struct qib_lkey_table *rkt, struct qib_mregion *mr)
 	 * unrestricted LKEY.
 	 */
 	rkt->gen++;
+	/*
+	 * bits are capped in qib_verbs.c to insure enough bits
+	 * for generation number
+	 */
 	mr->lkey = (r << (32 - ib_qib_lkey_table_size)) |
 		((((1 << (24 - ib_qib_lkey_table_size)) - 1) & rkt->gen)
 		 << 8);
diff --git a/drivers/infiniband/hw/qib/qib_verbs.c b/drivers/infiniband/hw/qib/qib_verbs.c
index 7b6c3bf..395d9d6 100644
--- a/drivers/infiniband/hw/qib/qib_verbs.c
+++ b/drivers/infiniband/hw/qib/qib_verbs.c
@@ -40,6 +40,7 @@
 #include <linux/rculist.h>
 #include <linux/mm.h>
 #include <linux/random.h>
+#include <linux/vmalloc.h>
 
 #include "qib.h"
 #include "qib_common.h"
@@ -2058,10 +2059,16 @@ int qib_register_ib_device(struct qib_devdata *dd)
 	 * the LKEY).  The remaining bits act as a generation number or tag.
 	 */
 	spin_lock_init(&dev->lk_table.lock);
+	/* insure generation is at least 4 bits see keys.c */
+	if (ib_qib_lkey_table_size > MAX_LKEY_TABLE_BITS) {
+		qib_dev_warn(dd, "lkey bits %u too large, reduced to %u\n",
+			ib_qib_lkey_table_size, MAX_LKEY_TABLE_BITS);
+		ib_qib_lkey_table_size = MAX_LKEY_TABLE_BITS;
+	}
 	dev->lk_table.max = 1 << ib_qib_lkey_table_size;
 	lk_tab_size = dev->lk_table.max * sizeof(*dev->lk_table.table);
 	dev->lk_table.table = (struct qib_mregion **)
-		__get_free_pages(GFP_KERNEL, get_order(lk_tab_size));
+		vmalloc(lk_tab_size);
 	if (dev->lk_table.table == NULL) {
 		ret = -ENOMEM;
 		goto err_lk;
@@ -2231,7 +2238,7 @@ int qib_register_ib_device(struct qib_devdata *dd)
 					sizeof(struct qib_pio_header),
 				  dev->pio_hdrs, dev->pio_hdrs_phys);
 err_hdrs:
-	free_pages((unsigned long) dev->lk_table.table, get_order(lk_tab_size));
+	vfree(dev->lk_table.table);
 err_lk:
 	kfree(dev->qp_table);
 err_qpt:
@@ -2285,7 +2292,6 @@ void qib_unregister_ib_device(struct qib_devdata *dd)
 					sizeof(struct qib_pio_header),
 				  dev->pio_hdrs, dev->pio_hdrs_phys);
 	lk_tab_size = dev->lk_table.max * sizeof(*dev->lk_table.table);
-	free_pages((unsigned long) dev->lk_table.table,
-		   get_order(lk_tab_size));
+	vfree(dev->lk_table.table);
 	kfree(dev->qp_table);
 }
diff --git a/drivers/infiniband/hw/qib/qib_verbs.h b/drivers/infiniband/hw/qib/qib_verbs.h
index 0c19ef0..66f7f62 100644
--- a/drivers/infiniband/hw/qib/qib_verbs.h
+++ b/drivers/infiniband/hw/qib/qib_verbs.h
@@ -622,6 +622,8 @@ struct qib_qpn_table {
 	struct qpn_map map[QPNMAP_ENTRIES];
 };
 
+#define MAX_LKEY_TABLE_BITS 23
+
 struct qib_lkey_table {
 	spinlock_t lock; /* protect changes in this struct */
 	u32 next;               /* next unused index (speeds search) */
diff --git a/drivers/mtd/maps/dc21285.c b/drivers/mtd/maps/dc21285.c
index 080f060..86598a1 100644
--- a/drivers/mtd/maps/dc21285.c
+++ b/drivers/mtd/maps/dc21285.c
@@ -38,9 +38,9 @@ static void nw_en_write(void)
 	 * we want to write a bit pattern XXX1 to Xilinx to enable
 	 * the write gate, which will be open for about the next 2ms.
 	 */
-	spin_lock_irqsave(&nw_gpio_lock, flags);
+	raw_spin_lock_irqsave(&nw_gpio_lock, flags);
 	nw_cpld_modify(CPLD_FLASH_WR_ENABLE, CPLD_FLASH_WR_ENABLE);
-	spin_unlock_irqrestore(&nw_gpio_lock, flags);
+	raw_spin_unlock_irqrestore(&nw_gpio_lock, flags);
 
 	/*
 	 * let the ISA bus to catch on...
diff --git a/drivers/mtd/mtd_blkdevs.c b/drivers/mtd/mtd_blkdevs.c
index 11c9dce..65dd2fd 100644
--- a/drivers/mtd/mtd_blkdevs.c
+++ b/drivers/mtd/mtd_blkdevs.c
@@ -214,6 +214,7 @@ static int blktrans_open(struct block_device *bdev, fmode_t mode)
 		return -ERESTARTSYS; /* FIXME: busy loop! -arnd*/
 
 	mutex_lock(&dev->lock);
+	mutex_lock(&mtd_table_mutex);
 
 	if (dev->open)
 		goto unlock;
@@ -237,6 +238,7 @@ static int blktrans_open(struct block_device *bdev, fmode_t mode)
 
 unlock:
 	dev->open++;
+	mutex_unlock(&mtd_table_mutex);
 	mutex_unlock(&dev->lock);
 	blktrans_dev_put(dev);
 	return ret;
@@ -247,6 +249,7 @@ static int blktrans_open(struct block_device *bdev, fmode_t mode)
 error_put:
 	module_put(dev->tr->owner);
 	kref_put(&dev->ref, blktrans_dev_release);
+	mutex_unlock(&mtd_table_mutex);
 	mutex_unlock(&dev->lock);
 	blktrans_dev_put(dev);
 	return ret;
@@ -261,6 +264,7 @@ static int blktrans_release(struct gendisk *disk, fmode_t mode)
 		return ret;
 
 	mutex_lock(&dev->lock);
+	mutex_lock(&mtd_table_mutex);
 
 	if (--dev->open)
 		goto unlock;
@@ -273,6 +277,7 @@ static int blktrans_release(struct gendisk *disk, fmode_t mode)
 		__put_mtd_device(dev->mtd);
 	}
 unlock:
+	mutex_unlock(&mtd_table_mutex);
 	mutex_unlock(&dev->lock);
 	blktrans_dev_put(dev);
 	return ret;
diff --git a/drivers/net/ethernet/stmicro/stmmac/descs.h b/drivers/net/ethernet/stmicro/stmmac/descs.h
index 9820ec8..e93a0bf 100644
--- a/drivers/net/ethernet/stmicro/stmmac/descs.h
+++ b/drivers/net/ethernet/stmicro/stmmac/descs.h
@@ -153,6 +153,8 @@ struct dma_desc {
 			u32 buffer2_size:13;
 			u32 reserved4:3;
 		} etx;		/* -- enhanced -- */
+
+		u64 all_flags;
 	} des01;
 	unsigned int des2;
 	unsigned int des3;
diff --git a/drivers/net/ethernet/stmicro/stmmac/enh_desc.c b/drivers/net/ethernet/stmicro/stmmac/enh_desc.c
index ad1b627..e0db6f6 100644
--- a/drivers/net/ethernet/stmicro/stmmac/enh_desc.c
+++ b/drivers/net/ethernet/stmicro/stmmac/enh_desc.c
@@ -232,6 +232,7 @@ static void enh_desc_init_rx_desc(struct dma_desc *p, unsigned int ring_size,
 {
 	int i;
 	for (i = 0; i < ring_size; i++) {
+		p->des01.all_flags = 0;
 		p->des01.erx.own = 1;
 		p->des01.erx.buffer1_size = BUF_SIZE_8KiB - 1;
 
@@ -248,7 +249,7 @@ static void enh_desc_init_tx_desc(struct dma_desc *p, unsigned int ring_size)
 	int i;
 
 	for (i = 0; i < ring_size; i++) {
-		p->des01.etx.own = 0;
+		p->des01.all_flags = 0;
 		ehn_desc_tx_set_on_ring_chain(p, (i == ring_size - 1));
 		p++;
 	}
@@ -271,6 +272,7 @@ static void enh_desc_set_tx_owner(struct dma_desc *p)
 
 static void enh_desc_set_rx_owner(struct dma_desc *p)
 {
+	p->des01.all_flags = 0;
 	p->des01.erx.own = 1;
 }
 
diff --git a/drivers/net/ethernet/stmicro/stmmac/norm_desc.c b/drivers/net/ethernet/stmicro/stmmac/norm_desc.c
index 25953bb..9703340 100644
--- a/drivers/net/ethernet/stmicro/stmmac/norm_desc.c
+++ b/drivers/net/ethernet/stmicro/stmmac/norm_desc.c
@@ -126,6 +126,7 @@ static void ndesc_init_rx_desc(struct dma_desc *p, unsigned int ring_size,
 {
 	int i;
 	for (i = 0; i < ring_size; i++) {
+		p->des01.all_flags = 0;
 		p->des01.rx.own = 1;
 		p->des01.rx.buffer1_size = BUF_SIZE_2KiB - 1;
 
@@ -141,7 +142,7 @@ static void ndesc_init_tx_desc(struct dma_desc *p, unsigned int ring_size)
 {
 	int i;
 	for (i = 0; i < ring_size; i++) {
-		p->des01.tx.own = 0;
+		p->des01.all_flags = 0;
 		ndesc_tx_set_on_ring_chain(p, (i == (ring_size - 1)));
 		p++;
 	}
@@ -164,6 +165,7 @@ static void ndesc_set_tx_owner(struct dma_desc *p)
 
 static void ndesc_set_rx_owner(struct dma_desc *p)
 {
+	p->des01.all_flags = 0;
 	p->des01.rx.own = 1;
 }
 
diff --git a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
index 9bdfaba..88c8645 100644
--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
@@ -424,19 +424,17 @@ static void init_dma_desc_rings(struct net_device *dev)
 	priv->rx_skbuff =
 	    kmalloc(sizeof(struct sk_buff *) * rxsize, GFP_KERNEL);
 	priv->dma_rx =
-	    (struct dma_desc *)dma_alloc_coherent(priv->device,
-						  rxsize *
-						  sizeof(struct dma_desc),
-						  &priv->dma_rx_phy,
-						  GFP_KERNEL);
+	    (struct dma_desc *)dma_zalloc_coherent(priv->device, rxsize *
+						   sizeof(struct dma_desc),
+						   &priv->dma_rx_phy,
+						   GFP_KERNEL);
 	priv->tx_skbuff = kmalloc(sizeof(struct sk_buff *) * txsize,
 				       GFP_KERNEL);
 	priv->dma_tx =
-	    (struct dma_desc *)dma_alloc_coherent(priv->device,
-						  txsize *
-						  sizeof(struct dma_desc),
-						  &priv->dma_tx_phy,
-						  GFP_KERNEL);
+	    (struct dma_desc *)dma_zalloc_coherent(priv->device, txsize *
+						   sizeof(struct dma_desc),
+						   &priv->dma_tx_phy,
+						   GFP_KERNEL);
 
 	if ((priv->dma_rx == NULL) || (priv->dma_tx == NULL)) {
 		pr_err("%s:ERROR allocating the DMA Tx/Rx desc\n", __func__);
diff --git a/drivers/net/wireless/ath/ath9k/main.c b/drivers/net/wireless/ath/ath9k/main.c
index ef26056..7e7bd15 100644
--- a/drivers/net/wireless/ath/ath9k/main.c
+++ b/drivers/net/wireless/ath/ath9k/main.c
@@ -235,7 +235,7 @@ static bool ath_prepare_reset(struct ath_softc *sc, bool retry_tx, bool flush)
 {
 	struct ath_hw *ah = sc->sc_ah;
 	struct ath_common *common = ath9k_hw_common(ah);
-	bool ret;
+	bool ret = true;
 
 	ieee80211_stop_queues(sc->hw);
 
@@ -245,10 +245,13 @@ static bool ath_prepare_reset(struct ath_softc *sc, bool retry_tx, bool flush)
 	ath9k_debug_samp_bb_mac(sc);
 	ath9k_hw_disable_interrupts(ah);
 
-	ret = ath_drain_all_txq(sc, retry_tx);
-
-	if (!ath_stoprecv(sc))
-		ret = false;
+	if (AR_SREV_9300_20_OR_LATER(ah)) {
+		ret &= ath_stoprecv(sc);
+		ret &= ath_drain_all_txq(sc, retry_tx);
+	} else {
+		ret &= ath_drain_all_txq(sc, retry_tx);
+		ret &= ath_stoprecv(sc);
+	}
 
 	if (!flush) {
 		if (ah->caps.hw_caps & ATH9K_HW_CAP_EDMA)
diff --git a/drivers/net/wireless/rndis_wlan.c b/drivers/net/wireless/rndis_wlan.c
index d66e298..414ac49 100644
--- a/drivers/net/wireless/rndis_wlan.c
+++ b/drivers/net/wireless/rndis_wlan.c
@@ -407,9 +407,9 @@ struct ndis_80211_pmkid {
 #define CAP_MODE_80211G		4
 #define CAP_MODE_MASK		7
 
-#define WORK_LINK_UP		(1<<0)
-#define WORK_LINK_DOWN		(1<<1)
-#define WORK_SET_MULTICAST_LIST	(1<<2)
+#define WORK_LINK_UP		0
+#define WORK_LINK_DOWN		1
+#define WORK_SET_MULTICAST_LIST	2
 
 #define RNDIS_WLAN_ALG_NONE	0
 #define RNDIS_WLAN_ALG_WEP	(1<<0)
diff --git a/drivers/pcmcia/topic.h b/drivers/pcmcia/topic.h
index 615a45a..582688fe 100644
--- a/drivers/pcmcia/topic.h
+++ b/drivers/pcmcia/topic.h
@@ -104,6 +104,9 @@
 #define TOPIC_EXCA_IF_CONTROL		0x3e	/* 8 bit */
 #define TOPIC_EXCA_IFC_33V_ENA		0x01
 
+#define TOPIC_PCI_CFG_PPBCN		0x3e	/* 16-bit */
+#define TOPIC_PCI_CFG_PPBCN_WBEN	0x0400
+
 static void topic97_zoom_video(struct pcmcia_socket *sock, int onoff)
 {
 	struct yenta_socket *socket = container_of(sock, struct yenta_socket, socket);
@@ -138,6 +141,7 @@ static int topic97_override(struct yenta_socket *socket)
 static int topic95_override(struct yenta_socket *socket)
 {
 	u8 fctrl;
+	u16 ppbcn;
 
 	/* enable 3.3V support for 16bit cards */
 	fctrl = exca_readb(socket, TOPIC_EXCA_IF_CONTROL);
@@ -146,6 +150,18 @@ static int topic95_override(struct yenta_socket *socket)
 	/* tell yenta to use exca registers to power 16bit cards */
 	socket->flags |= YENTA_16BIT_POWER_EXCA | YENTA_16BIT_POWER_DF;
 
+	/* Disable write buffers to prevent lockups under load with numerous
+	   Cardbus cards, observed on Tecra 500CDT and reported elsewhere on the
+	   net.  This is not a power-on default according to the datasheet
+	   but some BIOSes seem to set it. */
+	if (pci_read_config_word(socket->dev, TOPIC_PCI_CFG_PPBCN, &ppbcn) == 0
+	    && socket->dev->revision <= 7
+	    && (ppbcn & TOPIC_PCI_CFG_PPBCN_WBEN)) {
+		ppbcn &= ~TOPIC_PCI_CFG_PPBCN_WBEN;
+		pci_write_config_word(socket->dev, TOPIC_PCI_CFG_PPBCN, ppbcn);
+		dev_info(&socket->dev->dev, "Disabled ToPIC95 Cardbus write buffers.\n");
+	}
+
 	return 0;
 }
 
diff --git a/drivers/platform/x86/dell-laptop.c b/drivers/platform/x86/dell-laptop.c
index e6c08ee..3d67591 100644
--- a/drivers/platform/x86/dell-laptop.c
+++ b/drivers/platform/x86/dell-laptop.c
@@ -216,7 +216,6 @@ static struct dmi_system_id __devinitdata dell_quirks[] = {
 };
 
 static struct calling_interface_buffer *buffer;
-static struct page *bufferpage;
 static DEFINE_MUTEX(buffer_mutex);
 
 static int hwswitch_state;
@@ -714,11 +713,10 @@ static int __init dell_init(void)
 	 * Allocate buffer below 4GB for SMI data--only 32-bit physical addr
 	 * is passed to SMI handler.
 	 */
-	bufferpage = alloc_page(GFP_KERNEL | GFP_DMA32);
+	buffer = (void *)__get_free_page(GFP_KERNEL | GFP_DMA32);
 
-	if (!bufferpage)
+	if (!buffer)
 		goto fail_buffer;
-	buffer = page_address(bufferpage);
 
 	ret = dell_setup_rfkill();
 
@@ -787,7 +785,7 @@ static int __init dell_init(void)
 fail_filter:
 	dell_cleanup_rfkill();
 fail_rfkill:
-	free_page((unsigned long)bufferpage);
+	free_page((unsigned long)buffer);
 fail_buffer:
 	platform_device_del(platform_device);
 fail_platform_device2:
diff --git a/drivers/platform/x86/ideapad-laptop.c b/drivers/platform/x86/ideapad-laptop.c
index ac902f7..34e9fcf 100644
--- a/drivers/platform/x86/ideapad-laptop.c
+++ b/drivers/platform/x86/ideapad-laptop.c
@@ -407,7 +407,8 @@ const struct ideapad_rfk_data ideapad_rfk_data[] = {
 
 static int ideapad_rfk_set(void *data, bool blocked)
 {
-	unsigned long opcode = (unsigned long)data;
+	unsigned long dev = (unsigned long)data;
+	int opcode = ideapad_rfk_data[dev].opcode;
 
 	return write_ec_cmd(ideapad_handle, opcode, !blocked);
 }
diff --git a/drivers/regulator/core.c b/drivers/regulator/core.c
index 98ccd6a..73fb775 100644
--- a/drivers/regulator/core.c
+++ b/drivers/regulator/core.c
@@ -779,7 +779,7 @@ static int suspend_prepare(struct regulator_dev *rdev, suspend_state_t state)
 static void print_constraints(struct regulator_dev *rdev)
 {
 	struct regulation_constraints *constraints = rdev->constraints;
-	char buf[80] = "";
+	char buf[160] = "";
 	int count = 0;
 	int ret;
 
diff --git a/drivers/scsi/ipr.h b/drivers/scsi/ipr.h
index 153b8bd..19ff8b2 100644
--- a/drivers/scsi/ipr.h
+++ b/drivers/scsi/ipr.h
@@ -251,7 +251,7 @@
 #define IPR_RUNTIME_RESET				0x40000000
 
 #define IPR_IPL_INIT_MIN_STAGE_TIME			5
-#define IPR_IPL_INIT_DEFAULT_STAGE_TIME                 15
+#define IPR_IPL_INIT_DEFAULT_STAGE_TIME                 30
 #define IPR_IPL_INIT_STAGE_UNKNOWN			0x0
 #define IPR_IPL_INIT_STAGE_TRANSOP			0xB0000000
 #define IPR_IPL_INIT_STAGE_MASK				0xff000000
diff --git a/drivers/staging/rtl8712/rtl8712_recv.c b/drivers/staging/rtl8712/rtl8712_recv.c
index 887a807..549b8ab 100644
--- a/drivers/staging/rtl8712/rtl8712_recv.c
+++ b/drivers/staging/rtl8712/rtl8712_recv.c
@@ -1074,7 +1074,8 @@ static int recvbuf2recvframe(struct _adapter *padapter, struct sk_buff *pskb)
 		/* for first fragment packet, driver need allocate 1536 +
 		 * drvinfo_sz + RXDESC_SIZE to defrag packet. */
 		if ((mf == 1) && (frag == 0))
-			alloc_sz = 1658;/*1658+6=1664, 1664 is 128 alignment.*/
+			/*1658+6=1664, 1664 is 128 alignment.*/
+			alloc_sz = max_t(u16, tmp_len, 1658);
 		else
 			alloc_sz = tmp_len;
 		/* 2 is for IP header 4 bytes alignment in QoS packet case.
diff --git a/drivers/tty/serial/atmel_serial.c b/drivers/tty/serial/atmel_serial.c
index ff58d28..85c28e3 100644
--- a/drivers/tty/serial/atmel_serial.c
+++ b/drivers/tty/serial/atmel_serial.c
@@ -229,8 +229,7 @@ void atmel_config_rs485(struct uart_port *port, struct serial_rs485 *rs485conf)
 	if (rs485conf->flags & SER_RS485_ENABLED) {
 		dev_dbg(port->dev, "Setting UART to RS485\n");
 		atmel_port->tx_done_mask = ATMEL_US_TXEMPTY;
-		if ((rs485conf->delay_rts_after_send) > 0)
-			UART_PUT_TTGR(port, rs485conf->delay_rts_after_send);
+		UART_PUT_TTGR(port, rs485conf->delay_rts_after_send);
 		mode |= ATMEL_US_USMODE_RS485;
 	} else {
 		dev_dbg(port->dev, "Setting UART to RS232\n");
@@ -305,9 +304,7 @@ static void atmel_set_mctrl(struct uart_port *port, u_int mctrl)
 
 	if (atmel_port->rs485.flags & SER_RS485_ENABLED) {
 		dev_dbg(port->dev, "Setting UART to RS485\n");
-		if ((atmel_port->rs485.delay_rts_after_send) > 0)
-			UART_PUT_TTGR(port,
-					atmel_port->rs485.delay_rts_after_send);
+		UART_PUT_TTGR(port, atmel_port->rs485.delay_rts_after_send);
 		mode |= ATMEL_US_USMODE_RS485;
 	} else {
 		dev_dbg(port->dev, "Setting UART to RS232\n");
@@ -1239,9 +1236,7 @@ static void atmel_set_termios(struct uart_port *port, struct ktermios *termios,
 
 	if (atmel_port->rs485.flags & SER_RS485_ENABLED) {
 		dev_dbg(port->dev, "Setting UART to RS485\n");
-		if ((atmel_port->rs485.delay_rts_after_send) > 0)
-			UART_PUT_TTGR(port,
-					atmel_port->rs485.delay_rts_after_send);
+		UART_PUT_TTGR(port, atmel_port->rs485.delay_rts_after_send);
 		mode |= ATMEL_US_USMODE_RS485;
 	} else {
 		dev_dbg(port->dev, "Setting UART to RS232\n");
diff --git a/drivers/usb/core/hub.c b/drivers/usb/core/hub.c
index 05564d2..068183f 100644
--- a/drivers/usb/core/hub.c
+++ b/drivers/usb/core/hub.c
@@ -2257,9 +2257,6 @@ static unsigned hub_is_wusb(struct usb_hub *hub)
 #define HUB_LONG_RESET_TIME	200
 #define HUB_RESET_TIMEOUT	800
 
-static int hub_port_reset(struct usb_hub *hub, int port1,
-			struct usb_device *udev, unsigned int delay, bool warm);
-
 /* Is a USB 3.0 port in the Inactive or Complinance Mode state?
  * Port worm reset is required to recover
  */
@@ -2339,44 +2336,6 @@ static int hub_port_wait_reset(struct usb_hub *hub, int port1,
 	return -EBUSY;
 }
 
-static void hub_port_finish_reset(struct usb_hub *hub, int port1,
-			struct usb_device *udev, int *status)
-{
-	switch (*status) {
-	case 0:
-		/* TRSTRCY = 10 ms; plus some extra */
-		msleep(10 + 40);
-		if (udev) {
-			struct usb_hcd *hcd = bus_to_hcd(udev->bus);
-
-			update_devnum(udev, 0);
-			/* The xHC may think the device is already reset,
-			 * so ignore the status.
-			 */
-			if (hcd->driver->reset_device)
-				hcd->driver->reset_device(hcd, udev);
-		}
-		/* FALL THROUGH */
-	case -ENOTCONN:
-	case -ENODEV:
-		clear_port_feature(hub->hdev,
-				port1, USB_PORT_FEAT_C_RESET);
-		if (hub_is_superspeed(hub->hdev)) {
-			clear_port_feature(hub->hdev, port1,
-					USB_PORT_FEAT_C_BH_PORT_RESET);
-			clear_port_feature(hub->hdev, port1,
-					USB_PORT_FEAT_C_PORT_LINK_STATE);
-			clear_port_feature(hub->hdev, port1,
-					USB_PORT_FEAT_C_CONNECTION);
-		}
-		if (udev)
-			usb_set_device_state(udev, *status
-					? USB_STATE_NOTATTACHED
-					: USB_STATE_DEFAULT);
-		break;
-	}
-}
-
 /* Handle port reset and port warm(BH) reset (for USB3 protocol ports) */
 static int hub_port_reset(struct usb_hub *hub, int port1,
 			struct usb_device *udev, unsigned int delay, bool warm)
@@ -2399,13 +2358,9 @@ static int hub_port_reset(struct usb_hub *hub, int port1,
 		 * If the caller hasn't explicitly requested a warm reset,
 		 * double check and see if one is needed.
 		 */
-		status = hub_port_status(hub, port1,
-					&portstatus, &portchange);
-		if (status < 0)
-			goto done;
-
-		if (hub_port_warm_reset_required(hub, portstatus))
-			warm = true;
+		if (hub_port_status(hub, port1, &portstatus, &portchange) == 0)
+			if (hub_port_warm_reset_required(hub, portstatus))
+				warm = true;
 	}
 
 	/* Reset the port */
@@ -2428,11 +2383,19 @@ static int hub_port_reset(struct usb_hub *hub, int port1,
 
 		/* Check for disconnect or reset */
 		if (status == 0 || status == -ENOTCONN || status == -ENODEV) {
-			hub_port_finish_reset(hub, port1, udev, &status);
+			clear_port_feature(hub->hdev, port1,
+					USB_PORT_FEAT_C_RESET);
 
 			if (!hub_is_superspeed(hub->hdev))
 				goto done;
 
+			clear_port_feature(hub->hdev, port1,
+					USB_PORT_FEAT_C_BH_PORT_RESET);
+			clear_port_feature(hub->hdev, port1,
+					USB_PORT_FEAT_C_PORT_LINK_STATE);
+			clear_port_feature(hub->hdev, port1,
+					USB_PORT_FEAT_C_CONNECTION);
+
 			/*
 			 * If a USB 3.0 device migrates from reset to an error
 			 * state, re-issue the warm reset.
@@ -2466,6 +2429,26 @@ static int hub_port_reset(struct usb_hub *hub, int port1,
 		port1);
 
 done:
+	if (status == 0) {
+		/* TRSTRCY = 10 ms; plus some extra */
+		msleep(10 + 40);
+		if (udev) {
+			struct usb_hcd *hcd = bus_to_hcd(udev->bus);
+
+			update_devnum(udev, 0);
+			/* The xHC may think the device is already reset,
+			 * so ignore the status.
+			 */
+			if (hcd->driver->reset_device)
+				hcd->driver->reset_device(hcd, udev);
+
+			usb_set_device_state(udev, USB_STATE_DEFAULT);
+		}
+	} else {
+		if (udev)
+			usb_set_device_state(udev, USB_STATE_NOTATTACHED);
+	}
+
 	if (!hub_is_superspeed(hub->hdev))
 		up_read(&ehci_cf_port_reset_rwsem);
 
diff --git a/drivers/watchdog/omap_wdt.c b/drivers/watchdog/omap_wdt.c
index 8285d65..c080be5 100644
--- a/drivers/watchdog/omap_wdt.c
+++ b/drivers/watchdog/omap_wdt.c
@@ -152,6 +152,13 @@ static int omap_wdt_open(struct inode *inode, struct file *file)
 
 	pm_runtime_get_sync(wdev->dev);
 
+	/*
+	 * Make sure the watchdog is disabled. This is unfortunately required
+	 * because writing to various registers with the watchdog running has no
+	 * effect.
+	 */
+	omap_wdt_disable(wdev);
+
 	/* initialize prescaler */
 	while (__raw_readl(base + OMAP_WATCHDOG_WPS) & 0x01)
 		cpu_relax();
diff --git a/fs/dcache.c b/fs/dcache.c
index 09e2eda..9f8c58d 100644
--- a/fs/dcache.c
+++ b/fs/dcache.c
@@ -2510,6 +2510,8 @@ static int prepend_path(const struct path *path,
 	struct dentry *dentry = path->dentry;
 	struct vfsmount *vfsmnt = path->mnt;
 	struct mount *mnt = real_mount(vfsmnt);
+	char *orig_buffer = *buffer;
+	int orig_len = *buflen;
 	bool slash = false;
 	int error = 0;
 
@@ -2517,6 +2519,14 @@ static int prepend_path(const struct path *path,
 		struct dentry * parent;
 
 		if (dentry == vfsmnt->mnt_root || IS_ROOT(dentry)) {
+			/* Escaped? */
+			if (dentry != vfsmnt->mnt_root) {
+				*buffer = orig_buffer;
+				*buflen = orig_len;
+				slash = false;
+				error = 3;
+				goto global_root;
+			}
 			/* Global root? */
 			if (!mnt_has_parent(mnt))
 				goto global_root;
diff --git a/fs/ext4/indirect.c b/fs/ext4/indirect.c
index 6dc6153..f819837 100644
--- a/fs/ext4/indirect.c
+++ b/fs/ext4/indirect.c
@@ -705,7 +705,7 @@ int ext4_ind_map_blocks(handle_t *handle, struct inode *inode,
 				       EXT4_FEATURE_RO_COMPAT_BIGALLOC)) {
 		EXT4_ERROR_INODE(inode, "Can't allocate blocks for "
 				 "non-extent mapped inodes with bigalloc");
-		return -ENOSPC;
+		return -EUCLEAN;
 	}
 
 	goal = ext4_find_goal(inode, map->m_lblk, partial);
diff --git a/fs/ext4/inode.c b/fs/ext4/inode.c
index c68d3e1..9256acb 100644
--- a/fs/ext4/inode.c
+++ b/fs/ext4/inode.c
@@ -1848,18 +1848,32 @@ static int __ext4_journalled_writepage(struct page *page,
 	page_bufs = page_buffers(page);
 	BUG_ON(!page_bufs);
 	walk_page_buffers(handle, page_bufs, 0, len, NULL, bget_one);
-	/* As soon as we unlock the page, it can go away, but we have
-	 * references to buffers so we are safe */
+	/*
+	 * We need to release the page lock before we start the
+	 * journal, so grab a reference so the page won't disappear
+	 * out from under us.
+	 */
+	get_page(page);
 	unlock_page(page);
 
 	handle = ext4_journal_start(inode, ext4_writepage_trans_blocks(inode));
 	if (IS_ERR(handle)) {
 		ret = PTR_ERR(handle);
-		goto out;
+		put_page(page);
+		goto out_no_pagelock;
 	}
 
 	BUG_ON(!ext4_handle_valid(handle));
 
+	lock_page(page);
+	put_page(page);
+	if (page->mapping != mapping) {
+		/* The page got truncated from under us */
+		ext4_journal_stop(handle);
+		ret = 0;
+		goto out;
+	}
+
 	ret = walk_page_buffers(handle, page_bufs, 0, len, NULL,
 				do_journal_get_write_access);
 
@@ -1875,6 +1889,8 @@ static int __ext4_journalled_writepage(struct page *page,
 	walk_page_buffers(handle, page_bufs, 0, len, NULL, bput_one);
 	ext4_set_inode_state(inode, EXT4_STATE_JDATA);
 out:
+	unlock_page(page);
+out_no_pagelock:
 	return ret;
 }
 
diff --git a/fs/ext4/super.c b/fs/ext4/super.c
index c222d25..c7875cb 100644
--- a/fs/ext4/super.c
+++ b/fs/ext4/super.c
@@ -889,6 +889,7 @@ static void ext4_put_super(struct super_block *sb)
 		dump_orphan_list(sb, sbi);
 	J_ASSERT(list_empty(&sbi->s_orphan));
 
+	sync_blockdev(sb->s_bdev);
 	invalidate_bdev(sb->s_bdev);
 	if (sbi->journal_bdev && sbi->journal_bdev != sb->s_bdev) {
 		/*
diff --git a/fs/fuse/inode.c b/fs/fuse/inode.c
index a5c8b34..d8bc0a8 100644
--- a/fs/fuse/inode.c
+++ b/fs/fuse/inode.c
@@ -981,6 +981,7 @@ static int fuse_fill_super(struct super_block *sb, void *data, int silent)
 		goto err_fput;
 
 	fuse_conn_init(fc);
+	fc->release = fuse_free_conn;
 
 	fc->dev = sb->s_dev;
 	fc->sb = sb;
@@ -995,7 +996,6 @@ static int fuse_fill_super(struct super_block *sb, void *data, int silent)
 		fc->dont_mask = 1;
 	sb->s_flags |= MS_POSIXACL;
 
-	fc->release = fuse_free_conn;
 	fc->flags = d.flags;
 	fc->user_id = d.user_id;
 	fc->group_id = d.group_id;
diff --git a/fs/jbd2/checkpoint.c b/fs/jbd2/checkpoint.c
index c78841e..4fd7856 100644
--- a/fs/jbd2/checkpoint.c
+++ b/fs/jbd2/checkpoint.c
@@ -440,7 +440,7 @@ int jbd2_cleanup_journal_tail(journal_t *journal)
 	unsigned long	blocknr;
 
 	if (is_journal_aborted(journal))
-		return 1;
+		return -EIO;
 
 	if (!jbd2_journal_get_log_tail(journal, &first_tid, &blocknr))
 		return 1;
@@ -455,10 +455,9 @@ int jbd2_cleanup_journal_tail(journal_t *journal)
 	 * jbd2_cleanup_journal_tail() doesn't get called all that often.
 	 */
 	if (journal->j_flags & JBD2_BARRIER)
-		blkdev_issue_flush(journal->j_fs_dev, GFP_KERNEL, NULL);
+		blkdev_issue_flush(journal->j_fs_dev, GFP_NOFS, NULL);
 
-	__jbd2_update_log_tail(journal, first_tid, blocknr);
-	return 0;
+	return __jbd2_update_log_tail(journal, first_tid, blocknr);
 }
 
 
@@ -468,14 +467,14 @@ int jbd2_cleanup_journal_tail(journal_t *journal)
  * journal_clean_one_cp_list
  *
  * Find all the written-back checkpoint buffers in the given list and
- * release them.
+ * release them. If 'destroy' is set, clean all buffers unconditionally.
  *
  * Called with the journal locked.
  * Called with j_list_lock held.
  * Returns number of buffers reaped (for debug)
  */
 
-static int journal_clean_one_cp_list(struct journal_head *jh, int *released)
+static int journal_clean_one_cp_list(struct journal_head *jh, int *released, bool destroy)
 {
 	struct journal_head *last_jh;
 	struct journal_head *next_jh = jh;
@@ -489,7 +488,10 @@ static int journal_clean_one_cp_list(struct journal_head *jh, int *released)
 	do {
 		jh = next_jh;
 		next_jh = jh->b_cpnext;
-		ret = __try_to_free_cp_buf(jh);
+		if (!destroy)
+			ret = __try_to_free_cp_buf(jh);
+		else
+			ret = __jbd2_journal_remove_checkpoint(jh) + 1;
 		if (ret) {
 			freed++;
 			if (ret == 2) {
@@ -515,12 +517,14 @@ static int journal_clean_one_cp_list(struct journal_head *jh, int *released)
  *
  * Find all the written-back checkpoint buffers in the journal and release them.
  *
+ * If 'destroy' is set, release all buffers unconditionally.
+ *
  * Called with the journal locked.
  * Called with j_list_lock held.
  * Returns number of buffers reaped (for debug)
  */
 
-int __jbd2_journal_clean_checkpoint_list(journal_t *journal)
+int __jbd2_journal_clean_checkpoint_list(journal_t *journal, bool destroy)
 {
 	transaction_t *transaction, *last_transaction, *next_transaction;
 	int ret = 0;
@@ -536,7 +540,7 @@ int __jbd2_journal_clean_checkpoint_list(journal_t *journal)
 		transaction = next_transaction;
 		next_transaction = transaction->t_cpnext;
 		ret += journal_clean_one_cp_list(transaction->
-				t_checkpoint_list, &released);
+				t_checkpoint_list, &released, destroy);
 		/*
 		 * This function only frees up some memory if possible so we
 		 * dont have an obligation to finish processing. Bail out if
@@ -552,7 +556,7 @@ int __jbd2_journal_clean_checkpoint_list(journal_t *journal)
 		 * we can possibly see not yet submitted buffers on io_list
 		 */
 		ret += journal_clean_one_cp_list(transaction->
-				t_checkpoint_io_list, &released);
+				t_checkpoint_io_list, &released, destroy);
 		if (need_resched())
 			goto out;
 	} while (transaction != last_transaction);
@@ -561,6 +565,28 @@ int __jbd2_journal_clean_checkpoint_list(journal_t *journal)
 }
 
 /*
+ * Remove buffers from all checkpoint lists as journal is aborted and we just
+ * need to free memory
+ */
+void jbd2_journal_destroy_checkpoint(journal_t *journal)
+{
+	/*
+	 * We loop because __jbd2_journal_clean_checkpoint_list() may abort
+	 * early due to a need of rescheduling.
+	 */
+	while (1) {
+		spin_lock(&journal->j_list_lock);
+		if (!journal->j_checkpoint_transactions) {
+			spin_unlock(&journal->j_list_lock);
+			break;
+		}
+		__jbd2_journal_clean_checkpoint_list(journal, true);
+		spin_unlock(&journal->j_list_lock);
+		cond_resched();
+	}
+}
+
+/*
  * journal_remove_checkpoint: called after a buffer has been committed
  * to disk (either by being write-back flushed to disk, or being
  * committed to the log).
diff --git a/fs/jbd2/commit.c b/fs/jbd2/commit.c
index a0dcbd62..259f28d 100644
--- a/fs/jbd2/commit.c
+++ b/fs/jbd2/commit.c
@@ -438,7 +438,7 @@ void jbd2_journal_commit_transaction(journal_t *journal)
 	 * frees some memory
 	 */
 	spin_lock(&journal->j_list_lock);
-	__jbd2_journal_clean_checkpoint_list(journal);
+	__jbd2_journal_clean_checkpoint_list(journal, false);
 	spin_unlock(&journal->j_list_lock);
 
 	jbd_debug(3, "JBD2: commit phase 1\n");
diff --git a/fs/jbd2/journal.c b/fs/jbd2/journal.c
index f697468..a327944 100644
--- a/fs/jbd2/journal.c
+++ b/fs/jbd2/journal.c
@@ -823,9 +823,10 @@ int jbd2_journal_get_log_tail(journal_t *journal, tid_t *tid,
  *
  * Requires j_checkpoint_mutex
  */
-void __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block)
+int __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block)
 {
 	unsigned long freed;
+	int ret;
 
 	BUG_ON(!mutex_is_locked(&journal->j_checkpoint_mutex));
 
@@ -835,7 +836,10 @@ void __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block)
 	 * space and if we lose sb update during power failure we'd replay
 	 * old transaction with possibly newly overwritten data.
 	 */
-	jbd2_journal_update_sb_log_tail(journal, tid, block, WRITE_FUA);
+	ret = jbd2_journal_update_sb_log_tail(journal, tid, block, WRITE_FUA);
+	if (ret)
+		goto out;
+
 	write_lock(&journal->j_state_lock);
 	freed = block - journal->j_tail;
 	if (block < journal->j_tail)
@@ -851,6 +855,9 @@ void __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block)
 	journal->j_tail_sequence = tid;
 	journal->j_tail = block;
 	write_unlock(&journal->j_state_lock);
+
+out:
+	return ret;
 }
 
 /*
@@ -1264,7 +1271,7 @@ static int journal_reset(journal_t *journal)
 	return jbd2_journal_start_thread(journal);
 }
 
-static void jbd2_write_superblock(journal_t *journal, int write_op)
+static int jbd2_write_superblock(journal_t *journal, int write_op)
 {
 	struct buffer_head *bh = journal->j_sb_buffer;
 	int ret;
@@ -1301,7 +1308,10 @@ static void jbd2_write_superblock(journal_t *journal, int write_op)
 		printk(KERN_ERR "JBD2: Error %d detected when updating "
 		       "journal superblock for %s.\n", ret,
 		       journal->j_devname);
+		jbd2_journal_abort(journal, ret);
 	}
+
+	return ret;
 }
 
 /**
@@ -1314,10 +1324,11 @@ static void jbd2_write_superblock(journal_t *journal, int write_op)
  * Update a journal's superblock information about log tail and write it to
  * disk, waiting for the IO to complete.
  */
-void jbd2_journal_update_sb_log_tail(journal_t *journal, tid_t tail_tid,
+int jbd2_journal_update_sb_log_tail(journal_t *journal, tid_t tail_tid,
 				     unsigned long tail_block, int write_op)
 {
 	journal_superblock_t *sb = journal->j_superblock;
+	int ret;
 
 	BUG_ON(!mutex_is_locked(&journal->j_checkpoint_mutex));
 	jbd_debug(1, "JBD2: updating superblock (start %lu, seq %u)\n",
@@ -1326,13 +1337,18 @@ void jbd2_journal_update_sb_log_tail(journal_t *journal, tid_t tail_tid,
 	sb->s_sequence = cpu_to_be32(tail_tid);
 	sb->s_start    = cpu_to_be32(tail_block);
 
-	jbd2_write_superblock(journal, write_op);
+	ret = jbd2_write_superblock(journal, write_op);
+	if (ret)
+		goto out;
 
 	/* Log is no longer empty */
 	write_lock(&journal->j_state_lock);
 	WARN_ON(!sb->s_sequence);
 	journal->j_flags &= ~JBD2_FLUSHED;
 	write_unlock(&journal->j_state_lock);
+
+out:
+	return ret;
 }
 
 /**
@@ -1575,8 +1591,17 @@ int jbd2_journal_destroy(journal_t *journal)
 	while (journal->j_checkpoint_transactions != NULL) {
 		spin_unlock(&journal->j_list_lock);
 		mutex_lock(&journal->j_checkpoint_mutex);
-		jbd2_log_do_checkpoint(journal);
+		err = jbd2_log_do_checkpoint(journal);
 		mutex_unlock(&journal->j_checkpoint_mutex);
+		/*
+		 * If checkpointing failed, just free the buffers to avoid
+		 * looping forever
+		 */
+		if (err) {
+			jbd2_journal_destroy_checkpoint(journal);
+			spin_lock(&journal->j_list_lock);
+			break;
+		}
 		spin_lock(&journal->j_list_lock);
 	}
 
@@ -1785,7 +1810,14 @@ int jbd2_journal_flush(journal_t *journal)
 		return -EIO;
 
 	mutex_lock(&journal->j_checkpoint_mutex);
-	jbd2_cleanup_journal_tail(journal);
+	if (!err) {
+		err = jbd2_cleanup_journal_tail(journal);
+		if (err < 0) {
+			mutex_unlock(&journal->j_checkpoint_mutex);
+			goto out;
+		}
+		err = 0;
+	}
 
 	/* Finally, mark the journal as really needing no recovery.
 	 * This sets s_start==0 in the underlying superblock, which is
@@ -1801,7 +1833,8 @@ int jbd2_journal_flush(journal_t *journal)
 	J_ASSERT(journal->j_head == journal->j_tail);
 	J_ASSERT(journal->j_tail_sequence == journal->j_transaction_sequence);
 	write_unlock(&journal->j_state_lock);
-	return 0;
+out:
+	return err;
 }
 
 /**
diff --git a/fs/namei.c b/fs/namei.c
index ba642f0..d7a1b84 100644
--- a/fs/namei.c
+++ b/fs/namei.c
@@ -399,6 +399,24 @@ void path_put(struct path *path)
 }
 EXPORT_SYMBOL(path_put);
 
+/**
+ * path_connected - Verify that a path->dentry is below path->mnt.mnt_root
+ * @path: nameidate to verify
+ *
+ * Rename can sometimes move a file or directory outside of a bind
+ * mount, path_connected allows those cases to be detected.
+ */
+static bool path_connected(const struct path *path)
+{
+	struct vfsmount *mnt = path->mnt;
+
+	/* Only bind mounts can have disconnected paths */
+	if (mnt->mnt_root == mnt->mnt_sb->s_root)
+		return true;
+
+	return is_subdir(path->dentry, mnt->mnt_root);
+}
+
 /*
  * Path walking has 2 modes, rcu-walk and ref-walk (see
  * Documentation/filesystems/path-lookup.txt).  In situations when we can't
@@ -947,6 +965,8 @@ static int follow_dotdot_rcu(struct nameidata *nd)
 				goto failed;
 			nd->path.dentry = parent;
 			nd->seq = seq;
+			if (unlikely(!path_connected(&nd->path)))
+				goto failed;
 			break;
 		}
 		if (!follow_up_rcu(&nd->path))
@@ -1031,7 +1051,7 @@ static void follow_mount(struct path *path)
 	}
 }
 
-static void follow_dotdot(struct nameidata *nd)
+static int follow_dotdot(struct nameidata *nd)
 {
 	if (!nd->root.mnt)
 		set_root(nd);
@@ -1047,6 +1067,10 @@ static void follow_dotdot(struct nameidata *nd)
 			/* rare case of legitimate dget_parent()... */
 			nd->path.dentry = dget_parent(nd->path.dentry);
 			dput(old);
+			if (unlikely(!path_connected(&nd->path))) {
+				path_put(&nd->path);
+				return -ENOENT;
+			}
 			break;
 		}
 		if (!follow_up(&nd->path))
@@ -1054,6 +1078,7 @@ static void follow_dotdot(struct nameidata *nd)
 	}
 	follow_mount(&nd->path);
 	nd->inode = nd->path.dentry->d_inode;
+	return 0;
 }
 
 /*
@@ -1254,7 +1279,7 @@ static inline int handle_dots(struct nameidata *nd, int type)
 			if (follow_dotdot_rcu(nd))
 				return -ECHILD;
 		} else
-			follow_dotdot(nd);
+			return follow_dotdot(nd);
 	}
 	return 0;
 }
diff --git a/fs/nfs/nfs3xdr.c b/fs/nfs/nfs3xdr.c
index a77cc9a..e60bbe2 100644
--- a/fs/nfs/nfs3xdr.c
+++ b/fs/nfs/nfs3xdr.c
@@ -1333,7 +1333,7 @@ static void nfs3_xdr_enc_setacl3args(struct rpc_rqst *req,
 	if (args->npages != 0)
 		xdr_write_pages(xdr, args->pages, 0, args->len);
 	else
-		xdr_reserve_space(xdr, NFS_ACL_INLINE_BUFSIZE);
+		xdr_reserve_space(xdr, args->len);
 
 	error = nfsacl_encode(xdr->buf, base, args->inode,
 			    (args->mask & NFS_ACL) ?
diff --git a/fs/nfs/nfs4state.c b/fs/nfs/nfs4state.c
index c4600b5..282af88 100644
--- a/fs/nfs/nfs4state.c
+++ b/fs/nfs/nfs4state.c
@@ -1279,6 +1279,8 @@ static int nfs4_reclaim_open_state(struct nfs4_state_owner *sp, const struct nfs
 				}
 				spin_unlock(&state->state_lock);
 				nfs4_put_open_state(state);
+				clear_bit(NFS_STATE_RECLAIM_NOGRACE,
+					&state->flags);
 				goto restart;
 			}
 		}
diff --git a/include/acpi/actypes.h b/include/acpi/actypes.h
index 6d52429..0460073 100644
--- a/include/acpi/actypes.h
+++ b/include/acpi/actypes.h
@@ -495,6 +495,7 @@ typedef u64 acpi_integer;
 #define ACPI_NO_ACPI_ENABLE             0x10
 #define ACPI_NO_DEVICE_INIT             0x20
 #define ACPI_NO_OBJECT_INIT             0x40
+#define ACPI_NO_FACS_INIT               0x80
 
 /*
  * Initialization state
diff --git a/include/linux/jbd2.h b/include/linux/jbd2.h
index 2ffbf99..2179d78 100644
--- a/include/linux/jbd2.h
+++ b/include/linux/jbd2.h
@@ -974,15 +974,16 @@ extern struct journal_head * jbd2_journal_get_descriptor_buffer(journal_t *);
 int jbd2_journal_next_log_block(journal_t *, unsigned long long *);
 int jbd2_journal_get_log_tail(journal_t *journal, tid_t *tid,
 			      unsigned long *block);
-void __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block);
+int __jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block);
 void jbd2_update_log_tail(journal_t *journal, tid_t tid, unsigned long block);
 
 /* Commit management */
 extern void jbd2_journal_commit_transaction(journal_t *);
 
 /* Checkpoint list management */
-int __jbd2_journal_clean_checkpoint_list(journal_t *journal);
+int __jbd2_journal_clean_checkpoint_list(journal_t *journal, bool destroy);
 int __jbd2_journal_remove_checkpoint(struct journal_head *);
+void jbd2_journal_destroy_checkpoint(journal_t *journal);
 void __jbd2_journal_insert_checkpoint(struct journal_head *, transaction_t *);
 
 
@@ -1093,7 +1094,7 @@ extern int	   jbd2_journal_recover    (journal_t *journal);
 extern int	   jbd2_journal_wipe       (journal_t *, int);
 extern int	   jbd2_journal_skip_recovery	(journal_t *);
 extern void	   jbd2_journal_update_sb_errno(journal_t *);
-extern void	   jbd2_journal_update_sb_log_tail	(journal_t *, tid_t,
+extern int	   jbd2_journal_update_sb_log_tail	(journal_t *, tid_t,
 				unsigned long, int);
 extern void	   __jbd2_journal_abort_hard	(journal_t *);
 extern void	   jbd2_journal_abort      (journal_t *, int);
diff --git a/include/linux/nfs_xdr.h b/include/linux/nfs_xdr.h
index 7ba3551..845b402 100644
--- a/include/linux/nfs_xdr.h
+++ b/include/linux/nfs_xdr.h
@@ -1061,7 +1061,7 @@ struct nfstime4 {
 };
 
 #ifdef CONFIG_NFS_V4_1
-#define NFS4_EXCHANGE_ID_LEN	(48)
+#define NFS4_EXCHANGE_ID_LEN	(127)
 struct nfs41_exchange_id_args {
 	struct nfs_client		*client;
 	nfs4_verifier			*verifier;
diff --git a/include/net/sctp/structs.h b/include/net/sctp/structs.h
index 88949a9..4ea0ec6 100644
--- a/include/net/sctp/structs.h
+++ b/include/net/sctp/structs.h
@@ -209,6 +209,7 @@ extern struct sctp_globals {
 	struct list_head addr_waitq;
 	struct timer_list addr_wq_timer;
 	struct list_head auto_asconf_splist;
+	/* Lock that protects both addr_waitq and auto_asconf_splist */
 	spinlock_t addr_wq_lock;
 
 	/* Lock that protects the local_addr_list writers */
@@ -355,6 +356,10 @@ struct sctp_sock {
 	atomic_t pd_mode;
 	/* Receive to here while partial delivery is in effect. */
 	struct sk_buff_head pd_lobby;
+
+	/* These must be the last fields, as they will skipped on copies,
+	 * like on accept and peeloff operations
+	 */
 	struct list_head auto_asconf_list;
 	int do_auto_asconf;
 };
diff --git a/kernel/hrtimer.c b/kernel/hrtimer.c
index 3c9ca94..db4dc6b 100644
--- a/kernel/hrtimer.c
+++ b/kernel/hrtimer.c
@@ -854,6 +854,9 @@ u64 hrtimer_forward(struct hrtimer *timer, ktime_t now, ktime_t interval)
 	if (delta.tv64 < 0)
 		return 0;
 
+	if (WARN_ON(timer->state & HRTIMER_STATE_ENQUEUED))
+		return 0;
+
 	if (interval.tv64 < timer->base->resolution.tv64)
 		interval.tv64 = timer->base->resolution.tv64;
 
@@ -1266,11 +1269,14 @@ static void __run_hrtimer(struct hrtimer *timer, ktime_t *now)
 	 * Note: We clear the CALLBACK bit after enqueue_hrtimer and
 	 * we do not reprogramm the event hardware. Happens either in
 	 * hrtimer_start_range_ns() or in hrtimer_interrupt()
+	 *
+	 * Note: Because we dropped the cpu_base->lock above,
+	 * hrtimer_start_range_ns() can have popped in and enqueued the timer
+	 * for us already.
 	 */
-	if (restart != HRTIMER_NORESTART) {
-		BUG_ON(timer->state != HRTIMER_STATE_CALLBACK);
+	if (restart != HRTIMER_NORESTART &&
+	    !(timer->state & HRTIMER_STATE_ENQUEUED))
 		enqueue_hrtimer(timer, base);
-	}
 
 	WARN_ON_ONCE(!(timer->state & HRTIMER_STATE_CALLBACK));
 
diff --git a/kernel/rcutiny.c b/kernel/rcutiny.c
index 37a5444..60a56f4 100644
--- a/kernel/rcutiny.c
+++ b/kernel/rcutiny.c
@@ -279,6 +279,11 @@ static void __rcu_process_callbacks(struct rcu_ctrlblk *rcp)
 
 	/* Move the ready-to-invoke callbacks to a local list. */
 	local_irq_save(flags);
+	if (rcp->donetail == &rcp->rcucblist) {
+		/* No callbacks ready, so just leave. */
+		local_irq_restore(flags);
+		return;
+	}
 	RCU_TRACE(trace_rcu_batch_start(rcp->name, 0, rcp->qlen, -1));
 	list = rcp->rcucblist;
 	rcp->rcucblist = *rcp->donetail;
diff --git a/kernel/trace/trace_events_filter.c b/kernel/trace/trace_events_filter.c
index 196f46b..b155328 100644
--- a/kernel/trace/trace_events_filter.c
+++ b/kernel/trace/trace_events_filter.c
@@ -1044,6 +1044,9 @@ static void parse_init(struct filter_parse_state *ps,
 
 static char infix_next(struct filter_parse_state *ps)
 {
+	if (!ps->infix.cnt)
+		return 0;
+
 	ps->infix.cnt--;
 
 	return ps->infix.string[ps->infix.tail++];
@@ -1059,6 +1062,9 @@ static char infix_peek(struct filter_parse_state *ps)
 
 static void infix_advance(struct filter_parse_state *ps)
 {
+	if (!ps->infix.cnt)
+		return;
+
 	ps->infix.cnt--;
 	ps->infix.tail++;
 }
@@ -1372,7 +1378,9 @@ static int check_preds(struct filter_parse_state *ps)
 		}
 		cnt--;
 		n_normal_preds++;
-		WARN_ON_ONCE(cnt < 0);
+		/* all ops should have operands */
+		if (cnt < 0)
+			break;
 	}
 
 	if (cnt != 1 || !n_normal_preds || n_logical_preds >= n_normal_preds) {
diff --git a/lib/bitmap.c b/lib/bitmap.c
index b46ce02..3ed0f82 100644
--- a/lib/bitmap.c
+++ b/lib/bitmap.c
@@ -605,12 +605,12 @@ static int __bitmap_parselist(const char *buf, unsigned int buflen,
 	unsigned a, b;
 	int c, old_c, totaldigits;
 	const char __user __force *ubuf = (const char __user __force *)buf;
-	int exp_digit, in_range;
+	int at_start, in_range;
 
 	totaldigits = c = 0;
 	bitmap_zero(maskp, nmaskbits);
 	do {
-		exp_digit = 1;
+		at_start = 1;
 		in_range = 0;
 		a = b = 0;
 
@@ -639,11 +639,10 @@ static int __bitmap_parselist(const char *buf, unsigned int buflen,
 				break;
 
 			if (c == '-') {
-				if (exp_digit || in_range)
+				if (at_start || in_range)
 					return -EINVAL;
 				b = 0;
 				in_range = 1;
-				exp_digit = 1;
 				continue;
 			}
 
@@ -653,16 +652,18 @@ static int __bitmap_parselist(const char *buf, unsigned int buflen,
 			b = b * 10 + (c - '0');
 			if (!in_range)
 				a = b;
-			exp_digit = 0;
+			at_start = 0;
 			totaldigits++;
 		}
 		if (!(a <= b))
 			return -EINVAL;
 		if (b >= nmaskbits)
 			return -ERANGE;
-		while (a <= b) {
-			set_bit(a, maskp);
-			a++;
+		if (!at_start) {
+			while (a <= b) {
+				set_bit(a, maskp);
+				a++;
+			}
 		}
 	} while (buflen && c == ',');
 	return 0;
diff --git a/mm/kmemleak.c b/mm/kmemleak.c
index ad6ee88..c74827c 100644
--- a/mm/kmemleak.c
+++ b/mm/kmemleak.c
@@ -193,6 +193,8 @@ static struct kmem_cache *scan_area_cache;
 
 /* set if tracing memory operations is enabled */
 static atomic_t kmemleak_enabled = ATOMIC_INIT(0);
+/* same as above but only for the kmemleak_free() callback */
+static int kmemleak_free_enabled;
 /* set in the late_initcall if there were no errors */
 static atomic_t kmemleak_initialized = ATOMIC_INIT(0);
 /* enables or disables early logging of the memory operations */
@@ -936,7 +938,7 @@ void __ref kmemleak_free(const void *ptr)
 {
 	pr_debug("%s(0x%p)\n", __func__, ptr);
 
-	if (atomic_read(&kmemleak_enabled) && ptr && !IS_ERR(ptr))
+	if (kmemleak_free_enabled && ptr && !IS_ERR(ptr))
 		delete_object_full((unsigned long)ptr);
 	else if (atomic_read(&kmemleak_early_log))
 		log_early(KMEMLEAK_FREE, ptr, 0, 0);
@@ -976,7 +978,7 @@ void __ref kmemleak_free_percpu(const void __percpu *ptr)
 
 	pr_debug("%s(0x%p)\n", __func__, ptr);
 
-	if (atomic_read(&kmemleak_enabled) && ptr && !IS_ERR(ptr))
+	if (kmemleak_free_enabled && ptr && !IS_ERR(ptr))
 		for_each_possible_cpu(cpu)
 			delete_object_full((unsigned long)per_cpu_ptr(ptr,
 								      cpu));
@@ -1690,6 +1692,13 @@ static void kmemleak_do_cleanup(struct work_struct *work)
 	mutex_lock(&scan_mutex);
 	stop_scan_thread();
 
+	/*
+	 * Once the scan thread has stopped, it is safe to no longer track
+	 * object freeing. Ordering of the scan thread stopping and the memory
+	 * accesses below is guaranteed by the kthread_stop() function.
+	  */
+	kmemleak_free_enabled = 0;
+
 	if (cleanup) {
 		rcu_read_lock();
 		list_for_each_entry_rcu(object, &object_list, object_list)
@@ -1717,6 +1726,8 @@ static void kmemleak_disable(void)
 	/* check whether it is too early for a kernel thread */
 	if (atomic_read(&kmemleak_initialized))
 		schedule_work(&cleanup_work);
+	else
+		kmemleak_free_enabled = 0;
 
 	pr_info("Kernel memory leak detector disabled\n");
 }
@@ -1782,8 +1793,10 @@ void __init kmemleak_init(void)
 	if (atomic_read(&kmemleak_error)) {
 		local_irq_restore(flags);
 		return;
-	} else
+	} else {
 		atomic_set(&kmemleak_enabled, 1);
+		kmemleak_free_enabled = 1;
+	}
 	local_irq_restore(flags);
 
 	/*
diff --git a/net/9p/client.c b/net/9p/client.c
index b23a17c..32df0a3 100644
--- a/net/9p/client.c
+++ b/net/9p/client.c
@@ -833,7 +833,8 @@ static struct p9_req_t *p9_client_zc_rpc(struct p9_client *c, int8_t type,
 	if (err < 0) {
 		if (err == -EIO)
 			c->status = Disconnected;
-		goto reterr;
+		if (err != -ERESTARTSYS)
+			goto reterr;
 	}
 	if (req->status == REQ_STATUS_ERROR) {
 		p9_debug(P9_DEBUG_ERROR, "req_status error %d\n", req->t_err);
diff --git a/net/bridge/br_ioctl.c b/net/bridge/br_ioctl.c
index 7222fe1..ea0e15c 100644
--- a/net/bridge/br_ioctl.c
+++ b/net/bridge/br_ioctl.c
@@ -246,9 +246,7 @@ static int old_dev_ioctl(struct net_device *dev, struct ifreq *rq, int cmd)
 		if (!capable(CAP_NET_ADMIN))
 			return -EPERM;
 
-		spin_lock_bh(&br->lock);
 		br_stp_set_bridge_priority(br, args[1]);
-		spin_unlock_bh(&br->lock);
 		return 0;
 
 	case BRCTL_SET_PORT_PRIORITY:
diff --git a/net/bridge/br_multicast.c b/net/bridge/br_multicast.c
index a41051a..87ae8c3 100644
--- a/net/bridge/br_multicast.c
+++ b/net/bridge/br_multicast.c
@@ -36,6 +36,9 @@
 #define mlock_dereference(X, br) \
 	rcu_dereference_protected(X, lockdep_is_held(&br->multicast_lock))
 
+static void br_multicast_add_router(struct net_bridge *br,
+				    struct net_bridge_port *port);
+
 #if IS_ENABLED(CONFIG_IPV6)
 static inline int ipv6_is_transient_multicast(const struct in6_addr *addr)
 {
@@ -842,6 +845,8 @@ void br_multicast_enable_port(struct net_bridge_port *port)
 		goto out;
 
 	__br_multicast_enable_port(port);
+	if (port->multicast_router == 2 && hlist_unhashed(&port->rlist))
+		br_multicast_add_router(br, port);
 
 out:
 	spin_unlock(&br->multicast_lock);
diff --git a/net/bridge/br_stp_if.c b/net/bridge/br_stp_if.c
index 2f100cc..23ea159 100644
--- a/net/bridge/br_stp_if.c
+++ b/net/bridge/br_stp_if.c
@@ -242,12 +242,13 @@ bool br_stp_recalculate_bridge_id(struct net_bridge *br)
 	return true;
 }
 
-/* called under bridge lock */
+/* Acquires and releases bridge lock */
 void br_stp_set_bridge_priority(struct net_bridge *br, u16 newprio)
 {
 	struct net_bridge_port *p;
 	int wasroot;
 
+	spin_lock_bh(&br->lock);
 	wasroot = br_is_root_bridge(br);
 
 	list_for_each_entry(p, &br->port_list, list) {
@@ -265,6 +266,7 @@ void br_stp_set_bridge_priority(struct net_bridge *br, u16 newprio)
 	br_port_state_selection(br);
 	if (br_is_root_bridge(br) && !wasroot)
 		br_become_root_bridge(br);
+	spin_unlock_bh(&br->lock);
 }
 
 /* called under bridge lock */
diff --git a/net/ceph/osdmap.c b/net/ceph/osdmap.c
index 7fbe210..d4fbcb6 100644
--- a/net/ceph/osdmap.c
+++ b/net/ceph/osdmap.c
@@ -102,7 +102,7 @@ static int crush_decode_tree_bucket(void **p, void *end,
 {
 	int j;
 	dout("crush_decode_tree_bucket %p to %p\n", *p, end);
-	ceph_decode_32_safe(p, end, b->num_nodes, bad);
+	ceph_decode_8_safe(p, end, b->num_nodes, bad);
 	b->node_weights = kcalloc(b->num_nodes, sizeof(u32), GFP_NOFS);
 	if (b->node_weights == NULL)
 		return -ENOMEM;
diff --git a/net/core/pktgen.c b/net/core/pktgen.c
index 83d5a6a..e71766c 100644
--- a/net/core/pktgen.c
+++ b/net/core/pktgen.c
@@ -554,7 +554,7 @@ static int pktgen_if_show(struct seq_file *seq, void *v)
 			   "     dst_min: %s  dst_max: %s\n",
 			   pkt_dev->dst_min, pkt_dev->dst_max);
 		seq_printf(seq,
-			   "        src_min: %s  src_max: %s\n",
+			   "     src_min: %s  src_max: %s\n",
 			   pkt_dev->src_min, pkt_dev->src_max);
 	}
 
diff --git a/net/packet/af_packet.c b/net/packet/af_packet.c
index 030bd3f..d678fda 100644
--- a/net/packet/af_packet.c
+++ b/net/packet/af_packet.c
@@ -1169,16 +1169,6 @@ static void packet_sock_destruct(struct sock *sk)
 	sk_refcnt_debug_dec(sk);
 }
 
-static int fanout_rr_next(struct packet_fanout *f, unsigned int num)
-{
-	int x = atomic_read(&f->rr_cur) + 1;
-
-	if (x >= num)
-		x = 0;
-
-	return x;
-}
-
 static struct sock *fanout_demux_hash(struct packet_fanout *f, struct sk_buff *skb, unsigned int num)
 {
 	u32 idx, hash = skb->rxhash;
@@ -1190,13 +1180,9 @@ static struct sock *fanout_demux_hash(struct packet_fanout *f, struct sk_buff *s
 
 static struct sock *fanout_demux_lb(struct packet_fanout *f, struct sk_buff *skb, unsigned int num)
 {
-	int cur, old;
+	unsigned int val = atomic_inc_return(&f->rr_cur);
 
-	cur = atomic_read(&f->rr_cur);
-	while ((old = atomic_cmpxchg(&f->rr_cur, cur,
-				     fanout_rr_next(f, num))) != cur)
-		cur = old;
-	return f->arr[cur];
+	return f->arr[val % num];
 }
 
 static struct sock *fanout_demux_cpu(struct packet_fanout *f, struct sk_buff *skb, unsigned int num)
@@ -1210,7 +1196,7 @@ static int packet_rcv_fanout(struct sk_buff *skb, struct net_device *dev,
 			     struct packet_type *pt, struct net_device *orig_dev)
 {
 	struct packet_fanout *f = pt->af_packet_priv;
-	unsigned int num = f->num_members;
+	unsigned int num = ACCESS_ONCE(f->num_members);
 	struct packet_sock *po;
 	struct sock *sk;
 
diff --git a/net/sctp/socket.c b/net/sctp/socket.c
index 0c0bd2f..bc7b5de 100644
--- a/net/sctp/socket.c
+++ b/net/sctp/socket.c
@@ -1539,8 +1539,10 @@ SCTP_STATIC void sctp_close(struct sock *sk, long timeout)
 
 	/* Supposedly, no process has access to the socket, but
 	 * the net layers still may.
+	 * Also, sctp_destroy_sock() needs to be called with addr_wq_lock
+	 * held and that should be grabbed before socket lock.
 	 */
-	sctp_local_bh_disable();
+	spin_lock_bh(&sctp_globals.addr_wq_lock);
 	sctp_bh_lock_sock(sk);
 
 	/* Hold the sock, since sk_common_release() will put sock_put()
@@ -1550,7 +1552,7 @@ SCTP_STATIC void sctp_close(struct sock *sk, long timeout)
 	sk_common_release(sk);
 
 	sctp_bh_unlock_sock(sk);
-	sctp_local_bh_enable();
+	spin_unlock_bh(&sctp_globals.addr_wq_lock);
 
 	sock_put(sk);
 
@@ -3492,6 +3494,7 @@ static int sctp_setsockopt_auto_asconf(struct sock *sk, char __user *optval,
 	if ((val && sp->do_auto_asconf) || (!val && !sp->do_auto_asconf))
 		return 0;
 
+	spin_lock_bh(&sctp_globals.addr_wq_lock);
 	if (val == 0 && sp->do_auto_asconf) {
 		list_del(&sp->auto_asconf_list);
 		sp->do_auto_asconf = 0;
@@ -3500,6 +3503,7 @@ static int sctp_setsockopt_auto_asconf(struct sock *sk, char __user *optval,
 		    &sctp_auto_asconf_splist);
 		sp->do_auto_asconf = 1;
 	}
+	spin_unlock_bh(&sctp_globals.addr_wq_lock);
 	return 0;
 }
 
@@ -3935,18 +3939,28 @@ SCTP_STATIC int sctp_init_sock(struct sock *sk)
 	local_bh_disable();
 	percpu_counter_inc(&sctp_sockets_allocated);
 	sock_prot_inuse_add(sock_net(sk), sk->sk_prot, 1);
+
+	/* Nothing can fail after this block, otherwise
+	 * sctp_destroy_sock() will be called without addr_wq_lock held
+	 */
 	if (sctp_default_auto_asconf) {
+		spin_lock(&sctp_globals.addr_wq_lock);
 		list_add_tail(&sp->auto_asconf_list,
 		    &sctp_auto_asconf_splist);
 		sp->do_auto_asconf = 1;
-	} else
+		spin_unlock(&sctp_globals.addr_wq_lock);
+	} else {
 		sp->do_auto_asconf = 0;
+	}
+
 	local_bh_enable();
 
 	return 0;
 }
 
-/* Cleanup any SCTP per socket resources.  */
+/* Cleanup any SCTP per socket resources. Must be called with
+ * sctp_globals.addr_wq_lock held if sp->do_auto_asconf is true
+ */
 SCTP_STATIC void sctp_destroy_sock(struct sock *sk)
 {
 	struct sctp_sock *sp;
@@ -6746,6 +6760,19 @@ void sctp_copy_sock(struct sock *newsk, struct sock *sk,
 	newinet->mc_list = NULL;
 }
 
+static inline void sctp_copy_descendant(struct sock *sk_to,
+					const struct sock *sk_from)
+{
+	int ancestor_size = sizeof(struct inet_sock) +
+			    sizeof(struct sctp_sock) -
+			    offsetof(struct sctp_sock, auto_asconf_list);
+
+	if (sk_from->sk_family == PF_INET6)
+		ancestor_size += sizeof(struct ipv6_pinfo);
+
+	__inet_sk_copy_descendant(sk_to, sk_from, ancestor_size);
+}
+
 /* Populate the fields of the newsk from the oldsk and migrate the assoc
  * and its messages to the newsk.
  */
@@ -6760,7 +6787,6 @@ static void sctp_sock_migrate(struct sock *oldsk, struct sock *newsk,
 	struct sk_buff *skb, *tmp;
 	struct sctp_ulpevent *event;
 	struct sctp_bind_hashbucket *head;
-	struct list_head tmplist;
 
 	/* Migrate socket buffer sizes and all the socket level options to the
 	 * new socket.
@@ -6768,12 +6794,7 @@ static void sctp_sock_migrate(struct sock *oldsk, struct sock *newsk,
 	newsk->sk_sndbuf = oldsk->sk_sndbuf;
 	newsk->sk_rcvbuf = oldsk->sk_rcvbuf;
 	/* Brute force copy old sctp opt. */
-	if (oldsp->do_auto_asconf) {
-		memcpy(&tmplist, &newsp->auto_asconf_list, sizeof(tmplist));
-		inet_sk_copy_descendant(newsk, oldsk);
-		memcpy(&newsp->auto_asconf_list, &tmplist, sizeof(tmplist));
-	} else
-		inet_sk_copy_descendant(newsk, oldsk);
+	sctp_copy_descendant(newsk, oldsk);
 
 	/* Restore the ep value that was overwritten with the above structure
 	 * copy.
diff --git a/net/sunrpc/backchannel_rqst.c b/net/sunrpc/backchannel_rqst.c
index 31def68..617b955 100644
--- a/net/sunrpc/backchannel_rqst.c
+++ b/net/sunrpc/backchannel_rqst.c
@@ -60,7 +60,7 @@ static void xprt_free_allocation(struct rpc_rqst *req)
 
 	dprintk("RPC:        free allocations for req= %p\n", req);
 	BUG_ON(test_bit(RPC_BC_PA_IN_USE, &req->rq_bc_pa_state));
-	xbufp = &req->rq_private_buf;
+	xbufp = &req->rq_rcv_buf;
 	free_page((unsigned long)xbufp->head[0].iov_base);
 	xbufp = &req->rq_snd_buf;
 	free_page((unsigned long)xbufp->head[0].iov_base);
diff --git a/sound/soc/codecs/wm8737.c b/sound/soc/codecs/wm8737.c
index 4fe9d19..80460d2 100644
--- a/sound/soc/codecs/wm8737.c
+++ b/sound/soc/codecs/wm8737.c
@@ -484,7 +484,8 @@ static int wm8737_set_bias_level(struct snd_soc_codec *codec,
 
 			/* Fast VMID ramp at 2*2.5k */
 			snd_soc_update_bits(codec, WM8737_MISC_BIAS_CONTROL,
-					    WM8737_VMIDSEL_MASK, 0x4);
+					    WM8737_VMIDSEL_MASK,
+					    2 << WM8737_VMIDSEL_SHIFT);
 
 			/* Bring VMID up */
 			snd_soc_update_bits(codec, WM8737_POWER_MANAGEMENT,
@@ -498,7 +499,8 @@ static int wm8737_set_bias_level(struct snd_soc_codec *codec,
 
 		/* VMID at 2*300k */
 		snd_soc_update_bits(codec, WM8737_MISC_BIAS_CONTROL,
-				    WM8737_VMIDSEL_MASK, 2);
+				    WM8737_VMIDSEL_MASK,
+				    1 << WM8737_VMIDSEL_SHIFT);
 
 		break;
 
diff --git a/sound/soc/codecs/wm8903.h b/sound/soc/codecs/wm8903.h
index db94931..0bb4a64 100644
--- a/sound/soc/codecs/wm8903.h
+++ b/sound/soc/codecs/wm8903.h
@@ -172,7 +172,7 @@ extern int wm8903_mic_detect(struct snd_soc_codec *codec,
 #define WM8903_VMID_BUF_ENA_WIDTH                    1  /* VMID_BUF_ENA */
 
 #define WM8903_VMID_RES_50K                          2
-#define WM8903_VMID_RES_250K                         3
+#define WM8903_VMID_RES_250K                         4
 #define WM8903_VMID_RES_5K                           6
 
 /*
diff --git a/sound/soc/codecs/wm8955.c b/sound/soc/codecs/wm8955.c
index 4696f66..07b78a9 100644
--- a/sound/soc/codecs/wm8955.c
+++ b/sound/soc/codecs/wm8955.c
@@ -298,7 +298,7 @@ static int wm8955_configure_clocking(struct snd_soc_codec *codec)
 		snd_soc_update_bits(codec, WM8955_PLL_CONTROL_2,
 				    WM8955_K_17_9_MASK,
 				    (pll.k >> 9) & WM8955_K_17_9_MASK);
-		snd_soc_update_bits(codec, WM8955_PLL_CONTROL_2,
+		snd_soc_update_bits(codec, WM8955_PLL_CONTROL_3,
 				    WM8955_K_8_0_MASK,
 				    pll.k & WM8955_K_8_0_MASK);
 		if (pll.k)
diff --git a/sound/soc/codecs/wm8960.c b/sound/soc/codecs/wm8960.c
index ed986e6..bd3c6ef 100644
--- a/sound/soc/codecs/wm8960.c
+++ b/sound/soc/codecs/wm8960.c
@@ -183,7 +183,7 @@ SOC_SINGLE("PCM Playback -6dB Switch", WM8960_DACCTL1, 7, 1, 0),
 SOC_ENUM("ADC Polarity", wm8960_enum[0]),
 SOC_SINGLE("ADC High Pass Filter Switch", WM8960_DACCTL1, 0, 1, 0),
 
-SOC_ENUM("DAC Polarity", wm8960_enum[2]),
+SOC_ENUM("DAC Polarity", wm8960_enum[1]),
 SOC_SINGLE_BOOL_EXT("DAC Deemphasis Switch", 0,
 		    wm8960_get_deemph, wm8960_put_deemph),
 
