From 25ef22166357fa72e257db6b9e56e32f676ed7ae Mon Sep 17 00:00:00 2001
From: Tad <tad@spotco.us>
Date: Wed, 28 Oct 2015 10:27:26 -0400
Subject: [PATCH] Linux 3.4.106 -> 3.4.107

---
 Documentation/kernel-parameters.txt          |   1 +
 Makefile                                     |   2 +-
 arch/alpha/mm/fault.c                        |   2 +
 arch/arm/mm/proc-xscale.S                    |   4 +-
 arch/avr32/mm/fault.c                        |   2 +
 arch/cris/mm/fault.c                         |   2 +
 arch/frv/mm/fault.c                          |   2 +
 arch/ia64/mm/fault.c                         |   2 +
 arch/m32r/mm/fault.c                         |   2 +
 arch/m68k/mm/fault.c                         |   2 +
 arch/microblaze/mm/fault.c                   |   2 +
 arch/mips/kernel/irq_cpu.c                   |   4 +
 arch/mips/kernel/smp.c                       |   2 +-
 arch/mips/loongson/common/Makefile           |   3 +-
 arch/mips/mm/fault.c                         |   2 +
 arch/mn10300/mm/fault.c                      |   2 +
 arch/openrisc/mm/fault.c                     |   2 +
 arch/parisc/mm/fault.c                       |   2 +
 arch/powerpc/mm/fault.c                      |   6 +-
 arch/powerpc/platforms/cell/spu_fault.c      |   2 +-
 arch/powerpc/xmon/xmon.c                     |   7 +-
 arch/s390/mm/fault.c                         |   6 ++
 arch/score/mm/fault.c                        |   2 +
 arch/sh/mm/fault_32.c                        |   2 +
 arch/sh/mm/tlbflush_64.c                     |   2 +
 arch/sparc/mm/fault_32.c                     |   2 +
 arch/sparc/mm/fault_64.c                     |   2 +
 arch/tile/mm/fault.c                         |   2 +
 arch/um/kernel/trap.c                        |   2 +
 arch/x86/include/asm/ldt.h                   |   7 ++
 arch/x86/include/asm/msr-index.h             |   1 +
 arch/x86/kernel/cpu/amd.c                    |  10 ++
 arch/x86/kernel/cpu/mshyperv.c               |   1 +
 arch/x86/kernel/kprobes.c                    |  20 +++-
 arch/x86/kernel/process_64.c                 | 101 +++++++++++++-----
 arch/x86/kernel/tls.c                        |  16 +++
 arch/x86/mm/fault.c                          |   2 +
 arch/x86/mm/mmap.c                           |   6 +-
 arch/x86/um/sys_call_table_32.c              |   2 +-
 arch/x86/um/sys_call_table_64.c              |   2 +-
 arch/x86/vdso/vma.c                          |  36 +++++--
 arch/xtensa/mm/fault.c                       |   2 +
 block/genhd.c                                |  11 +-
 crypto/af_alg.c                              |   3 +
 drivers/ata/ahci.c                           |  26 +++++
 drivers/ata/libata-core.c                    |   5 +-
 drivers/ata/libata-sff.c                     |  12 +++
 drivers/ata/sata_dwc_460ex.c                 |  26 +++--
 drivers/ata/sata_fsl.c                       |   2 +-
 drivers/ata/sata_sil24.c                     |   2 +-
 drivers/base/bus.c                           |   8 +-
 drivers/base/core.c                          | 111 +++++++++++++++-----
 drivers/block/drbd/drbd_req.c                |   1 +
 drivers/gpio/gpiolib.c                       | 147 +++++++++++++++------------
 drivers/gpu/drm/i915/i915_gem.c              |  14 +++
 drivers/gpu/drm/i915/intel_lvds.c            |  24 ++---
 drivers/gpu/drm/radeon/radeon_kms.c          |   2 +
 drivers/gpu/drm/radeon/radeon_ttm.c          |   2 +-
 drivers/gpu/drm/vmwgfx/vmwgfx_fence.c        |  38 ++-----
 drivers/hid/hid-roccat-pyra.c                |   7 ++
 drivers/hv/vmbus_drv.c                       |   8 +-
 drivers/i2c/busses/i2c-davinci.c             |   8 +-
 drivers/input/joystick/xpad.c                |  16 ++-
 drivers/input/serio/i8042-x86ia64io.h        |  39 +++++++
 drivers/input/serio/i8042.c                  |  14 +++
 drivers/iommu/intel-iommu.c                  |   8 +-
 drivers/mfd/tc6393xb.c                       |  13 ++-
 drivers/mtd/ubi/upd.c                        |  10 +-
 drivers/net/can/dev.c                        |   8 +-
 drivers/net/can/usb/peak_usb/pcan_usb_core.c |  17 ++--
 drivers/net/can/usb/peak_usb/pcan_usb_pro.c  |   3 +-
 drivers/net/wireless/ath/ath5k/qcu.c         |   8 +-
 drivers/net/wireless/ath/ath9k/hw.h          |   4 +-
 drivers/net/wireless/ath/ath9k/mac.c         |   9 +-
 drivers/pci/probe.c                          |   3 +
 drivers/pci/quirks.c                         |  41 +++++++-
 drivers/platform/x86/hp_accel.c              |   1 +
 drivers/regulator/core.c                     |   2 +
 drivers/s390/char/con3215.c                  |  20 +++-
 drivers/scsi/NCR5380.c                       |  12 +--
 drivers/scsi/aha1740.c                       |   2 +-
 drivers/scsi/atari_NCR5380.c                 |   2 +-
 drivers/scsi/bnx2fc/bnx2fc_fcoe.c            |   7 ++
 drivers/scsi/megaraid.c                      |   8 +-
 drivers/scsi/megaraid/megaraid_sas_base.c    |   2 +-
 drivers/scsi/sd.c                            |   5 +-
 drivers/scsi/storvsc_drv.c                   |   7 +-
 drivers/scsi/sun3_NCR5380.c                  |  10 +-
 drivers/spi/spi-dw-mid.c                     |   1 -
 drivers/spi/spi-dw.c                         |  10 +-
 drivers/staging/comedi/drivers/cb_pcidas64.c | 123 +++++++++++++---------
 drivers/staging/iio/events.h                 |   2 +-
 drivers/target/iscsi/iscsi_target_util.c     |  26 ++---
 drivers/tty/serial/samsung.c                 |   4 +
 drivers/usb/class/cdc-acm.c                  |  10 +-
 drivers/usb/core/config.c                    |  11 ++
 drivers/usb/core/quirks.c                    |  11 ++
 drivers/usb/host/pci-quirks.c                |  18 +++-
 drivers/usb/host/xhci-pci.c                  |   2 +-
 drivers/usb/host/xhci-ring.c                 |  43 ++------
 drivers/usb/host/xhci.c                      | 102 ++++++++++---------
 drivers/usb/host/xhci.h                      |   2 +-
 drivers/usb/renesas_usbhs/mod_gadget.c       |   3 +
 drivers/usb/serial/console.c                 |  15 ++-
 drivers/usb/serial/cp210x.c                  |   3 +
 drivers/usb/serial/ftdi_sio.c                |  33 ++++++
 drivers/usb/serial/ftdi_sio_ids.h            |  39 ++++++-
 drivers/usb/serial/keyspan.c                 |  97 +++++++++++-------
 drivers/usb/serial/ssu100.c                  |  11 +-
 drivers/usb/storage/scsiglue.c               |   4 +
 drivers/usb/storage/unusual_devs.h           |  14 +++
 drivers/video/logo/logo.c                    |  17 +++-
 drivers/virtio/virtio.c                      |  19 ++--
 drivers/virtio/virtio_pci.c                  |  13 +--
 fs/binfmt_elf.c                              |   5 +-
 fs/btrfs/disk-io.c                           |   6 --
 fs/btrfs/extent-tree.c                       |  10 +-
 fs/ecryptfs/file.c                           |  12 ---
 fs/ecryptfs/main.c                           |  16 ++-
 fs/fs-writeback.c                            |  28 +++--
 fs/isofs/rock.c                              |   9 ++
 fs/jfs/jfs_dtree.c                           |   4 +-
 fs/ncpfs/ioctl.c                             |   1 -
 fs/nfsd/nfs4callback.c                       |   8 +-
 fs/nilfs2/nilfs.h                            |   2 -
 fs/nilfs2/segment.c                          |  45 +++++++-
 fs/nilfs2/segment.h                          |   5 +
 fs/notify/inode_mark.c                       |  17 ++--
 fs/ocfs2/aops.c                              |  16 ++-
 fs/proc/stat.c                               |   2 +-
 fs/proc/task_mmu.c                           |  10 ++
 fs/udf/dir.c                                 |   3 +-
 fs/udf/inode.c                               |  14 +++
 fs/udf/namei.c                               |   3 +-
 fs/udf/symlink.c                             |  57 +++++++++--
 fs/udf/udfdecl.h                             |   3 +-
 fs/udf/unicode.c                             |  28 ++---
 include/linux/device.h                       |   5 +
 include/linux/kernel_stat.h                  |   5 +
 include/linux/libata.h                       |   1 +
 include/linux/mm.h                           |   7 +-
 include/linux/rmap.h                         |  10 ++
 include/linux/sysfs.h                        |   9 ++
 include/linux/time.h                         |  13 +++
 include/linux/usb/quirks.h                   |  11 ++
 include/linux/usb_usual.h                    |   4 +-
 include/linux/virtio.h                       |   6 +-
 include/linux/writeback.h                    |   1 -
 include/net/sctp/sctp.h                      |   5 +
 include/net/sctp/sm.h                        |   6 +-
 include/scsi/scsi_device.h                   |   1 +
 include/sound/ak4113.h                       |   2 +-
 include/sound/ak4114.h                       |   2 +-
 kernel/irq/internals.h                       |   8 ++
 kernel/irq/irqdesc.c                         |  52 ++++++++++
 kernel/irq/proc.c                            |  22 +++-
 kernel/sched/rt.c                            |  17 +++-
 kernel/time.c                                |   4 +
 kernel/time/ntp.c                            |  11 ++
 lib/checksum.c                               |  12 ++-
 mm/ksm.c                                     |   2 +-
 mm/memory.c                                  |  63 +++++++-----
 mm/mmap.c                                    |  14 ++-
 mm/page-writeback.c                          |  43 +++-----
 mm/rmap.c                                    |  49 ++++++++-
 net/caif/chnl_net.c                          |   1 -
 net/compat.c                                 |   7 ++
 net/core/dev.c                               |  14 +--
 net/ipv6/ip6_fib.c                           |  45 ++++----
 net/mac80211/rx.c                            |  11 +-
 net/netfilter/ipvs/ip_vs_core.c              |  32 ++++--
 net/sctp/associola.c                         |   3 +-
 net/sctp/sm_make_chunk.c                     | 104 +++++++++++--------
 net/sctp/sm_statefuns.c                      |  18 +---
 net/socket.c                                 |   3 +
 net/sunrpc/svcsock.c                         |  27 +++--
 net/wireless/nl80211.c                       |   9 +-
 scripts/recordmcount.pl                      |   1 -
 security/keys/encrypted-keys/encrypted.c     |   5 +-
 sound/core/seq/seq_dummy.c                   |  31 ------
 sound/i2c/other/ak4113.c                     |  17 ++--
 sound/i2c/other/ak4114.c                     |  18 ++--
 sound/pci/hda/hda_intel.c                    |  14 ++-
 sound/pci/hda/patch_sigmatel.c               |   4 +-
 sound/soc/atmel/atmel_ssc_dai.c              |  18 +---
 sound/soc/codecs/sgtl5000.c                  |   3 +
 sound/soc/codecs/sigmadsp.c                  |   7 ++
 sound/soc/codecs/wm8960.c                    |   2 +-
 sound/usb/midi.c                             |   2 +
 sound/usb/mixer.c                            |   1 +
 sound/usb/mixer_maps.c                       |  15 ++-
 191 files changed, 1862 insertions(+), 881 deletions(-)

diff --git a/Documentation/kernel-parameters.txt b/Documentation/kernel-parameters.txt
index 719a853..7b6fa39 100644
--- a/Documentation/kernel-parameters.txt
+++ b/Documentation/kernel-parameters.txt
@@ -988,6 +988,7 @@ bytes respectively. Such letter suffixes can also be entirely omitted.
 	i8042.notimeout	[HW] Ignore timeout condition signalled by controller
 	i8042.reset	[HW] Reset the controller during init and cleanup
 	i8042.unlock	[HW] Unlock (ignore) the keylock
+	i8042.kbdreset  [HW] Reset device connected to KBD port
 
 	i810=		[HW,DRM]
 
diff --git a/Makefile b/Makefile
index e08bf16..9830710 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 4
-SUBLEVEL = 106
+SUBLEVEL = 107
 EXTRAVERSION =
 NAME = Saber-toothed Squirrel
 
diff --git a/arch/alpha/mm/fault.c b/arch/alpha/mm/fault.c
index 5eecab1..f153733 100644
--- a/arch/alpha/mm/fault.c
+++ b/arch/alpha/mm/fault.c
@@ -149,6 +149,8 @@ do_page_fault(unsigned long address, unsigned long mmcsr,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/arm/mm/proc-xscale.S b/arch/arm/mm/proc-xscale.S
index e766f88..08b51b7 100644
--- a/arch/arm/mm/proc-xscale.S
+++ b/arch/arm/mm/proc-xscale.S
@@ -535,7 +535,7 @@ ENTRY(cpu_xscale_do_suspend)
 	mrc	p15, 0, r5, c15, c1, 0	@ CP access reg
 	mrc	p15, 0, r6, c13, c0, 0	@ PID
 	mrc	p15, 0, r7, c3, c0, 0	@ domain ID
-	mrc	p15, 0, r8, c1, c1, 0	@ auxiliary control reg
+	mrc	p15, 0, r8, c1, c0, 1	@ auxiliary control reg
 	mrc	p15, 0, r9, c1, c0, 0	@ control reg
 	bic	r4, r4, #2		@ clear frequency change bit
 	stmia	r0, {r4 - r9}		@ store cp regs
@@ -552,7 +552,7 @@ ENTRY(cpu_xscale_do_resume)
 	mcr	p15, 0, r6, c13, c0, 0	@ PID
 	mcr	p15, 0, r7, c3, c0, 0	@ domain ID
 	mcr	p15, 0, r1, c2, c0, 0	@ translation table base addr
-	mcr	p15, 0, r8, c1, c1, 0	@ auxiliary control reg
+	mcr	p15, 0, r8, c1, c0, 1	@ auxiliary control reg
 	mov	r0, r9			@ control register
 	b	cpu_resume_mmu
 ENDPROC(cpu_xscale_do_resume)
diff --git a/arch/avr32/mm/fault.c b/arch/avr32/mm/fault.c
index f7040a1..632b649 100644
--- a/arch/avr32/mm/fault.c
+++ b/arch/avr32/mm/fault.c
@@ -136,6 +136,8 @@ asmlinkage void do_page_fault(unsigned long ecr, struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/cris/mm/fault.c b/arch/cris/mm/fault.c
index b4760d8..b07c00c 100644
--- a/arch/cris/mm/fault.c
+++ b/arch/cris/mm/fault.c
@@ -167,6 +167,8 @@ do_page_fault(unsigned long address, struct pt_regs *regs,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/frv/mm/fault.c b/arch/frv/mm/fault.c
index 331c1e2..8545496 100644
--- a/arch/frv/mm/fault.c
+++ b/arch/frv/mm/fault.c
@@ -166,6 +166,8 @@ asmlinkage void do_page_fault(int datammu, unsigned long esr0, unsigned long ear
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/ia64/mm/fault.c b/arch/ia64/mm/fault.c
index 02d29c2..3c820ea 100644
--- a/arch/ia64/mm/fault.c
+++ b/arch/ia64/mm/fault.c
@@ -162,6 +162,8 @@ ia64_do_page_fault (unsigned long address, unsigned long isr, struct pt_regs *re
 		 */
 		if (fault & VM_FAULT_OOM) {
 			goto out_of_memory;
+		} else if (fault & VM_FAULT_SIGSEGV) {
+			goto bad_area;
 		} else if (fault & VM_FAULT_SIGBUS) {
 			signal = SIGBUS;
 			goto bad_area;
diff --git a/arch/m32r/mm/fault.c b/arch/m32r/mm/fault.c
index 3cdfa9c..06827fc 100644
--- a/arch/m32r/mm/fault.c
+++ b/arch/m32r/mm/fault.c
@@ -198,6 +198,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long error_code,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/m68k/mm/fault.c b/arch/m68k/mm/fault.c
index 6b020a8..8646409 100644
--- a/arch/m68k/mm/fault.c
+++ b/arch/m68k/mm/fault.c
@@ -146,6 +146,8 @@ int do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto map_err;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto bus_err;
 		BUG();
diff --git a/arch/microblaze/mm/fault.c b/arch/microblaze/mm/fault.c
index c38a265..c7fe3da 100644
--- a/arch/microblaze/mm/fault.c
+++ b/arch/microblaze/mm/fault.c
@@ -214,6 +214,8 @@ void do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/mips/kernel/irq_cpu.c b/arch/mips/kernel/irq_cpu.c
index 972263b..0ed44be 100644
--- a/arch/mips/kernel/irq_cpu.c
+++ b/arch/mips/kernel/irq_cpu.c
@@ -55,6 +55,8 @@ static struct irq_chip mips_cpu_irq_controller = {
 	.irq_mask_ack	= mask_mips_irq,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 /*
@@ -91,6 +93,8 @@ static struct irq_chip mips_mt_cpu_irq_controller = {
 	.irq_mask_ack	= mips_mt_cpu_irq_ack,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 void __init mips_cpu_irq_init(void)
diff --git a/arch/mips/kernel/smp.c b/arch/mips/kernel/smp.c
index 41079b2..1a9bcc2 100644
--- a/arch/mips/kernel/smp.c
+++ b/arch/mips/kernel/smp.c
@@ -105,10 +105,10 @@ asmlinkage __cpuinit void start_secondary(void)
 	if ((read_c0_tcbind() & TCBIND_CURTC) == 0)
 #endif /* CONFIG_MIPS_MT_SMTC */
 	cpu_probe();
-	cpu_report();
 	per_cpu_trap_init();
 	mips_clockevent_init();
 	mp_ops->init_secondary();
+	cpu_report();
 
 	/*
 	 * XXX parity protection should be folded in here when it's converted
diff --git a/arch/mips/loongson/common/Makefile b/arch/mips/loongson/common/Makefile
index e526488..ce415f7 100644
--- a/arch/mips/loongson/common/Makefile
+++ b/arch/mips/loongson/common/Makefile
@@ -10,7 +10,8 @@ obj-$(CONFIG_GENERIC_GPIO) += gpio.o
 # Serial port support
 #
 obj-$(CONFIG_EARLY_PRINTK) += early_printk.o
-obj-$(CONFIG_SERIAL_8250) += serial.o
+loongson-serial-$(CONFIG_SERIAL_8250) := serial.o
+obj-y += $(loongson-serial-m) $(loongson-serial-y)
 obj-$(CONFIG_LOONGSON_UART_BASE) += uart_base.o
 obj-$(CONFIG_LOONGSON_MC146818) += rtc.o
 
diff --git a/arch/mips/mm/fault.c b/arch/mips/mm/fault.c
index c14f6df..5c9ba6a 100644
--- a/arch/mips/mm/fault.c
+++ b/arch/mips/mm/fault.c
@@ -155,6 +155,8 @@ asmlinkage void __kprobes do_page_fault(struct pt_regs *regs, unsigned long writ
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/mn10300/mm/fault.c b/arch/mn10300/mm/fault.c
index 90f346f..eb411b3 100644
--- a/arch/mn10300/mm/fault.c
+++ b/arch/mn10300/mm/fault.c
@@ -255,6 +255,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long fault_code,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/openrisc/mm/fault.c b/arch/openrisc/mm/fault.c
index a5dce82..162abfb 100644
--- a/arch/openrisc/mm/fault.c
+++ b/arch/openrisc/mm/fault.c
@@ -163,6 +163,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long address,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/parisc/mm/fault.c b/arch/parisc/mm/fault.c
index 18162ce..a9b765a 100644
--- a/arch/parisc/mm/fault.c
+++ b/arch/parisc/mm/fault.c
@@ -210,6 +210,8 @@ void do_page_fault(struct pt_regs *regs, unsigned long code,
 		 */
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto bad_area;
 		BUG();
diff --git a/arch/powerpc/mm/fault.c b/arch/powerpc/mm/fault.c
index 08ffcf5..3d30a4a 100644
--- a/arch/powerpc/mm/fault.c
+++ b/arch/powerpc/mm/fault.c
@@ -419,7 +419,11 @@ int __kprobes do_page_fault(struct pt_regs *regs, unsigned long address,
 	 */
 	fault = handle_mm_fault(mm, vma, address, flags);
 	if (unlikely(fault & (VM_FAULT_RETRY|VM_FAULT_ERROR))) {
-		int rc = mm_fault_error(regs, address, fault);
+		int rc;
+
+		if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
+		rc = mm_fault_error(regs, address, fault);
 		if (rc >= MM_FAULT_RETURN)
 			return rc;
 	}
diff --git a/arch/powerpc/platforms/cell/spu_fault.c b/arch/powerpc/platforms/cell/spu_fault.c
index 641e727..62f3e4e 100644
--- a/arch/powerpc/platforms/cell/spu_fault.c
+++ b/arch/powerpc/platforms/cell/spu_fault.c
@@ -75,7 +75,7 @@ int spu_handle_mm_fault(struct mm_struct *mm, unsigned long ea,
 		if (*flt & VM_FAULT_OOM) {
 			ret = -ENOMEM;
 			goto out_unlock;
-		} else if (*flt & VM_FAULT_SIGBUS) {
+		} else if (*flt & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV)) {
 			ret = -EFAULT;
 			goto out_unlock;
 		}
diff --git a/arch/powerpc/xmon/xmon.c b/arch/powerpc/xmon/xmon.c
index eab3492..7729c6c 100644
--- a/arch/powerpc/xmon/xmon.c
+++ b/arch/powerpc/xmon/xmon.c
@@ -285,10 +285,11 @@ static inline void disable_surveillance(void)
 	args.token = rtas_token("set-indicator");
 	if (args.token == RTAS_UNKNOWN_SERVICE)
 		return;
-	args.nargs = 3;
-	args.nret = 1;
+	args.token = cpu_to_be32(args.token);
+	args.nargs = cpu_to_be32(3);
+	args.nret = cpu_to_be32(1);
 	args.rets = &args.args[3];
-	args.args[0] = SURVEILLANCE_TOKEN;
+	args.args[0] = cpu_to_be32(SURVEILLANCE_TOKEN);
 	args.args[1] = 0;
 	args.args[2] = 0;
 	enter_rtas(__pa(&args));
diff --git a/arch/s390/mm/fault.c b/arch/s390/mm/fault.c
index f2b11ee..68ba1bb 100644
--- a/arch/s390/mm/fault.c
+++ b/arch/s390/mm/fault.c
@@ -237,6 +237,12 @@ static noinline void do_fault_error(struct pt_regs *regs, int fault)
 				do_no_context(regs);
 			else
 				pagefault_out_of_memory();
+		} else if (fault & VM_FAULT_SIGSEGV) {
+			/* Kernel mode? Handle exceptions or die */
+			if (!user_mode(regs))
+				do_no_context(regs);
+			else
+				do_sigsegv(regs, SEGV_MAPERR);
 		} else if (fault & VM_FAULT_SIGBUS) {
 			/* Kernel mode? Handle exceptions or die */
 			if (!(regs->psw.mask & PSW_MASK_PSTATE))
diff --git a/arch/score/mm/fault.c b/arch/score/mm/fault.c
index 47b600e..b3744ca 100644
--- a/arch/score/mm/fault.c
+++ b/arch/score/mm/fault.c
@@ -110,6 +110,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long write,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/sh/mm/fault_32.c b/arch/sh/mm/fault_32.c
index e99b104..a491963 100644
--- a/arch/sh/mm/fault_32.c
+++ b/arch/sh/mm/fault_32.c
@@ -206,6 +206,8 @@ asmlinkage void __kprobes do_page_fault(struct pt_regs *regs,
 			goto out_of_memory;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		BUG();
 	}
 	if (fault & VM_FAULT_MAJOR) {
diff --git a/arch/sh/mm/tlbflush_64.c b/arch/sh/mm/tlbflush_64.c
index 11c5a18f..92f0df9 100644
--- a/arch/sh/mm/tlbflush_64.c
+++ b/arch/sh/mm/tlbflush_64.c
@@ -194,6 +194,8 @@ asmlinkage void do_page_fault(struct pt_regs *regs, unsigned long writeaccess,
 			goto out_of_memory;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		BUG();
 	}
 
diff --git a/arch/sparc/mm/fault_32.c b/arch/sparc/mm/fault_32.c
index df3155a..5c6238d 100644
--- a/arch/sparc/mm/fault_32.c
+++ b/arch/sparc/mm/fault_32.c
@@ -300,6 +300,8 @@ asmlinkage void do_sparc_fault(struct pt_regs *regs, int text_fault, int write,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/sparc/mm/fault_64.c b/arch/sparc/mm/fault_64.c
index 1387aca..0dc7b90 100644
--- a/arch/sparc/mm/fault_64.c
+++ b/arch/sparc/mm/fault_64.c
@@ -443,6 +443,8 @@ asmlinkage void __kprobes do_sparc64_fault(struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/tile/mm/fault.c b/arch/tile/mm/fault.c
index 22e58f5..a362926 100644
--- a/arch/tile/mm/fault.c
+++ b/arch/tile/mm/fault.c
@@ -433,6 +433,8 @@ static int handle_page_fault(struct pt_regs *regs,
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/arch/um/kernel/trap.c b/arch/um/kernel/trap.c
index dafc947..f79ffc9 100644
--- a/arch/um/kernel/trap.c
+++ b/arch/um/kernel/trap.c
@@ -69,6 +69,8 @@ int handle_page_fault(unsigned long address, unsigned long ip,
 		if (unlikely(fault & VM_FAULT_ERROR)) {
 			if (fault & VM_FAULT_OOM) {
 				goto out_of_memory;
+			} else if (fault & VM_FAULT_SIGSEGV) {
+				goto out;
 			} else if (fault & VM_FAULT_SIGBUS) {
 				err = -EACCES;
 				goto out;
diff --git a/arch/x86/include/asm/ldt.h b/arch/x86/include/asm/ldt.h
index 46727eb..6e1aaf7 100644
--- a/arch/x86/include/asm/ldt.h
+++ b/arch/x86/include/asm/ldt.h
@@ -28,6 +28,13 @@ struct user_desc {
 	unsigned int  seg_not_present:1;
 	unsigned int  useable:1;
 #ifdef __x86_64__
+	/*
+	 * Because this bit is not present in 32-bit user code, user
+	 * programs can pass uninitialized values here.  Therefore, in
+	 * any context in which a user_desc comes from a 32-bit program,
+	 * the kernel must act as though lm == 0, regardless of the
+	 * actual value.
+	 */
 	unsigned int  lm:1;
 #endif
 };
diff --git a/arch/x86/include/asm/msr-index.h b/arch/x86/include/asm/msr-index.h
index ccb8059..e92e1e4 100644
--- a/arch/x86/include/asm/msr-index.h
+++ b/arch/x86/include/asm/msr-index.h
@@ -130,6 +130,7 @@
 #define MSR_AMD64_PATCH_LOADER		0xc0010020
 #define MSR_AMD64_OSVW_ID_LENGTH	0xc0010140
 #define MSR_AMD64_OSVW_STATUS		0xc0010141
+#define MSR_AMD64_LS_CFG		0xc0011020
 #define MSR_AMD64_DC_CFG		0xc0011022
 #define MSR_AMD64_IBSFETCHCTL		0xc0011030
 #define MSR_AMD64_IBSFETCHLINAD		0xc0011031
diff --git a/arch/x86/kernel/cpu/amd.c b/arch/x86/kernel/cpu/amd.c
index a9c8a46..5beec8a 100644
--- a/arch/x86/kernel/cpu/amd.c
+++ b/arch/x86/kernel/cpu/amd.c
@@ -417,6 +417,16 @@ static void __cpuinit early_init_amd_mc(struct cpuinfo_x86 *c)
 
 	c->x86_coreid_bits = bits;
 #endif
+
+	/* F16h erratum 793, CVE-2013-6885 */
+	if (c->x86 == 0x16 && c->x86_model <= 0xf) {
+		u64 val;
+
+		if (!rdmsrl_amd_safe(MSR_AMD64_LS_CFG, &val) &&
+		    !(val & BIT(15)))
+			wrmsrl_amd_safe(MSR_AMD64_LS_CFG, val | BIT(15));
+	}
+
 }
 
 static void __cpuinit bsp_init_amd(struct cpuinfo_x86 *c)
diff --git a/arch/x86/kernel/cpu/mshyperv.c b/arch/x86/kernel/cpu/mshyperv.c
index 646d192..c465584 100644
--- a/arch/x86/kernel/cpu/mshyperv.c
+++ b/arch/x86/kernel/cpu/mshyperv.c
@@ -55,6 +55,7 @@ static struct clocksource hyperv_cs = {
 	.rating		= 400, /* use this when running on Hyperv*/
 	.read		= read_hv_clock,
 	.mask		= CLOCKSOURCE_MASK(64),
+	.flags		= CLOCK_SOURCE_IS_CONTINUOUS,
 };
 
 static void __init ms_hyperv_init_platform(void)
diff --git a/arch/x86/kernel/kprobes.c b/arch/x86/kernel/kprobes.c
index e213fc8..15d3c45 100644
--- a/arch/x86/kernel/kprobes.c
+++ b/arch/x86/kernel/kprobes.c
@@ -1003,6 +1003,15 @@ int __kprobes setjmp_pre_handler(struct kprobe *p, struct pt_regs *regs)
 	regs->flags &= ~X86_EFLAGS_IF;
 	trace_hardirqs_off();
 	regs->ip = (unsigned long)(jp->entry);
+
+	/*
+	 * jprobes use jprobe_return() which skips the normal return
+	 * path of the function, and this messes up the accounting of the
+	 * function graph tracer to get messed up.
+	 *
+	 * Pause function graph tracing while performing the jprobe function.
+	 */
+	pause_graph_tracing();
 	return 1;
 }
 
@@ -1028,24 +1037,25 @@ int __kprobes longjmp_break_handler(struct kprobe *p, struct pt_regs *regs)
 	struct kprobe_ctlblk *kcb = get_kprobe_ctlblk();
 	u8 *addr = (u8 *) (regs->ip - 1);
 	struct jprobe *jp = container_of(p, struct jprobe, kp);
+	void *saved_sp = kcb->jprobe_saved_sp;
 
 	if ((addr > (u8 *) jprobe_return) &&
 	    (addr < (u8 *) jprobe_return_end)) {
-		if (stack_addr(regs) != kcb->jprobe_saved_sp) {
+		if (stack_addr(regs) != saved_sp) {
 			struct pt_regs *saved_regs = &kcb->jprobe_saved_regs;
 			printk(KERN_ERR
 			       "current sp %p does not match saved sp %p\n",
-			       stack_addr(regs), kcb->jprobe_saved_sp);
+			       stack_addr(regs), saved_sp);
 			printk(KERN_ERR "Saved registers for jprobe %p\n", jp);
 			show_registers(saved_regs);
 			printk(KERN_ERR "Current registers\n");
 			show_registers(regs);
 			BUG();
 		}
+		/* It's OK to start function graph tracing again */
+		unpause_graph_tracing();
 		*regs = kcb->jprobe_saved_regs;
-		memcpy((kprobe_opcode_t *)(kcb->jprobe_saved_sp),
-		       kcb->jprobes_stack,
-		       MIN_STACK_SIZE(kcb->jprobe_saved_sp));
+		memcpy(saved_sp, kcb->jprobes_stack, MIN_STACK_SIZE(saved_sp));
 		preempt_enable_no_resched();
 		return 1;
 	}
diff --git a/arch/x86/kernel/process_64.c b/arch/x86/kernel/process_64.c
index 43d8b48..bb390e1 100644
--- a/arch/x86/kernel/process_64.c
+++ b/arch/x86/kernel/process_64.c
@@ -286,24 +286,9 @@ __switch_to(struct task_struct *prev_p, struct task_struct *next_p)
 
 	fpu = switch_fpu_prepare(prev_p, next_p, cpu);
 
-	/*
-	 * Reload esp0, LDT and the page table pointer:
-	 */
+	/* Reload esp0 and ss1. */
 	load_sp0(tss, next);
 
-	/*
-	 * Switch DS and ES.
-	 * This won't pick up thread selector changes, but I guess that is ok.
-	 */
-	savesegment(es, prev->es);
-	if (unlikely(next->es | prev->es))
-		loadsegment(es, next->es);
-
-	savesegment(ds, prev->ds);
-	if (unlikely(next->ds | prev->ds))
-		loadsegment(ds, next->ds);
-
-
 	/* We must save %fs and %gs before load_TLS() because
 	 * %fs and %gs may be cleared by load_TLS().
 	 *
@@ -312,41 +297,101 @@ __switch_to(struct task_struct *prev_p, struct task_struct *next_p)
 	savesegment(fs, fsindex);
 	savesegment(gs, gsindex);
 
+	/*
+	 * Load TLS before restoring any segments so that segment loads
+	 * reference the correct GDT entries.
+	 */
 	load_TLS(next, cpu);
 
 	/*
-	 * Leave lazy mode, flushing any hypercalls made here.
-	 * This must be done before restoring TLS segments so
-	 * the GDT and LDT are properly updated, and must be
-	 * done before math_state_restore, so the TS bit is up
-	 * to date.
+	 * Leave lazy mode, flushing any hypercalls made here.  This
+	 * must be done after loading TLS entries in the GDT but before
+	 * loading segments that might reference them, and and it must
+	 * be done before math_state_restore, so the TS bit is up to
+	 * date.
 	 */
 	arch_end_context_switch(next_p);
 
+	/* Switch DS and ES.
+	 *
+	 * Reading them only returns the selectors, but writing them (if
+	 * nonzero) loads the full descriptor from the GDT or LDT.  The
+	 * LDT for next is loaded in switch_mm, and the GDT is loaded
+	 * above.
+	 *
+	 * We therefore need to write new values to the segment
+	 * registers on every context switch unless both the new and old
+	 * values are zero.
+	 *
+	 * Note that we don't need to do anything for CS and SS, as
+	 * those are saved and restored as part of pt_regs.
+	 */
+	savesegment(es, prev->es);
+	if (unlikely(next->es | prev->es))
+		loadsegment(es, next->es);
+
+	savesegment(ds, prev->ds);
+	if (unlikely(next->ds | prev->ds))
+		loadsegment(ds, next->ds);
+
 	/*
 	 * Switch FS and GS.
 	 *
-	 * Segment register != 0 always requires a reload.  Also
-	 * reload when it has changed.  When prev process used 64bit
-	 * base always reload to avoid an information leak.
+	 * These are even more complicated than FS and GS: they have
+	 * 64-bit bases are that controlled by arch_prctl.  Those bases
+	 * only differ from the values in the GDT or LDT if the selector
+	 * is 0.
+	 *
+	 * Loading the segment register resets the hidden base part of
+	 * the register to 0 or the value from the GDT / LDT.  If the
+	 * next base address zero, writing 0 to the segment register is
+	 * much faster than using wrmsr to explicitly zero the base.
+	 *
+	 * The thread_struct.fs and thread_struct.gs values are 0
+	 * if the fs and gs bases respectively are not overridden
+	 * from the values implied by fsindex and gsindex.  They
+	 * are nonzero, and store the nonzero base addresses, if
+	 * the bases are overridden.
+	 *
+	 * (fs != 0 && fsindex != 0) || (gs != 0 && gsindex != 0) should
+	 * be impossible.
+	 *
+	 * Therefore we need to reload the segment registers if either
+	 * the old or new selector is nonzero, and we need to override
+	 * the base address if next thread expects it to be overridden.
+	 *
+	 * This code is unnecessarily slow in the case where the old and
+	 * new indexes are zero and the new base is nonzero -- it will
+	 * unnecessarily write 0 to the selector before writing the new
+	 * base address.
+	 *
+	 * Note: This all depends on arch_prctl being the only way that
+	 * user code can override the segment base.  Once wrfsbase and
+	 * wrgsbase are enabled, most of this code will need to change.
 	 */
 	if (unlikely(fsindex | next->fsindex | prev->fs)) {
 		loadsegment(fs, next->fsindex);
+
 		/*
-		 * Check if the user used a selector != 0; if yes
-		 *  clear 64bit base, since overloaded base is always
-		 *  mapped to the Null selector
+		 * If user code wrote a nonzero value to FS, then it also
+		 * cleared the overridden base address.
+		 *
+		 * XXX: if user code wrote 0 to FS and cleared the base
+		 * address itself, we won't notice and we'll incorrectly
+		 * restore the prior base address next time we reschdule
+		 * the process.
 		 */
 		if (fsindex)
 			prev->fs = 0;
 	}
-	/* when next process has a 64bit base use it */
 	if (next->fs)
 		wrmsrl(MSR_FS_BASE, next->fs);
 	prev->fsindex = fsindex;
 
 	if (unlikely(gsindex | next->gsindex | prev->gs)) {
 		load_gs_index(next->gsindex);
+
+		/* This works (and fails) the same way as fsindex above. */
 		if (gsindex)
 			prev->gs = 0;
 	}
diff --git a/arch/x86/kernel/tls.c b/arch/x86/kernel/tls.c
index 9d25a6e..fe2e363 100644
--- a/arch/x86/kernel/tls.c
+++ b/arch/x86/kernel/tls.c
@@ -60,6 +60,22 @@ static bool tls_desc_okay(const struct user_desc *info)
 	if (!info->seg_32bit)
 		return false;
 
+	/* Only allow data segments in the TLS array. */
+	if (info->contents > 1)
+		return false;
+
+	/*
+	 * Non-present segments with DPL 3 present an interesting attack
+	 * surface.  The kernel should handle such segments correctly,
+	 * but TLS is very difficult to protect in a sandbox, so prevent
+	 * such segments from being created.
+	 *
+	 * If userspace needs to remove a TLS entry, it can still delete
+	 * it outright.
+	 */
+	if (info->seg_not_present)
+		return false;
+
 	return true;
 }
 
diff --git a/arch/x86/mm/fault.c b/arch/x86/mm/fault.c
index 4a0a2e8..b723f2e 100644
--- a/arch/x86/mm/fault.c
+++ b/arch/x86/mm/fault.c
@@ -887,6 +887,8 @@ mm_fault_error(struct pt_regs *regs, unsigned long error_code,
 		if (fault & (VM_FAULT_SIGBUS|VM_FAULT_HWPOISON|
 			     VM_FAULT_HWPOISON_LARGE))
 			do_sigbus(regs, error_code, address, fault);
+		else if (fault & VM_FAULT_SIGSEGV)
+			bad_area_nosemaphore(regs, error_code, address);
 		else
 			BUG();
 	}
diff --git a/arch/x86/mm/mmap.c b/arch/x86/mm/mmap.c
index 5c1ae28..75f9e5d 100644
--- a/arch/x86/mm/mmap.c
+++ b/arch/x86/mm/mmap.c
@@ -35,12 +35,12 @@ struct __read_mostly va_alignment va_align = {
 	.flags = -1,
 };
 
-static unsigned int stack_maxrandom_size(void)
+static unsigned long stack_maxrandom_size(void)
 {
-	unsigned int max = 0;
+	unsigned long max = 0;
 	if ((current->flags & PF_RANDOMIZE) &&
 		!(current->personality & ADDR_NO_RANDOMIZE)) {
-		max = ((-1U) & STACK_RND_MASK) << PAGE_SHIFT;
+		max = ((-1UL) & STACK_RND_MASK) << PAGE_SHIFT;
 	}
 
 	return max;
diff --git a/arch/x86/um/sys_call_table_32.c b/arch/x86/um/sys_call_table_32.c
index 68d1dc9..bd8b159 100644
--- a/arch/x86/um/sys_call_table_32.c
+++ b/arch/x86/um/sys_call_table_32.c
@@ -43,7 +43,7 @@ typedef asmlinkage void (*sys_call_ptr_t)(void);
 
 extern asmlinkage void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/arch/x86/um/sys_call_table_64.c b/arch/x86/um/sys_call_table_64.c
index 9924776..cbdab94 100644
--- a/arch/x86/um/sys_call_table_64.c
+++ b/arch/x86/um/sys_call_table_64.c
@@ -48,7 +48,7 @@ typedef void (*sys_call_ptr_t)(void);
 
 extern void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/arch/x86/vdso/vma.c b/arch/x86/vdso/vma.c
index 00aaf04..47aa108 100644
--- a/arch/x86/vdso/vma.c
+++ b/arch/x86/vdso/vma.c
@@ -117,23 +117,39 @@ subsys_initcall(init_vdso);
 
 struct linux_binprm;
 
-/* Put the vdso above the (randomized) stack with another randomized offset.
-   This way there is no hole in the middle of address space.
-   To save memory make sure it is still in the same PTE as the stack top.
-   This doesn't give that many random bits */
+/*
+ * Put the vdso above the (randomized) stack with another randomized
+ * offset.  This way there is no hole in the middle of address space.
+ * To save memory make sure it is still in the same PTE as the stack
+ * top.  This doesn't give that many random bits.
+ *
+ * Note that this algorithm is imperfect: the distribution of the vdso
+ * start address within a PMD is biased toward the end.
+ *
+ */
 static unsigned long vdso_addr(unsigned long start, unsigned len)
 {
 	unsigned long addr, end;
 	unsigned offset;
-	end = (start + PMD_SIZE - 1) & PMD_MASK;
+
+	/*
+	 * Round up the start address.  It can start out unaligned as a result
+	 * of stack start randomization.
+	 */
+	start = PAGE_ALIGN(start);
+
+	/* Round the lowest possible end address up to a PMD boundary. */
+	end = (start + len + PMD_SIZE - 1) & PMD_MASK;
 	if (end >= TASK_SIZE_MAX)
 		end = TASK_SIZE_MAX;
 	end -= len;
-	/* This loses some more bits than a modulo, but is cheaper */
-	offset = get_random_int() & (PTRS_PER_PTE - 1);
-	addr = start + (offset << PAGE_SHIFT);
-	if (addr >= end)
-		addr = end;
+
+	if (end > start) {
+		offset = get_random_int() % (((end - start) >> PAGE_SHIFT) + 1);
+		addr = start + (offset << PAGE_SHIFT);
+	} else {
+		addr = start;
+	}
 
 	/*
 	 * page-align it here so that get_unmapped_area doesn't
diff --git a/arch/xtensa/mm/fault.c b/arch/xtensa/mm/fault.c
index b17885a..b3877be 100644
--- a/arch/xtensa/mm/fault.c
+++ b/arch/xtensa/mm/fault.c
@@ -108,6 +108,8 @@ void do_page_fault(struct pt_regs *regs)
 	if (unlikely(fault & VM_FAULT_ERROR)) {
 		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGSEGV)
+			goto bad_area;
 		else if (fault & VM_FAULT_SIGBUS)
 			goto do_sigbus;
 		BUG();
diff --git a/block/genhd.c b/block/genhd.c
index da61520..6542b9b 100644
--- a/block/genhd.c
+++ b/block/genhd.c
@@ -1069,9 +1069,16 @@ int disk_expand_part_tbl(struct gendisk *disk, int partno)
 	struct disk_part_tbl *old_ptbl = disk->part_tbl;
 	struct disk_part_tbl *new_ptbl;
 	int len = old_ptbl ? old_ptbl->len : 0;
-	int target = partno + 1;
+	int i, target;
 	size_t size;
-	int i;
+
+	/*
+	 * check for int overflow, since we can get here from blkpg_ioctl()
+	 * with a user passed 'partno'.
+	 */
+	target = partno + 1;
+	if (target < 0)
+		return -EINVAL;
 
 	/* disk_max_parts() is zero during initialization, ignore if so */
 	if (disk_max_parts(disk) && target > disk_max_parts(disk))
diff --git a/crypto/af_alg.c b/crypto/af_alg.c
index bf948e1..6ef6e2a 100644
--- a/crypto/af_alg.c
+++ b/crypto/af_alg.c
@@ -449,6 +449,9 @@ void af_alg_complete(struct crypto_async_request *req, int err)
 {
 	struct af_alg_completion *completion = req->data;
 
+	if (err == -EINPROGRESS)
+		return;
+
 	completion->err = err;
 	complete(&completion->completion);
 }
diff --git a/drivers/ata/ahci.c b/drivers/ata/ahci.c
index ca9a287..6fc61eb 100644
--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -61,6 +61,8 @@ enum board_ids {
 	/* board IDs by feature in alphabetical order */
 	board_ahci,
 	board_ahci_ign_iferr,
+	board_ahci_nomsi,
+	board_ahci_noncq,
 	board_ahci_nosntf,
 	board_ahci_yes_fbs,
 
@@ -121,6 +123,20 @@ static const struct ata_port_info ahci_port_info[] = {
 		.udma_mask	= ATA_UDMA6,
 		.port_ops	= &ahci_ops,
 	},
+	[board_ahci_nomsi] = {
+		AHCI_HFLAGS	(AHCI_HFLAG_NO_MSI),
+		.flags		= AHCI_FLAG_COMMON,
+		.pio_mask	= ATA_PIO4,
+		.udma_mask	= ATA_UDMA6,
+		.port_ops	= &ahci_ops,
+	},
+	[board_ahci_noncq] = {
+		AHCI_HFLAGS	(AHCI_HFLAG_NO_NCQ),
+		.flags		= AHCI_FLAG_COMMON,
+		.pio_mask	= ATA_PIO4,
+		.udma_mask	= ATA_UDMA6,
+		.port_ops	= &ahci_ops,
+	},
 	[board_ahci_nosntf] =
 	{
 		AHCI_HFLAGS	(AHCI_HFLAG_NO_SNTF),
@@ -313,6 +329,9 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(INTEL, 0x8c87), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8e), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8f), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d03), board_ahci }, /* Sunrise Point-LP AHCI */
+	{ PCI_VDEVICE(INTEL, 0x9d05), board_ahci }, /* Sunrise Point-LP RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d07), board_ahci }, /* Sunrise Point-LP RAID */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H AHCI */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H RAID */
 	{ PCI_VDEVICE(INTEL, 0xa105), board_ahci }, /* Sunrise Point-H RAID */
@@ -469,6 +488,13 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(ASMEDIA, 0x0611), board_ahci },	/* ASM1061 */
 	{ PCI_VDEVICE(ASMEDIA, 0x0612), board_ahci },	/* ASM1062 */
 
+	/*
+	 * Samsung SSDs found on some macbooks.  NCQ times out if MSI is
+	 * enabled.  https://bugzilla.kernel.org/show_bug.cgi?id=60731
+	 */
+	{ PCI_VDEVICE(SAMSUNG, 0x1600), board_ahci_nomsi },
+	{ PCI_VDEVICE(SAMSUNG, 0xa800), board_ahci_nomsi },
+
 	/* Enmotus */
 	{ PCI_DEVICE(0x1c44, 0x8000), board_ahci },
 
diff --git a/drivers/ata/libata-core.c b/drivers/ata/libata-core.c
index 6b92236..adaf994 100644
--- a/drivers/ata/libata-core.c
+++ b/drivers/ata/libata-core.c
@@ -4712,7 +4712,10 @@ static struct ata_queued_cmd *ata_qc_new(struct ata_port *ap)
 		return NULL;
 
 	for (i = 0, tag = ap->last_tag + 1; i < max_queue; i++, tag++) {
-		tag = tag < max_queue ? tag : 0;
+		if (ap->flags & ATA_FLAG_LOWTAG)
+			tag = i;
+		else
+			tag = tag < max_queue ? tag : 0;
 
 		/* the last tag is reserved for internal command. */
 		if (tag == ATA_TAG_INTERNAL)
diff --git a/drivers/ata/libata-sff.c b/drivers/ata/libata-sff.c
index 3723e5e..fad2734 100644
--- a/drivers/ata/libata-sff.c
+++ b/drivers/ata/libata-sff.c
@@ -1333,7 +1333,19 @@ void ata_sff_flush_pio_task(struct ata_port *ap)
 	DPRINTK("ENTER\n");
 
 	cancel_delayed_work_sync(&ap->sff_pio_task);
+
+	/*
+	 * We wanna reset the HSM state to IDLE.  If we do so without
+	 * grabbing the port lock, critical sections protected by it which
+	 * expect the HSM state to stay stable may get surprised.  For
+	 * example, we may set IDLE in between the time
+	 * __ata_sff_port_intr() checks for HSM_ST_IDLE and before it calls
+	 * ata_sff_hsm_move() causing ata_sff_hsm_move() to BUG().
+	 */
+	spin_lock_irq(ap->lock);
 	ap->hsm_task_state = HSM_ST_IDLE;
+	spin_unlock_irq(ap->lock);
+
 	ap->sff_pio_task_link = NULL;
 
 	if (ata_msg_ctl(ap))
diff --git a/drivers/ata/sata_dwc_460ex.c b/drivers/ata/sata_dwc_460ex.c
index 69f7cde..9d6eb14 100644
--- a/drivers/ata/sata_dwc_460ex.c
+++ b/drivers/ata/sata_dwc_460ex.c
@@ -791,7 +791,7 @@ static int dma_dwc_init(struct sata_dwc_device *hsdev, int irq)
 	if (err) {
 		dev_err(host_pvt.dwc_dev, "%s: dma_request_interrupts returns"
 			" %d\n", __func__, err);
-		goto error_out;
+		return err;
 	}
 
 	/* Enabe DMA */
@@ -802,11 +802,6 @@ static int dma_dwc_init(struct sata_dwc_device *hsdev, int irq)
 		sata_dma_regs);
 
 	return 0;
-
-error_out:
-	dma_dwc_exit(hsdev);
-
-	return err;
 }
 
 static int sata_dwc_scr_read(struct ata_link *link, unsigned int scr, u32 *val)
@@ -1634,7 +1629,7 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	char *ver = (char *)&versionr;
 	u8 *base = NULL;
 	int err = 0;
-	int irq, rc;
+	int irq;
 	struct ata_host *host;
 	struct ata_port_info pi = sata_dwc_port_info[0];
 	const struct ata_port_info *ppi[] = { &pi, NULL };
@@ -1688,7 +1683,7 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	if (irq == NO_IRQ) {
 		dev_err(&ofdev->dev, "no SATA DMA irq\n");
 		err = -ENODEV;
-		goto error_out;
+		goto error_iomap;
 	}
 
 	/* Get physical SATA DMA register base address */
@@ -1697,14 +1692,16 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 		dev_err(&ofdev->dev, "ioremap failed for AHBDMA register"
 			" address\n");
 		err = -ENODEV;
-		goto error_out;
+		goto error_iomap;
 	}
 
 	/* Save dev for later use in dev_xxx() routines */
 	host_pvt.dwc_dev = &ofdev->dev;
 
 	/* Initialize AHB DMAC */
-	dma_dwc_init(hsdev, irq);
+	err = dma_dwc_init(hsdev, irq);
+	if (err)
+		goto error_dma_iomap;
 
 	/* Enable SATA Interrupts */
 	sata_dwc_enable_interrupts(hsdev);
@@ -1722,9 +1719,8 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 	 * device discovery process, invoking our port_start() handler &
 	 * error_handler() to execute a dummy Softreset EH session
 	 */
-	rc = ata_host_activate(host, irq, sata_dwc_isr, 0, &sata_dwc_sht);
-
-	if (rc != 0)
+	err = ata_host_activate(host, irq, sata_dwc_isr, 0, &sata_dwc_sht);
+	if (err)
 		dev_err(&ofdev->dev, "failed to activate host");
 
 	dev_set_drvdata(&ofdev->dev, host);
@@ -1733,7 +1729,8 @@ static int sata_dwc_probe(struct platform_device *ofdev)
 error_out:
 	/* Free SATA DMA resources */
 	dma_dwc_exit(hsdev);
-
+error_dma_iomap:
+	iounmap((void __iomem *)host_pvt.sata_dma_regs);
 error_iomap:
 	iounmap(base);
 error_kmalloc:
@@ -1754,6 +1751,7 @@ static int sata_dwc_remove(struct platform_device *ofdev)
 	/* Free SATA DMA resources */
 	dma_dwc_exit(hsdev);
 
+	iounmap((void __iomem *)host_pvt.sata_dma_regs);
 	iounmap(hsdev->reg_base);
 	kfree(hsdev);
 	kfree(host);
diff --git a/drivers/ata/sata_fsl.c b/drivers/ata/sata_fsl.c
index d6577b9..3d3b59a 100644
--- a/drivers/ata/sata_fsl.c
+++ b/drivers/ata/sata_fsl.c
@@ -1426,7 +1426,7 @@ static int sata_fsl_probe(struct platform_device *ofdev)
 	host_priv->csr_base = csr_base;
 
 	irq = irq_of_parse_and_map(ofdev->dev.of_node, 0);
-	if (irq < 0) {
+	if (!irq) {
 		dev_err(&ofdev->dev, "invalid irq from platform\n");
 		goto error_exit_with_cleanup;
 	}
diff --git a/drivers/ata/sata_sil24.c b/drivers/ata/sata_sil24.c
index e7e610a..cb68aa3 100644
--- a/drivers/ata/sata_sil24.c
+++ b/drivers/ata/sata_sil24.c
@@ -246,7 +246,7 @@ enum {
 	/* host flags */
 	SIL24_COMMON_FLAGS	= ATA_FLAG_SATA | ATA_FLAG_PIO_DMA |
 				  ATA_FLAG_NCQ | ATA_FLAG_ACPI_SATA |
-				  ATA_FLAG_AN | ATA_FLAG_PMP,
+				  ATA_FLAG_AN | ATA_FLAG_PMP | ATA_FLAG_LOWTAG,
 	SIL24_FLAG_PCIX_IRQ_WOC	= (1 << 24), /* IRQ loss errata on PCI-X */
 
 	IRQ_STAT_4PORTS		= 0xf,
diff --git a/drivers/base/bus.c b/drivers/base/bus.c
index feb30c1..b23bb9c 100644
--- a/drivers/base/bus.c
+++ b/drivers/base/bus.c
@@ -245,13 +245,15 @@ static ssize_t store_drivers_probe(struct bus_type *bus,
 				   const char *buf, size_t count)
 {
 	struct device *dev;
+	int err = -EINVAL;
 
 	dev = bus_find_device_by_name(bus, NULL, buf);
 	if (!dev)
 		return -ENODEV;
-	if (bus_rescan_devices_helper(dev, NULL) != 0)
-		return -EINVAL;
-	return count;
+	if (bus_rescan_devices_helper(dev, NULL) == 0)
+		err = count;
+	put_device(dev);
+	return err;
 }
 #endif
 
diff --git a/drivers/base/core.c b/drivers/base/core.c
index bde1832..b1726a0 100644
--- a/drivers/base/core.c
+++ b/drivers/base/core.c
@@ -1500,34 +1500,11 @@ static void device_create_release(struct device *dev)
 	kfree(dev);
 }
 
-/**
- * device_create_vargs - creates a device and registers it with sysfs
- * @class: pointer to the struct class that this device should be registered to
- * @parent: pointer to the parent struct device of this new device, if any
- * @devt: the dev_t for the char device to be added
- * @drvdata: the data to be added to the device for callbacks
- * @fmt: string for the device's name
- * @args: va_list for the device's name
- *
- * This function can be used by char device classes.  A struct device
- * will be created in sysfs, registered to the specified class.
- *
- * A "dev" file will be created, showing the dev_t for the device, if
- * the dev_t is not 0,0.
- * If a pointer to a parent struct device is passed in, the newly created
- * struct device will be a child of that device in sysfs.
- * The pointer to the struct device will be returned from the call.
- * Any further sysfs files that might be required can be created using this
- * pointer.
- *
- * Returns &struct device pointer on success, or ERR_PTR() on error.
- *
- * Note: the struct class passed to this function must have previously
- * been created with a call to class_create().
- */
-struct device *device_create_vargs(struct class *class, struct device *parent,
-				   dev_t devt, void *drvdata, const char *fmt,
-				   va_list args)
+static struct device *
+device_create_groups_vargs(struct class *class, struct device *parent,
+			   dev_t devt, void *drvdata,
+			   const struct attribute_group **groups,
+			   const char *fmt, va_list args)
 {
 	struct device *dev = NULL;
 	int retval = -ENODEV;
@@ -1544,6 +1521,7 @@ struct device *device_create_vargs(struct class *class, struct device *parent,
 	dev->devt = devt;
 	dev->class = class;
 	dev->parent = parent;
+	dev->groups = groups;
 	dev->release = device_create_release;
 	dev_set_drvdata(dev, drvdata);
 
@@ -1561,6 +1539,39 @@ struct device *device_create_vargs(struct class *class, struct device *parent,
 	put_device(dev);
 	return ERR_PTR(retval);
 }
+
+/**
+ * device_create_vargs - creates a device and registers it with sysfs
+ * @class: pointer to the struct class that this device should be registered to
+ * @parent: pointer to the parent struct device of this new device, if any
+ * @devt: the dev_t for the char device to be added
+ * @drvdata: the data to be added to the device for callbacks
+ * @fmt: string for the device's name
+ * @args: va_list for the device's name
+ *
+ * This function can be used by char device classes.  A struct device
+ * will be created in sysfs, registered to the specified class.
+ *
+ * A "dev" file will be created, showing the dev_t for the device, if
+ * the dev_t is not 0,0.
+ * If a pointer to a parent struct device is passed in, the newly created
+ * struct device will be a child of that device in sysfs.
+ * The pointer to the struct device will be returned from the call.
+ * Any further sysfs files that might be required can be created using this
+ * pointer.
+ *
+ * Returns &struct device pointer on success, or ERR_PTR() on error.
+ *
+ * Note: the struct class passed to this function must have previously
+ * been created with a call to class_create().
+ */
+struct device *device_create_vargs(struct class *class, struct device *parent,
+				   dev_t devt, void *drvdata, const char *fmt,
+				   va_list args)
+{
+	return device_create_groups_vargs(class, parent, devt, drvdata, NULL,
+					  fmt, args);
+}
 EXPORT_SYMBOL_GPL(device_create_vargs);
 
 /**
@@ -1600,6 +1611,50 @@ struct device *device_create(struct class *class, struct device *parent,
 }
 EXPORT_SYMBOL_GPL(device_create);
 
+/**
+ * device_create_with_groups - creates a device and registers it with sysfs
+ * @class: pointer to the struct class that this device should be registered to
+ * @parent: pointer to the parent struct device of this new device, if any
+ * @devt: the dev_t for the char device to be added
+ * @drvdata: the data to be added to the device for callbacks
+ * @groups: NULL-terminated list of attribute groups to be created
+ * @fmt: string for the device's name
+ *
+ * This function can be used by char device classes.  A struct device
+ * will be created in sysfs, registered to the specified class.
+ * Additional attributes specified in the groups parameter will also
+ * be created automatically.
+ *
+ * A "dev" file will be created, showing the dev_t for the device, if
+ * the dev_t is not 0,0.
+ * If a pointer to a parent struct device is passed in, the newly created
+ * struct device will be a child of that device in sysfs.
+ * The pointer to the struct device will be returned from the call.
+ * Any further sysfs files that might be required can be created using this
+ * pointer.
+ *
+ * Returns &struct device pointer on success, or ERR_PTR() on error.
+ *
+ * Note: the struct class passed to this function must have previously
+ * been created with a call to class_create().
+ */
+struct device *device_create_with_groups(struct class *class,
+					 struct device *parent, dev_t devt,
+					 void *drvdata,
+					 const struct attribute_group **groups,
+					 const char *fmt, ...)
+{
+	va_list vargs;
+	struct device *dev;
+
+	va_start(vargs, fmt);
+	dev = device_create_groups_vargs(class, parent, devt, drvdata, groups,
+					 fmt, vargs);
+	va_end(vargs);
+	return dev;
+}
+EXPORT_SYMBOL_GPL(device_create_with_groups);
+
 static int __match_devt(struct device *dev, void *data)
 {
 	dev_t *devt = data;
diff --git a/drivers/block/drbd/drbd_req.c b/drivers/block/drbd/drbd_req.c
index be984e0..43da226 100644
--- a/drivers/block/drbd/drbd_req.c
+++ b/drivers/block/drbd/drbd_req.c
@@ -1184,6 +1184,7 @@ int drbd_merge_bvec(struct request_queue *q, struct bvec_merge_data *bvm, struct
 		struct request_queue * const b =
 			mdev->ldev->backing_bdev->bd_disk->queue;
 		if (b->merge_bvec_fn) {
+			bvm->bi_bdev = mdev->ldev->backing_bdev;
 			backing_limit = b->merge_bvec_fn(b, bvm, bvec);
 			limit = min(limit, backing_limit);
 		}
diff --git a/drivers/gpio/gpiolib.c b/drivers/gpio/gpiolib.c
index 234cb1e..06d916b 100644
--- a/drivers/gpio/gpiolib.c
+++ b/drivers/gpio/gpiolib.c
@@ -60,6 +60,7 @@ struct gpio_desc {
 #define FLAG_ACTIVE_LOW	7	/* sysfs value has active low */
 #define FLAG_OPEN_DRAIN	8	/* Gpio is open drain type */
 #define FLAG_OPEN_SOURCE 9	/* Gpio is open source type */
+#define FLAG_SYSFS_DIR	10	/* show sysfs direction attribute */
 
 #define ID_SHIFT	16	/* add new flags before this one */
 
@@ -319,7 +320,7 @@ static ssize_t gpio_value_store(struct device *dev,
 	return status;
 }
 
-static const DEVICE_ATTR(value, 0644,
+static DEVICE_ATTR(value, 0644,
 		gpio_value_show, gpio_value_store);
 
 static irqreturn_t gpio_sysfs_irq(int irq, void *priv)
@@ -542,17 +543,47 @@ static ssize_t gpio_active_low_store(struct device *dev,
 	return status ? : size;
 }
 
-static const DEVICE_ATTR(active_low, 0644,
+static DEVICE_ATTR(active_low, 0644,
 		gpio_active_low_show, gpio_active_low_store);
 
-static const struct attribute *gpio_attrs[] = {
+static umode_t gpio_is_visible(struct kobject *kobj, struct attribute *attr,
+			       int n)
+{
+	struct device *dev = container_of(kobj, struct device, kobj);
+	struct gpio_desc *desc = dev_get_drvdata(dev);
+	unsigned gpio = desc - gpio_desc;
+	umode_t mode = attr->mode;
+	bool show_direction = test_bit(FLAG_SYSFS_DIR, &desc->flags);
+
+	if (attr == &dev_attr_direction.attr) {
+		if (!show_direction)
+			mode = 0;
+	} else if (attr == &dev_attr_edge.attr) {
+		if (gpio_to_irq(gpio) < 0)
+			mode = 0;
+		if (!show_direction && test_bit(FLAG_IS_OUT, &desc->flags))
+			mode = 0;
+	}
+
+	return mode;
+}
+
+static struct attribute *gpio_attrs[] = {
+	&dev_attr_direction.attr,
+	&dev_attr_edge.attr,
 	&dev_attr_value.attr,
 	&dev_attr_active_low.attr,
 	NULL,
 };
 
-static const struct attribute_group gpio_attr_group = {
-	.attrs = (struct attribute **) gpio_attrs,
+static const struct attribute_group gpio_group = {
+	.attrs = gpio_attrs,
+	.is_visible = gpio_is_visible,
+};
+
+static const struct attribute_group *gpio_groups[] = {
+	&gpio_group,
+	NULL
 };
 
 /*
@@ -589,16 +620,13 @@ static ssize_t chip_ngpio_show(struct device *dev,
 }
 static DEVICE_ATTR(ngpio, 0444, chip_ngpio_show, NULL);
 
-static const struct attribute *gpiochip_attrs[] = {
+static struct attribute *gpiochip_attrs[] = {
 	&dev_attr_base.attr,
 	&dev_attr_label.attr,
 	&dev_attr_ngpio.attr,
 	NULL,
 };
-
-static const struct attribute_group gpiochip_attr_group = {
-	.attrs = (struct attribute **) gpiochip_attrs,
-};
+ATTRIBUTE_GROUPS(gpiochip);
 
 /*
  * /sys/class/gpio/export ... write-only
@@ -704,8 +732,9 @@ int gpio_export(unsigned gpio, bool direction_may_change)
 {
 	unsigned long		flags;
 	struct gpio_desc	*desc;
-	int			status = -EINVAL;
+	int			status;
 	const char		*ioname = NULL;
+	struct device		*dev;
 
 	/* can't export until sysfs is available ... */
 	if (!gpio_class.p) {
@@ -713,59 +742,50 @@ int gpio_export(unsigned gpio, bool direction_may_change)
 		return -ENOENT;
 	}
 
-	if (!gpio_is_valid(gpio))
-		goto done;
+	if (!gpio_is_valid(gpio)) {
+		pr_debug("%s: gpio %d is not valid\n", __func__, gpio);
+		return -EINVAL;
+	}
 
 	mutex_lock(&sysfs_lock);
 
 	spin_lock_irqsave(&gpio_lock, flags);
 	desc = &gpio_desc[gpio];
-	if (test_bit(FLAG_REQUESTED, &desc->flags)
-			&& !test_bit(FLAG_EXPORT, &desc->flags)) {
-		status = 0;
-		if (!desc->chip->direction_input
-				|| !desc->chip->direction_output)
-			direction_may_change = false;
+	if (!test_bit(FLAG_REQUESTED, &desc->flags) ||
+	     test_bit(FLAG_EXPORT, &desc->flags)) {
+		spin_unlock_irqrestore(&gpio_lock, flags);
+		pr_debug("%s: gpio %d unavailable (requested=%d, exported=%d)\n",
+				__func__, gpio,
+				test_bit(FLAG_REQUESTED, &desc->flags),
+				test_bit(FLAG_EXPORT, &desc->flags));
+		return -EPERM;
+	}
+
+	if (desc->chip->direction_input && desc->chip->direction_output &&
+			direction_may_change) {
+		set_bit(FLAG_SYSFS_DIR, &desc->flags);
 	}
+
 	spin_unlock_irqrestore(&gpio_lock, flags);
 
 	if (desc->chip->names && desc->chip->names[gpio - desc->chip->base])
 		ioname = desc->chip->names[gpio - desc->chip->base];
 
-	if (status == 0) {
-		struct device	*dev;
-
-		dev = device_create(&gpio_class, desc->chip->dev, MKDEV(0, 0),
-				desc, ioname ? ioname : "gpio%u", gpio);
-		if (!IS_ERR(dev)) {
-			status = sysfs_create_group(&dev->kobj,
-						&gpio_attr_group);
-
-			if (!status && direction_may_change)
-				status = device_create_file(dev,
-						&dev_attr_direction);
-
-			if (!status && gpio_to_irq(gpio) >= 0
-					&& (direction_may_change
-						|| !test_bit(FLAG_IS_OUT,
-							&desc->flags)))
-				status = device_create_file(dev,
-						&dev_attr_edge);
-
-			if (status != 0)
-				device_unregister(dev);
-		} else
-			status = PTR_ERR(dev);
-		if (status == 0)
-			set_bit(FLAG_EXPORT, &desc->flags);
+	dev = device_create_with_groups(&gpio_class, desc->chip->dev,
+					MKDEV(0, 0), desc, gpio_groups,
+					ioname ? ioname : "gpio%u", gpio);
+	if (IS_ERR(dev)) {
+		status = PTR_ERR(dev);
+		goto fail_unlock;
 	}
 
+	set_bit(FLAG_EXPORT, &desc->flags);
 	mutex_unlock(&sysfs_lock);
+	return 0;
 
-done:
-	if (status)
-		pr_debug("%s: gpio%d status %d\n", __func__, gpio, status);
-
+fail_unlock:
+	mutex_unlock(&sysfs_lock);
+	pr_debug("%s: gpio%d status %d\n", __func__, gpio, status);
 	return status;
 }
 EXPORT_SYMBOL_GPL(gpio_export);
@@ -805,6 +825,7 @@ int gpio_export_link(struct device *dev, const char *name, unsigned gpio)
 		if (tdev != NULL) {
 			status = sysfs_create_link(&dev->kobj, &tdev->kobj,
 						name);
+			put_device(tdev);
 		} else {
 			status = -ENODEV;
 		}
@@ -855,7 +876,7 @@ int gpio_sysfs_set_active_low(unsigned gpio, int value)
 	}
 
 	status = sysfs_set_active_low(desc, dev, value);
-
+	put_device(dev);
 unlock:
 	mutex_unlock(&sysfs_lock);
 
@@ -893,6 +914,7 @@ void gpio_unexport(unsigned gpio)
 		dev = class_find_device(&gpio_class, NULL, desc, match_export);
 		if (dev) {
 			gpio_setup_irq(desc, dev, 0);
+			clear_bit(FLAG_SYSFS_DIR, &desc->flags);
 			clear_bit(FLAG_EXPORT, &desc->flags);
 		} else
 			status = -ENODEV;
@@ -924,13 +946,13 @@ static int gpiochip_export(struct gpio_chip *chip)
 
 	/* use chip->base for the ID; it's already known to be unique */
 	mutex_lock(&sysfs_lock);
-	dev = device_create(&gpio_class, chip->dev, MKDEV(0, 0), chip,
-				"gpiochip%d", chip->base);
-	if (!IS_ERR(dev)) {
-		status = sysfs_create_group(&dev->kobj,
-				&gpiochip_attr_group);
-	} else
+	dev = device_create_with_groups(&gpio_class, chip->dev, MKDEV(0, 0),
+					chip, gpiochip_groups,
+					"gpiochip%d", chip->base);
+	if (IS_ERR(dev))
 		status = PTR_ERR(dev);
+	else
+		status = 0;
 	chip->exported = (status == 0);
 	mutex_unlock(&sysfs_lock);
 
@@ -1081,23 +1103,22 @@ int gpiochip_add(struct gpio_chip *chip)
 				? (1 << FLAG_IS_OUT)
 				: 0;
 		}
-	}
 
 #ifdef CONFIG_PINCTRL
 	INIT_LIST_HEAD(&chip->pin_ranges);
 #endif
-
-	of_gpiochip_add(chip);
+	
+		of_gpiochip_add(chip);
+	}
 
 unlock:
 	spin_unlock_irqrestore(&gpio_lock, flags);
 
-	if (status)
-		goto fail;
-
 	status = gpiochip_export(chip);
-	if (status)
+	if (status) {
+		of_gpiochip_remove(chip);
 		goto fail;
+	}
 
 	pr_info("gpiochip_add: registered GPIOs %d to %d on device: %s\n",
 		chip->base, chip->base + chip->ngpio - 1,
diff --git a/drivers/gpu/drm/i915/i915_gem.c b/drivers/gpu/drm/i915/i915_gem.c
index 2ac4ded..b1f1d10 100644
--- a/drivers/gpu/drm/i915/i915_gem.c
+++ b/drivers/gpu/drm/i915/i915_gem.c
@@ -2193,6 +2193,13 @@ static int sandybridge_write_fence_reg(struct drm_i915_gem_object *obj,
 	int regnum = obj->fence_reg;
 	uint64_t val;
 
+	/* Adjust fence size to match tiled area */
+	if (obj->tiling_mode != I915_TILING_NONE) {
+		uint32_t row_size = obj->stride *
+			(obj->tiling_mode == I915_TILING_Y ? 32 : 8);
+		size = (size / row_size) * row_size;
+	}
+
 	val = (uint64_t)((obj->gtt_offset + size - 4096) &
 			 0xfffff000) << 32;
 	val |= obj->gtt_offset & 0xfffff000;
@@ -2230,6 +2237,13 @@ static int i965_write_fence_reg(struct drm_i915_gem_object *obj,
 	int regnum = obj->fence_reg;
 	uint64_t val;
 
+	/* Adjust fence size to match tiled area */
+	if (obj->tiling_mode != I915_TILING_NONE) {
+		uint32_t row_size = obj->stride *
+			(obj->tiling_mode == I915_TILING_Y ? 32 : 8);
+		size = (size / row_size) * row_size;
+	}
+
 	val = (uint64_t)((obj->gtt_offset + size - 4096) &
 		    0xfffff000) << 32;
 	val |= obj->gtt_offset & 0xfffff000;
diff --git a/drivers/gpu/drm/i915/intel_lvds.c b/drivers/gpu/drm/i915/intel_lvds.c
index 77190cc..3febe29 100644
--- a/drivers/gpu/drm/i915/intel_lvds.c
+++ b/drivers/gpu/drm/i915/intel_lvds.c
@@ -932,6 +932,17 @@ bool intel_lvds_init(struct drm_device *dev)
 	int pipe;
 	u8 pin;
 
+	/*
+	 * Unlock registers and just leave them unlocked. Do this before
+	 * checking quirk lists to avoid bogus WARNINGs.
+	 */
+	if (HAS_PCH_SPLIT(dev)) {
+		I915_WRITE(PCH_PP_CONTROL,
+			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
+	} else {
+		I915_WRITE(PP_CONTROL,
+			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
+	}
 	if (!intel_lvds_supported(dev))
 		return false;
 
@@ -1109,19 +1120,6 @@ bool intel_lvds_init(struct drm_device *dev)
 		pwm = I915_READ(BLC_PWM_PCH_CTL1);
 		pwm |= PWM_PCH_ENABLE;
 		I915_WRITE(BLC_PWM_PCH_CTL1, pwm);
-		/*
-		 * Unlock registers and just
-		 * leave them unlocked
-		 */
-		I915_WRITE(PCH_PP_CONTROL,
-			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
-	} else {
-		/*
-		 * Unlock registers and just
-		 * leave them unlocked
-		 */
-		I915_WRITE(PP_CONTROL,
-			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
 	}
 	dev_priv->lid_notifier.notifier_call = intel_lid_notify;
 	if (acpi_lid_notifier_register(&dev_priv->lid_notifier)) {
diff --git a/drivers/gpu/drm/radeon/radeon_kms.c b/drivers/gpu/drm/radeon/radeon_kms.c
index 9b46238..b731686 100644
--- a/drivers/gpu/drm/radeon/radeon_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_kms.c
@@ -428,6 +428,8 @@ int radeon_get_vblank_timestamp_kms(struct drm_device *dev, int crtc,
 
 	/* Get associated drm_crtc: */
 	drmcrtc = &rdev->mode_info.crtcs[crtc]->base;
+	if (!drmcrtc)
+		return -EINVAL;
 
 	/* Helper routine in DRM core does all the work: */
 	return drm_calc_vbltimestamp_from_scanoutpos(dev, crtc, max_error,
diff --git a/drivers/gpu/drm/radeon/radeon_ttm.c b/drivers/gpu/drm/radeon/radeon_ttm.c
index 49b55ed..15042d0 100644
--- a/drivers/gpu/drm/radeon/radeon_ttm.c
+++ b/drivers/gpu/drm/radeon/radeon_ttm.c
@@ -188,7 +188,7 @@ static void radeon_evict_flags(struct ttm_buffer_object *bo,
 	rbo = container_of(bo, struct radeon_bo, tbo);
 	switch (bo->mem.mem_type) {
 	case TTM_PL_VRAM:
-		if (rbo->rdev->ring[RADEON_RING_TYPE_GFX_INDEX].ready == false)
+		if (rbo->rdev->ring[radeon_copy_ring_index(rbo->rdev)].ready == false)
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_CPU);
 		else
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_GTT);
diff --git a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
index 7e07433..992b46b 100644
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
@@ -485,14 +485,7 @@ void vmw_fence_obj_flush(struct vmw_fence_obj *fence)
 
 static void vmw_fence_destroy(struct vmw_fence_obj *fence)
 {
-	struct vmw_fence_manager *fman = fence->fman;
-
 	kfree(fence);
-	/*
-	 * Free kernel space accounting.
-	 */
-	ttm_mem_global_free(vmw_mem_glob(fman->dev_priv),
-			    fman->fence_size);
 }
 
 int vmw_fence_create(struct vmw_fence_manager *fman,
@@ -500,20 +493,12 @@ int vmw_fence_create(struct vmw_fence_manager *fman,
 		     uint32_t mask,
 		     struct vmw_fence_obj **p_fence)
 {
-	struct ttm_mem_global *mem_glob = vmw_mem_glob(fman->dev_priv);
 	struct vmw_fence_obj *fence;
 	int ret;
 
-	ret = ttm_mem_global_alloc(mem_glob, fman->fence_size,
-				   false, false);
-	if (unlikely(ret != 0))
-		return ret;
-
 	fence = kzalloc(sizeof(*fence), GFP_KERNEL);
-	if (unlikely(fence == NULL)) {
-		ret = -ENOMEM;
-		goto out_no_object;
-	}
+	if (unlikely(fence == NULL))
+		return -ENOMEM;
 
 	ret = vmw_fence_obj_init(fman, fence, seqno, mask,
 				 vmw_fence_destroy);
@@ -525,8 +510,6 @@ int vmw_fence_create(struct vmw_fence_manager *fman,
 
 out_err_init:
 	kfree(fence);
-out_no_object:
-	ttm_mem_global_free(mem_glob, fman->fence_size);
 	return ret;
 }
 
@@ -1049,6 +1032,8 @@ int vmw_event_fence_action_create(struct drm_file *file_priv,
 	if (ret != 0)
 		goto out_no_queue;
 
+	return 0;
+
 out_no_queue:
 	event->base.destroy(&event->base);
 out_no_event:
@@ -1123,17 +1108,10 @@ int vmw_fence_event_ioctl(struct drm_device *dev, void *data,
 
 	BUG_ON(fence == NULL);
 
-	if (arg->flags & DRM_VMW_FE_FLAG_REQ_TIME)
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-	else
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-
+	ret = vmw_event_fence_action_create(file_priv, fence,
+					    arg->flags,
+					    arg->user_data,
+					    true);
 	if (unlikely(ret != 0)) {
 		if (ret != -ERESTARTSYS)
 			DRM_ERROR("Failed to attach event to fence.\n");
diff --git a/drivers/hid/hid-roccat-pyra.c b/drivers/hid/hid-roccat-pyra.c
index df05c1b1..5346647 100644
--- a/drivers/hid/hid-roccat-pyra.c
+++ b/drivers/hid/hid-roccat-pyra.c
@@ -35,6 +35,8 @@ static struct class *pyra_class;
 static void profile_activated(struct pyra_device *pyra,
 		unsigned int new_profile)
 {
+	if (new_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return;
 	pyra->actual_profile = new_profile;
 	pyra->actual_cpi = pyra->profile_settings[pyra->actual_profile].y_cpi;
 }
@@ -299,10 +301,15 @@ static ssize_t pyra_sysfs_write_settings(struct file *fp,
 	int retval = 0;
 	int difference;
 	struct pyra_roccat_report roccat_report;
+	struct pyra_settings const *settings;
 
 	if (off != 0 || count != sizeof(struct pyra_settings))
 		return -EINVAL;
 
+	settings = (struct pyra_settings const *)buf;
+	if (settings->startup_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return -EINVAL;
+
 	mutex_lock(&pyra->pyra_lock);
 	difference = memcmp(buf, &pyra->settings, sizeof(struct pyra_settings));
 	if (difference) {
diff --git a/drivers/hv/vmbus_drv.c b/drivers/hv/vmbus_drv.c
index 10619b3..1ec309d 100644
--- a/drivers/hv/vmbus_drv.c
+++ b/drivers/hv/vmbus_drv.c
@@ -681,7 +681,7 @@ int vmbus_device_register(struct hv_device *child_device_obj)
 	if (ret)
 		pr_err("Unable to register child device\n");
 	else
-		pr_info("child device %s registered\n",
+		pr_debug("child device %s registered\n",
 			dev_name(&child_device_obj->device));
 
 	return ret;
@@ -693,14 +693,14 @@ int vmbus_device_register(struct hv_device *child_device_obj)
  */
 void vmbus_device_unregister(struct hv_device *device_obj)
 {
+	pr_debug("child device %s unregistered\n",
+		dev_name(&device_obj->device));
+
 	/*
 	 * Kick off the process of unregistering the device.
 	 * This will call vmbus_remove() and eventually vmbus_device_release()
 	 */
 	device_unregister(&device_obj->device);
-
-	pr_info("child device %s unregistered\n",
-		dev_name(&device_obj->device));
 }
 
 
diff --git a/drivers/i2c/busses/i2c-davinci.c b/drivers/i2c/busses/i2c-davinci.c
index 79b4bcb..1837fe6 100644
--- a/drivers/i2c/busses/i2c-davinci.c
+++ b/drivers/i2c/busses/i2c-davinci.c
@@ -416,11 +416,9 @@ i2c_davinci_xfer_msg(struct i2c_adapter *adap, struct i2c_msg *msg, int stop)
 	if (dev->cmd_err & DAVINCI_I2C_STR_NACK) {
 		if (msg->flags & I2C_M_IGNORE_NAK)
 			return msg->len;
-		if (stop) {
-			w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
-			w |= DAVINCI_I2C_MDR_STP;
-			davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
-		}
+		w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
+		w |= DAVINCI_I2C_MDR_STP;
+		davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
 		return -EREMOTEIO;
 	}
 	return -EIO;
diff --git a/drivers/input/joystick/xpad.c b/drivers/input/joystick/xpad.c
index 42f7b25..b4e8db8 100644
--- a/drivers/input/joystick/xpad.c
+++ b/drivers/input/joystick/xpad.c
@@ -979,9 +979,19 @@ static int xpad_probe(struct usb_interface *intf, const struct usb_device_id *id
 		}
 
 		ep_irq_in = &intf->cur_altsetting->endpoint[1].desc;
-		usb_fill_bulk_urb(xpad->bulk_out, udev,
-				usb_sndbulkpipe(udev, ep_irq_in->bEndpointAddress),
-				xpad->bdata, XPAD_PKT_LEN, xpad_bulk_out, xpad);
+		if (usb_endpoint_is_bulk_out(ep_irq_in)) {
+			usb_fill_bulk_urb(xpad->bulk_out, udev,
+					  usb_sndbulkpipe(udev,
+							  ep_irq_in->bEndpointAddress),
+					  xpad->bdata, XPAD_PKT_LEN,
+					  xpad_bulk_out, xpad);
+		} else {
+			usb_fill_int_urb(xpad->bulk_out, udev,
+					 usb_sndintpipe(udev,
+							ep_irq_in->bEndpointAddress),
+					 xpad->bdata, XPAD_PKT_LEN,
+					 xpad_bulk_out, xpad, 0);
+		}
 
 		/*
 		 * Submit the int URB immediately rather than waiting for open
diff --git a/drivers/input/serio/i8042-x86ia64io.h b/drivers/input/serio/i8042-x86ia64io.h
index ce715b1..78227f3 100644
--- a/drivers/input/serio/i8042-x86ia64io.h
+++ b/drivers/input/serio/i8042-x86ia64io.h
@@ -408,6 +408,13 @@ static const struct dmi_system_id __initconst i8042_dmi_nomux_table[] = {
 		},
 	},
 	{
+		/* Acer Aspire 7738 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "Acer"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "Aspire 7738"),
+		},
+	},
+	{
 		/* Gericom Bellagio */
 		.matches = {
 			DMI_MATCH(DMI_SYS_VENDOR, "Gericom"),
@@ -721,6 +728,35 @@ static const struct dmi_system_id __initconst i8042_dmi_dritek_table[] = {
 	{ }
 };
 
+/*
+ * Some laptops need keyboard reset before probing for the trackpad to get
+ * it detected, initialised & finally work.
+ */
+static const struct dmi_system_id __initconst i8042_dmi_kbdreset_table[] = {
+	{
+		/* Gigabyte P35 v2 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P35V2"),
+		},
+	},
+		{
+		/* Aorus branded Gigabyte X3 Plus - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "X3"),
+		},
+	},
+	{
+		/* Gigabyte P34 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P34"),
+		},
+	},
+	{ }
+};
+
 #endif /* CONFIG_X86 */
 
 #ifdef CONFIG_PNP
@@ -1001,6 +1037,9 @@ static int __init i8042_platform_init(void)
 	if (dmi_check_system(i8042_dmi_dritek_table))
 		i8042_dritek = true;
 
+	if (dmi_check_system(i8042_dmi_kbdreset_table))
+		i8042_kbdreset = true;
+
 	/*
 	 * A20 was already enabled during early kernel init. But some buggy
 	 * BIOSes (in MSI Laptops) require A20 to be enabled using 8042 to
diff --git a/drivers/input/serio/i8042.c b/drivers/input/serio/i8042.c
index 8656441..178e75d 100644
--- a/drivers/input/serio/i8042.c
+++ b/drivers/input/serio/i8042.c
@@ -67,6 +67,10 @@ static bool i8042_notimeout;
 module_param_named(notimeout, i8042_notimeout, bool, 0);
 MODULE_PARM_DESC(notimeout, "Ignore timeouts signalled by i8042");
 
+static bool i8042_kbdreset;
+module_param_named(kbdreset, i8042_kbdreset, bool, 0);
+MODULE_PARM_DESC(kbdreset, "Reset device connected to KBD port");
+
 #ifdef CONFIG_X86
 static bool i8042_dritek;
 module_param_named(dritek, i8042_dritek, bool, 0);
@@ -783,6 +787,16 @@ static int __init i8042_check_aux(void)
 		return -1;
 
 /*
+ * Reset keyboard (needed on some laptops to successfully detect
+ * touchpad, e.g., some Gigabyte laptop models with Elantech
+ * touchpads).
+ */
+	if (i8042_kbdreset) {
+		pr_warn("Attempting to reset device connected to KBD port\n");
+		i8042_kbd_write(NULL, (unsigned char) 0xff);
+	}
+
+/*
  * Test AUX IRQ delivery to make sure BIOS did not grab the IRQ and
  * used it for a PCI card or somethig else.
  */
diff --git a/drivers/iommu/intel-iommu.c b/drivers/iommu/intel-iommu.c
index a5f4359..2e48b22 100644
--- a/drivers/iommu/intel-iommu.c
+++ b/drivers/iommu/intel-iommu.c
@@ -1792,7 +1792,7 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 	struct dma_pte *first_pte = NULL, *pte = NULL;
 	phys_addr_t uninitialized_var(pteval);
 	int addr_width = agaw_to_width(domain->agaw) - VTD_PAGE_SHIFT;
-	unsigned long sg_res;
+	unsigned long sg_res = 0;
 	unsigned int largepage_lvl = 0;
 	unsigned long lvl_pages = 0;
 
@@ -1803,10 +1803,8 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 
 	prot &= DMA_PTE_READ | DMA_PTE_WRITE | DMA_PTE_SNP;
 
-	if (sg)
-		sg_res = 0;
-	else {
-		sg_res = nr_pages + 1;
+	if (!sg) {
+		sg_res = nr_pages;
 		pteval = ((phys_addr_t)phys_pfn << VTD_PAGE_SHIFT) | prot;
 	}
 
diff --git a/drivers/mfd/tc6393xb.c b/drivers/mfd/tc6393xb.c
index 9612264..b69d91b 100644
--- a/drivers/mfd/tc6393xb.c
+++ b/drivers/mfd/tc6393xb.c
@@ -263,6 +263,17 @@ static int tc6393xb_ohci_disable(struct platform_device *dev)
 	return 0;
 }
 
+static int tc6393xb_ohci_suspend(struct platform_device *dev)
+{
+	struct tc6393xb_platform_data *tcpd = dev_get_platdata(dev->dev.parent);
+
+	/* We can't properly store/restore OHCI state, so fail here */
+	if (tcpd->resume_restore)
+		return -EBUSY;
+
+	return tc6393xb_ohci_disable(dev);
+}
+
 static int tc6393xb_fb_enable(struct platform_device *dev)
 {
 	struct tc6393xb *tc6393xb = dev_get_drvdata(dev->dev.parent);
@@ -403,7 +414,7 @@ static struct mfd_cell __devinitdata tc6393xb_cells[] = {
 		.num_resources = ARRAY_SIZE(tc6393xb_ohci_resources),
 		.resources = tc6393xb_ohci_resources,
 		.enable = tc6393xb_ohci_enable,
-		.suspend = tc6393xb_ohci_disable,
+		.suspend = tc6393xb_ohci_suspend,
 		.resume = tc6393xb_ohci_enable,
 		.disable = tc6393xb_ohci_disable,
 	},
diff --git a/drivers/mtd/ubi/upd.c b/drivers/mtd/ubi/upd.c
index 425bf5a..068a246 100644
--- a/drivers/mtd/ubi/upd.c
+++ b/drivers/mtd/ubi/upd.c
@@ -135,6 +135,10 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 	ubi_assert(!vol->updating && !vol->changing_leb);
 	vol->updating = 1;
 
+	vol->upd_buf = vmalloc(ubi->leb_size);
+	if (!vol->upd_buf)
+		return -ENOMEM;
+
 	err = set_update_marker(ubi, vol);
 	if (err)
 		return err;
@@ -154,14 +158,12 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 		err = clear_update_marker(ubi, vol, 0);
 		if (err)
 			return err;
+
+		vfree(vol->upd_buf);
 		vol->updating = 0;
 		return 0;
 	}
 
-	vol->upd_buf = vmalloc(ubi->leb_size);
-	if (!vol->upd_buf)
-		return -ENOMEM;
-
 	vol->upd_ebs = div_u64(bytes + vol->usable_leb_size - 1,
 			       vol->usable_leb_size);
 	vol->upd_bytes = bytes;
diff --git a/drivers/net/can/dev.c b/drivers/net/can/dev.c
index d4f7f95..88c39e4 100644
--- a/drivers/net/can/dev.c
+++ b/drivers/net/can/dev.c
@@ -612,10 +612,14 @@ static int can_changelink(struct net_device *dev,
 		if (dev->flags & IFF_UP)
 			return -EBUSY;
 		cm = nla_data(data[IFLA_CAN_CTRLMODE]);
-		if (cm->flags & ~priv->ctrlmode_supported)
+
+		/* check whether changed bits are allowed to be modified */
+		if (cm->mask & ~priv->ctrlmode_supported)
 			return -EOPNOTSUPP;
+
+		/* clear bits to be modified and copy the flag values */
 		priv->ctrlmode &= ~cm->mask;
-		priv->ctrlmode |= cm->flags;
+		priv->ctrlmode |= (cm->flags & cm->mask);
 	}
 
 	if (data[IFLA_CAN_BITTIMING]) {
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_core.c b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
index d2f91f7..925c7e1 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_core.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
@@ -737,7 +737,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 		dev_err(&intf->dev, "%s: couldn't alloc cmd buffer\n",
 			PCAN_USB_DRIVER_NAME);
 		err = -ENOMEM;
-		goto lbl_set_intf_data;
+		goto lbl_free_candev;
 	}
 
 	dev->udev = usb_dev;
@@ -776,7 +776,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	err = register_candev(netdev);
 	if (err) {
 		dev_err(&intf->dev, "couldn't register CAN device: %d\n", err);
-		goto lbl_free_cmd_buf;
+		goto lbl_restore_intf_data;
 	}
 
 	if (dev->prev_siblings)
@@ -789,14 +789,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	if (dev->adapter->dev_init) {
 		err = dev->adapter->dev_init(dev);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* set bus off */
 	if (dev->adapter->dev_set_bus) {
 		err = dev->adapter->dev_set_bus(dev, 0);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* get device number early */
@@ -808,11 +808,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 
 	return 0;
 
-lbl_free_cmd_buf:
-	kfree(dev->cmd_buf);
+lbl_unregister_candev:
+	unregister_candev(netdev);
 
-lbl_set_intf_data:
+lbl_restore_intf_data:
 	usb_set_intfdata(intf, dev->prev_siblings);
+	kfree(dev->cmd_buf);
+
+lbl_free_candev:
 	free_candev(netdev);
 
 	return err;
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
index c95913a..5fe28be 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
@@ -333,8 +333,6 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	if (!(dev->state & PCAN_USB_STATE_CONNECTED))
 		return 0;
 
-	memset(req_addr, '\0', req_size);
-
 	req_type = USB_TYPE_VENDOR | USB_RECIP_OTHER;
 
 	switch (req_id) {
@@ -345,6 +343,7 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	default:
 		p = usb_rcvctrlpipe(dev->udev, 0);
 		req_type |= USB_DIR_IN;
+		memset(req_addr, '\0', req_size);
 		break;
 	}
 
diff --git a/drivers/net/wireless/ath/ath5k/qcu.c b/drivers/net/wireless/ath/ath5k/qcu.c
index 30b50f9..19ba204 100644
--- a/drivers/net/wireless/ath/ath5k/qcu.c
+++ b/drivers/net/wireless/ath/ath5k/qcu.c
@@ -223,13 +223,7 @@ ath5k_hw_setup_tx_queue(struct ath5k_hw *ah, enum ath5k_tx_queue queue_type,
 	} else {
 		switch (queue_type) {
 		case AR5K_TX_QUEUE_DATA:
-			for (queue = AR5K_TX_QUEUE_ID_DATA_MIN;
-				ah->ah_txq[queue].tqi_type !=
-				AR5K_TX_QUEUE_INACTIVE; queue++) {
-
-				if (queue > AR5K_TX_QUEUE_ID_DATA_MAX)
-					return -EINVAL;
-			}
+			queue = queue_info->tqi_subtype;
 			break;
 		case AR5K_TX_QUEUE_UAPSD:
 			queue = AR5K_TX_QUEUE_ID_UAPSD;
diff --git a/drivers/net/wireless/ath/ath9k/hw.h b/drivers/net/wireless/ath/ath9k/hw.h
index f49be96..d4f09b4 100644
--- a/drivers/net/wireless/ath/ath9k/hw.h
+++ b/drivers/net/wireless/ath/ath9k/hw.h
@@ -181,8 +181,8 @@
 #define PAPRD_IDEAL_AGC2_PWR_RANGE	0xe0
 
 enum ath_hw_txq_subtype {
-	ATH_TXQ_AC_BE = 0,
-	ATH_TXQ_AC_BK = 1,
+	ATH_TXQ_AC_BK = 0,
+	ATH_TXQ_AC_BE = 1,
 	ATH_TXQ_AC_VI = 2,
 	ATH_TXQ_AC_VO = 3,
 };
diff --git a/drivers/net/wireless/ath/ath9k/mac.c b/drivers/net/wireless/ath/ath9k/mac.c
index f7bd253..2d628f9 100644
--- a/drivers/net/wireless/ath/ath9k/mac.c
+++ b/drivers/net/wireless/ath/ath9k/mac.c
@@ -303,14 +303,7 @@ int ath9k_hw_setuptxqueue(struct ath_hw *ah, enum ath9k_tx_queue type,
 		q = ATH9K_NUM_TX_QUEUES - 3;
 		break;
 	case ATH9K_TX_QUEUE_DATA:
-		for (q = 0; q < ATH9K_NUM_TX_QUEUES; q++)
-			if (ah->txq[q].tqi_type ==
-			    ATH9K_TX_QUEUE_INACTIVE)
-				break;
-		if (q == ATH9K_NUM_TX_QUEUES) {
-			ath_err(common, "No available TX queue\n");
-			return -1;
-		}
+		q = qinfo->tqi_subtype;
 		break;
 	default:
 		ath_err(common, "Invalid TX queue type: %u\n", type);
diff --git a/drivers/pci/probe.c b/drivers/pci/probe.c
index 63e0199..d62ad0b 100644
--- a/drivers/pci/probe.c
+++ b/drivers/pci/probe.c
@@ -254,14 +254,17 @@ int __pci_read_base(struct pci_dev *dev, enum pci_bar_type type,
 		res->flags |= IORESOURCE_SIZEALIGN;
 		if (res->flags & IORESOURCE_IO) {
 			l &= PCI_BASE_ADDRESS_IO_MASK;
+			sz &= PCI_BASE_ADDRESS_IO_MASK;
 			mask = PCI_BASE_ADDRESS_IO_MASK & (u32) IO_SPACE_LIMIT;
 		} else {
 			l &= PCI_BASE_ADDRESS_MEM_MASK;
+			sz &= PCI_BASE_ADDRESS_MEM_MASK;
 			mask = (u32)PCI_BASE_ADDRESS_MEM_MASK;
 		}
 	} else {
 		res->flags |= (l & IORESOURCE_ROM_ENABLE);
 		l &= PCI_ROM_ADDRESS_MASK;
+		sz &= PCI_ROM_ADDRESS_MASK;
 		mask = (u32)PCI_ROM_ADDRESS_MASK;
 	}
 
diff --git a/drivers/pci/quirks.c b/drivers/pci/quirks.c
index e587d00..ffde183 100644
--- a/drivers/pci/quirks.c
+++ b/drivers/pci/quirks.c
@@ -327,19 +327,52 @@ static void __devinit quirk_s3_64M(struct pci_dev *dev)
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_S3,	PCI_DEVICE_ID_S3_868,		quirk_s3_64M);
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_S3,	PCI_DEVICE_ID_S3_968,		quirk_s3_64M);
 
+static void quirk_io(struct pci_dev *dev, int pos, unsigned size,
+		     const char *name)
+{
+	u32 region;
+	struct pci_bus_region bus_region;
+	struct resource *res = dev->resource + pos;
+
+	pci_read_config_dword(dev, PCI_BASE_ADDRESS_0 + (pos << 2), &region);
+
+	if (!region)
+		return;
+
+	res->name = pci_name(dev);
+	res->flags = region & ~PCI_BASE_ADDRESS_IO_MASK;
+	res->flags |=
+		(IORESOURCE_IO | IORESOURCE_PCI_FIXED | IORESOURCE_SIZEALIGN);
+	region &= ~(size - 1);
+
+	/* Convert from PCI bus to resource space */
+	bus_region.start = region;
+	bus_region.end = region + size - 1;
+	pcibios_bus_to_resource(dev->bus, res, &bus_region);
+
+	dev_info(&dev->dev, FW_BUG "%s quirk: reg 0x%x: %pR\n",
+		 name, PCI_BASE_ADDRESS_0 + (pos << 2), res);
+}
+
 /*
  * Some CS5536 BIOSes (for example, the Soekris NET5501 board w/ comBIOS
  * ver. 1.33  20070103) don't set the correct ISA PCI region header info.
  * BAR0 should be 8 bytes; instead, it may be set to something like 8k
  * (which conflicts w/ BAR1's memory range).
+ *
+ * CS553x's ISA PCI BARs may also be read-only (ref:
+ * https://bugzilla.kernel.org/show_bug.cgi?id=85991 - Comment #4 forward).
  */
 static void __devinit quirk_cs5536_vsa(struct pci_dev *dev)
 {
+	static char *name = "CS5536 ISA bridge";
+
 	if (pci_resource_len(dev, 0) != 8) {
-		struct resource *res = &dev->resource[0];
-		res->end = res->start + 8 - 1;
-		dev_info(&dev->dev, "CS5536 ISA bridge bug detected "
-				"(incorrect header); workaround applied.\n");
+		quirk_io(dev, 0,   8, name);	/* SMB */
+		quirk_io(dev, 1, 256, name);	/* GPIO */
+		quirk_io(dev, 2,  64, name);	/* MFGPT */
+		dev_info(&dev->dev, "%s bug detected (incorrect header); workaround applied\n",
+			 name);
 	}
 }
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_AMD, PCI_DEVICE_ID_AMD_CS5536_ISA, quirk_cs5536_vsa);
diff --git a/drivers/platform/x86/hp_accel.c b/drivers/platform/x86/hp_accel.c
index 0076fea..be6b648 100644
--- a/drivers/platform/x86/hp_accel.c
+++ b/drivers/platform/x86/hp_accel.c
@@ -237,6 +237,7 @@ static struct dmi_system_id lis3lv02d_dmi_ids[] = {
 	AXIS_DMI_MATCH("HPB64xx", "HP ProBook 64", xy_swap),
 	AXIS_DMI_MATCH("HPB64xx", "HP EliteBook 84", xy_swap),
 	AXIS_DMI_MATCH("HPB65xx", "HP ProBook 65", x_inverted),
+	AXIS_DMI_MATCH("HPZBook15", "HP ZBook 15", x_inverted),
 	{ NULL, }
 /* Laptop models without axis info (yet):
  * "NC6910" "HP Compaq 6910"
diff --git a/drivers/regulator/core.c b/drivers/regulator/core.c
index c45c2dc..98ccd6a 100644
--- a/drivers/regulator/core.c
+++ b/drivers/regulator/core.c
@@ -1427,12 +1427,14 @@ void regulator_put(struct regulator *regulator)
 		device_remove_file(regulator->dev, &regulator->dev_attr);
 		kfree(regulator->dev_attr.attr.name);
 	}
+	mutex_lock(&rdev->mutex);
 	kfree(regulator->supply_name);
 	list_del(&regulator->list);
 	kfree(regulator);
 
 	rdev->open_count--;
 	rdev->exclusive = 0;
+	mutex_unlock(&rdev->mutex);
 
 	module_put(rdev->owner);
 	mutex_unlock(&regulator_list_mutex);
diff --git a/drivers/s390/char/con3215.c b/drivers/s390/char/con3215.c
index 4f9f1dc..fa47d8d 100644
--- a/drivers/s390/char/con3215.c
+++ b/drivers/s390/char/con3215.c
@@ -997,12 +997,26 @@ static int tty3215_write(struct tty_struct * tty,
 			 const unsigned char *buf, int count)
 {
 	struct raw3215_info *raw;
+	int i, written;
 
 	if (!tty)
 		return 0;
 	raw = (struct raw3215_info *) tty->driver_data;
-	raw3215_write(raw, buf, count);
-	return count;
+	written = count;
+	while (count > 0) {
+		for (i = 0; i < count; i++)
+			if (buf[i] == '\t' || buf[i] == '\n')
+				break;
+		raw3215_write(raw, buf, i);
+		count -= i;
+		buf += i;
+		if (count > 0) {
+			raw3215_putchar(raw, *buf);
+			count--;
+			buf++;
+		}
+	}
+	return written;
 }
 
 /*
@@ -1149,7 +1163,7 @@ static int __init tty3215_init(void)
 	driver->subtype = SYSTEM_TYPE_TTY;
 	driver->init_termios = tty_std_termios;
 	driver->init_termios.c_iflag = IGNBRK | IGNPAR;
-	driver->init_termios.c_oflag = ONLCR | XTABS;
+	driver->init_termios.c_oflag = ONLCR;
 	driver->init_termios.c_lflag = ISIG;
 	driver->flags = TTY_DRIVER_REAL_RAW;
 	tty_set_operations(driver, &tty3215_ops);
diff --git a/drivers/scsi/NCR5380.c b/drivers/scsi/NCR5380.c
index 165e4dd86..a57f85a 100644
--- a/drivers/scsi/NCR5380.c
+++ b/drivers/scsi/NCR5380.c
@@ -2662,14 +2662,14 @@ static void NCR5380_dma_complete(NCR5380_instance * instance) {
  *
  * Purpose : abort a command
  *
- * Inputs : cmd - the Scsi_Cmnd to abort, code - code to set the 
- *      host byte of the result field to, if zero DID_ABORTED is 
+ * Inputs : cmd - the Scsi_Cmnd to abort, code - code to set the
+ *      host byte of the result field to, if zero DID_ABORTED is
  *      used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
- *	XXX - there is no way to abort the command that is currently 
- *	connected, you have to wait for it to complete.  If this is 
+ *	XXX - there is no way to abort the command that is currently
+ *	connected, you have to wait for it to complete.  If this is
  *	a problem, we could implement longjmp() / setjmp(), setjmp()
  *	called where the loop started in NCR5380_main().
  *
@@ -2719,7 +2719,7 @@ static int NCR5380_abort(Scsi_Cmnd * cmd) {
  * aborted flag and get back into our main loop.
  */
 
-		return 0;
+		return SUCCESS;
 	}
 #endif
 
diff --git a/drivers/scsi/aha1740.c b/drivers/scsi/aha1740.c
index a3e6ed3..d0fa3e7 100644
--- a/drivers/scsi/aha1740.c
+++ b/drivers/scsi/aha1740.c
@@ -550,7 +550,7 @@ static int aha1740_eh_abort_handler (Scsi_Cmnd *dummy)
  * quiet as possible...
  */
 
-	return 0;
+	return SUCCESS;
 }
 
 static struct scsi_host_template aha1740_template = {
diff --git a/drivers/scsi/atari_NCR5380.c b/drivers/scsi/atari_NCR5380.c
index 2db79b4..589c2a3 100644
--- a/drivers/scsi/atari_NCR5380.c
+++ b/drivers/scsi/atari_NCR5380.c
@@ -2638,7 +2638,7 @@ static void NCR5380_reselect(struct Scsi_Host *instance)
  *	host byte of the result field to, if zero DID_ABORTED is
  *	used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
  * XXX - there is no way to abort the command that is currently
  *	 connected, you have to wait for it to complete.  If this is
diff --git a/drivers/scsi/bnx2fc/bnx2fc_fcoe.c b/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
index c1c6a92..cabfbf3 100644
--- a/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
+++ b/drivers/scsi/bnx2fc/bnx2fc_fcoe.c
@@ -406,6 +406,7 @@ static int bnx2fc_rcv(struct sk_buff *skb, struct net_device *dev,
 	struct fc_frame_header *fh;
 	struct fcoe_rcv_info *fr;
 	struct fcoe_percpu_s *bg;
+	struct sk_buff *tmp_skb;
 	unsigned short oxid;
 
 	interface = container_of(ptype, struct bnx2fc_interface,
@@ -417,6 +418,12 @@ static int bnx2fc_rcv(struct sk_buff *skb, struct net_device *dev,
 		goto err;
 	}
 
+	tmp_skb = skb_share_check(skb, GFP_ATOMIC);
+	if (!tmp_skb)
+		goto err;
+
+	skb = tmp_skb;
+
 	if (unlikely(eth_hdr(skb)->h_proto != htons(ETH_P_FCOE))) {
 		printk(KERN_ERR PFX "bnx2fc_rcv: Wrong FC type frame\n");
 		goto err;
diff --git a/drivers/scsi/megaraid.c b/drivers/scsi/megaraid.c
index 4d39a9f..152fe62 100644
--- a/drivers/scsi/megaraid.c
+++ b/drivers/scsi/megaraid.c
@@ -1967,7 +1967,7 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 	     cmd->device->id, cmd->device->lun);
 
 	if(list_empty(&adapter->pending_list))
-		return FALSE;
+		return FAILED;
 
 	list_for_each_safe(pos, next, &adapter->pending_list) {
 
@@ -1990,7 +1990,7 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 					(aor==SCB_ABORT) ? "ABORTING":"RESET",
 					scb->idx);
 
-				return FALSE;
+				return FAILED;
 			}
 			else {
 
@@ -2015,12 +2015,12 @@ megaraid_abort_and_reset(adapter_t *adapter, Scsi_Cmnd *cmd, int aor)
 				list_add_tail(SCSI_LIST(cmd),
 						&adapter->completed_list);
 
-				return TRUE;
+				return SUCCESS;
 			}
 		}
 	}
 
-	return FALSE;
+	return FAILED;
 }
 
 static inline int
diff --git a/drivers/scsi/megaraid/megaraid_sas_base.c b/drivers/scsi/megaraid/megaraid_sas_base.c
index 6188700..bacd344 100644
--- a/drivers/scsi/megaraid/megaraid_sas_base.c
+++ b/drivers/scsi/megaraid/megaraid_sas_base.c
@@ -919,7 +919,7 @@ megasas_issue_blocked_abort_cmd(struct megasas_instance *instance,
 	abort_fr->abort_mfi_phys_addr_hi = 0;
 
 	cmd->sync_cmd = 1;
-	cmd->cmd_status = 0xFF;
+	cmd->cmd_status = ENODATA;
 
 	instance->instancet->issue_dcmd(instance, cmd);
 
diff --git a/drivers/scsi/sd.c b/drivers/scsi/sd.c
index 71459d5..e127ceb 100644
--- a/drivers/scsi/sd.c
+++ b/drivers/scsi/sd.c
@@ -2227,7 +2227,10 @@ sd_read_cache_type(struct scsi_disk *sdkp, unsigned char *buffer)
 		}
 
 		sdkp->DPOFUA = (data.device_specific & 0x10) != 0;
-		if (sdkp->DPOFUA && !sdkp->device->use_10_for_rw) {
+		if (sdp->broken_fua) {
+			sd_printk(KERN_NOTICE, sdkp, "Disabling FUA\n");
+			sdkp->DPOFUA = 0;
+		} else if (sdkp->DPOFUA && !sdkp->device->use_10_for_rw) {
 			sd_printk(KERN_NOTICE, sdkp,
 				  "Uses READ/WRITE(6), disabling FUA\n");
 			sdkp->DPOFUA = 0;
diff --git a/drivers/scsi/storvsc_drv.c b/drivers/scsi/storvsc_drv.c
index 446c023..a0df0fb 100644
--- a/drivers/scsi/storvsc_drv.c
+++ b/drivers/scsi/storvsc_drv.c
@@ -1359,13 +1359,12 @@ static int storvsc_queuecommand(struct Scsi_Host *host, struct scsi_cmnd *scmnd)
 	if (ret == -EAGAIN) {
 		/* no more space */
 
-		if (cmd_request->bounce_sgl_count) {
+		if (cmd_request->bounce_sgl_count)
 			destroy_bounce_buffer(cmd_request->bounce_sgl,
 					cmd_request->bounce_sgl_count);
 
-			ret = SCSI_MLQUEUE_DEVICE_BUSY;
-			goto queue_error;
-		}
+		ret = SCSI_MLQUEUE_DEVICE_BUSY;
+		goto queue_error;
 	}
 
 	return 0;
diff --git a/drivers/scsi/sun3_NCR5380.c b/drivers/scsi/sun3_NCR5380.c
index 7e12a2e..9aaf084 100644
--- a/drivers/scsi/sun3_NCR5380.c
+++ b/drivers/scsi/sun3_NCR5380.c
@@ -2624,15 +2624,15 @@ static void NCR5380_reselect (struct Scsi_Host *instance)
  * Purpose : abort a command
  *
  * Inputs : cmd - the struct scsi_cmnd to abort, code - code to set the
- * 	host byte of the result field to, if zero DID_ABORTED is 
+ *	host byte of the result field to, if zero DID_ABORTED is
  *	used.
  *
- * Returns : 0 - success, -1 on failure.
+ * Returns : SUCCESS - success, FAILED on failure.
  *
- * XXX - there is no way to abort the command that is currently 
- * 	 connected, you have to wait for it to complete.  If this is 
+ * XXX - there is no way to abort the command that is currently
+ *	 connected, you have to wait for it to complete.  If this is
  *	 a problem, we could implement longjmp() / setjmp(), setjmp()
- * 	 called where the loop started in NCR5380_main().
+ *	 called where the loop started in NCR5380_main().
  */
 
 static int NCR5380_abort(struct scsi_cmnd *cmd)
diff --git a/drivers/spi/spi-dw-mid.c b/drivers/spi/spi-dw-mid.c
index efc494a..f15f624 100644
--- a/drivers/spi/spi-dw-mid.c
+++ b/drivers/spi/spi-dw-mid.c
@@ -219,7 +219,6 @@ int dw_spi_mid_init(struct dw_spi *dws)
 	iounmap(clk_reg);
 
 	dws->num_cs = 16;
-	dws->fifo_len = 40;	/* FIFO has 40 words buffer */
 
 #ifdef CONFIG_SPI_DW_MID_DMA
 	dws->dma_priv = kzalloc(sizeof(struct mid_dma), GFP_KERNEL);
diff --git a/drivers/spi/spi-dw.c b/drivers/spi/spi-dw.c
index d1a495f..cce2d7b 100644
--- a/drivers/spi/spi-dw.c
+++ b/drivers/spi/spi-dw.c
@@ -394,9 +394,6 @@ static void pump_transfers(unsigned long data)
 	chip = dws->cur_chip;
 	spi = message->spi;
 
-	if (unlikely(!chip->clk_div))
-		chip->clk_div = dws->max_freq / chip->speed_hz;
-
 	if (message->state == ERROR_STATE) {
 		message->status = -EIO;
 		goto early_exit;
@@ -438,7 +435,7 @@ static void pump_transfers(unsigned long data)
 	if (transfer->speed_hz) {
 		speed = chip->speed_hz;
 
-		if (transfer->speed_hz != speed) {
+		if ((transfer->speed_hz != speed) || (!chip->clk_div)) {
 			speed = transfer->speed_hz;
 			if (speed > dws->max_freq) {
 				printk(KERN_ERR "MRST SPI0: unsupported"
@@ -677,7 +674,6 @@ static int dw_spi_setup(struct spi_device *spi)
 		dev_err(&spi->dev, "No max speed HZ parameter\n");
 		return -EINVAL;
 	}
-	chip->speed_hz = spi->max_speed_hz;
 
 	chip->tmode = 0; /* Tx & Rx */
 	/* Default SPI mode is SCPOL = 0, SCPH = 0 */
@@ -784,13 +780,13 @@ static void spi_hw_init(struct dw_spi *dws)
 	 */
 	if (!dws->fifo_len) {
 		u32 fifo;
-		for (fifo = 2; fifo <= 257; fifo++) {
+		for (fifo = 1; fifo < 256; fifo++) {
 			dw_writew(dws, DW_SPI_TXFLTR, fifo);
 			if (fifo != dw_readw(dws, DW_SPI_TXFLTR))
 				break;
 		}
 
-		dws->fifo_len = (fifo == 257) ? 0 : fifo;
+		dws->fifo_len = (fifo == 1) ? 0 : fifo;
 		dw_writew(dws, DW_SPI_TXFLTR, 0);
 	}
 }
diff --git a/drivers/staging/comedi/drivers/cb_pcidas64.c b/drivers/staging/comedi/drivers/cb_pcidas64.c
index 915157d..6f743df 100644
--- a/drivers/staging/comedi/drivers/cb_pcidas64.c
+++ b/drivers/staging/comedi/drivers/cb_pcidas64.c
@@ -423,6 +423,29 @@ static const struct comedi_lrange ai_ranges_64xx = {
 	 }
 };
 
+static const uint8_t ai_range_code_64xx[8] = {
+	0x0, 0x1, 0x2, 0x3,	/* bipolar 10, 5, 2,5, 1.25 */
+	0x8, 0x9, 0xa, 0xb	/* unipolar 10, 5, 2.5, 1.25 */
+};
+
+/* analog input ranges for 64-Mx boards */
+static const struct comedi_lrange ai_ranges_64_mx = {
+	7, {
+		BIP_RANGE(5),
+		BIP_RANGE(2.5),
+		BIP_RANGE(1.25),
+		BIP_RANGE(0.625),
+		UNI_RANGE(5),
+		UNI_RANGE(2.5),
+		UNI_RANGE(1.25)
+	}
+};
+
+static const uint8_t ai_range_code_64_mx[7] = {
+	0x0, 0x1, 0x2, 0x3,	/* bipolar 5, 2.5, 1.25, 0.625 */
+	0x9, 0xa, 0xb		/* unipolar 5, 2.5, 1.25 */
+};
+
 /* analog input ranges for 60xx boards */
 static const struct comedi_lrange ai_ranges_60xx = {
 	4,
@@ -434,6 +457,10 @@ static const struct comedi_lrange ai_ranges_60xx = {
 	 }
 };
 
+static const uint8_t ai_range_code_60xx[4] = {
+	0x0, 0x1, 0x4, 0x7	/* bipolar 10, 5, 0.5, 0.05 */
+};
+
 /* analog input ranges for 6030, etc boards */
 static const struct comedi_lrange ai_ranges_6030 = {
 	14,
@@ -455,6 +482,11 @@ static const struct comedi_lrange ai_ranges_6030 = {
 	 }
 };
 
+static const uint8_t ai_range_code_6030[14] = {
+	0x0, 0x1, 0x2, 0x3, 0x4, 0x5, 0x6, /* bip 10, 5, 2, 1, 0.5, 0.2, 0.1 */
+	0x9, 0xa, 0xb, 0xc, 0xd, 0xe, 0xf  /* uni 10, 5, 2, 1, 0.5, 0.2, 0.1 */
+};
+
 /* analog input ranges for 6052, etc boards */
 static const struct comedi_lrange ai_ranges_6052 = {
 	15,
@@ -477,6 +509,11 @@ static const struct comedi_lrange ai_ranges_6052 = {
 	 }
 };
 
+static const uint8_t ai_range_code_6052[15] = {
+	0x0, 0x1, 0x2, 0x3, 0x4, 0x5, 0x6, 0x7,	/* bipolar 10 ... 0.05 */
+	0x9, 0xa, 0xb, 0xc, 0xd, 0xe, 0xf	/* unipolar 10 ... 0.1 */
+};
+
 /* analog input ranges for 4020 board */
 static const struct comedi_lrange ai_ranges_4020 = {
 	2,
@@ -561,6 +598,7 @@ struct pcidas64_board {
 	int ai_bits;		/*  analog input resolution */
 	int ai_speed;		/*  fastest conversion period in ns */
 	const struct comedi_lrange *ai_range_table;
+	const uint8_t *ai_range_code;
 	int ao_nchan;		/*  number of analog out channels */
 	int ao_bits;		/*  analog output resolution */
 	int ao_scan_speed;	/*  analog output speed (for a scan, not conversion) */
@@ -619,6 +657,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -635,6 +674,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -650,7 +690,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -666,7 +707,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -682,7 +724,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ao_range_table = &ao_ranges_64xx,
 	 .ao_range_code = ao_range_code_64xx,
 	 .ai_fifo = &ai_fifo_64xx,
@@ -698,6 +741,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_bits = 16,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -714,6 +758,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -729,6 +774,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -745,6 +791,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -761,6 +808,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -777,6 +825,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -791,6 +840,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -803,6 +853,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6030,
+	 .ai_range_code = ai_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -816,6 +867,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 0,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
 	 .has_8255 = 0,
 	 },
@@ -830,6 +882,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -846,6 +899,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 100000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_60xx,
+	 .ai_range_code = ai_range_code_60xx,
 	 .ao_range_table = &ao_ranges_60xx,
 	 .ao_range_code = ao_range_code_60xx,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -862,6 +916,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -878,6 +933,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 3333,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -894,6 +950,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -910,6 +967,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 1000,
 	 .layout = LAYOUT_60XX,
 	 .ai_range_table = &ai_ranges_6052,
+	 .ai_range_code = ai_range_code_6052,
 	 .ao_range_table = &ao_ranges_6030,
 	 .ao_range_code = ao_range_code_6030,
 	 .ai_fifo = &ai_fifo_60xx,
@@ -942,6 +1000,7 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
 	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_code = ai_range_code_64xx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -954,7 +1013,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -967,7 +1027,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -980,7 +1041,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 0,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -993,7 +1055,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1006,7 +1069,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1019,7 +1083,8 @@ static const struct pcidas64_board pcidas64_boards[] = {
 	 .ao_nchan = 2,
 	 .ao_scan_speed = 10000,
 	 .layout = LAYOUT_64XX,
-	 .ai_range_table = &ai_ranges_64xx,
+	 .ai_range_table = &ai_ranges_64_mx,
+	 .ai_range_code = ai_range_code_64_mx,
 	 .ai_fifo = ai_fifo_64xx,
 	 .has_8255 = 1,
 	 },
@@ -1257,45 +1322,7 @@ module_exit(driver_cb_pcidas_cleanup_module);
 static unsigned int ai_range_bits_6xxx(const struct comedi_device *dev,
 				       unsigned int range_index)
 {
-	const struct comedi_krange *range =
-	    &board(dev)->ai_range_table->range[range_index];
-	unsigned int bits = 0;
-
-	switch (range->max) {
-	case 10000000:
-		bits = 0x000;
-		break;
-	case 5000000:
-		bits = 0x100;
-		break;
-	case 2000000:
-	case 2500000:
-		bits = 0x200;
-		break;
-	case 1000000:
-	case 1250000:
-		bits = 0x300;
-		break;
-	case 500000:
-		bits = 0x400;
-		break;
-	case 200000:
-	case 250000:
-		bits = 0x500;
-		break;
-	case 100000:
-		bits = 0x600;
-		break;
-	case 50000:
-		bits = 0x700;
-		break;
-	default:
-		comedi_error(dev, "bug! in ai_range_bits_6xxx");
-		break;
-	}
-	if (range->min == 0)
-		bits += 0x900;
-	return bits;
+	return board(dev)->ai_range_code[range_index] << 8;
 }
 
 static unsigned int hw_revision(const struct comedi_device *dev,
diff --git a/drivers/staging/iio/events.h b/drivers/staging/iio/events.h
index c25f0e3..a6f999c 100644
--- a/drivers/staging/iio/events.h
+++ b/drivers/staging/iio/events.h
@@ -90,7 +90,7 @@ enum iio_event_direction {
 
 #define IIO_EVENT_CODE_EXTRACT_TYPE(mask) ((mask >> 56) & 0xFF)
 
-#define IIO_EVENT_CODE_EXTRACT_DIR(mask) ((mask >> 48) & 0xCF)
+#define IIO_EVENT_CODE_EXTRACT_DIR(mask) ((mask >> 48) & 0x7F)
 
 #define IIO_EVENT_CODE_EXTRACT_CHAN_TYPE(mask) ((mask >> 32) & 0xFF)
 
diff --git a/drivers/target/iscsi/iscsi_target_util.c b/drivers/target/iscsi/iscsi_target_util.c
index 4c05ed6..8d57ab3 100644
--- a/drivers/target/iscsi/iscsi_target_util.c
+++ b/drivers/target/iscsi/iscsi_target_util.c
@@ -1480,15 +1480,15 @@ static int iscsit_do_tx_data(
 	struct iscsi_conn *conn,
 	struct iscsi_data_count *count)
 {
-	int data = count->data_length, total_tx = 0, tx_loop = 0, iov_len;
+	int ret, iov_len;
 	struct kvec *iov_p;
 	struct msghdr msg;
 
 	if (!conn || !conn->sock || !conn->conn_ops)
 		return -1;
 
-	if (data <= 0) {
-		pr_err("Data length is: %d\n", data);
+	if (count->data_length <= 0) {
+		pr_err("Data length is: %d\n", count->data_length);
 		return -1;
 	}
 
@@ -1497,20 +1497,16 @@ static int iscsit_do_tx_data(
 	iov_p = count->iov;
 	iov_len = count->iov_count;
 
-	while (total_tx < data) {
-		tx_loop = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
-					(data - total_tx));
-		if (tx_loop <= 0) {
-			pr_debug("tx_loop: %d total_tx %d\n",
-				tx_loop, total_tx);
-			return tx_loop;
-		}
-		total_tx += tx_loop;
-		pr_debug("tx_loop: %d, total_tx: %d, data: %d\n",
-					tx_loop, total_tx, data);
+	ret = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
+			     count->data_length);
+	if (ret != count->data_length) {
+		pr_err("Unexpected ret: %d send data %d\n",
+		       ret, count->data_length);
+		return -EPIPE;
 	}
+	pr_debug("ret: %d, sent data: %d\n", ret, count->data_length);
 
-	return total_tx;
+	return ret;
 }
 
 int rx_data(
diff --git a/drivers/tty/serial/samsung.c b/drivers/tty/serial/samsung.c
index c49f3bf..8b409d4 100644
--- a/drivers/tty/serial/samsung.c
+++ b/drivers/tty/serial/samsung.c
@@ -528,11 +528,15 @@ static void s3c24xx_serial_pm(struct uart_port *port, unsigned int level,
 			      unsigned int old)
 {
 	struct s3c24xx_uart_port *ourport = to_ourport(port);
+	int timeout = 10000;
 
 	ourport->pm_level = level;
 
 	switch (level) {
 	case 3:
+		while (--timeout && !s3c24xx_serial_txempty_nofifo(port))
+			udelay(100);
+
 		if (!IS_ERR(ourport->baudclk) && ourport->baudclk != NULL)
 			clk_disable(ourport->baudclk);
 
diff --git a/drivers/usb/class/cdc-acm.c b/drivers/usb/class/cdc-acm.c
index 8f4a628..0532577 100644
--- a/drivers/usb/class/cdc-acm.c
+++ b/drivers/usb/class/cdc-acm.c
@@ -1108,10 +1108,11 @@ static int acm_probe(struct usb_interface *intf,
 	} else {
 		control_interface = usb_ifnum_to_if(usb_dev, union_header->bMasterInterface0);
 		data_interface = usb_ifnum_to_if(usb_dev, (data_interface_num = union_header->bSlaveInterface0));
-		if (!control_interface || !data_interface) {
-			dev_dbg(&intf->dev, "no interfaces\n");
-			return -ENODEV;
-		}
+	}
+
+	if (!control_interface || !data_interface) {
+		dev_dbg(&intf->dev, "no interfaces\n");
+		return -ENODEV;
 	}
 
 	if (data_interface_num != call_interface_num)
@@ -1429,6 +1430,7 @@ static void acm_disconnect(struct usb_interface *intf)
 				&dev_attr_wCountryCodes);
 		device_remove_file(&acm->control->dev,
 				&dev_attr_iCountryCodeRelDate);
+		kfree(acm->country_codes);
 	}
 	device_remove_file(&acm->control->dev, &dev_attr_bmCapabilities);
 	usb_set_intfdata(acm->control, NULL);
diff --git a/drivers/usb/core/config.c b/drivers/usb/core/config.c
index 6ed7e7c..cc1004a 100644
--- a/drivers/usb/core/config.c
+++ b/drivers/usb/core/config.c
@@ -201,6 +201,17 @@ static int usb_parse_endpoint(struct device *ddev, int cfgno, int inum,
 			if (n == 0)
 				n = 9;	/* 32 ms = 2^(9-1) uframes */
 			j = 16;
+
+			/*
+			 * Adjust bInterval for quirked devices.
+			 * This quirk fixes bIntervals reported in
+			 * linear microframes.
+			 */
+			if (to_usb_device(ddev)->quirks &
+				USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL) {
+				n = clamp(fls(d->bInterval), i, j);
+				i = j = n;
+			}
 			break;
 		default:		/* USB_SPEED_FULL or _LOW */
 			/* For low-speed, 10 ms is the official minimum.
diff --git a/drivers/usb/core/quirks.c b/drivers/usb/core/quirks.c
index d482141..95f60d0 100644
--- a/drivers/usb/core/quirks.c
+++ b/drivers/usb/core/quirks.c
@@ -38,6 +38,9 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* Creative SB Audigy 2 NX */
 	{ USB_DEVICE(0x041e, 0x3020), .driver_info = USB_QUIRK_RESET_RESUME },
 
+	/* Microsoft Wireless Laser Mouse 6000 Receiver */
+	{ USB_DEVICE(0x045e, 0x00e1), .driver_info = USB_QUIRK_RESET_RESUME },
+
 	/* Microsoft LifeCam-VX700 v2.0 */
 	{ USB_DEVICE(0x045e, 0x0770), .driver_info = USB_QUIRK_RESET_RESUME },
 
@@ -174,6 +177,10 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* SKYMEDI USB_DRIVE */
 	{ USB_DEVICE(0x1516, 0x8628), .driver_info = USB_QUIRK_RESET_RESUME },
 
+	/* Razer - Razer Blade Keyboard */
+	{ USB_DEVICE(0x1532, 0x0116), .driver_info =
+			USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL },
+
 	/* BUILDWIN Photo Frame */
 	{ USB_DEVICE(0x1908, 0x1315), .driver_info =
 			USB_QUIRK_HONOR_BNUMINTERFACES },
@@ -184,6 +191,10 @@ static const struct usb_device_id usb_quirk_list[] = {
 	/* Protocol and OTG Electrical Test Device */
 	{ USB_DEVICE(0x1a0a, 0x0200), .driver_info = USB_QUIRK_OTG_PET },
 
+	/* Protocol and OTG Electrical Test Device */
+	{ USB_DEVICE(0x1a0a, 0x0200), .driver_info =
+			USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL },
+
 	{ }  /* terminating entry must be last */
 };
 
diff --git a/drivers/usb/host/pci-quirks.c b/drivers/usb/host/pci-quirks.c
index 90dcf54..1f230ed 100644
--- a/drivers/usb/host/pci-quirks.c
+++ b/drivers/usb/host/pci-quirks.c
@@ -470,7 +470,8 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 {
 	void __iomem *base;
 	u32 control;
-	u32 fminterval;
+	u32 fminterval = 0;
+	bool no_fminterval = false;
 	int cnt;
 
 	if (!mmio_resource_enabled(pdev, 0))
@@ -480,6 +481,13 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	if (base == NULL)
 		return;
 
+	/*
+	 * ULi M5237 OHCI controller locks the whole system when accessing
+	 * the OHCI_FMINTERVAL offset.
+	 */
+	if (pdev->vendor == PCI_VENDOR_ID_AL && pdev->device == 0x5237)
+		no_fminterval = true;
+
 	control = readl(base + OHCI_CONTROL);
 
 /* On PA-RISC, PDC can leave IR set incorrectly; ignore it there. */
@@ -518,7 +526,9 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	}
 
 	/* software reset of the controller, preserving HcFmInterval */
-	fminterval = readl(base + OHCI_FMINTERVAL);
+	if (!no_fminterval)
+		fminterval = readl(base + OHCI_FMINTERVAL);
+
 	writel(OHCI_HCR, base + OHCI_CMDSTATUS);
 
 	/* reset requires max 10 us delay */
@@ -527,7 +537,9 @@ static void __devinit quirk_usb_handoff_ohci(struct pci_dev *pdev)
 			break;
 		udelay(1);
 	}
-	writel(fminterval, base + OHCI_FMINTERVAL);
+
+	if (!no_fminterval)
+		writel(fminterval, base + OHCI_FMINTERVAL);
 
 	/* Now the controller is safely in SUSPEND and nothing can wake it up */
 	iounmap(base);
diff --git a/drivers/usb/host/xhci-pci.c b/drivers/usb/host/xhci-pci.c
index 0e1f1f0..7d1a99dd 100644
--- a/drivers/usb/host/xhci-pci.c
+++ b/drivers/usb/host/xhci-pci.c
@@ -222,7 +222,7 @@ static int xhci_pci_suspend(struct usb_hcd *hcd, bool do_wakeup)
 			xhci->shared_hcd->state != HC_STATE_SUSPENDED)
 		return -EINVAL;
 
-	retval = xhci_suspend(xhci);
+	retval = xhci_suspend(xhci, do_wakeup);
 
 	return retval;
 }
diff --git a/drivers/usb/host/xhci-ring.c b/drivers/usb/host/xhci-ring.c
index 5cdb965..7a10a49 100644
--- a/drivers/usb/host/xhci-ring.c
+++ b/drivers/usb/host/xhci-ring.c
@@ -1182,9 +1182,8 @@ static void handle_reset_ep_completion(struct xhci_hcd *xhci,
 				false);
 		xhci_ring_cmd_db(xhci);
 	} else {
-		/* Clear our internal halted state and restart the ring(s) */
+		/* Clear our internal halted state */
 		xhci->devs[slot_id]->eps[ep_index].ep_state &= ~EP_HALTED;
-		ring_doorbell_for_active_rings(xhci, slot_id, ep_index);
 	}
 }
 
@@ -1922,23 +1921,12 @@ static int finish_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		ep->stopped_trb = event_trb;
 		return 0;
 	} else {
-		if (trb_comp_code == COMP_STALL) {
-			/* The transfer is completed from the driver's
-			 * perspective, but we need to issue a set dequeue
-			 * command for this stalled endpoint to move the dequeue
-			 * pointer past the TD.  We can't do that here because
-			 * the halt condition must be cleared first.  Let the
-			 * USB class driver clear the stall later.
-			 */
-			ep->stopped_td = td;
-			ep->stopped_trb = event_trb;
-			ep->stopped_stream = ep_ring->stream_id;
-		} else if (xhci_requires_manual_halt_cleanup(xhci,
-					ep_ctx, trb_comp_code)) {
-			/* Other types of errors halt the endpoint, but the
-			 * class driver doesn't call usb_reset_endpoint() unless
-			 * the error is -EPIPE.  Clear the halted status in the
-			 * xHCI hardware manually.
+		if (trb_comp_code == COMP_STALL ||
+		    xhci_requires_manual_halt_cleanup(xhci, ep_ctx,
+						      trb_comp_code)) {
+			/* Issue a reset endpoint command to clear the host side			 * halt, followed by a set dequeue command to move the
+			 * dequeue pointer past the TD.
+			 * The class driver clears the device side halt later.
 			 */
 			xhci_cleanup_halted_endpoint(xhci,
 					slot_id, ep_index, ep_ring->stream_id,
@@ -2058,9 +2046,7 @@ static int process_ctrl_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		else
 			td->urb->actual_length = 0;
 
-		xhci_cleanup_halted_endpoint(xhci,
-			slot_id, ep_index, 0, td, event_trb);
-		return finish_td(xhci, td, event_trb, event, ep, status, true);
+		return finish_td(xhci, td, event_trb, event, ep, status, false);
 	}
 	/*
 	 * Did we transfer any data, despite the errors that might have
@@ -2612,17 +2598,8 @@ static int handle_tx_event(struct xhci_hcd *xhci,
 		if (ret) {
 			urb = td->urb;
 			urb_priv = urb->hcpriv;
-			/* Leave the TD around for the reset endpoint function
-			 * to use(but only if it's not a control endpoint,
-			 * since we already queued the Set TR dequeue pointer
-			 * command for stalled control endpoints).
-			 */
-			if (usb_endpoint_xfer_control(&urb->ep->desc) ||
-				(trb_comp_code != COMP_STALL &&
-					trb_comp_code != COMP_BABBLE))
-				xhci_urb_free_priv(xhci, urb_priv);
-			else
-				kfree(urb_priv);
+
+			xhci_urb_free_priv(xhci, urb_priv);
 
 			usb_hcd_unlink_urb_from_ep(bus_to_hcd(urb->dev->bus), urb);
 			if ((urb->actual_length != urb->transfer_buffer_length &&
diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index 1bef534..b20962d 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -33,6 +33,8 @@
 #define DRIVER_AUTHOR "Sarah Sharp"
 #define DRIVER_DESC "'eXtensible' Host Controller (xHC) Driver"
 
+#define	PORT_WAKE_BITS	(PORT_WKOC_E | PORT_WKDISC_E | PORT_WKCONN_E)
+
 /* Some 0.95 hardware can't handle the chain bit on a Link TRB being cleared */
 static int link_quirk;
 module_param(link_quirk, int, S_IRUGO | S_IWUSR);
@@ -887,18 +889,56 @@ static void xhci_clear_command_ring(struct xhci_hcd *xhci)
 	xhci_set_cmd_ring_deq(xhci);
 }
 
+static void xhci_disable_port_wake_on_bits(struct xhci_hcd *xhci)
+{
+	int port_index;
+	__le32 __iomem **port_array;
+	unsigned long flags;
+	u32 t1, t2;
+
+	spin_lock_irqsave(&xhci->lock, flags);
+
+	/* disble usb3 ports Wake bits*/
+	port_index = xhci->num_usb3_ports;
+	port_array = xhci->usb3_ports;
+	while (port_index--) {
+		t1 = readl(port_array[port_index]);
+		t1 = xhci_port_state_to_neutral(t1);
+		t2 = t1 & ~PORT_WAKE_BITS;
+		if (t1 != t2)
+			writel(t2, port_array[port_index]);
+	}
+
+	/* disble usb2 ports Wake bits*/
+	port_index = xhci->num_usb2_ports;
+	port_array = xhci->usb2_ports;
+	while (port_index--) {
+		t1 = readl(port_array[port_index]);
+		t1 = xhci_port_state_to_neutral(t1);
+		t2 = t1 & ~PORT_WAKE_BITS;
+		if (t1 != t2)
+			writel(t2, port_array[port_index]);
+	}
+
+	spin_unlock_irqrestore(&xhci->lock, flags);
+}
+
 /*
  * Stop HC (not bus-specific)
  *
  * This is called when the machine transition into S3/S4 mode.
  *
  */
-int xhci_suspend(struct xhci_hcd *xhci)
+int xhci_suspend(struct xhci_hcd *xhci, bool do_wakeup)
 {
 	int			rc = 0;
 	struct usb_hcd		*hcd = xhci_to_hcd(xhci);
 	u32			command;
 
+	/* Clear root port wake on bits if wakeup not allowed. */
+	if (!do_wakeup)
+		xhci_disable_port_wake_on_bits(xhci);
+
 	/* Don't poll the roothubs on bus suspend. */
 	xhci_dbg(xhci, "%s: stopping port polling.\n", __func__);
 	clear_bit(HCD_FLAG_POLL_RH, &hcd->flags);
@@ -2851,61 +2891,31 @@ void xhci_cleanup_stalled_ring(struct xhci_hcd *xhci,
 	}
 }
 
-/* Deal with stalled endpoints.  The core should have sent the control message
- * to clear the halt condition.  However, we need to make the xHCI hardware
- * reset its sequence number, since a device will expect a sequence number of
- * zero after the halt condition is cleared.
+/* Called when clearing halted device. The core should have sent the control
+ * message to clear the device halt condition. The host side of the halt should
+ * already be cleared with a reset endpoint command issued when the STALL tx
+ * event was received.
+ *
  * Context: in_interrupt
  */
+
 void xhci_endpoint_reset(struct usb_hcd *hcd,
 		struct usb_host_endpoint *ep)
 {
 	struct xhci_hcd *xhci;
-	struct usb_device *udev;
-	unsigned int ep_index;
-	unsigned long flags;
-	int ret;
-	struct xhci_virt_ep *virt_ep;
 
 	xhci = hcd_to_xhci(hcd);
-	udev = (struct usb_device *) ep->hcpriv;
-	/* Called with a root hub endpoint (or an endpoint that wasn't added
-	 * with xhci_add_endpoint()
-	 */
-	if (!ep->hcpriv)
-		return;
-	ep_index = xhci_get_endpoint_index(&ep->desc);
-	virt_ep = &xhci->devs[udev->slot_id]->eps[ep_index];
-	if (!virt_ep->stopped_td) {
-		xhci_dbg(xhci, "Endpoint 0x%x not halted, refusing to reset.\n",
-				ep->desc.bEndpointAddress);
-		return;
-	}
-	if (usb_endpoint_xfer_control(&ep->desc)) {
-		xhci_dbg(xhci, "Control endpoint stall already handled.\n");
-		return;
-	}
-
-	xhci_dbg(xhci, "Queueing reset endpoint command\n");
-	spin_lock_irqsave(&xhci->lock, flags);
-	ret = xhci_queue_reset_ep(xhci, udev->slot_id, ep_index);
 	/*
-	 * Can't change the ring dequeue pointer until it's transitioned to the
-	 * stopped state, which is only upon a successful reset endpoint
-	 * command.  Better hope that last command worked!
+	 * We might need to implement the config ep cmd in xhci 4.8.1 note:
+	 * The Reset Endpoint Command may only be issued to endpoints in the
+	 * Halted state. If software wishes reset the Data Toggle or Sequence
+	 * Number of an endpoint that isn't in the Halted state, then software
+	 * may issue a Configure Endpoint Command with the Drop and Add bits set
+	 * for the target endpoint. that is in the Stopped state.
 	 */
-	if (!ret) {
-		xhci_cleanup_stalled_ring(xhci, udev, ep_index);
-		kfree(virt_ep->stopped_td);
-		xhci_ring_cmd_db(xhci);
-	}
-	virt_ep->stopped_td = NULL;
-	virt_ep->stopped_trb = NULL;
-	virt_ep->stopped_stream = 0;
-	spin_unlock_irqrestore(&xhci->lock, flags);
-
-	if (ret)
-		xhci_warn(xhci, "FIXME allocate a new ring segment\n");
+	/* For now just print debug to follow the situation */
+	xhci_dbg(xhci, "Endpoint 0x%x ep reset callback called\n",
+		 ep->desc.bEndpointAddress);
 }
 
 static int xhci_check_streams_endpoint(struct xhci_hcd *xhci,
diff --git a/drivers/usb/host/xhci.h b/drivers/usb/host/xhci.h
index d643c1a..16cc569 100644
--- a/drivers/usb/host/xhci.h
+++ b/drivers/usb/host/xhci.h
@@ -1755,7 +1755,7 @@ void xhci_shutdown(struct usb_hcd *hcd);
 int xhci_gen_setup(struct usb_hcd *hcd, xhci_get_quirks_t get_quirks);
 
 #ifdef	CONFIG_PM
-int xhci_suspend(struct xhci_hcd *xhci);
+int xhci_suspend(struct xhci_hcd *xhci, bool do_wakeup);
 int xhci_resume(struct xhci_hcd *xhci, bool hibernated);
 #else
 #define	xhci_suspend	NULL
diff --git a/drivers/usb/renesas_usbhs/mod_gadget.c b/drivers/usb/renesas_usbhs/mod_gadget.c
index 00bd2a5..056dc6e 100644
--- a/drivers/usb/renesas_usbhs/mod_gadget.c
+++ b/drivers/usb/renesas_usbhs/mod_gadget.c
@@ -672,6 +672,9 @@ static int __usbhsg_ep_set_halt_wedge(struct usb_ep *ep, int halt, int wedge)
 	struct device *dev = usbhsg_gpriv_to_dev(gpriv);
 	unsigned long flags;
 
+	if (!pipe)
+		return -EINVAL;
+
 	usbhsg_pipe_disable(uep);
 
 	dev_dbg(dev, "set halt %d (pipe %d)\n",
diff --git a/drivers/usb/serial/console.c b/drivers/usb/serial/console.c
index 1ee6b2a..87302dd 100644
--- a/drivers/usb/serial/console.c
+++ b/drivers/usb/serial/console.c
@@ -47,6 +47,8 @@ static struct console usbcons;
  * ------------------------------------------------------------
  */
 
+static const struct tty_operations usb_console_fake_tty_ops = {
+};
 
 /*
  * The parsing of the command line works exactly like the
@@ -141,14 +143,17 @@ static int usb_console_setup(struct console *co, char *options)
 				goto reset_open_count;
 			}
 			kref_init(&tty->kref);
-			tty_port_tty_set(&port->port, tty);
 			tty->driver = usb_serial_tty_driver;
 			tty->index = co->index;
+			INIT_LIST_HEAD(&tty->tty_files);
+			kref_get(&tty->driver->kref);
+			tty->ops = &usb_console_fake_tty_ops;
 			if (tty_init_termios(tty)) {
 				retval = -ENOMEM;
 				err("no more memory");
-				goto free_tty;
+				goto put_tty;
 			}
+			tty_port_tty_set(&port->port, tty);
 		}
 
 		/* only call the device specific open if this
@@ -170,7 +175,7 @@ static int usb_console_setup(struct console *co, char *options)
 			serial->type->set_termios(tty, port, &dummy);
 
 			tty_port_tty_set(&port->port, NULL);
-			kfree(tty);
+			tty_kref_put(tty);
 		}
 		set_bit(ASYNCB_INITIALIZED, &port->port.flags);
 	}
@@ -186,8 +191,8 @@ static int usb_console_setup(struct console *co, char *options)
 
  fail:
 	tty_port_tty_set(&port->port, NULL);
- free_tty:
-	kfree(tty);
+ put_tty:
+	tty_kref_put(tty);
  reset_open_count:
 	port->port.count = 0;
 	usb_autopm_put_interface(serial->interface);
diff --git a/drivers/usb/serial/cp210x.c b/drivers/usb/serial/cp210x.c
index 19074db..8137937 100644
--- a/drivers/usb/serial/cp210x.c
+++ b/drivers/usb/serial/cp210x.c
@@ -126,9 +126,12 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(0x10C4, 0x85F8) }, /* Virtenio Preon32 */
 	{ USB_DEVICE(0x10C4, 0x8664) }, /* AC-Services CAN-IF */
 	{ USB_DEVICE(0x10C4, 0x8665) }, /* AC-Services OBD-IF */
+	{ USB_DEVICE(0x10C4, 0x8856) },	/* CEL EM357 ZigBee USB Stick - LR */
+	{ USB_DEVICE(0x10C4, 0x8857) },	/* CEL EM357 ZigBee USB Stick */
 	{ USB_DEVICE(0x10C4, 0x88A4) }, /* MMB Networks ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x88A5) }, /* Planet Innovation Ingeni ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x8946) }, /* Ketra N1 Wireless Interface */
+	{ USB_DEVICE(0x10C4, 0x8977) },	/* CEL MeshWorks DevKit Device */
 	{ USB_DEVICE(0x10C4, 0xEA60) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA61) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA70) }, /* Silicon Labs factory default */
diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index a89433b..4bfcfa7 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -494,6 +494,39 @@ static struct usb_device_id id_table_combined [] = {
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FD_PID) },
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FE_PID) },
 	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_01FF_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_4701_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9300_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9301_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9302_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9303_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9304_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9305_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9306_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9307_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9308_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9309_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930A_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930B_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930C_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930D_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930E_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_930F_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9310_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9311_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9312_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9313_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9314_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9315_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9316_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9317_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9318_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_9319_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931A_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931B_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931C_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931D_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931E_PID) },
+	{ USB_DEVICE(MTXORB_VID, MTXORB_FTDI_RANGE_931F_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_PERLE_ULTRAPORT_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_PIEGROUP_PID) },
 	{ USB_DEVICE(FTDI_VID, FTDI_TNC_X_PID) },
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index 64ee791..ecb4dee 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -920,8 +920,8 @@
 #define BAYER_CONTOUR_CABLE_PID        0x6001
 
 /*
- * The following are the values for the Matrix Orbital FTDI Range
- * Anything in this range will use an FT232RL.
+ * Matrix Orbital Intelligent USB displays.
+ * http://www.matrixorbital.com
  */
 #define MTXORB_VID			0x1B3D
 #define MTXORB_FTDI_RANGE_0100_PID	0x0100
@@ -1180,8 +1180,39 @@
 #define MTXORB_FTDI_RANGE_01FD_PID	0x01FD
 #define MTXORB_FTDI_RANGE_01FE_PID	0x01FE
 #define MTXORB_FTDI_RANGE_01FF_PID	0x01FF
-
-
+#define MTXORB_FTDI_RANGE_4701_PID	0x4701
+#define MTXORB_FTDI_RANGE_9300_PID	0x9300
+#define MTXORB_FTDI_RANGE_9301_PID	0x9301
+#define MTXORB_FTDI_RANGE_9302_PID	0x9302
+#define MTXORB_FTDI_RANGE_9303_PID	0x9303
+#define MTXORB_FTDI_RANGE_9304_PID	0x9304
+#define MTXORB_FTDI_RANGE_9305_PID	0x9305
+#define MTXORB_FTDI_RANGE_9306_PID	0x9306
+#define MTXORB_FTDI_RANGE_9307_PID	0x9307
+#define MTXORB_FTDI_RANGE_9308_PID	0x9308
+#define MTXORB_FTDI_RANGE_9309_PID	0x9309
+#define MTXORB_FTDI_RANGE_930A_PID	0x930A
+#define MTXORB_FTDI_RANGE_930B_PID	0x930B
+#define MTXORB_FTDI_RANGE_930C_PID	0x930C
+#define MTXORB_FTDI_RANGE_930D_PID	0x930D
+#define MTXORB_FTDI_RANGE_930E_PID	0x930E
+#define MTXORB_FTDI_RANGE_930F_PID	0x930F
+#define MTXORB_FTDI_RANGE_9310_PID	0x9310
+#define MTXORB_FTDI_RANGE_9311_PID	0x9311
+#define MTXORB_FTDI_RANGE_9312_PID	0x9312
+#define MTXORB_FTDI_RANGE_9313_PID	0x9313
+#define MTXORB_FTDI_RANGE_9314_PID	0x9314
+#define MTXORB_FTDI_RANGE_9315_PID	0x9315
+#define MTXORB_FTDI_RANGE_9316_PID	0x9316
+#define MTXORB_FTDI_RANGE_9317_PID	0x9317
+#define MTXORB_FTDI_RANGE_9318_PID	0x9318
+#define MTXORB_FTDI_RANGE_9319_PID	0x9319
+#define MTXORB_FTDI_RANGE_931A_PID	0x931A
+#define MTXORB_FTDI_RANGE_931B_PID	0x931B
+#define MTXORB_FTDI_RANGE_931C_PID	0x931C
+#define MTXORB_FTDI_RANGE_931D_PID	0x931D
+#define MTXORB_FTDI_RANGE_931E_PID	0x931E
+#define MTXORB_FTDI_RANGE_931F_PID	0x931F
 
 /*
  * The Mobility Lab (TML)
diff --git a/drivers/usb/serial/keyspan.c b/drivers/usb/serial/keyspan.c
index 66d806e..0879ac7 100644
--- a/drivers/usb/serial/keyspan.c
+++ b/drivers/usb/serial/keyspan.c
@@ -323,24 +323,28 @@ static void	usa26_indat_callback(struct urb *urb)
 		if ((data[0] & 0x80) == 0) {
 			/* no errors on individual bytes, only
 			   possible overrun err */
-			if (data[0] & RXERROR_OVERRUN)
-				err = TTY_OVERRUN;
-			else
-				err = 0;
+			if (data[0] & RXERROR_OVERRUN) {
+				tty_insert_flip_char(tty, 0, TTY_OVERRUN);
+			}
 			for (i = 1; i < urb->actual_length ; ++i)
-				tty_insert_flip_char(tty, data[i], err);
+				tty_insert_flip_char(tty, data[i], TTY_NORMAL);
 		} else {
 			/* some bytes had errors, every byte has status */
 			dbg("%s - RX error!!!!", __func__);
 			for (i = 0; i + 1 < urb->actual_length; i += 2) {
-				int stat = data[i], flag = 0;
-				if (stat & RXERROR_OVERRUN)
-					flag |= TTY_OVERRUN;
-				if (stat & RXERROR_FRAMING)
-					flag |= TTY_FRAME;
-				if (stat & RXERROR_PARITY)
-					flag |= TTY_PARITY;
+				int stat = data[i];
+				int flag = TTY_NORMAL;
+
+				if (stat & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				/* XXX should handle break (0x10) */
+				if (stat & RXERROR_PARITY)
+					flag = TTY_PARITY;
+				else if (stat & RXERROR_FRAMING)
+					flag = TTY_FRAME;
+
 				tty_insert_flip_char(tty, data[i+1], flag);
 			}
 		}
@@ -712,14 +716,19 @@ static void	usa49_indat_callback(struct urb *urb)
 		} else {
 			/* some bytes had errors, every byte has status */
 			for (i = 0; i + 1 < urb->actual_length; i += 2) {
-				int stat = data[i], flag = 0;
-				if (stat & RXERROR_OVERRUN)
-					flag |= TTY_OVERRUN;
-				if (stat & RXERROR_FRAMING)
-					flag |= TTY_FRAME;
-				if (stat & RXERROR_PARITY)
-					flag |= TTY_PARITY;
+				int stat = data[i];
+				int flag = TTY_NORMAL;
+
+				if (stat & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				/* XXX should handle break (0x10) */
+				if (stat & RXERROR_PARITY)
+					flag = TTY_PARITY;
+				else if (stat & RXERROR_FRAMING)
+					flag = TTY_FRAME;
+
 				tty_insert_flip_char(tty, data[i+1], flag);
 			}
 		}
@@ -779,14 +788,19 @@ static void usa49wg_indat_callback(struct urb *urb)
 				 * some bytes had errors, every byte has status
 				 */
 				for (x = 0; x + 1 < len; x += 2) {
-					int stat = data[i], flag = 0;
-					if (stat & RXERROR_OVERRUN)
-						flag |= TTY_OVERRUN;
-					if (stat & RXERROR_FRAMING)
-						flag |= TTY_FRAME;
-					if (stat & RXERROR_PARITY)
-						flag |= TTY_PARITY;
+					int stat = data[i];
+					int flag = TTY_NORMAL;
+
+					if (stat & RXERROR_OVERRUN) {
+						tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+					}
 					/* XXX should handle break (0x10) */
+					if (stat & RXERROR_PARITY)
+						flag = TTY_PARITY;
+					else if (stat & RXERROR_FRAMING)
+						flag = TTY_FRAME;
+
 					tty_insert_flip_char(tty,
 							data[i+1], flag);
 					i += 2;
@@ -844,25 +858,32 @@ static void usa90_indat_callback(struct urb *urb)
 			if ((data[0] & 0x80) == 0) {
 				/* no errors on individual bytes, only
 				   possible overrun err*/
-				if (data[0] & RXERROR_OVERRUN)
-					err = TTY_OVERRUN;
-				else
-					err = 0;
+				if (data[0] & RXERROR_OVERRUN) {
+					tty_insert_flip_char(tty, 0,
+								TTY_OVERRUN);
+				}
 				for (i = 1; i < urb->actual_length ; ++i)
 					tty_insert_flip_char(tty, data[i],
-									err);
+								TTY_NORMAL);
 			}  else {
 			/* some bytes had errors, every byte has status */
 				dbg("%s - RX error!!!!", __func__);
 				for (i = 0; i + 1 < urb->actual_length; i += 2) {
-					int stat = data[i], flag = 0;
-					if (stat & RXERROR_OVERRUN)
-						flag |= TTY_OVERRUN;
-					if (stat & RXERROR_FRAMING)
-						flag |= TTY_FRAME;
-					if (stat & RXERROR_PARITY)
-						flag |= TTY_PARITY;
+					int stat = data[i];
+					int flag = TTY_NORMAL;
+
+					if (stat & RXERROR_OVERRUN) {
+						tty_insert_flip_char(
+								tty, 0,
+								TTY_OVERRUN);
+					}
+
 					/* XXX should handle break (0x10) */
+					if (stat & RXERROR_PARITY)
+						flag = TTY_PARITY;
+					else if (stat & RXERROR_FRAMING)
+						flag = TTY_FRAME;
+
 					tty_insert_flip_char(tty, data[i+1],
 									flag);
 				}
diff --git a/drivers/usb/serial/ssu100.c b/drivers/usb/serial/ssu100.c
index d19fa6a..f425507 100644
--- a/drivers/usb/serial/ssu100.c
+++ b/drivers/usb/serial/ssu100.c
@@ -598,10 +598,10 @@ static void ssu100_update_lsr(struct usb_serial_port *port, u8 lsr,
 			if (*tty_flag == TTY_NORMAL)
 				*tty_flag = TTY_FRAME;
 		}
-		if (lsr & UART_LSR_OE){
+		if (lsr & UART_LSR_OE) {
 			priv->icount.overrun++;
-			if (*tty_flag == TTY_NORMAL)
-				*tty_flag = TTY_OVERRUN;
+			tty_insert_flip_char(tty_port_tty_get(&port->port),
+					0, TTY_OVERRUN);
 		}
 	}
 
@@ -622,11 +622,8 @@ static int ssu100_process_packet(struct urb *urb,
 	if ((len >= 4) &&
 	    (packet[0] == 0x1b) && (packet[1] == 0x1b) &&
 	    ((packet[2] == 0x00) || (packet[2] == 0x01))) {
-		if (packet[2] == 0x00) {
+		if (packet[2] == 0x00)
 			ssu100_update_lsr(port, packet[3], &flag);
-			if (flag == TTY_OVERRUN)
-				tty_insert_flip_char(tty, 0, TTY_OVERRUN);
-		}
 		if (packet[2] == 0x01)
 			ssu100_update_msr(port, packet[3]);
 
diff --git a/drivers/usb/storage/scsiglue.c b/drivers/usb/storage/scsiglue.c
index a4f033b..b987c53 100644
--- a/drivers/usb/storage/scsiglue.c
+++ b/drivers/usb/storage/scsiglue.c
@@ -247,6 +247,10 @@ static int slave_configure(struct scsi_device *sdev)
 			sdev->use_rpm_auto = 1;
 			sdev->autosuspend_delay = us->sdev_autosuspend_delay;
 		}
+		
+		/* A few buggy USB-ATA bridges don't understand FUA */
+		if (us->fflags & US_FL_BROKEN_FUA)
+			sdev->broken_fua = 1;
 	} else {
 
 		/* Non-disk-type devices don't need to blacklist any pages
diff --git a/drivers/usb/storage/unusual_devs.h b/drivers/usb/storage/unusual_devs.h
index a280945..25174be 100644
--- a/drivers/usb/storage/unusual_devs.h
+++ b/drivers/usb/storage/unusual_devs.h
@@ -1940,6 +1940,13 @@ UNUSUAL_DEV(  0x14cd, 0x6600, 0x0201, 0x0201,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_IGNORE_RESIDUE ),
 
+/* Reported by Michael Büsch <m@bues.ch> */
+UNUSUAL_DEV(  0x152d, 0x0567, 0x0114, 0x0114,
+		"JMicron",
+		"USB to ATA/ATAPI Bridge",
+		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
+		US_FL_BROKEN_FUA ),
+
 /* Reported by Alexandre Oliva <oliva@lsd.ic.unicamp.br>
  * JMicron responds to USN and several other SCSI ioctls with a
  * residue that causes subsequent I/O requests to fail.  */
@@ -1949,6 +1956,13 @@ UNUSUAL_DEV(  0x152d, 0x2329, 0x0100, 0x0100,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_IGNORE_RESIDUE | US_FL_SANE_SENSE ),
 
+/* Reported by Dmitry Nezhevenko <dion@dion.org.ua> */
+UNUSUAL_DEV(  0x152d, 0x2566, 0x0114, 0x0114,
+		"JMicron",
+		"USB to ATA/ATAPI Bridge",
+		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
+		US_FL_BROKEN_FUA ),
+
 /* Entrega Technologies U1-SC25 (later Xircom PortGear PGSCSI)
  * and Mac USB Dock USB-SCSI */
 UNUSUAL_DEV(  0x1645, 0x0007, 0x0100, 0x0133,
diff --git a/drivers/video/logo/logo.c b/drivers/video/logo/logo.c
index 080c35b..cc5dbb5 100644
--- a/drivers/video/logo/logo.c
+++ b/drivers/video/logo/logo.c
@@ -25,6 +25,21 @@ static bool nologo;
 module_param(nologo, bool, 0);
 MODULE_PARM_DESC(nologo, "Disables startup logo");
 
+/*
+ * Logos are located in the initdata, and will be freed in kernel_init.
+ * Use late_init to mark the logos as freed to prevent any further use.
+ */
+
+static bool logos_freed;
+
+static int __init fb_logo_late_init(void)
+{
+	logos_freed = true;
+	return 0;
+}
+
+late_initcall(fb_logo_late_init);
+
 /* logo's are marked __initdata. Use __init_refok to tell
  * modpost that it is intended that this function uses data
  * marked __initdata.
@@ -33,7 +48,7 @@ const struct linux_logo * __init_refok fb_find_logo(int depth)
 {
 	const struct linux_logo *logo = NULL;
 
-	if (nologo)
+	if (nologo || logos_freed)
 		return NULL;
 
 	if (depth >= 1) {
diff --git a/drivers/virtio/virtio.c b/drivers/virtio/virtio.c
index 984c501..cc02a9b 100644
--- a/drivers/virtio/virtio.c
+++ b/drivers/virtio/virtio.c
@@ -9,33 +9,32 @@ static unsigned int dev_index;
 static ssize_t device_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%04x\n", dev->id.device);
 }
 static ssize_t vendor_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%04x\n", dev->id.vendor);
 }
 static ssize_t status_show(struct device *_d,
 			   struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "0x%08x\n", dev->config->get_status(dev));
 }
 static ssize_t modalias_show(struct device *_d,
 			     struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
-
+	struct virtio_device *dev = dev_to_virtio(_d);
 	return sprintf(buf, "virtio:d%08Xv%08X\n",
 		       dev->id.device, dev->id.vendor);
 }
 static ssize_t features_show(struct device *_d,
 			     struct device_attribute *attr, char *buf)
 {
-	struct virtio_device *dev = container_of(_d, struct virtio_device, dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	unsigned int i;
 	ssize_t len = 0;
 
@@ -70,7 +69,7 @@ static inline int virtio_id_match(const struct virtio_device *dev,
 static int virtio_dev_match(struct device *_dv, struct device_driver *_dr)
 {
 	unsigned int i;
-	struct virtio_device *dev = container_of(_dv,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_dv);
 	const struct virtio_device_id *ids;
 
 	ids = container_of(_dr, struct virtio_driver, driver)->id_table;
@@ -82,7 +81,7 @@ static int virtio_dev_match(struct device *_dv, struct device_driver *_dr)
 
 static int virtio_uevent(struct device *_dv, struct kobj_uevent_env *env)
 {
-	struct virtio_device *dev = container_of(_dv,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_dv);
 
 	return add_uevent_var(env, "MODALIAS=virtio:d%08Xv%08X",
 			      dev->id.device, dev->id.vendor);
@@ -110,7 +109,7 @@ EXPORT_SYMBOL_GPL(virtio_check_driver_offered_feature);
 static int virtio_dev_probe(struct device *_d)
 {
 	int err, i;
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	struct virtio_driver *drv = container_of(dev->dev.driver,
 						 struct virtio_driver, driver);
 	u32 device_features;
@@ -148,7 +147,7 @@ static int virtio_dev_probe(struct device *_d)
 
 static int virtio_dev_remove(struct device *_d)
 {
-	struct virtio_device *dev = container_of(_d,struct virtio_device,dev);
+	struct virtio_device *dev = dev_to_virtio(_d);
 	struct virtio_driver *drv = container_of(dev->dev.driver,
 						 struct virtio_driver, driver);
 
diff --git a/drivers/virtio/virtio_pci.c b/drivers/virtio/virtio_pci.c
index a41f264..cc56763 100644
--- a/drivers/virtio/virtio_pci.c
+++ b/drivers/virtio/virtio_pci.c
@@ -624,11 +624,13 @@ static struct virtio_config_ops virtio_pci_config_ops = {
 
 static void virtio_pci_release_dev(struct device *_d)
 {
-	/*
-	 * No need for a release method as we allocate/free
-	 * all devices together with the pci devices.
-	 * Provide an empty one to avoid getting a warning from core.
-	 */
+	struct virtio_device *vdev = dev_to_virtio(_d);
+	struct virtio_pci_device *vp_dev = to_vp_device(vdev);
+
+	/* As struct device is a kobject, it's not safe to
+	 * free the memory (including the reference counter itself)
+	 * until it's release callback. */
+	kfree(vp_dev);
 }
 
 /* the PCI probing function */
@@ -716,7 +718,6 @@ static void __devexit virtio_pci_remove(struct pci_dev *pci_dev)
 	pci_iounmap(pci_dev, vp_dev->ioaddr);
 	pci_release_regions(pci_dev);
 	pci_disable_device(pci_dev);
-	kfree(vp_dev);
 }
 
 #ifdef CONFIG_PM
diff --git a/fs/binfmt_elf.c b/fs/binfmt_elf.c
index a009b9e..6dacccef 100644
--- a/fs/binfmt_elf.c
+++ b/fs/binfmt_elf.c
@@ -539,11 +539,12 @@ static unsigned long load_elf_interp(struct elfhdr *interp_elf_ex,
 
 static unsigned long randomize_stack_top(unsigned long stack_top)
 {
-	unsigned int random_variable = 0;
+	unsigned long random_variable = 0;
 
 	if ((current->flags & PF_RANDOMIZE) &&
 		!(current->personality & ADDR_NO_RANDOMIZE)) {
-		random_variable = get_random_int() & STACK_RND_MASK;
+		random_variable = (unsigned long) get_random_int();
+		random_variable &= STACK_RND_MASK;
 		random_variable <<= PAGE_SHIFT;
 	}
 #ifdef CONFIG_STACK_GROWSUP
diff --git a/fs/btrfs/disk-io.c b/fs/btrfs/disk-io.c
index a7ffc88..7c23cd9 100644
--- a/fs/btrfs/disk-io.c
+++ b/fs/btrfs/disk-io.c
@@ -3556,12 +3556,6 @@ static int btrfs_destroy_pinned_extent(struct btrfs_root *root,
 		if (ret)
 			break;
 
-		/* opt_discard */
-		if (btrfs_test_opt(root, DISCARD))
-			ret = btrfs_error_discard_extent(root, start,
-							 end + 1 - start,
-							 NULL);
-
 		clear_extent_dirty(unpin, start, end, GFP_NOFS);
 		btrfs_error_unpin_extent_range(root, start, end);
 		cond_resched();
diff --git a/fs/btrfs/extent-tree.c b/fs/btrfs/extent-tree.c
index 224ce21..cf6e7f4 100644
--- a/fs/btrfs/extent-tree.c
+++ b/fs/btrfs/extent-tree.c
@@ -4892,7 +4892,8 @@ void btrfs_prepare_extent_commit(struct btrfs_trans_handle *trans,
 	update_global_block_rsv(fs_info);
 }
 
-static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
+static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end,
+			      const bool return_free_space)
 {
 	struct btrfs_fs_info *fs_info = root->fs_info;
 	struct btrfs_block_group_cache *cache = NULL;
@@ -4912,7 +4913,8 @@ static int unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
 
 		if (start < cache->last_byte_to_unpin) {
 			len = min(len, cache->last_byte_to_unpin - start);
-			btrfs_add_free_space(cache, start, len);
+			if (return_free_space)
+				btrfs_add_free_space(cache, start, len);
 		}
 
 		start += len;
@@ -4960,7 +4962,7 @@ int btrfs_finish_extent_commit(struct btrfs_trans_handle *trans,
 						   end + 1 - start, NULL);
 
 		clear_extent_dirty(unpin, start, end, GFP_NOFS);
-		unpin_extent_range(root, start, end);
+		unpin_extent_range(root, start, end, true);
 		cond_resched();
 	}
 
@@ -8008,7 +8010,7 @@ int btrfs_init_space_info(struct btrfs_fs_info *fs_info)
 
 int btrfs_error_unpin_extent_range(struct btrfs_root *root, u64 start, u64 end)
 {
-	return unpin_extent_range(root, start, end);
+	return unpin_extent_range(root, start, end, false);
 }
 
 int btrfs_error_discard_extent(struct btrfs_root *root, u64 bytenr,
diff --git a/fs/ecryptfs/file.c b/fs/ecryptfs/file.c
index d45ba45..f04aa33 100644
--- a/fs/ecryptfs/file.c
+++ b/fs/ecryptfs/file.c
@@ -195,24 +195,12 @@ static int ecryptfs_open(struct inode *inode, struct file *file)
 {
 	int rc = 0;
 	struct ecryptfs_crypt_stat *crypt_stat = NULL;
-	struct ecryptfs_mount_crypt_stat *mount_crypt_stat;
 	struct dentry *ecryptfs_dentry = file->f_path.dentry;
 	/* Private value of ecryptfs_dentry allocated in
 	 * ecryptfs_lookup() */
 	struct dentry *lower_dentry;
 	struct ecryptfs_file_info *file_info;
 
-	mount_crypt_stat = &ecryptfs_superblock_to_private(
-		ecryptfs_dentry->d_sb)->mount_crypt_stat;
-	if ((mount_crypt_stat->flags & ECRYPTFS_ENCRYPTED_VIEW_ENABLED)
-	    && ((file->f_flags & O_WRONLY) || (file->f_flags & O_RDWR)
-		|| (file->f_flags & O_CREAT) || (file->f_flags & O_TRUNC)
-		|| (file->f_flags & O_APPEND))) {
-		printk(KERN_WARNING "Mount has encrypted view enabled; "
-		       "files may only be read\n");
-		rc = -EPERM;
-		goto out;
-	}
 	/* Released in ecryptfs_release or end of function if failure */
 	file_info = kmem_cache_zalloc(ecryptfs_file_info_cache, GFP_KERNEL);
 	ecryptfs_set_file_private(file, file_info);
diff --git a/fs/ecryptfs/main.c b/fs/ecryptfs/main.c
index 240832e..93b7bec 100644
--- a/fs/ecryptfs/main.c
+++ b/fs/ecryptfs/main.c
@@ -494,6 +494,7 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 {
 	struct super_block *s;
 	struct ecryptfs_sb_info *sbi;
+	struct ecryptfs_mount_crypt_stat *mount_crypt_stat;
 	struct ecryptfs_dentry_info *root_info;
 	const char *err = "Getting sb failed";
 	struct inode *inode;
@@ -512,6 +513,7 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 		err = "Error parsing options";
 		goto out;
 	}
+	mount_crypt_stat = &sbi->mount_crypt_stat;
 
 	s = sget(fs_type, NULL, set_anon_super, NULL);
 	if (IS_ERR(s)) {
@@ -557,11 +559,19 @@ static struct dentry *ecryptfs_mount(struct file_system_type *fs_type, int flags
 
 	/**
 	 * Set the POSIX ACL flag based on whether they're enabled in the lower
-	 * mount. Force a read-only eCryptfs mount if the lower mount is ro.
-	 * Allow a ro eCryptfs mount even when the lower mount is rw.
+	 * mount.
 	 */
 	s->s_flags = flags & ~MS_POSIXACL;
-	s->s_flags |= path.dentry->d_sb->s_flags & (MS_RDONLY | MS_POSIXACL);
+	s->s_flags |= path.dentry->d_sb->s_flags & MS_POSIXACL;
+
+	/**
+	 * Force a read-only eCryptfs mount when:
+	 *   1) The lower mount is ro
+	 *   2) The ecryptfs_encrypted_view mount option is specified
+	 */
+	if (path.dentry->d_sb->s_flags & MS_RDONLY ||
+	    mount_crypt_stat->flags & ECRYPTFS_ENCRYPTED_VIEW_ENABLED)
+		s->s_flags |= MS_RDONLY;
 
 	s->s_maxbytes = path.dentry->d_sb->s_maxbytes;
 	s->s_blocksize = path.dentry->d_sb->s_blocksize;
diff --git a/fs/fs-writeback.c b/fs/fs-writeback.c
index e4926e5..6e748b1 100644
--- a/fs/fs-writeback.c
+++ b/fs/fs-writeback.c
@@ -403,7 +403,6 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 
 	/* Set I_SYNC, reset I_DIRTY_PAGES */
 	inode->i_state |= I_SYNC;
-	inode->i_state &= ~I_DIRTY_PAGES;
 	spin_unlock(&inode->i_lock);
 	spin_unlock(&wb->list_lock);
 
@@ -428,9 +427,28 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 	 * write_inode()
 	 */
 	spin_lock(&inode->i_lock);
+
 	dirty = inode->i_state & I_DIRTY;
-	inode->i_state &= ~(I_DIRTY_SYNC | I_DIRTY_DATASYNC);
+	inode->i_state &= ~I_DIRTY;
+
+	/*
+	 * Paired with smp_mb() in __mark_inode_dirty().  This allows
+	 * __mark_inode_dirty() to test i_state without grabbing i_lock -
+	 * either they see the I_DIRTY bits cleared or we see the dirtied
+	 * inode.
+	 *
+	 * I_DIRTY_PAGES is always cleared together above even if @mapping
+	 * still has dirty pages.  The flag is reinstated after smp_mb() if
+	 * necessary.  This guarantees that either __mark_inode_dirty()
+	 * sees clear I_DIRTY_PAGES or we see PAGECACHE_TAG_DIRTY.
+	 */
+	smp_mb();
+
+	if (mapping_tagged(mapping, PAGECACHE_TAG_DIRTY))
+		inode->i_state |= I_DIRTY_PAGES;
+
 	spin_unlock(&inode->i_lock);
+
 	/* Don't write the inode if only I_DIRTY_PAGES was set */
 	if (dirty & (I_DIRTY_SYNC | I_DIRTY_DATASYNC)) {
 		int err = write_inode(inode, wbc);
@@ -456,7 +474,6 @@ writeback_single_inode(struct inode *inode, struct bdi_writeback *wb,
 			 * We didn't write back all the pages.  nfs_writepages()
 			 * sometimes bales out without doing anything.
 			 */
-			inode->i_state |= I_DIRTY_PAGES;
 			if (wbc->nr_to_write <= 0) {
 				/*
 				 * slice used up: queue for next turn
@@ -1076,12 +1093,11 @@ void __mark_inode_dirty(struct inode *inode, int flags)
 	}
 
 	/*
-	 * make sure that changes are seen by all cpus before we test i_state
-	 * -- mikulas
+	 * Paired with smp_mb() in __writeback_single_inode() for the
+	 * following lockless i_state test.  See there for details.
 	 */
 	smp_mb();
 
-	/* avoid the locking if we can */
 	if ((inode->i_state & flags) == flags)
 		return;
 
diff --git a/fs/isofs/rock.c b/fs/isofs/rock.c
index ee62cc0..1780949 100644
--- a/fs/isofs/rock.c
+++ b/fs/isofs/rock.c
@@ -30,6 +30,7 @@ struct rock_state {
 	int cont_size;
 	int cont_extent;
 	int cont_offset;
+	int cont_loops;
 	struct inode *inode;
 };
 
@@ -73,6 +74,9 @@ static void init_rock_state(struct rock_state *rs, struct inode *inode)
 	rs->inode = inode;
 }
 
+/* Maximum number of Rock Ridge continuation entries */
+#define RR_MAX_CE_ENTRIES 32
+
 /*
  * Returns 0 if the caller should continue scanning, 1 if the scan must end
  * and -ve on error.
@@ -105,6 +109,8 @@ static int rock_continue(struct rock_state *rs)
 			goto out;
 		}
 		ret = -EIO;
+		if (++rs->cont_loops >= RR_MAX_CE_ENTRIES)
+			goto out;
 		bh = sb_bread(rs->inode->i_sb, rs->cont_extent);
 		if (bh) {
 			memcpy(rs->buffer, bh->b_data + rs->cont_offset,
@@ -356,6 +362,9 @@ parse_rock_ridge_inode_internal(struct iso_directory_record *de,
 			rs.cont_size = isonum_733(rr->u.CE.size);
 			break;
 		case SIG('E', 'R'):
+			/* Invalid length of ER tag id? */
+			if (rr->u.ER.len_id + offsetof(struct rock_ridge, u.ER.data) > rr->len)
+				goto out;
 			ISOFS_SB(inode->i_sb)->s_rock = 1;
 			printk(KERN_DEBUG "ISO 9660 Extensions: ");
 			{
diff --git a/fs/jfs/jfs_dtree.c b/fs/jfs/jfs_dtree.c
index b6f17c0..33c8624 100644
--- a/fs/jfs/jfs_dtree.c
+++ b/fs/jfs/jfs_dtree.c
@@ -3103,7 +3103,7 @@ int jfs_readdir(struct file *filp, void *dirent, filldir_t filldir)
 				 * self "."
 				 */
 				filp->f_pos = 1;
-				if (filldir(dirent, ".", 1, 0, ip->i_ino,
+				if (filldir(dirent, ".", 1, 1, ip->i_ino,
 					    DT_DIR))
 					return 0;
 			}
@@ -3111,7 +3111,7 @@ int jfs_readdir(struct file *filp, void *dirent, filldir_t filldir)
 			 * parent ".."
 			 */
 			filp->f_pos = 2;
-			if (filldir(dirent, "..", 2, 1, PARENT(ip), DT_DIR))
+			if (filldir(dirent, "..", 2, 2, PARENT(ip), DT_DIR))
 				return 0;
 
 			/*
diff --git a/fs/ncpfs/ioctl.c b/fs/ncpfs/ioctl.c
index 6958adf..0a76def 100644
--- a/fs/ncpfs/ioctl.c
+++ b/fs/ncpfs/ioctl.c
@@ -445,7 +445,6 @@ static long __ncp_ioctl(struct inode *inode, unsigned int cmd, unsigned long arg
 						result = -EIO;
 					}
 				}
-				result = 0;
 			}
 			mutex_unlock(&server->root_setup_lock);
 
diff --git a/fs/nfsd/nfs4callback.c b/fs/nfsd/nfs4callback.c
index c8e9f63..ebf3f59 100644
--- a/fs/nfsd/nfs4callback.c
+++ b/fs/nfsd/nfs4callback.c
@@ -784,8 +784,12 @@ static bool nfsd41_cb_get_slot(struct nfs4_client *clp, struct rpc_task *task)
 {
 	if (test_and_set_bit(0, &clp->cl_cb_slot_busy) != 0) {
 		rpc_sleep_on(&clp->cl_cb_waitq, task, NULL);
-		dprintk("%s slot is busy\n", __func__);
-		return false;
+		/* Race breaker */
+		if (test_and_set_bit(0, &clp->cl_cb_slot_busy) != 0) {
+			dprintk("%s slot is busy\n", __func__);
+			return false;
+		}
+		rpc_wake_up_queued_task(&clp->cl_cb_waitq, task);
 	}
 	return true;
 }
diff --git a/fs/nilfs2/nilfs.h b/fs/nilfs2/nilfs.h
index 250add8..161a10c 100644
--- a/fs/nilfs2/nilfs.h
+++ b/fs/nilfs2/nilfs.h
@@ -128,7 +128,6 @@ enum {
  * @ti_save: Backup of journal_info field of task_struct
  * @ti_flags: Flags
  * @ti_count: Nest level
- * @ti_garbage:	List of inode to be put when releasing semaphore
  */
 struct nilfs_transaction_info {
 	u32			ti_magic;
@@ -137,7 +136,6 @@ struct nilfs_transaction_info {
 				   one of other filesystems has a bug. */
 	unsigned short		ti_flags;
 	unsigned short		ti_count;
-	struct list_head	ti_garbage;
 };
 
 /* ti_magic */
diff --git a/fs/nilfs2/segment.c b/fs/nilfs2/segment.c
index e0a5a18..7bb866c 100644
--- a/fs/nilfs2/segment.c
+++ b/fs/nilfs2/segment.c
@@ -302,7 +302,6 @@ static void nilfs_transaction_lock(struct super_block *sb,
 	ti->ti_count = 0;
 	ti->ti_save = cur_ti;
 	ti->ti_magic = NILFS_TI_MAGIC;
-	INIT_LIST_HEAD(&ti->ti_garbage);
 	current->journal_info = ti;
 
 	for (;;) {
@@ -329,8 +328,6 @@ static void nilfs_transaction_unlock(struct super_block *sb)
 
 	up_write(&nilfs->ns_segctor_sem);
 	current->journal_info = ti->ti_save;
-	if (!list_empty(&ti->ti_garbage))
-		nilfs_dispose_list(nilfs, &ti->ti_garbage, 0);
 }
 
 static void *nilfs_segctor_map_segsum_entry(struct nilfs_sc_info *sci,
@@ -743,6 +740,15 @@ static void nilfs_dispose_list(struct the_nilfs *nilfs,
 	}
 }
 
+static void nilfs_iput_work_func(struct work_struct *work)
+{
+	struct nilfs_sc_info *sci = container_of(work, struct nilfs_sc_info,
+						 sc_iput_work);
+	struct the_nilfs *nilfs = sci->sc_super->s_fs_info;
+
+	nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 0);
+}
+
 static int nilfs_test_metadata_dirty(struct the_nilfs *nilfs,
 				     struct nilfs_root *root)
 {
@@ -1896,8 +1902,9 @@ static int nilfs_segctor_collect_dirty_files(struct nilfs_sc_info *sci,
 static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 					     struct the_nilfs *nilfs)
 {
-	struct nilfs_transaction_info *ti = current->journal_info;
 	struct nilfs_inode_info *ii, *n;
+	int during_mount = !(sci->sc_super->s_flags & MS_ACTIVE);
+	int defer_iput = false;
 
 	spin_lock(&nilfs->ns_inode_lock);
 	list_for_each_entry_safe(ii, n, &sci->sc_dirty_files, i_dirty) {
@@ -1908,9 +1915,24 @@ static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 		clear_bit(NILFS_I_BUSY, &ii->i_state);
 		brelse(ii->i_bh);
 		ii->i_bh = NULL;
-		list_move_tail(&ii->i_dirty, &ti->ti_garbage);
+		list_del_init(&ii->i_dirty);
+		if (!ii->vfs_inode.i_nlink || during_mount) {
+			/*
+			 * Defer calling iput() to avoid deadlocks if
+			 * i_nlink == 0 or mount is not yet finished.
+			 */
+			list_add_tail(&ii->i_dirty, &sci->sc_iput_queue);
+			defer_iput = true;
+		} else {
+			spin_unlock(&nilfs->ns_inode_lock);
+			iput(&ii->vfs_inode);
+			spin_lock(&nilfs->ns_inode_lock);
+		}
 	}
 	spin_unlock(&nilfs->ns_inode_lock);
+
+	if (defer_iput)
+		schedule_work(&sci->sc_iput_work);
 }
 
 /*
@@ -2577,6 +2599,8 @@ static struct nilfs_sc_info *nilfs_segctor_new(struct super_block *sb,
 	INIT_LIST_HEAD(&sci->sc_segbufs);
 	INIT_LIST_HEAD(&sci->sc_write_logs);
 	INIT_LIST_HEAD(&sci->sc_gc_inodes);
+	INIT_LIST_HEAD(&sci->sc_iput_queue);
+	INIT_WORK(&sci->sc_iput_work, nilfs_iput_work_func);
 	init_timer(&sci->sc_timer);
 
 	sci->sc_interval = HZ * NILFS_SC_DEFAULT_TIMEOUT;
@@ -2603,6 +2627,8 @@ static void nilfs_segctor_write_out(struct nilfs_sc_info *sci)
 		ret = nilfs_segctor_construct(sci, SC_LSEG_SR);
 		nilfs_transaction_unlock(sci->sc_super);
 
+		flush_work(&sci->sc_iput_work);
+
 	} while (ret && retrycount-- > 0);
 }
 
@@ -2627,6 +2653,9 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		|| sci->sc_seq_request != sci->sc_seq_done);
 	spin_unlock(&sci->sc_state_lock);
 
+	if (flush_work(&sci->sc_iput_work))
+		flag = true;
+
 	if (flag || !nilfs_segctor_confirm(sci))
 		nilfs_segctor_write_out(sci);
 
@@ -2636,6 +2665,12 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		nilfs_dispose_list(nilfs, &sci->sc_dirty_files, 1);
 	}
 
+	if (!list_empty(&sci->sc_iput_queue)) {
+		nilfs_warning(sci->sc_super, __func__,
+			      "iput queue is not empty\n");
+		nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 1);
+	}
+
 	WARN_ON(!list_empty(&sci->sc_segbufs));
 	WARN_ON(!list_empty(&sci->sc_write_logs));
 
diff --git a/fs/nilfs2/segment.h b/fs/nilfs2/segment.h
index 38a1d00..a48d6de 100644
--- a/fs/nilfs2/segment.h
+++ b/fs/nilfs2/segment.h
@@ -26,6 +26,7 @@
 #include <linux/types.h>
 #include <linux/fs.h>
 #include <linux/buffer_head.h>
+#include <linux/workqueue.h>
 #include <linux/nilfs2_fs.h>
 #include "nilfs.h"
 
@@ -92,6 +93,8 @@ struct nilfs_segsum_pointer {
  * @sc_nblk_inc: Block count of current generation
  * @sc_dirty_files: List of files to be written
  * @sc_gc_inodes: List of GC inodes having blocks to be written
+ * @sc_iput_queue: list of inodes for which iput should be done
+ * @sc_iput_work: work struct to defer iput call
  * @sc_freesegs: array of segment numbers to be freed
  * @sc_nfreesegs: number of segments on @sc_freesegs
  * @sc_dsync_inode: inode whose data pages are written for a sync operation
@@ -135,6 +138,8 @@ struct nilfs_sc_info {
 
 	struct list_head	sc_dirty_files;
 	struct list_head	sc_gc_inodes;
+	struct list_head	sc_iput_queue;
+	struct work_struct	sc_iput_work;
 
 	__u64		       *sc_freesegs;
 	size_t			sc_nfreesegs;
diff --git a/fs/notify/inode_mark.c b/fs/notify/inode_mark.c
index b13c00a..df6dacc 100644
--- a/fs/notify/inode_mark.c
+++ b/fs/notify/inode_mark.c
@@ -282,20 +282,25 @@ void fsnotify_unmount_inodes(struct list_head *list)
 		spin_unlock(&inode->i_lock);
 
 		/* In case the dropping of a reference would nuke next_i. */
-		if ((&next_i->i_sb_list != list) &&
-		    atomic_read(&next_i->i_count)) {
+		while (&next_i->i_sb_list != list) {
 			spin_lock(&next_i->i_lock);
-			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE))) {
+			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE)) &&
+						atomic_read(&next_i->i_count)) {
 				__iget(next_i);
 				need_iput = next_i;
+				spin_unlock(&next_i->i_lock);
+				break;
 			}
 			spin_unlock(&next_i->i_lock);
+			next_i = list_entry(next_i->i_sb_list.next,
+						struct inode, i_sb_list);
 		}
 
 		/*
-		 * We can safely drop inode_sb_list_lock here because we hold
-		 * references on both inode and next_i.  Also no new inodes
-		 * will be added since the umount has begun.
+		 * We can safely drop inode_sb_list_lock here because either
+		 * we actually hold references on both inode and next_i or
+		 * end of list.  Also no new inodes will be added since the
+		 * umount has begun.
 		 */
 		spin_unlock(&inode_sb_list_lock);
 
diff --git a/fs/ocfs2/aops.c b/fs/ocfs2/aops.c
index 340bd02..e9829ca 100644
--- a/fs/ocfs2/aops.c
+++ b/fs/ocfs2/aops.c
@@ -917,7 +917,7 @@ void ocfs2_unlock_and_free_pages(struct page **pages, int num_pages)
 	}
 }
 
-static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+static void ocfs2_unlock_pages(struct ocfs2_write_ctxt *wc)
 {
 	int i;
 
@@ -938,7 +938,11 @@ static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
 		page_cache_release(wc->w_target_page);
 	}
 	ocfs2_unlock_and_free_pages(wc->w_pages, wc->w_num_pages);
+}
 
+static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+{
+	ocfs2_unlock_pages(wc);
 	brelse(wc->w_di_bh);
 	kfree(wc);
 }
@@ -2059,11 +2063,19 @@ int ocfs2_write_end_nolock(struct address_space *mapping,
 	di->i_mtime_nsec = di->i_ctime_nsec = cpu_to_le32(inode->i_mtime.tv_nsec);
 	ocfs2_journal_dirty(handle, wc->w_di_bh);
 
+	/* unlock pages before dealloc since it needs acquiring j_trans_barrier
+	 * lock, or it will cause a deadlock since journal commit threads holds
+	 * this lock and will ask for the page lock when flushing the data.
+	 * put it here to preserve the unlock order.
+	 */
+	ocfs2_unlock_pages(wc);
+
 	ocfs2_commit_trans(osb, handle);
 
 	ocfs2_run_deallocs(osb, &wc->w_dealloc);
 
-	ocfs2_free_write_ctxt(wc);
+	brelse(wc->w_di_bh);
+	kfree(wc);
 
 	return copied;
 }
diff --git a/fs/proc/stat.c b/fs/proc/stat.c
index a1ca9bc..95f2e25 100644
--- a/fs/proc/stat.c
+++ b/fs/proc/stat.c
@@ -159,7 +159,7 @@ static int show_stat(struct seq_file *p, void *v)
 
 	/* sum again ? it could be updated? */
 	for_each_irq_nr(j)
-		seq_put_decimal_ull(p, ' ', kstat_irqs(j));
+		seq_put_decimal_ull(p, ' ', kstat_irqs_usr(j));
 
 	seq_printf(p,
 		"\nctxt %llu\n"
diff --git a/fs/proc/task_mmu.c b/fs/proc/task_mmu.c
index e4e423a..324eb57 100644
--- a/fs/proc/task_mmu.c
+++ b/fs/proc/task_mmu.c
@@ -1054,9 +1054,19 @@ static ssize_t pagemap_read(struct file *file, char __user *buf,
 	return ret;
 }
 
+static int pagemap_open(struct inode *inode, struct file *file)
+{
+	/* do not disclose physical addresses to unprivileged
+	   userspace (closes a rowhammer attack vector) */
+	if (!capable(CAP_SYS_ADMIN))
+		return -EPERM;
+	return 0;
+}
+
 const struct file_operations proc_pagemap_operations = {
 	.llseek		= mem_lseek, /* borrow this */
 	.read		= pagemap_read,
+	.open		= pagemap_open,
 };
 #endif /* CONFIG_PROC_PAGE_MONITOR */
 
diff --git a/fs/udf/dir.c b/fs/udf/dir.c
index eb8bfe2..56341af 100644
--- a/fs/udf/dir.c
+++ b/fs/udf/dir.c
@@ -163,7 +163,8 @@ static int do_udf_readdir(struct inode *dir, struct file *filp,
 			struct kernel_lb_addr tloc = lelb_to_cpu(cfi.icb.extLocation);
 
 			iblock = udf_get_lb_pblock(dir->i_sb, &tloc, 0);
-			flen = udf_get_filename(dir->i_sb, nameptr, fname, lfi);
+			flen = udf_get_filename(dir->i_sb, nameptr, lfi, fname,
+						UDF_NAME_LEN);
 			dt_type = DT_UNKNOWN;
 		}
 
diff --git a/fs/udf/inode.c b/fs/udf/inode.c
index aa70035..8053ee7 100644
--- a/fs/udf/inode.c
+++ b/fs/udf/inode.c
@@ -1392,6 +1392,20 @@ static void udf_fill_inode(struct inode *inode, struct buffer_head *bh)
 							iinfo->i_lenEAttr;
 	}
 
+	/* Sanity checks for files in ICB so that we don't get confused later */
+	if (iinfo->i_alloc_type == ICBTAG_FLAG_AD_IN_ICB) {
+		/*
+		 * For file in ICB data is stored in allocation descriptor
+		 * so sizes should match
+		 */
+		if (iinfo->i_lenAlloc != inode->i_size)
+			return;
+		/* File in ICB has to fit in there... */
+		if (inode->i_size > inode->i_sb->s_blocksize -
+					udf_file_entry_alloc_offset(inode))
+			return;
+	}
+
 	switch (fe->icbTag.fileType) {
 	case ICBTAG_FILE_TYPE_DIRECTORY:
 		inode->i_op = &udf_dir_inode_operations;
diff --git a/fs/udf/namei.c b/fs/udf/namei.c
index 78bff11..407c129 100644
--- a/fs/udf/namei.c
+++ b/fs/udf/namei.c
@@ -233,7 +233,8 @@ static struct fileIdentDesc *udf_find_entry(struct inode *dir,
 		if (!lfi)
 			continue;
 
-		flen = udf_get_filename(dir->i_sb, nameptr, fname, lfi);
+		flen = udf_get_filename(dir->i_sb, nameptr, lfi, fname,
+					UDF_NAME_LEN);
 		if (flen && udf_match(flen, fname, child->len, child->name))
 			goto out_ok;
 	}
diff --git a/fs/udf/symlink.c b/fs/udf/symlink.c
index d7c6dbe..0422b7b 100644
--- a/fs/udf/symlink.c
+++ b/fs/udf/symlink.c
@@ -30,49 +30,73 @@
 #include <linux/buffer_head.h>
 #include "udf_i.h"
 
-static void udf_pc_to_char(struct super_block *sb, unsigned char *from,
-			   int fromlen, unsigned char *to)
+static int udf_pc_to_char(struct super_block *sb, unsigned char *from,
+			  int fromlen, unsigned char *to, int tolen)
 {
 	struct pathComponent *pc;
 	int elen = 0;
+	int comp_len;
 	unsigned char *p = to;
 
+	/* Reserve one byte for terminating \0 */
+	tolen--;
 	while (elen < fromlen) {
 		pc = (struct pathComponent *)(from + elen);
+		elen += sizeof(struct pathComponent);
 		switch (pc->componentType) {
 		case 1:
 			/*
 			 * Symlink points to some place which should be agreed
  			 * upon between originator and receiver of the media. Ignore.
 			 */
-			if (pc->lengthComponentIdent > 0)
+			if (pc->lengthComponentIdent > 0) {
+				elen += pc->lengthComponentIdent;
 				break;
+			}
 			/* Fall through */
 		case 2:
+			if (tolen == 0)
+				return -ENAMETOOLONG;
 			p = to;
 			*p++ = '/';
+			tolen--;
 			break;
 		case 3:
+			if (tolen < 3)
+				return -ENAMETOOLONG;
 			memcpy(p, "../", 3);
 			p += 3;
+			tolen -= 3;
 			break;
 		case 4:
+			if (tolen < 2)
+				return -ENAMETOOLONG;
 			memcpy(p, "./", 2);
 			p += 2;
+			tolen -= 2;
 			/* that would be . - just ignore */
 			break;
 		case 5:
-			p += udf_get_filename(sb, pc->componentIdent, p,
-					      pc->lengthComponentIdent);
+			elen += pc->lengthComponentIdent;
+			if (elen > fromlen)
+				return -EIO;
+			comp_len = udf_get_filename(sb, pc->componentIdent,
+						    pc->lengthComponentIdent,
+						    p, tolen);
+			p += comp_len;
+			tolen -= comp_len;
+			if (tolen == 0)
+				return -ENAMETOOLONG;
 			*p++ = '/';
+			tolen--;
 			break;
 		}
-		elen += sizeof(struct pathComponent) + pc->lengthComponentIdent;
 	}
 	if (p > to + 1)
 		p[-1] = '\0';
 	else
 		p[0] = '\0';
+	return 0;
 }
 
 static int udf_symlink_filler(struct file *file, struct page *page)
@@ -80,11 +104,17 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	struct inode *inode = page->mapping->host;
 	struct buffer_head *bh = NULL;
 	unsigned char *symlink;
-	int err = -EIO;
+	int err;
 	unsigned char *p = kmap(page);
 	struct udf_inode_info *iinfo;
 	uint32_t pos;
 
+	/* We don't support symlinks longer than one block */
+	if (inode->i_size > inode->i_sb->s_blocksize) {
+		err = -ENAMETOOLONG;
+		goto out_unmap;
+	}
+
 	iinfo = UDF_I(inode);
 	pos = udf_block_map(inode, 0);
 
@@ -94,14 +124,18 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	} else {
 		bh = sb_bread(inode->i_sb, pos);
 
-		if (!bh)
-			goto out;
+		if (!bh) {
+			err = -EIO;
+			goto out_unlock_inode;
+		}
 
 		symlink = bh->b_data;
 	}
 
-	udf_pc_to_char(inode->i_sb, symlink, inode->i_size, p);
+	err = udf_pc_to_char(inode->i_sb, symlink, inode->i_size, p, PAGE_SIZE);
 	brelse(bh);
+	if (err)
+		goto out_unlock_inode;
 
 	up_read(&iinfo->i_data_sem);
 	SetPageUptodate(page);
@@ -109,9 +143,10 @@ static int udf_symlink_filler(struct file *file, struct page *page)
 	unlock_page(page);
 	return 0;
 
-out:
+out_unlock_inode:
 	up_read(&iinfo->i_data_sem);
 	SetPageError(page);
+out_unmap:
 	kunmap(page);
 	unlock_page(page);
 	return err;
diff --git a/fs/udf/udfdecl.h b/fs/udf/udfdecl.h
index ebe1031..375f648 100644
--- a/fs/udf/udfdecl.h
+++ b/fs/udf/udfdecl.h
@@ -207,7 +207,8 @@ udf_get_lb_pblock(struct super_block *sb, struct kernel_lb_addr *loc,
 }
 
 /* unicode.c */
-extern int udf_get_filename(struct super_block *, uint8_t *, uint8_t *, int);
+extern int udf_get_filename(struct super_block *, uint8_t *, int, uint8_t *,
+			    int);
 extern int udf_put_filename(struct super_block *, const uint8_t *, uint8_t *,
 			    int);
 extern int udf_build_ustr(struct ustr *, dstring *, int);
diff --git a/fs/udf/unicode.c b/fs/udf/unicode.c
index 44b815e..d29c06f 100644
--- a/fs/udf/unicode.c
+++ b/fs/udf/unicode.c
@@ -28,7 +28,8 @@
 
 #include "udf_sb.h"
 
-static int udf_translate_to_linux(uint8_t *, uint8_t *, int, uint8_t *, int);
+static int udf_translate_to_linux(uint8_t *, int, uint8_t *, int, uint8_t *,
+				  int);
 
 static int udf_char_to_ustr(struct ustr *dest, const uint8_t *src, int strlen)
 {
@@ -333,8 +334,8 @@ static int udf_NLStoCS0(struct nls_table *nls, dstring *ocu, struct ustr *uni,
 	return u_len + 1;
 }
 
-int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
-		     int flen)
+int udf_get_filename(struct super_block *sb, uint8_t *sname, int slen,
+		     uint8_t *dname, int dlen)
 {
 	struct ustr *filename, *unifilename;
 	int len = 0;
@@ -347,7 +348,7 @@ int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
 	if (!unifilename)
 		goto out1;
 
-	if (udf_build_ustr_exact(unifilename, sname, flen))
+	if (udf_build_ustr_exact(unifilename, sname, slen))
 		goto out2;
 
 	if (UDF_QUERY_FLAG(sb, UDF_FLAG_UTF8)) {
@@ -366,7 +367,8 @@ int udf_get_filename(struct super_block *sb, uint8_t *sname, uint8_t *dname,
 	} else
 		goto out2;
 
-	len = udf_translate_to_linux(dname, filename->u_name, filename->u_len,
+	len = udf_translate_to_linux(dname, dlen,
+				     filename->u_name, filename->u_len,
 				     unifilename->u_name, unifilename->u_len);
 out2:
 	kfree(unifilename);
@@ -403,10 +405,12 @@ int udf_put_filename(struct super_block *sb, const uint8_t *sname,
 #define EXT_MARK		'.'
 #define CRC_MARK		'#'
 #define EXT_SIZE 		5
+/* Number of chars we need to store generated CRC to make filename unique */
+#define CRC_LEN			5
 
-static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
-				  int udfLen, uint8_t *fidName,
-				  int fidNameLen)
+static int udf_translate_to_linux(uint8_t *newName, int newLen,
+				  uint8_t *udfName, int udfLen,
+				  uint8_t *fidName, int fidNameLen)
 {
 	int index, newIndex = 0, needsCRC = 0;
 	int extIndex = 0, newExtIndex = 0, hasExt = 0;
@@ -440,7 +444,7 @@ static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
 					newExtIndex = newIndex;
 				}
 			}
-			if (newIndex < 256)
+			if (newIndex < newLen)
 				newName[newIndex++] = curr;
 			else
 				needsCRC = 1;
@@ -468,13 +472,13 @@ static int udf_translate_to_linux(uint8_t *newName, uint8_t *udfName,
 				}
 				ext[localExtIndex++] = curr;
 			}
-			maxFilenameLen = 250 - localExtIndex;
+			maxFilenameLen = newLen - CRC_LEN - localExtIndex;
 			if (newIndex > maxFilenameLen)
 				newIndex = maxFilenameLen;
 			else
 				newIndex = newExtIndex;
-		} else if (newIndex > 250)
-			newIndex = 250;
+		} else if (newIndex > newLen - CRC_LEN)
+			newIndex = newLen - CRC_LEN;
 		newName[newIndex++] = CRC_MARK;
 		valueCRC = crc_itu_t(0, fidName, fidNameLen);
 		newName[newIndex++] = hexChar[(valueCRC & 0xf000) >> 12];
diff --git a/include/linux/device.h b/include/linux/device.h
index c297f25..5bf8909 100644
--- a/include/linux/device.h
+++ b/include/linux/device.h
@@ -849,6 +849,11 @@ extern __printf(5, 6)
 struct device *device_create(struct class *cls, struct device *parent,
 			     dev_t devt, void *drvdata,
 			     const char *fmt, ...);
+extern __printf(6, 7)
+struct device *device_create_with_groups(struct class *cls,
+			     struct device *parent, dev_t devt, void *drvdata,
+			     const struct attribute_group **groups,
+			     const char *fmt, ...);
 extern void device_destroy(struct class *cls, dev_t devt);
 
 /*
diff --git a/include/linux/kernel_stat.h b/include/linux/kernel_stat.h
index 2fbd905..8e62498 100644
--- a/include/linux/kernel_stat.h
+++ b/include/linux/kernel_stat.h
@@ -104,8 +104,13 @@ static inline unsigned int kstat_irqs(unsigned int irq)
 
 	return sum;
 }
+static inline unsigned int kstat_irqs_usr(unsigned int irq)
+{
+	return kstat_irqs(irq);
+}
 #else
 extern unsigned int kstat_irqs(unsigned int irq);
+extern unsigned int kstat_irqs_usr(unsigned int irq);
 #endif
 
 /*
diff --git a/include/linux/libata.h b/include/linux/libata.h
index dd16deb..764cd54 100644
--- a/include/linux/libata.h
+++ b/include/linux/libata.h
@@ -207,6 +207,7 @@ enum {
 	ATA_FLAG_SW_ACTIVITY	= (1 << 22), /* driver supports sw activity
 					      * led */
 	ATA_FLAG_NO_DIPM	= (1 << 23), /* host not happy with DIPM */
+	ATA_FLAG_LOWTAG		= (1 << 24), /* host wants lowest available tag */
 
 	/* bits 24:31 of ap->flags are reserved for LLD specific flags */
 
diff --git a/include/linux/mm.h b/include/linux/mm.h
index dcff232..e2309a7 100644
--- a/include/linux/mm.h
+++ b/include/linux/mm.h
@@ -871,6 +871,7 @@ static inline int page_mapped(struct page *page)
 #define VM_FAULT_WRITE	0x0008	/* Special case for get_user_pages */
 #define VM_FAULT_HWPOISON 0x0010	/* Hit poisoned small page */
 #define VM_FAULT_HWPOISON_LARGE 0x0020  /* Hit poisoned large page. Index encoded in upper bits */
+#define VM_FAULT_SIGSEGV 0x0040
 
 #define VM_FAULT_NOPAGE	0x0100	/* ->fault installed the pte, not return page */
 #define VM_FAULT_LOCKED	0x0200	/* ->fault locked the returned page */
@@ -878,8 +879,8 @@ static inline int page_mapped(struct page *page)
 
 #define VM_FAULT_HWPOISON_LARGE_MASK 0xf000 /* encodes hpage index for large hwpoison */
 
-#define VM_FAULT_ERROR	(VM_FAULT_OOM | VM_FAULT_SIGBUS | VM_FAULT_HWPOISON | \
-			 VM_FAULT_HWPOISON_LARGE)
+#define VM_FAULT_ERROR	(VM_FAULT_OOM | VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV | \
+			 VM_FAULT_HWPOISON | VM_FAULT_HWPOISON_LARGE)
 
 /* Encode hstate index for a hwpoisoned large page */
 #define VM_FAULT_SET_HINDEX(x) ((x) << 12)
@@ -1492,7 +1493,7 @@ extern int expand_downwards(struct vm_area_struct *vma,
 #if VM_GROWSUP
 extern int expand_upwards(struct vm_area_struct *vma, unsigned long address);
 #else
-  #define expand_upwards(vma, address) do { } while (0)
+  #define expand_upwards(vma, address) (0)
 #endif
 
 /* Look up the first VMA which satisfies  addr < vm_end,  NULL if none. */
diff --git a/include/linux/rmap.h b/include/linux/rmap.h
index a5ddc60..2f69ff4 100644
--- a/include/linux/rmap.h
+++ b/include/linux/rmap.h
@@ -37,6 +37,16 @@ struct anon_vma {
 	atomic_t refcount;
 
 	/*
+	 * Count of child anon_vmas and VMAs which points to this anon_vma.
+	 *
+	 * This counter is used for making decision about reusing anon_vma
+	 * instead of forking new one. See comments in function anon_vma_clone.
+	 */
+	unsigned degree;
+
+	struct anon_vma *parent;	/* Parent of this anon_vma */
+
+	/*
 	 * NOTE: the LSB of the head.next is set by
 	 * mm_take_all_locks() _after_ taking the above lock. So the
 	 * head must only be read/written after taking the above lock
diff --git a/include/linux/sysfs.h b/include/linux/sysfs.h
index 0010009..caf2e56 100644
--- a/include/linux/sysfs.h
+++ b/include/linux/sysfs.h
@@ -80,6 +80,15 @@ struct attribute_group {
 
 #define __ATTR_NULL { .attr = { .name = NULL } }
 
+#define ATTRIBUTE_GROUPS(name)					\
+static const struct attribute_group name##_group = {		\
+	.attrs = name##_attrs,					\
+};								\
+static const struct attribute_group *name##_groups[] = {	\
+	&name##_group,						\
+	NULL,							\
+}
+
 #define attr_name(_attr) (_attr).attr.name
 
 struct file;
diff --git a/include/linux/time.h b/include/linux/time.h
index af224eb..577e465 100644
--- a/include/linux/time.h
+++ b/include/linux/time.h
@@ -195,6 +195,19 @@ extern void getboottime(struct timespec *ts);
 extern void monotonic_to_bootbased(struct timespec *ts);
 extern void get_monotonic_boottime(struct timespec *ts);
 
+static inline bool timeval_valid(const struct timeval *tv)
+{
+	/* Dates before 1970 are bogus */
+	if (tv->tv_sec < 0)
+		return false;
+
+	/* Can't have more microseconds then a second */
+	if (tv->tv_usec < 0 || tv->tv_usec >= USEC_PER_SEC)
+		return false;
+
+	return true;
+}
+
 extern struct timespec timespec_trunc(struct timespec t, unsigned gran);
 extern int timekeeping_valid_for_hres(void);
 extern u64 timekeeping_max_deferment(void);
diff --git a/include/linux/usb/quirks.h b/include/linux/usb/quirks.h
index b1a7654..4bfff7a 100644
--- a/include/linux/usb/quirks.h
+++ b/include/linux/usb/quirks.h
@@ -35,4 +35,15 @@
 /* device can't handle device_qualifier descriptor requests */
 #define USB_QUIRK_DEVICE_QUALIFIER	0x00000100
 
+/*
+ * For high speed and super speed interupt endpoints, the USB 2.0 and
+ * USB 3.0 spec require the interval in microframes
+ * (1 microframe = 125 microseconds) to be calculated as
+ * interval = 2 ^ (bInterval-1).
+ *
+ * Devices with this quirk report their bInterval as the result of this
+ * calculation instead of the exponent variable used in the calculation.
+ */
+#define USB_QUIRK_LINEAR_UFRAME_INTR_BINTERVAL	0x00000080
+
 #endif /* __LINUX_USB_QUIRKS_H */
diff --git a/include/linux/usb_usual.h b/include/linux/usb_usual.h
index 17df360..f2000e9 100644
--- a/include/linux/usb_usual.h
+++ b/include/linux/usb_usual.h
@@ -64,7 +64,9 @@
 	US_FLAG(NO_READ_CAPACITY_16,	0x00080000)		\
 		/* cannot handle READ_CAPACITY_16 */		\
 	US_FLAG(INITIAL_READ10,	0x00100000)			\
-		/* Initial READ(10) (and others) must be retried */
+		/* Initial READ(10) (and others) must be retried */	\
+	US_FLAG(BROKEN_FUA,	0x01000000)			\
+		/* Cannot handle FUA in WRITE or READ CDBs */	\
 
 #define US_FLAG(name, value)	US_FL_##name = value ,
 enum { US_DO_ALL_FLAGS };
diff --git a/include/linux/virtio.h b/include/linux/virtio.h
index c2814ab..eba97bf 100644
--- a/include/linux/virtio.h
+++ b/include/linux/virtio.h
@@ -280,7 +280,11 @@ struct virtio_device {
 	void *priv;
 };
 
-#define dev_to_virtio(dev) container_of(dev, struct virtio_device, dev)
+static inline struct virtio_device *dev_to_virtio(struct device *_dev)
+{
+	return container_of(_dev, struct virtio_device, dev);
+}
+
 int register_virtio_device(struct virtio_device *dev);
 void unregister_virtio_device(struct virtio_device *dev);
 
diff --git a/include/linux/writeback.h b/include/linux/writeback.h
index 57b3695..4c5950c 100644
--- a/include/linux/writeback.h
+++ b/include/linux/writeback.h
@@ -187,7 +187,6 @@ int write_cache_pages(struct address_space *mapping,
 		      struct writeback_control *wbc, writepage_t writepage,
 		      void *data);
 int do_writepages(struct address_space *mapping, struct writeback_control *wbc);
-void set_page_dirty_balance(struct page *page, int page_mkwrite);
 void writeback_set_ratelimit(void);
 void tag_pages_for_writeback(struct address_space *mapping,
 			     pgoff_t start, pgoff_t end);
diff --git a/include/net/sctp/sctp.h b/include/net/sctp/sctp.h
index a2ef814..43c8bbcdb 100644
--- a/include/net/sctp/sctp.h
+++ b/include/net/sctp/sctp.h
@@ -524,6 +524,11 @@ static inline void sctp_assoc_pending_pmtu(struct sctp_association *asoc)
 	asoc->pmtu_pending = 0;
 }
 
+static inline bool sctp_chunk_pending(const struct sctp_chunk *chunk)
+{
+	return !list_empty(&chunk->list);
+}
+
 /* Walk through a list of TLV parameters.  Don't trust the
  * individual parameter lengths and instead depend on
  * the chunk length to indicate when to stop.  Make sure
diff --git a/include/net/sctp/sm.h b/include/net/sctp/sm.h
index 9148632..4d1be75 100644
--- a/include/net/sctp/sm.h
+++ b/include/net/sctp/sm.h
@@ -251,9 +251,9 @@ struct sctp_chunk *sctp_make_asconf_update_ip(struct sctp_association *,
 					      int, __be16);
 struct sctp_chunk *sctp_make_asconf_set_prim(struct sctp_association *asoc,
 					     union sctp_addr *addr);
-int sctp_verify_asconf(const struct sctp_association *asoc,
-		       struct sctp_paramhdr *param_hdr, void *chunk_end,
-		       struct sctp_paramhdr **errp);
+bool sctp_verify_asconf(const struct sctp_association *asoc,
+			struct sctp_chunk *chunk, bool addr_param_needed,
+			struct sctp_paramhdr **errp);
 struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 				       struct sctp_chunk *asconf);
 int sctp_process_asconf_ack(struct sctp_association *asoc,
diff --git a/include/scsi/scsi_device.h b/include/scsi/scsi_device.h
index 0564655..ef54805 100644
--- a/include/scsi/scsi_device.h
+++ b/include/scsi/scsi_device.h
@@ -154,6 +154,7 @@ struct scsi_device {
 	unsigned try_rc_10_first:1;	/* Try READ_CAPACACITY_10 first */
 	unsigned is_visible:1;	/* is the device visible in sysfs */
 	unsigned use_rpm_auto:1; /* Enable runtime PM auto suspend */
+	unsigned broken_fua:1;		/* Don't set FUA bit */
 
 #define SCSI_DEFAULT_AUTOSUSPEND_DELAY  -1
 	int autosuspend_delay;
diff --git a/include/sound/ak4113.h b/include/sound/ak4113.h
index 2609048..3a34f6e 100644
--- a/include/sound/ak4113.h
+++ b/include/sound/ak4113.h
@@ -286,7 +286,7 @@ struct ak4113 {
 	ak4113_write_t *write;
 	ak4113_read_t *read;
 	void *private_data;
-	unsigned int init:1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[AK4113_WRITABLE_REGS];
 	struct snd_kcontrol *kctls[AK4113_CONTROLS];
diff --git a/include/sound/ak4114.h b/include/sound/ak4114.h
index 3ce69fd..6944116 100644
--- a/include/sound/ak4114.h
+++ b/include/sound/ak4114.h
@@ -168,7 +168,7 @@ struct ak4114 {
 	ak4114_write_t * write;
 	ak4114_read_t * read;
 	void * private_data;
-	unsigned int init: 1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[7];
 	unsigned char txcsb[5];
diff --git a/kernel/irq/internals.h b/kernel/irq/internals.h
index 001fa5b..8a160e8 100644
--- a/kernel/irq/internals.h
+++ b/kernel/irq/internals.h
@@ -74,6 +74,14 @@ extern void irq_percpu_disable(struct irq_desc *desc, unsigned int cpu);
 extern void mask_irq(struct irq_desc *desc);
 extern void unmask_irq(struct irq_desc *desc);
 
+#ifdef CONFIG_SPARSE_IRQ
+extern void irq_lock_sparse(void);
+extern void irq_unlock_sparse(void);
+#else
+static inline void irq_lock_sparse(void) { }
+static inline void irq_unlock_sparse(void) { }
+#endif
+
 extern void init_kstat_irqs(struct irq_desc *desc, int node, int nr);
 
 irqreturn_t handle_irq_event_percpu(struct irq_desc *desc, struct irqaction *action);
diff --git a/kernel/irq/irqdesc.c b/kernel/irq/irqdesc.c
index 5413064..69772e5 100644
--- a/kernel/irq/irqdesc.c
+++ b/kernel/irq/irqdesc.c
@@ -132,6 +132,16 @@ static void free_masks(struct irq_desc *desc)
 static inline void free_masks(struct irq_desc *desc) { }
 #endif
 
+void irq_lock_sparse(void)
+{
+	mutex_lock(&sparse_irq_lock);
+}
+
+void irq_unlock_sparse(void)
+{
+	mutex_unlock(&sparse_irq_lock);
+}
+
 static struct irq_desc *alloc_desc(int irq, int node, struct module *owner)
 {
 	struct irq_desc *desc;
@@ -168,6 +178,12 @@ static void free_desc(unsigned int irq)
 
 	unregister_irq_proc(irq, desc);
 
+	/*
+	 * sparse_irq_lock protects also show_interrupts() and
+	 * kstat_irq_usr(). Once we deleted the descriptor from the
+	 * sparse tree we can free it. Access in proc will fail to
+	 * lookup the descriptor.
+	 */
 	mutex_lock(&sparse_irq_lock);
 	delete_irq_desc(irq);
 	mutex_unlock(&sparse_irq_lock);
@@ -499,6 +515,15 @@ void dynamic_irq_cleanup(unsigned int irq)
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
 }
 
+/**
+ * kstat_irqs_cpu - Get the statistics for an interrupt on a cpu
+ * @irq:	The interrupt number
+ * @cpu:	The cpu number
+ *
+ * Returns the sum of interrupt counts on @cpu since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -507,6 +532,14 @@ unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 			*per_cpu_ptr(desc->kstat_irqs, cpu) : 0;
 }
 
+/**
+ * kstat_irqs - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs(unsigned int irq)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -519,3 +552,22 @@ unsigned int kstat_irqs(unsigned int irq)
 		sum += *per_cpu_ptr(desc->kstat_irqs, cpu);
 	return sum;
 }
+
+/**
+ * kstat_irqs_usr - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. Contrary to kstat_irqs() this can be called from any
+ * preemptible context. It's protected against concurrent removal of
+ * an interrupt descriptor when sparse irqs are enabled.
+ */
+unsigned int kstat_irqs_usr(unsigned int irq)
+{
+	int sum;
+
+	irq_lock_sparse();
+	sum = kstat_irqs(irq);
+	irq_unlock_sparse();
+	return sum;
+}
diff --git a/kernel/irq/proc.c b/kernel/irq/proc.c
index 4bd4faa..fb655f5f 100644
--- a/kernel/irq/proc.c
+++ b/kernel/irq/proc.c
@@ -15,6 +15,23 @@
 
 #include "internals.h"
 
+/*
+ * Access rules:
+ *
+ * procfs protects read/write of /proc/irq/N/ files against a
+ * concurrent free of the interrupt descriptor. remove_proc_entry()
+ * immediately prevents new read/writes to happen and waits for
+ * already running read/write functions to complete.
+ *
+ * We remove the proc entries first and then delete the interrupt
+ * descriptor from the radix tree and free it. So it is guaranteed
+ * that irq_to_desc(N) is valid as long as the read/writes are
+ * permitted by procfs.
+ *
+ * The read from /proc/interrupts is a different problem because there
+ * is no protection. So the lookup and the access to irqdesc
+ * information must be protected by sparse_irq_lock.
+ */
 static struct proc_dir_entry *root_irq_dir;
 
 #ifdef CONFIG_SMP
@@ -441,9 +458,10 @@ int show_interrupts(struct seq_file *p, void *v)
 		seq_putc(p, '\n');
 	}
 
+	irq_lock_sparse();
 	desc = irq_to_desc(i);
 	if (!desc)
-		return 0;
+		goto outsparse;
 
 	raw_spin_lock_irqsave(&desc->lock, flags);
 	for_each_online_cpu(j)
@@ -481,6 +499,8 @@ int show_interrupts(struct seq_file *p, void *v)
 	seq_putc(p, '\n');
 out:
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
+outsparse:
+	irq_unlock_sparse();
 	return 0;
 }
 #endif
diff --git a/kernel/sched/rt.c b/kernel/sched/rt.c
index 526c77d..71429db 100644
--- a/kernel/sched/rt.c
+++ b/kernel/sched/rt.c
@@ -1293,7 +1293,12 @@ select_task_rq_rt(struct task_struct *p, int sd_flag, int flags)
 	    (p->rt.nr_cpus_allowed > 1)) {
 		int target = find_lowest_rq(p);
 
-		if (target != -1)
+		/*
+		 * Don't bother moving it if the destination CPU is
+		 * not running a lower priority task.
+		 */
+		if (target != -1 &&
+		    p->prio < cpu_rq(target)->rt.highest_prio.curr)
 			cpu = target;
 	}
 	rcu_read_unlock();
@@ -1570,6 +1575,16 @@ static struct rq *find_lock_lowest_rq(struct task_struct *task, struct rq *rq)
 
 		lowest_rq = cpu_rq(cpu);
 
+		if (lowest_rq->rt.highest_prio.curr <= task->prio) {
+			/*
+			 * Target rq has tasks of equal or higher priority,
+			 * retrying does not release any lock and is unlikely
+			 * to yield a different result.
+			 */
+			lowest_rq = NULL;
+			break;
+		}
+
 		/* if the prio of this runqueue changed, try again */
 		if (double_lock_balance(rq, lowest_rq)) {
 			/*
diff --git a/kernel/time.c b/kernel/time.c
index a095290..0864d70 100644
--- a/kernel/time.c
+++ b/kernel/time.c
@@ -186,6 +186,10 @@ SYSCALL_DEFINE2(settimeofday, struct timeval __user *, tv,
 	if (tv) {
 		if (copy_from_user(&user_tv, tv, sizeof(*tv)))
 			return -EFAULT;
+
+		if (!timeval_valid(&user_tv))
+			return -EINVAL;
+
 		new_ts.tv_sec = user_tv.tv_sec;
 		new_ts.tv_nsec = user_tv.tv_usec * NSEC_PER_USEC;
 	}
diff --git a/kernel/time/ntp.c b/kernel/time/ntp.c
index 8b70710..e32587e 100644
--- a/kernel/time/ntp.c
+++ b/kernel/time/ntp.c
@@ -660,6 +660,17 @@ int do_adjtimex(struct timex *txc)
 			return result;
 	}
 
+	/*
+	 * Check for potential multiplication overflows that can
+	 * only happen on 64-bit systems:
+	 */
+	if ((txc->modes & ADJ_FREQUENCY) && (BITS_PER_LONG == 64)) {
+		if (LLONG_MIN / PPM_SCALE > txc->freq)
+			return -EINVAL;
+		if (LLONG_MAX / PPM_SCALE < txc->freq)
+			return -EINVAL;
+	}
+
 	getnstimeofday(&ts);
 
 	spin_lock_irq(&ntp_lock);
diff --git a/lib/checksum.c b/lib/checksum.c
index 12dceb2..33f29f0 100644
--- a/lib/checksum.c
+++ b/lib/checksum.c
@@ -179,6 +179,15 @@ csum_partial_copy(const void *src, void *dst, int len, __wsum sum)
 EXPORT_SYMBOL(csum_partial_copy);
 
 #ifndef csum_tcpudp_nofold
+static inline u32 from64to32(u64 x)
+{
+	/* add up 32-bit and 32-bit for 32+c bit */
+	x = (x & 0xffffffff) + (x >> 32);
+	/* add up carry.. */
+	x = (x & 0xffffffff) + (x >> 32);
+	return (u32)x;
+}
+
 __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 			unsigned short len,
 			unsigned short proto,
@@ -193,8 +202,7 @@ __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 #else
 	s += (proto + len) << 8;
 #endif
-	s += (s >> 32);
-	return (__force __wsum)s;
+	return (__force __wsum)from64to32(s);
 }
 EXPORT_SYMBOL(csum_tcpudp_nofold);
 #endif
diff --git a/mm/ksm.c b/mm/ksm.c
index fa73fc6..c9a2934 100644
--- a/mm/ksm.c
+++ b/mm/ksm.c
@@ -345,7 +345,7 @@ static int break_ksm(struct vm_area_struct *vma, unsigned long addr)
 		else
 			ret = VM_FAULT_WRITE;
 		put_page(page);
-	} while (!(ret & (VM_FAULT_WRITE | VM_FAULT_SIGBUS | VM_FAULT_OOM)));
+	} while (!(ret & (VM_FAULT_WRITE | VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV | VM_FAULT_OOM)));
 	/*
 	 * We must loop because handle_mm_fault() may back out if there's
 	 * any difficulty e.g. if pte accessed bit gets updated concurrently.
diff --git a/mm/memory.c b/mm/memory.c
index 6d5e635..0e4c5fe 100644
--- a/mm/memory.c
+++ b/mm/memory.c
@@ -852,20 +852,20 @@ copy_one_pte(struct mm_struct *dst_mm, struct mm_struct *src_mm,
 		if (!pte_file(pte)) {
 			swp_entry_t entry = pte_to_swp_entry(pte);
 
-			if (swap_duplicate(entry) < 0)
-				return entry.val;
-
-			/* make sure dst_mm is on swapoff's mmlist. */
-			if (unlikely(list_empty(&dst_mm->mmlist))) {
-				spin_lock(&mmlist_lock);
-				if (list_empty(&dst_mm->mmlist))
-					list_add(&dst_mm->mmlist,
-						 &src_mm->mmlist);
-				spin_unlock(&mmlist_lock);
-			}
-			if (likely(!non_swap_entry(entry)))
+			if (likely(!non_swap_entry(entry))) {
+				if (swap_duplicate(entry) < 0)
+					return entry.val;
+
+				/* make sure dst_mm is on swapoff's mmlist. */
+				if (unlikely(list_empty(&dst_mm->mmlist))) {
+					spin_lock(&mmlist_lock);
+					if (list_empty(&dst_mm->mmlist))
+						list_add(&dst_mm->mmlist,
+							 &src_mm->mmlist);
+					spin_unlock(&mmlist_lock);
+				}
 				rss[MM_SWAPENTS]++;
-			else if (is_migration_entry(entry)) {
+			} else if (is_migration_entry(entry)) {
 				page = migration_entry_to_page(entry);
 
 				if (PageAnon(page))
@@ -1805,7 +1805,7 @@ int __get_user_pages(struct task_struct *tsk, struct mm_struct *mm,
 						else
 							return -EFAULT;
 					}
-					if (ret & VM_FAULT_SIGBUS)
+					if (ret & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV))
 						return i ? i : -EFAULT;
 					BUG();
 				}
@@ -1909,7 +1909,7 @@ int fixup_user_fault(struct task_struct *tsk, struct mm_struct *mm,
 			return -ENOMEM;
 		if (ret & (VM_FAULT_HWPOISON | VM_FAULT_HWPOISON_LARGE))
 			return -EHWPOISON;
-		if (ret & VM_FAULT_SIGBUS)
+		if (ret & (VM_FAULT_SIGBUS | VM_FAULT_SIGSEGV))
 			return -EFAULT;
 		BUG();
 	}
@@ -2699,18 +2699,25 @@ static int do_wp_page(struct mm_struct *mm, struct vm_area_struct *vma,
 		if (!dirty_page)
 			return ret;
 
-		/*
-		 * Yes, Virginia, this is actually required to prevent a race
-		 * with clear_page_dirty_for_io() from clearing the page dirty
-		 * bit after it clear all dirty ptes, but before a racing
-		 * do_wp_page installs a dirty pte.
-		 *
-		 * __do_fault is protected similarly.
-		 */
 		if (!page_mkwrite) {
-			wait_on_page_locked(dirty_page);
-			set_page_dirty_balance(dirty_page, page_mkwrite);
+			struct address_space *mapping;
+			int dirtied;
+
+			lock_page(dirty_page);
+			dirtied = set_page_dirty(dirty_page);
+			VM_BUG_ON(dirty_page);
+			mapping = dirty_page->mapping;
+			unlock_page(dirty_page);
+
+			if (dirtied && mapping) {
+				/*
+				 * Some device drivers do not set page.mapping
+				 * but still dirty their pages
+				 */
+				balance_dirty_pages_ratelimited(mapping);
+			}
 		}
+
 		put_page(dirty_page);
 		if (page_mkwrite) {
 			struct address_space *mapping = dirty_page->mapping;
@@ -3165,7 +3172,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (prev && prev->vm_end == address)
 			return prev->vm_flags & VM_GROWSDOWN ? 0 : -ENOMEM;
 
-		expand_downwards(vma, address - PAGE_SIZE);
+		return expand_downwards(vma, address - PAGE_SIZE);
 	}
 	if ((vma->vm_flags & VM_GROWSUP) && address + PAGE_SIZE == vma->vm_end) {
 		struct vm_area_struct *next = vma->vm_next;
@@ -3174,7 +3181,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (next && next->vm_start == address + PAGE_SIZE)
 			return next->vm_flags & VM_GROWSUP ? 0 : -ENOMEM;
 
-		expand_upwards(vma, address + PAGE_SIZE);
+		return expand_upwards(vma, address + PAGE_SIZE);
 	}
 	return 0;
 }
@@ -3196,7 +3203,7 @@ static int do_anonymous_page(struct mm_struct *mm, struct vm_area_struct *vma,
 
 	/* Check if we need to add a guard page to the stack */
 	if (check_stack_guard_page(vma, address) < 0)
-		return VM_FAULT_SIGBUS;
+		return VM_FAULT_SIGSEGV;
 
 	/* Use the zero-page for reads */
 	if (!(flags & FAULT_FLAG_WRITE)) {
diff --git a/mm/mmap.c b/mm/mmap.c
index eadef99..4cef37e 100644
--- a/mm/mmap.c
+++ b/mm/mmap.c
@@ -567,9 +567,12 @@ again:			remove_next = 1 + (end > next->vm_end);
 		 * shrinking vma had, to cover any anon pages imported.
 		 */
 		if (exporter && exporter->anon_vma && !importer->anon_vma) {
-			if (anon_vma_clone(importer, exporter))
-				return -ENOMEM;
+			int error;
+
 			importer->anon_vma = exporter->anon_vma;
+			error = anon_vma_clone(importer, exporter);
+			if (error)
+				return error;
 		}
 	}
 
@@ -1734,14 +1737,17 @@ static int acct_stack_growth(struct vm_area_struct *vma, unsigned long size, uns
 {
 	struct mm_struct *mm = vma->vm_mm;
 	struct rlimit *rlim = current->signal->rlim;
-	unsigned long new_start;
+	unsigned long new_start, actual_size;
 
 	/* address space limit tests */
 	if (!may_expand_vm(mm, grow))
 		return -ENOMEM;
 
 	/* Stack limit test */
-	if (size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
+	actual_size = size;
+	if (size && (vma->vm_flags & (VM_GROWSUP | VM_GROWSDOWN)))
+		actual_size -= PAGE_SIZE;
+	if (actual_size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
 		return -ENOMEM;
 
 	/* mlock limit tests */
diff --git a/mm/page-writeback.c b/mm/page-writeback.c
index e696d5e..0a49a2f 100644
--- a/mm/page-writeback.c
+++ b/mm/page-writeback.c
@@ -1397,16 +1397,6 @@ static void balance_dirty_pages(struct address_space *mapping,
 		bdi_start_background_writeback(bdi);
 }
 
-void set_page_dirty_balance(struct page *page, int page_mkwrite)
-{
-	if (set_page_dirty(page) || page_mkwrite) {
-		struct address_space *mapping = page_mapping(page);
-
-		if (mapping)
-			balance_dirty_pages_ratelimited(mapping);
-	}
-}
-
 static DEFINE_PER_CPU(int, bdp_ratelimits);
 
 /*
@@ -1984,32 +1974,25 @@ EXPORT_SYMBOL(account_page_writeback);
  * page dirty in that case, but not all the buffers.  This is a "bottom-up"
  * dirtying, whereas __set_page_dirty_buffers() is a "top-down" dirtying.
  *
- * Most callers have locked the page, which pins the address_space in memory.
- * But zap_pte_range() does not lock the page, however in that case the
- * mapping is pinned by the vma's ->vm_file reference.
- *
- * We take care to handle the case where the page was truncated from the
- * mapping by re-checking page_mapping() inside tree_lock.
+ * The caller must ensure this doesn't race with truncation.  Most will simply
+ * hold the page lock, but e.g. zap_pte_range() calls with the page mapped and
+ * the pte lock held, which also locks out truncat
  */
 int __set_page_dirty_nobuffers(struct page *page)
 {
 	if (!TestSetPageDirty(page)) {
 		struct address_space *mapping = page_mapping(page);
-		struct address_space *mapping2;
 		unsigned long flags;
 
 		if (!mapping)
 			return 1;
 
 		spin_lock_irqsave(&mapping->tree_lock, flags);
-		mapping2 = page_mapping(page);
-		if (mapping2) { /* Race with truncate? */
-			BUG_ON(mapping2 != mapping);
-			WARN_ON_ONCE(!PagePrivate(page) && !PageUptodate(page));
-			account_page_dirtied(page, mapping);
-			radix_tree_tag_set(&mapping->page_tree,
-				page_index(page), PAGECACHE_TAG_DIRTY);
-		}
+		BUG_ON(page_mapping(page) != mapping);
+		WARN_ON_ONCE(!PagePrivate(page) && !PageUptodate(page));
+		account_page_dirtied(page, mapping);
+		radix_tree_tag_set(&mapping->page_tree, page_index(page),
+				   PAGECACHE_TAG_DIRTY);
 		spin_unlock_irqrestore(&mapping->tree_lock, flags);
 		if (mapping->host) {
 			/* !PageAnon && !swapper_space */
@@ -2166,12 +2149,10 @@ int clear_page_dirty_for_io(struct page *page)
 		/*
 		 * We carefully synchronise fault handlers against
 		 * installing a dirty pte and marking the page dirty
-		 * at this point. We do this by having them hold the
-		 * page lock at some point after installing their
-		 * pte, but before marking the page dirty.
-		 * Pages are always locked coming in here, so we get
-		 * the desired exclusion. See mm/memory.c:do_wp_page()
-		 * for more comments.
+		 * at this point.  We do this by having them hold the
+		 * page lock while dirtying the page, and pages are
+		 * always locked coming in here, so we get the desired
+		 * exclusion.
 		 */
 		if (TestClearPageDirty(page)) {
 			dec_zone_page_state(page, NR_FILE_DIRTY);
diff --git a/mm/rmap.c b/mm/rmap.c
index ecce3ec..46dfc4e 100644
--- a/mm/rmap.c
+++ b/mm/rmap.c
@@ -72,6 +72,8 @@ static inline struct anon_vma *anon_vma_alloc(void)
 	anon_vma = kmem_cache_alloc(anon_vma_cachep, GFP_KERNEL);
 	if (anon_vma) {
 		atomic_set(&anon_vma->refcount, 1);
+		anon_vma->degree = 1;	/* Reference for first vma */
+		anon_vma->parent = anon_vma;
 		/*
 		 * Initialise the anon_vma root to point to itself. If called
 		 * from fork, the root will be reset to the parents anon_vma.
@@ -193,6 +195,8 @@ int anon_vma_prepare(struct vm_area_struct *vma)
 		if (likely(!vma->anon_vma)) {
 			vma->anon_vma = anon_vma;
 			anon_vma_chain_link(vma, avc, anon_vma);
+			/* vma reference or self-parent link for new root */
+			anon_vma->degree++;
 			allocated = NULL;
 			avc = NULL;
 		}
@@ -241,6 +245,14 @@ static inline void unlock_anon_vma_root(struct anon_vma *root)
 /*
  * Attach the anon_vmas from src to dst.
  * Returns 0 on success, -ENOMEM on failure.
+ *
+ * If dst->anon_vma is NULL this function tries to find and reuse existing
+ * anon_vma which has no vmas and only one child anon_vma. This prevents
+ * degradation of anon_vma hierarchy to endless linear chain in case of
+ * constantly forking task. On the other hand, an anon_vma with more than one
+ * child isn't reused even if there was no alive vma, thus rmap walker has a
+ * good chance of avoiding scanning the whole hierarchy when it searches where
+ * page is mapped.
  */
 int anon_vma_clone(struct vm_area_struct *dst, struct vm_area_struct *src)
 {
@@ -261,11 +273,32 @@ int anon_vma_clone(struct vm_area_struct *dst, struct vm_area_struct *src)
 		anon_vma = pavc->anon_vma;
 		root = lock_anon_vma_root(root, anon_vma);
 		anon_vma_chain_link(dst, avc, anon_vma);
+
+		/*
+		 * Reuse existing anon_vma if its degree lower than two,
+		 * that means it has no vma and only one anon_vma child.
+		 *
+		 * Do not chose parent anon_vma, otherwise first child
+		 * will always reuse it. Root anon_vma is never reused:
+		 * it has self-parent reference and at least one child.
+		 */
+		if (!dst->anon_vma && anon_vma != src->anon_vma &&
+				anon_vma->degree < 2)
+			dst->anon_vma = anon_vma;
 	}
+	if (dst->anon_vma)
+		dst->anon_vma->degree++;
 	unlock_anon_vma_root(root);
 	return 0;
 
  enomem_failure:
+	/*
+	 * dst->anon_vma is dropped here otherwise its degree can be incorrectly
+	 * decremented in unlink_anon_vmas().
+	 * We can safely do this because callers of anon_vma_clone() don't care
+	 * about dst->anon_vma if anon_vma_clone() failed.
+	 */
+	dst->anon_vma = NULL;
 	unlink_anon_vmas(dst);
 	return -ENOMEM;
 }
@@ -329,6 +362,9 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	if (!pvma->anon_vma)
 		return 0;
 
+	/* Drop inherited anon_vma, we'll reuse existing or allocate new. */
+	vma->anon_vma = NULL;
+
 	/*
 	 * First, attach the new VMA to the parent VMA's anon_vmas,
 	 * so rmap can find non-COWed pages in child processes.
@@ -336,6 +372,10 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	if (anon_vma_clone(vma, pvma))
 		return -ENOMEM;
 
+	/* An existing anon_vma has been reused, all done then. */
+	if (vma->anon_vma)
+		return 0;
+
 	/* Then add our own anon_vma. */
 	anon_vma = anon_vma_alloc();
 	if (!anon_vma)
@@ -349,6 +389,7 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	 * lock any of the anon_vmas in this anon_vma tree.
 	 */
 	anon_vma->root = pvma->anon_vma->root;
+	anon_vma->parent = pvma->anon_vma;
 	/*
 	 * With refcounts, an anon_vma can stay around longer than the
 	 * process it belongs to. The root anon_vma needs to be pinned until
@@ -359,6 +400,7 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	vma->anon_vma = anon_vma;
 	anon_vma_lock(anon_vma);
 	anon_vma_chain_link(vma, avc, anon_vma);
+	anon_vma->parent->degree++;
 	anon_vma_unlock(anon_vma);
 
 	return 0;
@@ -389,12 +431,16 @@ void unlink_anon_vmas(struct vm_area_struct *vma)
 		 * Leave empty anon_vmas on the list - we'll need
 		 * to free them outside the lock.
 		 */
-		if (list_empty(&anon_vma->head))
+		if (list_empty(&anon_vma->head)) {
+			anon_vma->parent->degree--;
 			continue;
+		}
 
 		list_del(&avc->same_vma);
 		anon_vma_chain_free(avc);
 	}
+	if (vma->anon_vma)
+		vma->anon_vma->degree--;
 	unlock_anon_vma_root(root);
 
 	/*
@@ -405,6 +451,7 @@ void unlink_anon_vmas(struct vm_area_struct *vma)
 	list_for_each_entry_safe(avc, next, &vma->anon_vma_chain, same_vma) {
 		struct anon_vma *anon_vma = avc->anon_vma;
 
+		BUG_ON(anon_vma->degree);
 		put_anon_vma(anon_vma);
 
 		list_del(&avc->same_vma);
diff --git a/net/caif/chnl_net.c b/net/caif/chnl_net.c
index d09340e..b8d9403 100644
--- a/net/caif/chnl_net.c
+++ b/net/caif/chnl_net.c
@@ -467,7 +467,6 @@ static int ipcaif_newlink(struct net *src_net, struct net_device *dev,
 	ASSERT_RTNL();
 	caifdev = netdev_priv(dev);
 	caif_netlink_parms(data, &caifdev->conn_req);
-	dev_net_set(caifdev->netdev, src_net);
 
 	ret = register_netdevice(dev);
 	if (ret)
diff --git a/net/compat.c b/net/compat.c
index f7f82ba..618ad24 100644
--- a/net/compat.c
+++ b/net/compat.c
@@ -71,6 +71,13 @@ int get_compat_msghdr(struct msghdr *kmsg, struct compat_msghdr __user *umsg)
 	    __get_user(kmsg->msg_controllen, &umsg->msg_controllen) ||
 	    __get_user(kmsg->msg_flags, &umsg->msg_flags))
 		return -EFAULT;
+
+	if (!tmp1)
+		kmsg->msg_namelen = 0;
+
+	if (kmsg->msg_namelen < 0)
+		return -EINVAL;
+
 	if (kmsg->msg_namelen > sizeof(struct sockaddr_storage))
 		kmsg->msg_namelen = sizeof(struct sockaddr_storage);
 	kmsg->msg_name = compat_ptr(tmp1);
diff --git a/net/core/dev.c b/net/core/dev.c
index 634f56d..06ea934 100644
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -2143,12 +2143,14 @@ netdev_features_t netif_skb_features(struct sk_buff *skb)
 	if (skb_shinfo(skb)->gso_segs > skb->dev->gso_max_segs)
 		features &= ~NETIF_F_GSO_MASK;
 
-	if (protocol == htons(ETH_P_8021Q)) {
-		struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
-		protocol = veh->h_vlan_encapsulated_proto;
-	} else if (!vlan_tx_tag_present(skb)) {
-		return harmonize_features(skb, protocol, features);
-	}
+	if (!vlan_tx_tag_present(skb)) {
+		if (unlikely(protocol == htons(ETH_P_8021Q))) {
+			struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
+			protocol = veh->h_vlan_encapsulated_proto;
+		} else {
+			return harmonize_features(skb, protocol, features);
+		}
+        }
 
 	features &= (skb->dev->vlan_features | NETIF_F_HW_VLAN_TX);
 
diff --git a/net/ipv6/ip6_fib.c b/net/ipv6/ip6_fib.c
index 5bb77a6..2cfcfb7 100644
--- a/net/ipv6/ip6_fib.c
+++ b/net/ipv6/ip6_fib.c
@@ -633,6 +633,29 @@ static struct fib6_node * fib6_add_1(struct fib6_node *root, void *addr,
 	return ln;
 }
 
+static void fib6_purge_rt(struct rt6_info *rt, struct fib6_node *fn,
+			  struct net *net)
+{
+	if (atomic_read(&rt->rt6i_ref) != 1) {
+		/* This route is used as dummy address holder in some split
+		 * nodes. It is not leaked, but it still holds other resources,
+		 * which must be released in time. So, scan ascendant nodes
+		 * and replace dummy references to this route with references
+		 * to still alive ones.
+		 */
+		while (fn) {
+			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
+				fn->leaf = fib6_find_prefix(net, fn);
+				atomic_inc(&fn->leaf->rt6i_ref);
+				rt6_release(rt);
+			}
+			fn = fn->parent;
+		}
+		/* No more references are possible at this point. */
+		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
+	}
+}
+
 /*
  *	Insert routing information in a node.
  */
@@ -723,11 +746,12 @@ static int fib6_add_rt2node(struct fib6_node *fn, struct rt6_info *rt,
 		rt->dst.rt6_next = iter->dst.rt6_next;
 		atomic_inc(&rt->rt6i_ref);
 		inet6_rt_notify(RTM_NEWROUTE, rt, info);
-		rt6_release(iter);
 		if (!(fn->fn_flags & RTN_RTINFO)) {
 			info->nl_net->ipv6.rt6_stats->fib_route_nodes++;
 			fn->fn_flags |= RTN_RTINFO;
 		}
+		fib6_purge_rt(iter, fn, info->nl_net);
+		rt6_release(iter);
 	}
 
 	return 0;
@@ -1229,24 +1253,7 @@ static void fib6_del_route(struct fib6_node *fn, struct rt6_info **rtp,
 		fn = fib6_repair_tree(net, fn);
 	}
 
-	if (atomic_read(&rt->rt6i_ref) != 1) {
-		/* This route is used as dummy address holder in some split
-		 * nodes. It is not leaked, but it still holds other resources,
-		 * which must be released in time. So, scan ascendant nodes
-		 * and replace dummy references to this route with references
-		 * to still alive ones.
-		 */
-		while (fn) {
-			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
-				fn->leaf = fib6_find_prefix(net, fn);
-				atomic_inc(&fn->leaf->rt6i_ref);
-				rt6_release(rt);
-			}
-			fn = fn->parent;
-		}
-		/* No more references are possible at this point. */
-		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
-	}
+	fib6_purge_rt(rt, fn, net);
 
 	inet6_rt_notify(RTM_DELROUTE, rt, info);
 	rt6_release(rt);
diff --git a/net/mac80211/rx.c b/net/mac80211/rx.c
index 32929b0..24f2a41 100644
--- a/net/mac80211/rx.c
+++ b/net/mac80211/rx.c
@@ -1486,14 +1486,14 @@ ieee80211_rx_h_defragment(struct ieee80211_rx_data *rx)
 	sc = le16_to_cpu(hdr->seq_ctrl);
 	frag = sc & IEEE80211_SCTL_FRAG;
 
-	if (likely(!ieee80211_has_morefrags(fc) && frag == 0))
-		goto out;
-
 	if (is_multicast_ether_addr(hdr->addr1)) {
 		rx->local->dot11MulticastReceivedFrameCount++;
-		goto out;
+		goto out_no_led;
 	}
 
+	if (likely(!ieee80211_has_morefrags(fc) && frag == 0))
+		goto out;
+
 	I802_DEBUG_INC(rx->local->rx_handlers_fragments);
 
 	if (skb_linearize(rx->skb))
@@ -1584,9 +1584,10 @@ ieee80211_rx_h_defragment(struct ieee80211_rx_data *rx)
 	status->rx_flags |= IEEE80211_RX_FRAGMENTED;
 
  out:
+	ieee80211_led_rx(rx->local);
+ out_no_led:
 	if (rx->sta)
 		rx->sta->rx_packets++;
-	ieee80211_led_rx(rx->local);
 	return RX_CONTINUE;
 }
 
diff --git a/net/netfilter/ipvs/ip_vs_core.c b/net/netfilter/ipvs/ip_vs_core.c
index 00bdb1d..abdb475 100644
--- a/net/netfilter/ipvs/ip_vs_core.c
+++ b/net/netfilter/ipvs/ip_vs_core.c
@@ -662,16 +662,24 @@ static inline int ip_vs_gather_frags_v6(struct sk_buff *skb, u_int32_t user)
 }
 #endif
 
-static int ip_vs_route_me_harder(int af, struct sk_buff *skb)
+static int ip_vs_route_me_harder(int af, struct sk_buff *skb,
+				 unsigned int hooknum)
 {
+	if (!sysctl_snat_reroute(skb))
+		return 0;
+	/* Reroute replies only to remote clients (FORWARD and LOCAL_OUT) */
+	if (NF_INET_LOCAL_IN == hooknum)
+		return 0;
 #ifdef CONFIG_IP_VS_IPV6
 	if (af == AF_INET6) {
-		if (sysctl_snat_reroute(skb) && ip6_route_me_harder(skb) != 0)
+		struct dst_entry *dst = skb_dst(skb);
+
+		if (dst->dev && !(dst->dev->flags & IFF_LOOPBACK) &&
+		    ip6_route_me_harder(skb) != 0)
 			return 1;
 	} else
 #endif
-		if ((sysctl_snat_reroute(skb) ||
-		     skb_rtable(skb)->rt_flags & RTCF_LOCAL) &&
+		if (!(skb_rtable(skb)->rt_flags & RTCF_LOCAL) &&
 		    ip_route_me_harder(skb, RTN_LOCAL) != 0)
 			return 1;
 
@@ -782,7 +790,8 @@ static int handle_response_icmp(int af, struct sk_buff *skb,
 				union nf_inet_addr *snet,
 				__u8 protocol, struct ip_vs_conn *cp,
 				struct ip_vs_protocol *pp,
-				unsigned int offset, unsigned int ihl)
+				unsigned int offset, unsigned int ihl,
+				unsigned int hooknum)
 {
 	unsigned int verdict = NF_DROP;
 
@@ -812,7 +821,7 @@ static int handle_response_icmp(int af, struct sk_buff *skb,
 #endif
 		ip_vs_nat_icmp(skb, pp, cp, 1);
 
-	if (ip_vs_route_me_harder(af, skb))
+	if (ip_vs_route_me_harder(af, skb, hooknum))
 		goto out;
 
 	/* do the statistics and put it back */
@@ -908,7 +917,7 @@ static int ip_vs_out_icmp(struct sk_buff *skb, int *related,
 
 	snet.ip = iph->saddr;
 	return handle_response_icmp(AF_INET, skb, &snet, cih->protocol, cp,
-				    pp, offset, ihl);
+				    pp, offset, ihl, hooknum);
 }
 
 #ifdef CONFIG_IP_VS_IPV6
@@ -985,7 +994,8 @@ static int ip_vs_out_icmp_v6(struct sk_buff *skb, int *related,
 
 	snet.in6 = iph->saddr;
 	return handle_response_icmp(AF_INET6, skb, &snet, cih->nexthdr, cp,
-				    pp, offset, sizeof(struct ipv6hdr));
+				    pp, offset, sizeof(struct ipv6hdr),
+				    hooknum);
 }
 #endif
 
@@ -1018,7 +1028,7 @@ static inline int is_tcp_reset(const struct sk_buff *skb, int nh_len)
  */
 static unsigned int
 handle_response(int af, struct sk_buff *skb, struct ip_vs_proto_data *pd,
-		struct ip_vs_conn *cp, int ihl)
+		struct ip_vs_conn *cp, int ihl, unsigned int hooknum)
 {
 	struct ip_vs_protocol *pp = pd->pp;
 
@@ -1056,7 +1066,7 @@ handle_response(int af, struct sk_buff *skb, struct ip_vs_proto_data *pd,
 	 * if it came from this machine itself.  So re-compute
 	 * the routing information.
 	 */
-	if (ip_vs_route_me_harder(af, skb))
+	if (ip_vs_route_me_harder(af, skb, hooknum))
 		goto drop;
 
 	IP_VS_DBG_PKT(10, af, pp, skb, 0, "After SNAT");
@@ -1169,7 +1179,7 @@ ip_vs_out(unsigned int hooknum, struct sk_buff *skb, int af)
 	cp = pp->conn_out_get(af, skb, &iph, iph.len, 0);
 
 	if (likely(cp))
-		return handle_response(af, skb, pd, cp, iph.len);
+		return handle_response(af, skb, pd, cp, iph.len, hooknum);
 	if (sysctl_nat_icmp_send(net) &&
 	    (pp->protocol == IPPROTO_TCP ||
 	     pp->protocol == IPPROTO_UDP ||
diff --git a/net/sctp/associola.c b/net/sctp/associola.c
index da54d29..d014b05 100644
--- a/net/sctp/associola.c
+++ b/net/sctp/associola.c
@@ -1272,7 +1272,6 @@ void sctp_assoc_update(struct sctp_association *asoc,
 	asoc->peer.peer_hmacs = new->peer.peer_hmacs;
 	new->peer.peer_hmacs = NULL;
 
-	sctp_auth_key_put(asoc->asoc_shared_key);
 	sctp_auth_asoc_init_active_key(asoc, GFP_ATOMIC);
 }
 
@@ -1638,6 +1637,8 @@ struct sctp_chunk *sctp_assoc_lookup_asconf_ack(
 	 * ack chunk whose serial number matches that of the request.
 	 */
 	list_for_each_entry(ack, &asoc->asconf_ack_list, transmitted_list) {
+		if (sctp_chunk_pending(ack))
+			continue;
 		if (ack->subh.addip_hdr->serial == serial) {
 			sctp_chunk_hold(ack);
 			return ack;
diff --git a/net/sctp/sm_make_chunk.c b/net/sctp/sm_make_chunk.c
index adb0287..f1249b3 100644
--- a/net/sctp/sm_make_chunk.c
+++ b/net/sctp/sm_make_chunk.c
@@ -2569,7 +2569,10 @@ static int sctp_process_param(struct sctp_association *asoc,
 
 		addr_param = param.v + sizeof(sctp_addip_param_t);
 
-		af = sctp_get_af_specific(param_type2af(param.p->type));
+		af = sctp_get_af_specific(param_type2af(addr_param->p.type));
+		if (af == NULL)
+			break;
+
 		af->from_addr_param(&addr, addr_param,
 				    htons(asoc->peer.port), 0);
 
@@ -3068,50 +3071,63 @@ static __be16 sctp_process_asconf_param(struct sctp_association *asoc,
 	return SCTP_ERROR_NO_ERROR;
 }
 
-/* Verify the ASCONF packet before we process it.  */
-int sctp_verify_asconf(const struct sctp_association *asoc,
-		       struct sctp_paramhdr *param_hdr, void *chunk_end,
-		       struct sctp_paramhdr **errp) {
-	sctp_addip_param_t *asconf_param;
+/* Verify the ASCONF packet before we process it. */
+bool sctp_verify_asconf(const struct sctp_association *asoc,
+			struct sctp_chunk *chunk, bool addr_param_needed,
+			struct sctp_paramhdr **errp)
+{
+	sctp_addip_chunk_t *addip = (sctp_addip_chunk_t *) chunk->chunk_hdr;
 	union sctp_params param;
-	int length, plen;
+	bool addr_param_seen = false;
 
-	param.v = (sctp_paramhdr_t *) param_hdr;
-	while (param.v <= chunk_end - sizeof(sctp_paramhdr_t)) {
-		length = ntohs(param.p->length);
-		*errp = param.p;
-
-		if (param.v > chunk_end - length ||
-		    length < sizeof(sctp_paramhdr_t))
-			return 0;
+	sctp_walk_params(param, addip, addip_hdr.params) {
+		size_t length = ntohs(param.p->length);
 
+		*errp = param.p;
 		switch (param.p->type) {
+		case SCTP_PARAM_ERR_CAUSE:
+			break;
+		case SCTP_PARAM_IPV4_ADDRESS:
+			if (length != sizeof(sctp_ipv4addr_param_t))
+				return false;
+			addr_param_seen = true;
+			break;
+		case SCTP_PARAM_IPV6_ADDRESS:
+			if (length != sizeof(sctp_ipv6addr_param_t))
+				return false;
+			addr_param_seen = true;
+			break;
 		case SCTP_PARAM_ADD_IP:
 		case SCTP_PARAM_DEL_IP:
 		case SCTP_PARAM_SET_PRIMARY:
-			asconf_param = (sctp_addip_param_t *)param.v;
-			plen = ntohs(asconf_param->param_hdr.length);
-			if (plen < sizeof(sctp_addip_param_t) +
-			    sizeof(sctp_paramhdr_t))
-				return 0;
+			/* In ASCONF chunks, these need to be first. */
+			if (addr_param_needed && !addr_param_seen)
+				return false;
+			length = ntohs(param.addip->param_hdr.length);
+			if (length < sizeof(sctp_addip_param_t) +
+				     sizeof(sctp_paramhdr_t))
+				return false;
 			break;
 		case SCTP_PARAM_SUCCESS_REPORT:
 		case SCTP_PARAM_ADAPTATION_LAYER_IND:
 			if (length != sizeof(sctp_addip_param_t))
-				return 0;
-
+				return false;
 			break;
 		default:
-			break;
+			/* This is unkown to us, reject! */
+			return false;
 		}
-
-		param.v += WORD_ROUND(length);
 	}
 
-	if (param.v != chunk_end)
-		return 0;
+	/* Remaining sanity checks. */
+	if (addr_param_needed && !addr_param_seen)
+		return false;
+	if (!addr_param_needed && addr_param_seen)
+		return false;
+	if (param.v != chunk->chunk_end)
+		return false;
 
-	return 1;
+	return true;
 }
 
 /* Process an incoming ASCONF chunk with the next expected serial no. and
@@ -3120,16 +3136,17 @@ int sctp_verify_asconf(const struct sctp_association *asoc,
 struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 				       struct sctp_chunk *asconf)
 {
+	sctp_addip_chunk_t *addip = (sctp_addip_chunk_t *) asconf->chunk_hdr;
+	bool all_param_pass = true;
+	union sctp_params param;
 	sctp_addiphdr_t		*hdr;
 	union sctp_addr_param	*addr_param;
 	sctp_addip_param_t	*asconf_param;
 	struct sctp_chunk	*asconf_ack;
-
 	__be16	err_code;
 	int	length = 0;
 	int	chunk_len;
 	__u32	serial;
-	int	all_param_pass = 1;
 
 	chunk_len = ntohs(asconf->chunk_hdr->length) - sizeof(sctp_chunkhdr_t);
 	hdr = (sctp_addiphdr_t *)asconf->skb->data;
@@ -3157,9 +3174,14 @@ struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 		goto done;
 
 	/* Process the TLVs contained within the ASCONF chunk. */
-	while (chunk_len > 0) {
+	sctp_walk_params(param, addip, addip_hdr.params) {
+		/* Skip preceeding address parameters. */
+		if (param.p->type == SCTP_PARAM_IPV4_ADDRESS ||
+		    param.p->type == SCTP_PARAM_IPV6_ADDRESS)
+			continue;
+
 		err_code = sctp_process_asconf_param(asoc, asconf,
-						     asconf_param);
+						     param.addip);
 		/* ADDIP 4.1 A7)
 		 * If an error response is received for a TLV parameter,
 		 * all TLVs with no response before the failed TLV are
@@ -3167,28 +3189,20 @@ struct sctp_chunk *sctp_process_asconf(struct sctp_association *asoc,
 		 * the failed response are considered unsuccessful unless
 		 * a specific success indication is present for the parameter.
 		 */
-		if (SCTP_ERROR_NO_ERROR != err_code)
-			all_param_pass = 0;
-
+		if (err_code != SCTP_ERROR_NO_ERROR)
+			all_param_pass = false;
 		if (!all_param_pass)
-			sctp_add_asconf_response(asconf_ack,
-						 asconf_param->crr_id, err_code,
-						 asconf_param);
+			sctp_add_asconf_response(asconf_ack, param.addip->crr_id,
+						 err_code, param.addip);
 
 		/* ADDIP 4.3 D11) When an endpoint receiving an ASCONF to add
 		 * an IP address sends an 'Out of Resource' in its response, it
 		 * MUST also fail any subsequent add or delete requests bundled
 		 * in the ASCONF.
 		 */
-		if (SCTP_ERROR_RSRC_LOW == err_code)
+		if (err_code == SCTP_ERROR_RSRC_LOW)
 			goto done;
-
-		/* Move to the next ASCONF param. */
-		length = ntohs(asconf_param->param_hdr.length);
-		asconf_param = (void *)asconf_param + length;
-		chunk_len -= length;
 	}
-
 done:
 	asoc->peer.addip_serial++;
 
diff --git a/net/sctp/sm_statefuns.c b/net/sctp/sm_statefuns.c
index 5ac33b6..a6a3006 100644
--- a/net/sctp/sm_statefuns.c
+++ b/net/sctp/sm_statefuns.c
@@ -3516,9 +3516,7 @@ sctp_disposition_t sctp_sf_do_asconf(const struct sctp_endpoint *ep,
 	struct sctp_chunk	*asconf_ack = NULL;
 	struct sctp_paramhdr	*err_param = NULL;
 	sctp_addiphdr_t		*hdr;
-	union sctp_addr_param	*addr_param;
 	__u32			serial;
-	int			length;
 
 	if (!sctp_vtag_verify(chunk, asoc)) {
 		sctp_add_cmd_sf(commands, SCTP_CMD_REPORT_BAD_TAG,
@@ -3543,17 +3541,8 @@ sctp_disposition_t sctp_sf_do_asconf(const struct sctp_endpoint *ep,
 	hdr = (sctp_addiphdr_t *)chunk->skb->data;
 	serial = ntohl(hdr->serial);
 
-	addr_param = (union sctp_addr_param *)hdr->params;
-	length = ntohs(addr_param->p.length);
-	if (length < sizeof(sctp_paramhdr_t))
-		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
-			   (void *)addr_param, commands);
-
 	/* Verify the ASCONF chunk before processing it. */
-	if (!sctp_verify_asconf(asoc,
-			    (sctp_paramhdr_t *)((void *)addr_param + length),
-			    (void *)chunk->chunk_end,
-			    &err_param))
+	if (!sctp_verify_asconf(asoc, chunk, true, &err_param))
 		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
 						  (void *)err_param, commands);
 
@@ -3670,10 +3659,7 @@ sctp_disposition_t sctp_sf_do_asconf_ack(const struct sctp_endpoint *ep,
 	rcvd_serial = ntohl(addip_hdr->serial);
 
 	/* Verify the ASCONF-ACK chunk before processing it. */
-	if (!sctp_verify_asconf(asoc,
-	    (sctp_paramhdr_t *)addip_hdr->params,
-	    (void *)asconf_ack->chunk_end,
-	    &err_param))
+	if (!sctp_verify_asconf(asoc, asconf_ack, false, &err_param))
 		return sctp_sf_violation_paramlen(ep, asoc, type, arg,
 			   (void *)err_param, commands);
 
diff --git a/net/socket.c b/net/socket.c
index 7e13992..efcf863 100644
--- a/net/socket.c
+++ b/net/socket.c
@@ -1929,6 +1929,9 @@ static int copy_msghdr_from_user(struct msghdr *kmsg,
 	if (copy_from_user(kmsg, umsg, sizeof(struct msghdr)))
 		return -EFAULT;
 
+	if (kmsg->msg_name == NULL)
+		kmsg->msg_namelen = 0;
+
 	if (kmsg->msg_namelen < 0)
 		return -EINVAL;
 
diff --git a/net/sunrpc/svcsock.c b/net/sunrpc/svcsock.c
index 4c23cfc..a0769e1 100644
--- a/net/sunrpc/svcsock.c
+++ b/net/sunrpc/svcsock.c
@@ -1055,17 +1055,12 @@ static int receive_cb_reply(struct svc_sock *svsk, struct svc_rqst *rqstp)
 	xid = *p++;
 	calldir = *p;
 
-	if (bc_xprt)
-		req = xprt_lookup_rqst(bc_xprt, xid);
-
-	if (!req) {
-		printk(KERN_NOTICE
-			"%s: Got unrecognized reply: "
-			"calldir 0x%x xpt_bc_xprt %p xid %08x\n",
-			__func__, ntohl(calldir),
-			bc_xprt, xid);
+	if (!bc_xprt)
 		return -EAGAIN;
-	}
+	spin_lock_bh(&bc_xprt->transport_lock);
+	req = xprt_lookup_rqst(bc_xprt, xid);
+	if (!req)
+		goto unlock_notfound;
 
 	memcpy(&req->rq_private_buf, &req->rq_rcv_buf, sizeof(struct xdr_buf));
 	/*
@@ -1076,11 +1071,21 @@ static int receive_cb_reply(struct svc_sock *svsk, struct svc_rqst *rqstp)
 	dst = &req->rq_private_buf.head[0];
 	src = &rqstp->rq_arg.head[0];
 	if (dst->iov_len < src->iov_len)
-		return -EAGAIN; /* whatever; just giving up. */
+		goto unlock_eagain; /* whatever; just giving up. */
 	memcpy(dst->iov_base, src->iov_base, src->iov_len);
 	xprt_complete_rqst(req->rq_task, svsk->sk_reclen);
 	rqstp->rq_arg.len = 0;
+	spin_unlock_bh(&bc_xprt->transport_lock);
 	return 0;
+unlock_notfound:
+	printk(KERN_NOTICE
+		"%s: Got unrecognized reply: "
+		"calldir 0x%x xpt_bc_xprt %p xid %08x\n",
+		__func__, ntohl(calldir),
+		bc_xprt, ntohl(xid));
+unlock_eagain:
+	spin_unlock_bh(&bc_xprt->transport_lock);
+	return -EAGAIN;
 }
 
 static int copy_pages_to_kvecs(struct kvec *vec, struct page **pages, int len)
diff --git a/net/wireless/nl80211.c b/net/wireless/nl80211.c
index be8244d..1bab426 100644
--- a/net/wireless/nl80211.c
+++ b/net/wireless/nl80211.c
@@ -1957,6 +1957,9 @@ static int nl80211_get_key(struct sk_buff *skb, struct genl_info *info)
 	if (!rdev->ops->get_key)
 		return -EOPNOTSUPP;
 
+	if (!pairwise && mac_addr && !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
+		return -ENOENT;
+
 	msg = nlmsg_new(NLMSG_DEFAULT_SIZE, GFP_KERNEL);
 	if (!msg)
 		return -ENOMEM;
@@ -1974,10 +1977,6 @@ static int nl80211_get_key(struct sk_buff *skb, struct genl_info *info)
 	if (mac_addr)
 		NLA_PUT(msg, NL80211_ATTR_MAC, ETH_ALEN, mac_addr);
 
-	if (pairwise && mac_addr &&
-	    !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
-		return -ENOENT;
-
 	err = rdev->ops->get_key(&rdev->wiphy, dev, key_idx, pairwise,
 				 mac_addr, &cookie, get_key_callback);
 
@@ -2149,7 +2148,7 @@ static int nl80211_del_key(struct sk_buff *skb, struct genl_info *info)
 	wdev_lock(dev->ieee80211_ptr);
 	err = nl80211_key_allowed(dev->ieee80211_ptr);
 
-	if (key.type == NL80211_KEYTYPE_PAIRWISE && mac_addr &&
+	if (key.type == NL80211_KEYTYPE_GROUP && mac_addr &&
 	    !(rdev->wiphy.flags & WIPHY_FLAG_IBSS_RSN))
 		err = -ENOENT;
 
diff --git a/scripts/recordmcount.pl b/scripts/recordmcount.pl
index 858966a..679218b 100755
--- a/scripts/recordmcount.pl
+++ b/scripts/recordmcount.pl
@@ -262,7 +262,6 @@ sub check_objcopy
     # force flags for this arch
     $ld .= " -m shlelf_linux";
     $objcopy .= " -O elf32-sh-linux";
-    $cc .= " -m32";
 
 } elsif ($arch eq "powerpc") {
     $local_regex = "^[0-9a-fA-F]+\\s+t\\s+(\\.?\\S+)";
diff --git a/security/keys/encrypted-keys/encrypted.c b/security/keys/encrypted-keys/encrypted.c
index 2d1bb8a..a02f923 100644
--- a/security/keys/encrypted-keys/encrypted.c
+++ b/security/keys/encrypted-keys/encrypted.c
@@ -1016,10 +1016,13 @@ static int __init init_encrypted(void)
 	ret = encrypted_shash_alloc();
 	if (ret < 0)
 		return ret;
+	ret = aes_get_sizes();
+	if (ret < 0)
+		goto out;
 	ret = register_key_type(&key_type_encrypted);
 	if (ret < 0)
 		goto out;
-	return aes_get_sizes();
+	return 0;
 out:
 	encrypted_shash_release();
 	return ret;
diff --git a/sound/core/seq/seq_dummy.c b/sound/core/seq/seq_dummy.c
index dbc5507..f60d814 100644
--- a/sound/core/seq/seq_dummy.c
+++ b/sound/core/seq/seq_dummy.c
@@ -82,36 +82,6 @@ struct snd_seq_dummy_port {
 static int my_client = -1;
 
 /*
- * unuse callback - send ALL_SOUNDS_OFF and RESET_CONTROLLERS events
- * to subscribers.
- * Note: this callback is called only after all subscribers are removed.
- */
-static int
-dummy_unuse(void *private_data, struct snd_seq_port_subscribe *info)
-{
-	struct snd_seq_dummy_port *p;
-	int i;
-	struct snd_seq_event ev;
-
-	p = private_data;
-	memset(&ev, 0, sizeof(ev));
-	if (p->duplex)
-		ev.source.port = p->connect;
-	else
-		ev.source.port = p->port;
-	ev.dest.client = SNDRV_SEQ_ADDRESS_SUBSCRIBERS;
-	ev.type = SNDRV_SEQ_EVENT_CONTROLLER;
-	for (i = 0; i < 16; i++) {
-		ev.data.control.channel = i;
-		ev.data.control.param = MIDI_CTL_ALL_SOUNDS_OFF;
-		snd_seq_kernel_client_dispatch(p->client, &ev, 0, 0);
-		ev.data.control.param = MIDI_CTL_RESET_CONTROLLERS;
-		snd_seq_kernel_client_dispatch(p->client, &ev, 0, 0);
-	}
-	return 0;
-}
-
-/*
  * event input callback - just redirect events to subscribers
  */
 static int
@@ -175,7 +145,6 @@ create_port(int idx, int type)
 		| SNDRV_SEQ_PORT_TYPE_PORT;
 	memset(&pcb, 0, sizeof(pcb));
 	pcb.owner = THIS_MODULE;
-	pcb.unuse = dummy_unuse;
 	pcb.event_input = dummy_input;
 	pcb.private_free = dummy_free;
 	pcb.private_data = rec;
diff --git a/sound/i2c/other/ak4113.c b/sound/i2c/other/ak4113.c
index dde5c9c..e1ab3ad 100644
--- a/sound/i2c/other/ak4113.c
+++ b/sound/i2c/other/ak4113.c
@@ -56,8 +56,7 @@ static inline unsigned char reg_read(struct ak4113 *ak4113, unsigned char reg)
 
 static void snd_ak4113_free(struct ak4113 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -89,6 +88,7 @@ int snd_ak4113_create(struct snd_card *card, ak4113_read_t *read,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4113_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < AK4113_WRITABLE_REGS ; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -139,13 +139,11 @@ static void ak4113_init_regs(struct ak4113 *chip)
 
 void snd_ak4113_reinit(struct ak4113 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work_sync(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4113_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 EXPORT_SYMBOL_GPL(snd_ak4113_reinit);
@@ -632,8 +630,9 @@ static void ak4113_stats(struct work_struct *work)
 {
 	struct ak4113 *chip = container_of(work, struct ak4113, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4113_check_rate_and_errors(chip, chip->check_flags);
 
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
diff --git a/sound/i2c/other/ak4114.c b/sound/i2c/other/ak4114.c
index fdf3c1b..4c6b379 100644
--- a/sound/i2c/other/ak4114.c
+++ b/sound/i2c/other/ak4114.c
@@ -66,8 +66,7 @@ static void reg_dump(struct ak4114 *ak4114)
 
 static void snd_ak4114_free(struct ak4114 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -100,6 +99,7 @@ int snd_ak4114_create(struct snd_card *card,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4114_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < 7; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -152,13 +152,11 @@ static void ak4114_init_regs(struct ak4114 *chip)
 
 void snd_ak4114_reinit(struct ak4114 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work_sync(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4114_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
@@ -612,10 +610,10 @@ static void ak4114_stats(struct work_struct *work)
 {
 	struct ak4114 *chip = container_of(work, struct ak4114, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4114_check_rate_and_errors(chip, chip->check_flags);
-
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
 EXPORT_SYMBOL(snd_ak4114_create);
diff --git a/sound/pci/hda/hda_intel.c b/sound/pci/hda/hda_intel.c
index 33e538f..f461737 100644
--- a/sound/pci/hda/hda_intel.c
+++ b/sound/pci/hda/hda_intel.c
@@ -2685,6 +2685,7 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	struct azx *chip;
 	int i, err;
 	unsigned short gcap;
+	unsigned int dma_bits = 64;
 	static struct snd_device_ops ops = {
 		.dev_free = azx_dev_free,
 	};
@@ -2780,9 +2781,14 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	gcap = azx_readw(chip, GCAP);
 	snd_printdd(SFX "chipset global capabilities = 0x%x\n", gcap);
 
+	/* AMD devices support 40 or 48bit DMA, take the safe one */
+	if (chip->pci->vendor == PCI_VENDOR_ID_AMD)
+		dma_bits = 40;
+
 	/* disable SB600 64bit support for safety */
 	if (chip->pci->vendor == PCI_VENDOR_ID_ATI) {
 		struct pci_dev *p_smbus;
+		dma_bits = 40;
 		p_smbus = pci_get_device(PCI_VENDOR_ID_ATI,
 					 PCI_DEVICE_ID_ATI_SBX00_SMBUS,
 					 NULL);
@@ -2812,9 +2818,11 @@ static int __devinit azx_create(struct snd_card *card, struct pci_dev *pci,
 	}
 
 	/* allow 64bit DMA address if supported by H/W */
-	if ((gcap & ICH6_GCAP_64OK) && !pci_set_dma_mask(pci, DMA_BIT_MASK(64)))
-		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(64));
-	else {
+	if (!(gcap & ICH6_GCAP_64OK))
+		dma_bits = 32;
+	if (!pci_set_dma_mask(pci, DMA_BIT_MASK(dma_bits))) {
+		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(dma_bits));
+	} else {
 		pci_set_dma_mask(pci, DMA_BIT_MASK(32));
 		pci_set_consistent_dma_mask(pci, DMA_BIT_MASK(32));
 	}
diff --git a/sound/pci/hda/patch_sigmatel.c b/sound/pci/hda/patch_sigmatel.c
index 137b67f..606f87a 100644
--- a/sound/pci/hda/patch_sigmatel.c
+++ b/sound/pci/hda/patch_sigmatel.c
@@ -4246,9 +4246,9 @@ static void stac_store_hints(struct hda_codec *codec)
 			spec->gpio_mask;
 	}
 	if (get_int_hint(codec, "gpio_dir", &spec->gpio_dir))
-		spec->gpio_mask &= spec->gpio_mask;
-	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
 		spec->gpio_dir &= spec->gpio_mask;
+	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
+		spec->gpio_data &= spec->gpio_mask;
 	if (get_int_hint(codec, "eapd_mask", &spec->eapd_mask))
 		spec->eapd_mask &= spec->gpio_mask;
 	if (get_int_hint(codec, "gpio_mute", &spec->gpio_mute))
diff --git a/sound/soc/atmel/atmel_ssc_dai.c b/sound/soc/atmel/atmel_ssc_dai.c
index 354341e..8d7d29c 100644
--- a/sound/soc/atmel/atmel_ssc_dai.c
+++ b/sound/soc/atmel/atmel_ssc_dai.c
@@ -341,7 +341,6 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 	struct atmel_pcm_dma_params *dma_params;
 	int dir, channels, bits;
 	u32 tfmr, rfmr, tcmr, rcmr;
-	int start_event;
 	int ret;
 
 	/*
@@ -460,19 +459,10 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		 * The SSC transmit clock is obtained from the BCLK signal on
 		 * on the TK line, and the SSC receive clock is
 		 * generated from the transmit clock.
-		 *
-		 *  For single channel data, one sample is transferred
-		 * on the falling edge of the LRC clock.
-		 * For two channel data, one sample is
-		 * transferred on both edges of the LRC clock.
 		 */
-		start_event = ((channels == 1)
-				? SSC_START_FALLING_RF
-				: SSC_START_EDGE_RF);
-
 		rcmr =	  SSC_BF(RCMR_PERIOD, 0)
 			| SSC_BF(RCMR_STTDLY, START_DELAY)
-			| SSC_BF(RCMR_START, start_event)
+			| SSC_BF(RCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(RCMR_CKI, SSC_CKI_RISING)
 			| SSC_BF(RCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(RCMR_CKS, SSC_CKS_CLOCK);
@@ -480,14 +470,14 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		rfmr =	  SSC_BF(RFMR_FSEDGE, SSC_FSEDGE_POSITIVE)
 			| SSC_BF(RFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(RFMR_FSLEN, 0)
-			| SSC_BF(RFMR_DATNB, 0)
+			| SSC_BF(RFMR_DATNB, (channels - 1))
 			| SSC_BIT(RFMR_MSBF)
 			| SSC_BF(RFMR_LOOP, 0)
 			| SSC_BF(RFMR_DATLEN, (bits - 1));
 
 		tcmr =	  SSC_BF(TCMR_PERIOD, 0)
 			| SSC_BF(TCMR_STTDLY, START_DELAY)
-			| SSC_BF(TCMR_START, start_event)
+			| SSC_BF(TCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(TCMR_CKI, SSC_CKI_FALLING)
 			| SSC_BF(TCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(TCMR_CKS, SSC_CKS_PIN);
@@ -496,7 +486,7 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 			| SSC_BF(TFMR_FSDEN, 0)
 			| SSC_BF(TFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(TFMR_FSLEN, 0)
-			| SSC_BF(TFMR_DATNB, 0)
+			| SSC_BF(TFMR_DATNB, (channels - 1))
 			| SSC_BIT(TFMR_MSBF)
 			| SSC_BF(TFMR_DATDEF, 0)
 			| SSC_BF(TFMR_DATLEN, (bits - 1));
diff --git a/sound/soc/codecs/sgtl5000.c b/sound/soc/codecs/sgtl5000.c
index c40b7ca..87cbf14 100644
--- a/sound/soc/codecs/sgtl5000.c
+++ b/sound/soc/codecs/sgtl5000.c
@@ -1238,6 +1238,9 @@ static int sgtl5000_enable_regulators(struct snd_soc_codec *codec)
 	/* wait for all power rails bring up */
 	udelay(10);
 
+	/* Need 8 clocks before I2C accesses */
+	udelay(1);
+
 	/* read chip information */
 	reg = snd_soc_read(codec, SGTL5000_CHIP_ID);
 	if (((reg & SGTL5000_PARTID_MASK) >> SGTL5000_PARTID_SHIFT) !=
diff --git a/sound/soc/codecs/sigmadsp.c b/sound/soc/codecs/sigmadsp.c
index 4068f24..bb3878c 100644
--- a/sound/soc/codecs/sigmadsp.c
+++ b/sound/soc/codecs/sigmadsp.c
@@ -176,6 +176,13 @@ static int _process_sigma_firmware(struct device *dev,
 		goto done;
 	}
 
+	if (ssfw_head->version != 1) {
+		dev_err(dev,
+			"Failed to load firmware: Invalid version %d. Supported firmware versions: 1\n",
+			ssfw_head->version);
+		goto done;
+	}
+
 	crc = crc32(0, fw->data + sizeof(*ssfw_head),
 			fw->size - sizeof(*ssfw_head));
 	pr_debug("%s: crc=%x\n", __func__, crc);
diff --git a/sound/soc/codecs/wm8960.c b/sound/soc/codecs/wm8960.c
index ddb0d90..a09d7eb 100644
--- a/sound/soc/codecs/wm8960.c
+++ b/sound/soc/codecs/wm8960.c
@@ -496,7 +496,7 @@ static struct {
 	{ 22050, 2 },
 	{ 24000, 2 },
 	{ 16000, 3 },
-	{ 11250, 4 },
+	{ 11025, 4 },
 	{ 12000, 4 },
 	{  8000, 5 },
 };
diff --git a/sound/usb/midi.c b/sound/usb/midi.c
index 2778815..c6ded49 100644
--- a/sound/usb/midi.c
+++ b/sound/usb/midi.c
@@ -365,6 +365,8 @@ static void snd_usbmidi_error_timer(unsigned long data)
 		if (in && in->error_resubmit) {
 			in->error_resubmit = 0;
 			for (j = 0; j < INPUT_URBS; ++j) {
+				if (atomic_read(&in->urbs[j]->use_count))
+					continue;
 				in->urbs[j]->dev = umidi->dev;
 				snd_usbmidi_submit_urb(in->urbs[j], GFP_ATOMIC);
 			}
diff --git a/sound/usb/mixer.c b/sound/usb/mixer.c
index 42d34c3..c44f605 100644
--- a/sound/usb/mixer.c
+++ b/sound/usb/mixer.c
@@ -909,6 +909,7 @@ static void volume_control_quirks(struct usb_mixer_elem_info *cval,
 	case USB_ID(0x046d, 0x0807): /* Logitech Webcam C500 */
 	case USB_ID(0x046d, 0x0808):
 	case USB_ID(0x046d, 0x0809):
+	case USB_ID(0x046d, 0x0819): /* Logitech Webcam C210 */
 	case USB_ID(0x046d, 0x081d): /* HD Webcam c510 */
 	case USB_ID(0x046d, 0x0991):
 	/* Most audio usb devices lie about volume resolution.
diff --git a/sound/usb/mixer_maps.c b/sound/usb/mixer_maps.c
index d1d72ff..621bc9e 100644
--- a/sound/usb/mixer_maps.c
+++ b/sound/usb/mixer_maps.c
@@ -328,8 +328,11 @@ static struct usbmix_name_map gamecom780_map[] = {
 	{}
 };
 
-static const struct usbmix_name_map kef_x300a_map[] = {
-	{ 10, NULL }, /* firmware locks up (?) when we try to access this FU */
+/* some (all?) SCMS USB3318 devices are affected by a firmware lock up
+ * when anything attempts to access FU 10 (control)
+ */
+static const struct usbmix_name_map scms_usb3318_map[] = {
+	{ 10, NULL },
 	{ 0 }
 };
 
@@ -425,8 +428,14 @@ static struct usbmix_ctl_map usbmix_ctl_maps[] = {
 		.map = ebox44_map,
 	},
 	{
+		/* KEF X300A */
 		.id = USB_ID(0x27ac, 0x1000),
-		.map = kef_x300a_map,
+		.map = scms_usb3318_map,
+	},
+	{
+		/* Arcam rPAC */
+		.id = USB_ID(0x25c4, 0x0003),
+		.map = scms_usb3318_map,
 	},
 	{ 0 } /* terminator */
 };
