From 87a5b2ff5c53d13f937bdcb20ab462e4aaa61e3b Mon Sep 17 00:00:00 2001
From: Tad <tad@spotco.us>
Date: Fri, 18 Nov 2016 12:38:14 -0500
Subject: [PATCH] Enable overclock by default

Change-Id: Idc640d7f58271892ae91678de847d9d1fcc4b281
---
 drivers/cpufreq/qcom-cpufreq.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/cpufreq/qcom-cpufreq.c b/drivers/cpufreq/qcom-cpufreq.c
index dd3a589..4cc8680 100644
--- a/drivers/cpufreq/qcom-cpufreq.c
+++ b/drivers/cpufreq/qcom-cpufreq.c
@@ -31,7 +31,7 @@
 
 static DEFINE_MUTEX(l2bw_lock);
 
-static unsigned long arg_cpu_max_a53 = 1440000;
+static unsigned long arg_cpu_max_a53 = 1632000;
 
 static int __init cpufreq_read_cpu_max_a53(char *cpu_max_a53)
 {
@@ -48,7 +48,7 @@ static int __init cpufreq_read_cpu_max_a53(char *cpu_max_a53)
 }
 __setup("cpu_max_a53=", cpufreq_read_cpu_max_a53);
 
-static unsigned long arg_cpu_max_a57 = 1824000;
+static unsigned long arg_cpu_max_a57 = 2016000;
 
 static int __init cpufreq_read_cpu_max_a57(char *cpu_max_a57)
 {
-- 
2.9.3

