From b75779de1c7fd9f624d0523a8ff9020b91f918ed Mon Sep 17 00:00:00 2001
From: Tad <tad@spotco.us>
Date: Thu, 12 Apr 2018 08:05:32 -0400
Subject: [PATCH] Fix -user builds for many LGE devices

Change-Id: I3649cf211a356c57e129fbda1f5184a4bebc85af
---
 public/domain.te | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/public/domain.te b/public/domain.te
index 8640baaa..4b5b0bc6 100644
--- a/public/domain.te
+++ b/public/domain.te
@@ -486,6 +486,9 @@ neverallow { domain -recovery -update_engine } system_block_device:blk_file writ
 # No domains other than install_recovery or recovery can write to recovery.
 neverallow { domain -install_recovery -recovery } recovery_block_device:blk_file write;
 
+# Select devices have policies prevented by the following neverallow
+attribute misc_block_device_exception;
+
 # No domains other than a select few can access the misc_block_device. This
 # block device is reserved for OTA use.
 # Do not assert this rule on userdebug/eng builds, due to some devices using
@@ -500,6 +503,7 @@ neverallow {
   -vold
   -recovery
   -ueventd
+  -misc_block_device_exception
 } misc_block_device:blk_file { append link relabelfrom rename write open read ioctl lock };
 
 # Only (hw|vnd|)servicemanager should be able to register with binder as the context manager
-- 
2.17.0

